(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 123.5 98.5 136.500001 111.500001)
    (thickness 1.6)
    (drawings 2)
    (tracks 0)
    (zones 0)
    (modules 2)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(U1-Pad1)")
  (net 4 "Net-(U1-Pad2)")
  (net 5 "Net-(U1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 574F49E8)
    (at 128.7 107.6)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference "" (at -3.3 -1.1) (layer F.SilkS))
    (fp_text value "" (at 3 2.6) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connect:PINHEAD1-3 (layer F.Cu) (tedit 574F49DE)
    (at 130 103.7)
    (attr virtual)
    (fp_text reference "" (at -4.8 -2.45) (layer F.SilkS))
    (fp_text value "" (at 1.4 -3.9) (layer F.Fab))
    (pad 1 thru_hole oval (at -2.54 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at 0 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad3)"))
  )
  (gr_text "626-90000\nRev P2" (at 130 100.8) (layer B.SilkS))
  (gr_circle (center 130 105) (end 136.35 105) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.5 111.5) (xy 123.5 111.5) (xy 123.5 98.5) (xy 136.5 98.5) (xy 136.5 111.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.5 111.5) (xy 123.5 111.5) (xy 123.5 98.5) (xy 136.5 98.5) (xy 136.5 111.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.5 101.5) (xy 127 101.5) (xy 127 100) (xy 133.5 100) (xy 133.5 101.5)
      )
    )
  )
)
