(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 118)
    (zones 0)
    (modules 8)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 LED_IN)
  (net 3 "Net-(D1-Pad2)")
  (net 4 5V)
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 LED_OUT)
  (net 8 M1)
  (net 9 M2)
  (net 10 M3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5V)
    (add_net GND)
    (add_net LED_IN)
    (add_net LED_OUT)
    (add_net M1)
    (add_net M2)
    (add_net M3)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
  )
  (module LED_Racewire:house_fpv_logo_10mm_10mm (layer B.Cu) (tedit 5F64E60A)
    (at 82.6 38.7)
    (fp_text reference G*** (at 4 4) (layer Cmts.User) hide)
    (fp_text value LOGO (at 10 4) (layer B.SilkS) hide)
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 75.3 38.7 270)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D1 (at 0 -3.5 90) (layer Cmts.User) hide)
    (fp_text value WS2812B (at 0 4 90) (layer Cmts.User) hide)
    (fp_text user 1 (at -4.15 -1.6 90) (layer Cmts.User) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 2.45 1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.45 -1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 LED_IN))
    (pad 2 smd rect (at -2.45 1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2.45 -1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 80.8 38.7 270)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D2 (at 0 -3.5 90) (layer Cmts.User) hide)
    (fp_text value WS2812B (at 0 4 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -2.45 -1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 5V))
    (pad 2 smd rect (at -2.45 1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 86.3 38.7 270)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D3 (at 0 -3.5 90) (layer Cmts.User) hide)
    (fp_text value WS2812B (at 0 4 90) (layer F.Fab) hide)
    (fp_text user 1 (at -4.15 -1.6 90) (layer Cmts.User) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 2.45 1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.45 -1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at -2.45 1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -2.45 -1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 91.8 38.7 270)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D4 (at 0 -3.5 90) (layer Cmts.User) hide)
    (fp_text value WS2812B (at 0 4 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -2.45 -1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 5V))
    (pad 2 smd rect (at -2.45 1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 7 LED_OUT))
    (pad 4 smd rect (at 2.45 -1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_Racewire:LED_PINS (layer F.Cu) (tedit 5F64CB41)
    (at 67.3 34.7)
    (fp_text reference J2 (at 2 9) (layer Cmts.User) hide)
    (fp_text value Conn_01x04_Male (at -1 4 90) (layer Cmts.User) hide)
    (pad 1 smd circle (at 4 1) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 5V))
    (pad 2 smd circle (at 4 3) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 4 7) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 LED_OUT))
    (pad 3 smd circle (at 4 5) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 LED_IN))
  )
  (module LED_Racewire:Racewire_3w_2mm (layer F.Cu) (tedit 5F64CF0F)
    (at 67.3 34.7)
    (fp_text reference J1 (at 2 9) (layer Cmts.User) hide)
    (fp_text value Conn_01x03_Male (at -1 4 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at 1 1) (size 2.7 2.7) (layers F.Cu F.Paste F.Mask)
      (net 8 M1))
    (pad 2 smd rect (at 1 4) (size 2.7 2.7) (layers F.Cu F.Paste F.Mask)
      (net 9 M2))
    (pad 3 smd rect (at 1 7) (size 2.7 2.7) (layers F.Cu F.Paste F.Mask)
      (net 10 M3))
  )
  (module LED_Racewire:Racewire_3w_2mm (layer F.Cu) (tedit 5F64CF0F)
    (at 95.4 34.7)
    (fp_text reference J3 (at 2 9) (layer Cmts.User) hide)
    (fp_text value Conn_01x03_Male (at -1 4 90) (layer Cmts.User) hide)
    (pad 3 smd rect (at 1 7) (size 2.7 2.7) (layers F.Cu F.Paste F.Mask)
      (net 10 M3))
    (pad 2 smd rect (at 1 4) (size 2.7 2.7) (layers F.Cu F.Paste F.Mask)
      (net 9 M2))
    (pad 1 smd rect (at 1 1) (size 2.7 2.7) (layers F.Cu F.Paste F.Mask)
      (net 8 M1))
  )
  (gr_text FPV (at 87.9 36.9 90) (layer B.SilkS))
  (gr_text House (at 77.5 38.1 90) (layer B.SilkS))
  (gr_text R1.0 (at 94.3 41.7 90) (layer B.SilkS))
  (dimension 31.3 (width 0.12) (layer F.Fab)
    (gr_text "31.300 mm" (at 82.35 31.83) (layer F.Fab))
    (feature1 (pts (xy 98 34.1) (xy 98 32.513579)))
    (feature2 (pts (xy 66.7 34.1) (xy 66.7 32.513579)))
    (crossbar (pts (xy 66.7 33.1) (xy 98 33.1)))
    (arrow1a (pts (xy 98 33.1) (xy 96.873496 33.686421)))
    (arrow1b (pts (xy 98 33.1) (xy 96.873496 32.513579)))
    (arrow2a (pts (xy 66.7 33.1) (xy 67.826504 33.686421)))
    (arrow2b (pts (xy 66.7 33.1) (xy 67.826504 32.513579)))
  )
  (dimension 9.2 (width 0.12) (layer F.Fab)
    (gr_text "9.200 mm" (at 63.13 38.7 90) (layer F.Fab))
    (feature1 (pts (xy 66.7 34.1) (xy 63.813579 34.1)))
    (feature2 (pts (xy 66.7 43.3) (xy 63.813579 43.3)))
    (crossbar (pts (xy 64.4 43.3) (xy 64.4 34.1)))
    (arrow1a (pts (xy 64.4 34.1) (xy 64.986421 35.226504)))
    (arrow1b (pts (xy 64.4 34.1) (xy 63.813579 35.226504)))
    (arrow2a (pts (xy 64.4 43.3) (xy 64.986421 42.173496)))
    (arrow2b (pts (xy 64.4 43.3) (xy 63.813579 42.173496)))
  )
  (gr_text I (at 70.1 39.7) (layer F.SilkS))
  (gr_text O (at 70.1 41.8) (layer F.SilkS))
  (gr_text G (at 70.1 37.7) (layer F.SilkS))
  (gr_text 5 (at 70.1 35.7) (layer F.SilkS))
  (gr_line (start 66.7 43.3) (end 66.7 34.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98 43.3) (end 66.7 43.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98 34.1) (end 98 43.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.7 34.1) (end 98 34.1) (layer Edge.Cuts) (width 0.05))
  (zone (net 10) (net_name M3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 40.4) (xy 67 43) (xy 97.7 43) (xy 97.7 40.4)
      )
    )
  )
  (zone (net 9) (net_name M2) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.7 40) (xy 97.7 37.4) (xy 67 37.4) (xy 67 40)
      )
    )
  )
  (zone (net 8) (net_name M1) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 34.4) (xy 67 37) (xy 97.6 37) (xy 97.7 37) (xy 97.7 34.4)
      )
    )
  )
  (zone (net 8) (net_name M1) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 34.4) (xy 67 37) (xy 97.6 37) (xy 97.7 37) (xy 97.7 34.4)
      )
    )
  )
  (zone (net 8) (net_name M1) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 34.4) (xy 67 37) (xy 97.6 37) (xy 97.7 37) (xy 97.7 34.4)
      )
    )
  )
  (zone (net 9) (net_name M2) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.7 40) (xy 97.7 37.4) (xy 67 37.4) (xy 67 40)
      )
    )
  )
  (zone (net 9) (net_name M2) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.7 40) (xy 97.7 37.4) (xy 67 37.4) (xy 67 40)
      )
    )
  )
  (zone (net 10) (net_name M3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 40.4) (xy 67 43) (xy 97.7 43) (xy 97.7 40.4)
      )
    )
  )
  (zone (net 10) (net_name M3) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 40.4) (xy 67 43) (xy 97.7 43) (xy 97.7 40.4)
      )
    )
  )
)
