<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="-2.54" y1="-2.54" x2="38.1" y2="-2.54" width="0.2032" layer="20"/>
<wire x1="38.1" y1="-2.54" x2="38.1" y2="45.72" width="0.2032" layer="20"/>
<wire x1="38.1" y1="45.72" x2="-2.54" y2="45.72" width="0.2032" layer="20"/>
<wire x1="-2.54" y1="45.72" x2="-2.54" y2="-2.54" width="0.2032" layer="20"/>
<text>Load on</text>
<text>5V USB</text>
<text>Status</text>
<text>GND</text>
<text>MonkeyTurk
Feather M0 Shield
mil @ DiCarlo Lab </text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X12_LOCK">
<description>&lt;h3&gt;Plated Through Hole -12 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X16_LOCK">
<description>&lt;h3&gt;Plated Through Hole -16 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_16&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_SLOT">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector PTH Slot Pads&lt;/h3&gt;
Extended soldering pads. 
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Barrel-Connector-PJ-202A.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO5">
<description>&lt;b&gt;TO 5&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="M9040P">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Marquardt</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_3MM">
<description>&lt;h3&gt;LED 3MM PTH&lt;/h3&gt;

3 mm, round.

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="SparkFun-Connectors" package="1X12_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X16_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_SLOT" value="POWER_JACKSLT">
<attribute name="PROD_ID" value="PRT-00119"/>
</element>
<element name="Q1" library="transistor-npn" package="TO5" value="2N1893">
<attribute name="POPULARITY" value="0"/>
</element>
<element name="S1" library="switch" package="M9040P" value="">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO41-10" value="1N4004">
<attribute name="POPULARITY" value="82"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED_3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08306"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED_3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="RST">
<contactref element="J3" pad="16"/>
</signal>
<signal name="3V">
<contactref element="J3" pad="15"/>
</signal>
<signal name="ARF">
<contactref element="J3" pad="14"/>
</signal>
<signal name="GND">
<contactref element="J3" pad="13"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="GND@2"/>
<contactref element="J1" pad="GND@1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="A0">
<contactref element="J3" pad="12"/>
</signal>
<signal name="A1">
<contactref element="J3" pad="11"/>
</signal>
<signal name="A2">
<contactref element="J3" pad="10"/>
</signal>
<signal name="A3">
<contactref element="J3" pad="9"/>
</signal>
<signal name="A4">
<contactref element="J3" pad="8"/>
</signal>
<signal name="A5">
<contactref element="J3" pad="7"/>
</signal>
<signal name="SCK">
<contactref element="J3" pad="6"/>
</signal>
<signal name="MOSI">
<contactref element="J3" pad="5"/>
</signal>
<signal name="MISO">
<contactref element="J3" pad="4"/>
</signal>
<signal name="0RX">
<contactref element="J3" pad="3"/>
</signal>
<signal name="1TX">
<contactref element="J3" pad="2"/>
</signal>
<signal name="DFU">
<contactref element="J3" pad="1"/>
</signal>
<signal name="BAT">
<contactref element="J2" pad="12"/>
</signal>
<signal name="EN">
<contactref element="J2" pad="11"/>
</signal>
<signal name="USB">
<contactref element="J2" pad="10"/>
<contactref element="Q1" pad="3"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="12">
<contactref element="J2" pad="8"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="11">
<contactref element="J2" pad="7"/>
</signal>
<signal name="10">
<contactref element="J2" pad="6"/>
</signal>
<signal name="9">
<contactref element="J2" pad="5"/>
</signal>
<signal name="6">
<contactref element="J2" pad="4"/>
</signal>
<signal name="5">
<contactref element="J2" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="J2" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="J2" pad="1"/>
</signal>
<signal name="13">
<contactref element="J2" pad="9"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="S1" pad="3"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="D3" pad="K"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="K"/>
<contactref element="J1" pad="PWR"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
