(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 74)
    (zones 0)
    (modules 20)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.408)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.6576 2.032)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 2.000000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 12V)
  (net 3 5V)
  (net 4 LATCH_OUT)
  (net 5 24_32_SWITCH)
  (net 6 READER_LED)
  (net 7 READER_BUZZ)
  (net 8 DOOR)
  (net 9 WIEGAND_IN2)
  (net 10 WIEGAND_IN1)
  (net 11 "Net-(D1-Pad1)")
  (net 12 "Net-(D2-Pad1)")
  (net 13 "Net-(D4-Pad1)")
  (net 14 WIEGAND_OUT2)
  (net 15 WIEGAND_OUT1)
  (net 16 "Net-(J4-Pad12)")
  (net 17 "Net-(J4-Pad11)")
  (net 18 "Net-(J4-Pad10)")
  (net 19 "Net-(J4-Pad9)")
  (net 20 "Net-(J4-Pad8)")
  (net 21 "Net-(J4-Pad7)")
  (net 22 "Net-(J4-Pad3)")
  (net 23 "Net-(J4-Pad2)")
  (net 24 "Net-(J4-Pad1)")
  (net 25 "Net-(J5-Pad3)")
  (net 26 "Net-(J5-Pad4)")
  (net 27 "Net-(J5-Pad5)")
  (net 28 "Net-(J5-Pad6)")
  (net 29 "Net-(J5-Pad7)")
  (net 30 "Net-(J5-Pad8)")
  (net 31 "Net-(J5-Pad9)")
  (net 32 "Net-(J5-Pad10)")
  (net 33 "Net-(J5-Pad11)")
  (net 34 "Net-(J5-Pad12)")
  (net 35 "Net-(J5-Pad13)")
  (net 36 "Net-(J5-Pad15)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net 12V)
    (add_net 24_32_SWITCH)
    (add_net 5V)
    (add_net DOOR)
    (add_net GND)
    (add_net LATCH_OUT)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad10)")
    (add_net "Net-(J4-Pad11)")
    (add_net "Net-(J4-Pad12)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J4-Pad9)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad11)")
    (add_net "Net-(J5-Pad12)")
    (add_net "Net-(J5-Pad13)")
    (add_net "Net-(J5-Pad15)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J5-Pad9)")
    (add_net READER_BUZZ)
    (add_net READER_LED)
    (add_net WIEGAND_IN1)
    (add_net WIEGAND_IN2)
    (add_net WIEGAND_OUT1)
    (add_net WIEGAND_OUT2)
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD)
    (at 115.85 133.575)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 12V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 6150E14B)
    (at 107.306001 128.597001)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at -3.581001 5.527999) (layer F.SilkS))
    (fp_text value ZXMP4A16G (at 0 0.762) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask)
      (net 4 LATCH_OUT))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 4 LATCH_OUT))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 8 DOOR))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 118.48 116.23 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D4 (at 0 -2 90) (layer F.SilkS))
    (fp_text value LED (at 0 2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 5V))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D4-Pad1)"))
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD)
    (at 120.6 133.575 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -2.074 -2.128) (layer F.SilkS))
    (fp_text value 22uF (at 0 2.3) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 5V))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07 (layer F.Cu) (tedit 0)
    (at 105.664 100.076 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value Conn_01x07_Male (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 24_32_SWITCH))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 READER_LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 READER_BUZZ))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 WIEGAND_IN2))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 WIEGAND_IN1))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 12V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07.wrl
      (offset (xyz 0 -7.619999885559082 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 563007E4)
    (at 103.75 143.256)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J2 (at 2.5 5.9) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 2.5 -6.6) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 4 LATCH_OUT))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 12V))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (offset (xyz 2.499359962463379 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 563007E4)
    (at 117.348 143.256)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J3 (at 2.5 5.9) (layer F.SilkS) hide)
    (fp_text value Barrel_Jack (at 2.5 -6.6) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 12V))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (offset (xyz 2.499359962463379 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 0)
    (at 100 100)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J4 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value WROOM32_1 (at 0 -3.1) (layer F.Fab))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 5V))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 DOOR))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J4-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J4-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J4-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J4-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J4-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J4-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 READER_BUZZ))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 READER_LED))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 24_32_SWITCH))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J4-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (offset (xyz 0 -17.77999973297119 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 0)
    (at 125.4 100)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J5 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value WROOM32_2 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 WIEGAND_OUT2))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 WIEGAND_OUT1))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J5-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J5-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J5-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J5-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J5-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J5-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J5-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J5-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J5-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J5-Pad15)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (offset (xyz 0 -17.77999973297119 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 5415D182)
    (at 112.55 109.15 90)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R1 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 5415D182)
    (at 106.05 109.15 90)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R2 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.7 90) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 5415D182)
    (at 118.48 109.2 90)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R3 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 112.55 116.1 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -2 90) (layer F.SilkS))
    (fp_text value LED (at 0 2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 12V))
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 106.05 116.1 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -2 90) (layer F.SilkS))
    (fp_text value LED (at 0 2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 8 DOOR))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D2-Pad1)"))
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 0)
    (at 109.8 136.3 180)
    (attr smd)
    (fp_text reference D3 (at 0 2) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 12V))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 4 LATCH_OUT))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 5415D182)
    (at 111 104 180)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R4 (at 1.2 -2.4) (layer F.SilkS))
    (fp_text value 1k (at 0 2.7) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 14 WIEGAND_OUT2))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 WIEGAND_IN2))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 5415D182)
    (at 106.2 104 180)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R5 (at 3 -2.4) (layer F.SilkS))
    (fp_text value 2k (at 0 2.7) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 14 WIEGAND_OUT2))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 5415D182)
    (at 116.4 104)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R6 (at -1.4 2.4) (layer F.SilkS))
    (fp_text value 1k (at 0 2.7) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 15 WIEGAND_OUT1))
    (pad 1 smd rect (at -1.45 0) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 WIEGAND_IN1))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 5415D182)
    (at 121 104)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R7 (at -1.8 2.4) (layer F.SilkS))
    (fp_text value 2k (at 0 2.7) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 15 WIEGAND_OUT1))
    (pad 2 smd rect (at 1.45 0) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 0)
    (at 117.75 125.3)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference U1 (at 0 -5.08) (layer F.SilkS))
    (fp_text value L7805 (at 0 3.81) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 12V))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 5V))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 24/32 (at 105.85 105.175 90) (layer B.SilkS))
  (gr_text LED (at 108.35 103.425 90) (layer B.SilkS))
  (gr_text BUZZ (at 110.95 104.2 90) (layer B.SilkS))
  (gr_text W2 (at 113.525 103 90) (layer B.SilkS))
  (gr_text W1 (at 116.075 103.125 90) (layer B.SilkS))
  (gr_text GND (at 118.4 103.7 270) (layer B.SilkS))
  (gr_text +12V (at 121.2 104.4 270) (layer B.SilkS))
  (gr_text "ESP32 Doorbot v5\nBy Timm Murray\nCopyright © 2021\nBY-CC" (at 117.8 110) (layer B.SilkS))
  (gr_line (start 127.25 98) (end 98 98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.25 149.75) (end 127.25 98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98 149.75) (end 127.25 149.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98 98) (end 98 149.75) (layer Edge.Cuts) (width 0.05))
  (gr_text Door (at 99.5 143.25 90) (layer F.SilkS))
  (gr_text 12/24V (at 113 143.25 90) (layer F.SilkS))
  (gr_text GND (at 126.25 143.25 90) (layer F.SilkS))
  (gr_text Door (at 106.4 112.4) (layer F.SilkS))
  (gr_text 12V (at 112.4 112.4) (layer F.SilkS))
  (gr_text 5V (at 118.65 112.65) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.25 149.75) (xy 98 149.75) (xy 98 98) (xy 127.25 98)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.408))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.25 149.75) (xy 98 149.75) (xy 98 98) (xy 127.25 98)
      )
    )
  )
)
