(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 83)
    (tracks 1408)
    (zones 0)
    (modules 112)
    (nets 85)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.082)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.6)
    (via_min_drill 0.2)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FEFFAE7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 EXT_PWR_GROUND)
  (net 2 "Net-(BT101-Pad1)")
  (net 3 +3V3)
  (net 4 "Net-(C103-Pad2)")
  (net 5 /AUDIO_OUT)
  (net 6 Vproc)
  (net 7 /ADC6)
  (net 8 /AUDIO_IN)
  (net 9 /ADC7)
  (net 10 EXT_BATTERY)
  (net 11 "Net-(J101-Pad1)")
  (net 12 /PTT_OUT)
  (net 13 "Net-(J103-Pad1)")
  (net 14 D5)
  (net 15 D4)
  (net 16 D3)
  (net 17 D2)
  (net 18 D1)
  (net 19 D0)
  (net 20 TONE_LOGIC)
  (net 21 CW_KEY_LOGIC)
  (net 22 PTT_LOGIC)
  (net 23 ~RESET~)
  (net 24 RTC_SQW)
  (net 25 PWDN)
  (net 26 "Net-(MOD101-Pad22)")
  (net 27 SCL)
  (net 28 SDA)
  (net 29 "Net-(Q102-Pad3)")
  (net 30 "Net-(R101-Pad2)")
  (net 31 "Net-(R102-Pad1)")
  (net 32 "Net-(U101-Pad4)")
  (net 33 "Net-(U102-Pad13)")
  (net 34 "Net-(U102-Pad16)")
  (net 35 "Net-(U104-Pad3)")
  (net 36 "Net-(U104-Pad4)")
  (net 37 "Net-(J104-Pad3)")
  (net 38 "Net-(J104-Pad4)")
  (net 39 "Net-(J104-Pad5)")
  (net 40 "Net-(J104-Pad6)")
  (net 41 "Net-(J104-Pad7)")
  (net 42 "Net-(J104-Pad8)")
  (net 43 Controlled_Power)
  (net 44 TXD)
  (net 45 VDC)
  (net 46 "Net-(C104-Pad1)")
  (net 47 "Net-(Q101-Pad1)")
  (net 48 RXD)
  (net 49 EXTERNAL_PWR_SOURCE)
  (net 50 /PC0)
  (net 51 /PC1)
  (net 52 /PC2)
  (net 53 /PC3)
  (net 54 /PD1)
  (net 55 "Net-(Q103-Pad1)")
  (net 56 "Net-(Q104-Pad1)")
  (net 57 "Net-(R103-Pad1)")
  (net 58 "Net-(R111-Pad1)")
  (net 59 "Net-(R113-Pad1)")
  (net 60 CW_KEY)
  (net 61 DTR)
  (net 62 /PD3)
  (net 63 "Net-(Q103-Pad3)")
  (net 64 Power_In)
  (net 65 "Net-(J111-Pad4)")
  (net 66 "Net-(J111-Pad3)")
  (net 67 "Net-(J111-Pad2)")
  (net 68 "Net-(J111-Pad1)")
  (net 69 "Net-(J111-Pad5)")
  (net 70 "Net-(J111-Pad6)")
  (net 71 "Net-(J111-Pad7)")
  (net 72 "Net-(J111-Pad8)")
  (net 73 "Net-(J111-Pad9)")
  (net 74 "Net-(D102-Pad2)")
  (net 75 GND1)
  (net 76 "Net-(D101-Pad1)")
  (net 77 /GROUND)
  (net 78 /RADIO_V+)
  (net 79 "Net-(FB103-Pad1)")
  (net 80 "Net-(FB105-Pad1)")
  (net 81 "Net-(FB106-Pad1)")
  (net 82 "Net-(U105-Pad1)")
  (net 83 "Net-(U105-Pad4)")
  (net 84 "Net-(U103-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /ADC6)
    (add_net /ADC7)
    (add_net /AUDIO_IN)
    (add_net /AUDIO_OUT)
    (add_net /GROUND)
    (add_net /PC0)
    (add_net /PC1)
    (add_net /PC2)
    (add_net /PC3)
    (add_net /PD1)
    (add_net /PD3)
    (add_net /PTT_OUT)
    (add_net /RADIO_V+)
    (add_net CW_KEY)
    (add_net CW_KEY_LOGIC)
    (add_net Controlled_Power)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net DTR)
    (add_net EXTERNAL_PWR_SOURCE)
    (add_net EXT_BATTERY)
    (add_net GND1)
    (add_net "Net-(BT101-Pad1)")
    (add_net "Net-(C103-Pad2)")
    (add_net "Net-(C104-Pad1)")
    (add_net "Net-(D101-Pad1)")
    (add_net "Net-(D102-Pad2)")
    (add_net "Net-(FB103-Pad1)")
    (add_net "Net-(FB105-Pad1)")
    (add_net "Net-(FB106-Pad1)")
    (add_net "Net-(J103-Pad1)")
    (add_net "Net-(J104-Pad3)")
    (add_net "Net-(J104-Pad4)")
    (add_net "Net-(J104-Pad5)")
    (add_net "Net-(J104-Pad6)")
    (add_net "Net-(J104-Pad7)")
    (add_net "Net-(J104-Pad8)")
    (add_net "Net-(J111-Pad1)")
    (add_net "Net-(J111-Pad2)")
    (add_net "Net-(J111-Pad3)")
    (add_net "Net-(J111-Pad4)")
    (add_net "Net-(J111-Pad5)")
    (add_net "Net-(J111-Pad6)")
    (add_net "Net-(J111-Pad7)")
    (add_net "Net-(J111-Pad8)")
    (add_net "Net-(J111-Pad9)")
    (add_net "Net-(MOD101-Pad22)")
    (add_net "Net-(Q101-Pad1)")
    (add_net "Net-(Q102-Pad3)")
    (add_net "Net-(Q103-Pad1)")
    (add_net "Net-(Q103-Pad3)")
    (add_net "Net-(Q104-Pad1)")
    (add_net "Net-(R101-Pad2)")
    (add_net "Net-(R102-Pad1)")
    (add_net "Net-(R103-Pad1)")
    (add_net "Net-(R111-Pad1)")
    (add_net "Net-(R113-Pad1)")
    (add_net "Net-(U101-Pad4)")
    (add_net "Net-(U102-Pad13)")
    (add_net "Net-(U102-Pad16)")
    (add_net "Net-(U103-Pad6)")
    (add_net "Net-(U104-Pad3)")
    (add_net "Net-(U104-Pad4)")
    (add_net "Net-(U105-Pad1)")
    (add_net "Net-(U105-Pad4)")
    (add_net PTT_LOGIC)
    (add_net PWDN)
    (add_net Power_In)
    (add_net RTC_SQW)
    (add_net RXD)
    (add_net SCL)
    (add_net SDA)
    (add_net TONE_LOGIC)
    (add_net TXD)
    (add_net VDC)
    (add_net Vproc)
    (add_net ~RESET~)
  )
  (net_class Stripline ""
    (clearance 0.05)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.2)
    (diff_pair_gap 0.3)
    (add_net EXT_PWR_GROUND)
    (add_net "Net-(J101-Pad1)")
  )
  (module Diodes_SMD:DO-219AD (layer F.Cu) (tedit 60958D8A)
    (at 120.93 111.33)
    (descr MicroSMP)
    (tags "DO-219SD diode")
    (attr smd)
    (fp_text reference D108 (at -0.32 -1.79) (layer F.SilkS))
    (fp_text value MSS1P2L-M3/89A (at 0 3) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 2 1.1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C104-Pad1)"))
    (pad 2 smd rect (at 0.9 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 Vproc))
  )
  (module Diodes_SMD:DO-219AD (layer F.Cu) (tedit 60958D57)
    (at 118.24 102.4 90)
    (descr MicroSMP)
    (tags "DO-219SD diode")
    (attr smd)
    (fp_text reference D109 (at 1.57 1.84 90) (layer F.SilkS))
    (fp_text value MSS1P2L-M3/89A (at 0 3 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 2 1.1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C104-Pad1)"))
    (pad 2 smd rect (at 0.9 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT101-Pad1)"))
  )
  (module Diodes_SMD:DO-219AD (layer F.Cu) (tedit 60958B8B)
    (at 125.24 90.4 90)
    (descr MicroSMP)
    (tags "DO-219SD diode")
    (attr smd)
    (fp_text reference D101 (at 0.85 1.99 90) (layer F.SilkS))
    (fp_text value MSS1P2L-M3/89A (at -0.14 4.81 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 2 1.1) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D101-Pad1)"))
    (pad 2 smd rect (at 0.9 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 EXT_BATTERY))
  )
  (module Oddities:RV-3028-C7 (layer F.Cu) (tedit 6095896F)
    (at 121.35 106.99 90)
    (descr "Low Power RTC Module")
    (tags RV-3028-C7)
    (solder_mask_margin 0.06)
    (clearance 0.06)
    (attr smd)
    (fp_text reference U103 (at 0.3 1.84 270) (layer F.SilkS))
    (fp_text value RV-8803-C7 (at 0 -3.048 90) (layer F.Fab))
    (pad 8 smd rect (at -0.9 -0.6 90) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 27 SCL))
    (pad 7 smd rect (at 0 -0.6 90) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R103-Pad1)"))
    (pad 6 smd rect (at 0.9 -0.6 90) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U103-Pad6)"))
    (pad 5 smd rect (at 1.8 -0.6 90) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 1 smd rect (at -0.9 0.6 90) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 SDA))
    (pad 2 smd rect (at 0 0.6 90) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R113-Pad1)"))
    (pad 3 smd rect (at 0.9 0.6 90) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C104-Pad1)"))
    (pad 4 smd rect (at 1.8 0.6 90) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R111-Pad1)"))
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 60958907)
    (at 141.63 112.01)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U102 (at 0.01 6.22) (layer F.SilkS))
    (fp_text value CD74HC4050M96 (at 0 6) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J104-Pad8)"))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 D0))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J104-Pad7)"))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 D1))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J104-Pad6)"))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 D2))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 D3))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J104-Pad5)"))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 D4))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J104-Pad4)"))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U102-Pad13)"))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 D5))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J104-Pad3)"))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U102-Pad16)"))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-20-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 609588AF)
    (at 163.57 108.97 90)
    (descr "20-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U104 (at 0 -3.33 90) (layer F.SilkS))
    (fp_text value F1975NCGI (at 0 3.33 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.965 -1 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(J104-Pad3)") (solder_mask_margin 0.06) (clearance 0.06))
    (pad 2 smd roundrect (at -1.965 -0.5 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(J101-Pad1)") (solder_mask_margin 0.06) (clearance 0.06))
    (pad 3 smd roundrect (at -1.965 0 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(U104-Pad3)") (solder_mask_margin 0.06) (clearance 0.06))
    (pad 4 smd roundrect (at -1.965 0.5 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(U104-Pad4)") (solder_mask_margin 0.06) (clearance 0.06))
    (pad 5 smd roundrect (at -1.965 1 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 VDC) (solder_mask_margin 0.06) (clearance 0.06))
    (pad 6 smd roundrect (at -1 1.965 180) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 VDC) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 7 smd roundrect (at -0.5 1.965 180) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 8 smd roundrect (at 0 1.965 180) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 9 smd roundrect (at 0.5 1.965 180) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 10 smd roundrect (at 1 1.965 180) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 11 smd roundrect (at 1.965 1 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 12 smd roundrect (at 1.965 0.5 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 13 smd roundrect (at 1.965 0 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 14 smd roundrect (at 1.965 -0.5 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(J103-Pad1)") (solder_mask_margin 0.06) (clearance 0.06))
    (pad 15 smd roundrect (at 1.965 -1 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(J104-Pad4)") (solder_mask_margin 0.06) (clearance 0.06))
    (pad 16 smd roundrect (at 1 -1.965 180) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(J104-Pad5)") (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 17 smd roundrect (at 0.5 -1.965 180) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(J104-Pad6)") (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 18 smd roundrect (at 0 -1.965 180) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 19 smd roundrect (at -0.5 -1.965 180) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(J104-Pad7)") (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 20 smd roundrect (at -1 -1.965 180) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(J104-Pad8)") (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 0))
    (pad 21 smd rect (at 0.625 0.625 90) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 75 GND1) (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at 0.625 -0.625 90) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 75 GND1) (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at -0.625 0.625 90) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 75 GND1) (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at -0.625 -0.625 90) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 75 GND1) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SO16 (layer F.Cu) (tedit 609587C3)
    (at 105.02 96.51 270)
    (attr smd)
    (fp_text reference U105 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value DS3231 (at 0.381 -1.905 270) (layer F.Fab))
    (pad 1 smd rect (at -4.495 4.4 270) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U105-Pad1)"))
    (pad 2 smd rect (at -3.175 4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 6 Vproc))
    (pad 3 smd rect (at -1.905 4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 24 RTC_SQW))
    (pad 4 smd rect (at -0.635 4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U105-Pad4)"))
    (pad 5 smd rect (at 0.635 4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 6 smd rect (at 1.905 4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 7 smd rect (at 3.175 4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 8 smd rect (at 4.495 4.4 270) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 9 smd rect (at 4.495 -4.4 270) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 10 smd rect (at 3.175 -4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 11 smd rect (at 1.905 -4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 12 smd rect (at 0.635 -4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 13 smd rect (at -0.635 -4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 14 smd rect (at -1.905 -4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT101-Pad1)"))
    (pad 15 smd rect (at -3.175 -4.4 270) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 28 SDA))
    (pad 16 smd rect (at -4.495 -4.4 270) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 27 SCL))
    (model SMD_Packages.3dshapes/SO-16-L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.6 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Modules:Arduino_Pro_Mini (layer F.Cu) (tedit 60954C7E)
    (at 121.72 94.58)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference MOD101 (at -0.73 1.29) (layer F.SilkS))
    (fp_text value "Arduino Pro Mini (5V Version)" (at -0.225001 -6.865001) (layer F.Fab))
    (fp_text user A7 (at 2.84 19.13) (layer B.SilkS))
    (fp_text user A6 (at 2.79 21.5) (layer B.SilkS))
    (fp_text user SCL (at 2.46 8.99) (layer B.SilkS))
    (fp_text user SDA (at 2.41 11.44) (layer B.SilkS))
    (fp_text user DTR (at 6.36 -4.39) (layer B.SilkS))
    (fp_text user Vcc (at 10.28 7.72) (layer B.SilkS))
    (fp_text user RAW (at 10.61 -0.09) (layer B.SilkS))
    (fp_text user GND (at 10.66 2.41) (layer B.SilkS))
    (fp_text user RST (at 10.56 5.11) (layer B.SilkS))
    (fp_text user A3 (at 9.96 10.3) (layer B.SilkS))
    (fp_text user A2 (at 9.96 12.73) (layer B.SilkS))
    (fp_text user A1 (at 9.85 15.2) (layer B.SilkS))
    (fp_text user A0 (at 9.91 17.79) (layer B.SilkS))
    (fp_text user 13 (at 9.96 20.32) (layer B.SilkS))
    (fp_text user 12 (at 9.96 22.79) (layer B.SilkS))
    (fp_text user 11 (at 9.91 25.32) (layer B.SilkS))
    (fp_text user 10 (at 10.02 27.85) (layer B.SilkS))
    (fp_text user 9 (at -9.58 27.75) (layer B.SilkS))
    (fp_text user 8 (at -9.58 25.27) (layer B.SilkS))
    (fp_text user 7 (at -9.53 22.79) (layer B.SilkS))
    (fp_text user 6 (at -9.53 20.1) (layer B.SilkS))
    (fp_text user 5 (at -9.58 17.73) (layer B.SilkS))
    (fp_text user 4 (at -9.58 15.09) (layer B.SilkS))
    (fp_text user 3 (at -9.58 12.67) (layer B.SilkS))
    (fp_text user 2 (at -9.58 10.2) (layer B.SilkS))
    (fp_text user DTR (at -6.34 -4.29) (layer B.SilkS))
    (fp_text user A6 (at 2.64 26.02 -90) (layer B.SilkS))
    (fp_text user A7 (at 5.01 26.07 -90) (layer B.SilkS))
    (fp_text user GND (at -0.01 25.54 -90) (layer B.SilkS))
    (pad 32 thru_hole oval (at 4.71 19.05) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /ADC7))
    (pad 31 thru_hole oval (at 4.71 21.59) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /ADC6))
    (pad 33 thru_hole oval (at 4.71 11.43) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 SDA))
    (pad 34 thru_hole oval (at 4.71 8.89) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 SCL))
    (pad 13 thru_hole oval (at 7.63 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 D2))
    (pad 14 thru_hole oval (at 7.63 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 D3))
    (pad 12 thru_hole oval (at -7.6249 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 D1))
    (pad 11 thru_hole oval (at -7.6249 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 D0))
    (pad 15 thru_hole oval (at 7.63 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 D4))
    (pad 16 thru_hole oval (at 7.63 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 D5))
    (pad 17 thru_hole oval (at 7.63 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /PC0))
    (pad 18 thru_hole oval (at 7.63 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /PC1))
    (pad 19 thru_hole oval (at 7.63 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /PC2))
    (pad 20 thru_hole oval (at 7.63 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /PC3))
    (pad 21 thru_hole oval (at 7.63 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 Vproc))
    (pad 22 thru_hole oval (at 7.63 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(MOD101-Pad22)"))
    (pad 23 thru_hole rect (at 7.63 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 EXT_PWR_GROUND))
    (pad 24 thru_hole oval (at 7.62 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(D101-Pad1)"))
    (pad 10 thru_hole oval (at -7.6249 22.8854) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 PWDN))
    (pad 9 thru_hole oval (at -7.6249 20.3454) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 CW_KEY_LOGIC))
    (pad 8 thru_hole oval (at -7.6249 17.8054) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 TONE_LOGIC))
    (pad 7 thru_hole oval (at -7.6249 15.2654) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 PTT_LOGIC))
    (pad 6 thru_hole oval (at -7.6249 12.7254) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /PD3))
    (pad 5 thru_hole oval (at -7.6249 10.1854) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 RTC_SQW))
    (pad 4 thru_hole rect (at -7.6249 7.6454) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 EXT_PWR_GROUND))
    (pad 3 thru_hole oval (at -7.6249 5.1054) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 ~RESET~))
    (pad 2 thru_hole oval (at -7.6249 2.5654) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 RXD))
    (pad 1 thru_hole oval (at -7.62 0.0254) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /PD1))
    (pad 30 thru_hole oval (at 6.29285 -2.51485 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 DTR))
    (pad 30 thru_hole oval (at -6.29315 -2.51485 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 DTR))
    (pad 32 thru_hole oval (at 5.09 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /ADC7))
    (pad 31 thru_hole oval (at 2.55 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /ADC6))
    (pad 23 thru_hole rect (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 EXT_PWR_GROUND))
  )
  (module Connect:CON-SMA-EDGE-S (layer F.Cu) (tedit 608EFDA9)
    (at 163.07 99.4 90)
    (attr smd)
    (fp_text reference J103 (at -3.41 -0.09) (layer F.SilkS))
    (fp_text value "To Antenna" (at -2.17 4.61 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0 90) (size 4.5 6.35) (layers B.Cu B.Mask)
      (net 75 GND1))
    (pad 2 smd rect (at 0 2.77 90) (size 4.5 0.8128) (layers F.Cu F.Mask)
      (net 75 GND1))
    (pad 1 smd rect (at 0 0 90) (size 4.5 0.76) (layers F.Cu F.Mask)
      (net 13 "Net-(J103-Pad1)"))
    (pad 2 smd rect (at 0 -2.77 90) (size 4.5 0.8128) (layers F.Cu F.Mask)
      (net 75 GND1))
  )
  (module Connect:CON-SMA-EDGE-S (layer F.Cu) (tedit 608EFD6C)
    (at 163.07 117.57 270)
    (attr smd)
    (fp_text reference J101 (at -3.41 -0.15) (layer F.SilkS))
    (fp_text value "To Radio" (at -1.38 -4.71 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0 270) (size 4.5 6.35) (layers B.Cu B.Mask)
      (net 75 GND1))
    (pad 2 smd rect (at 0 2.77 270) (size 4.5 0.8128) (layers F.Cu F.Mask)
      (net 75 GND1))
    (pad 1 smd rect (at 0 0 270) (size 4.5 0.76) (layers F.Cu F.Mask)
      (net 11 "Net-(J101-Pad1)"))
    (pad 2 smd rect (at 0 -2.77 270) (size 4.5 0.8128) (layers F.Cu F.Mask)
      (net 75 GND1))
  )
  (module Connect:CON-SMA-EDGE-S (layer F.Cu) (tedit 608EFC9C)
    (at 170.2 104.2)
    (attr smd)
    (fp_text reference J113 (at -3.12 0.02 90) (layer F.SilkS))
    (fp_text value "To Stub" (at 0 4.8 180) (layer F.Fab) hide)
    (fp_text user STUB (at -0.42 3.79) (layer F.SilkS))
    (pad 2 smd rect (at 0 -2.77) (size 4.5 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 75 GND1))
    (pad 1 smd rect (at 0 0) (size 4.5 0.76) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J103-Pad1)"))
    (pad 2 smd rect (at 0 2.77) (size 4.5 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 75 GND1))
    (pad 2 smd rect (at 0 0) (size 4.5 6.35) (layers B.Cu B.Mask)
      (net 75 GND1))
  )
  (module Oddities:Waveguide_T_50_ohms (layer F.Cu) (tedit 60885106)
    (at 163.07 104.2)
    (solder_mask_margin 0.06)
    (clearance 0.06)
    (attr smd)
    (fp_text reference WG1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Waveguide_T_50_ohms (at 0 -0.5) (layer F.Fab))
    (pad 2 smd rect (at 2.875 0 270) (size 0.25 6) (layers F.Cu)
      (net 13 "Net-(J103-Pad1)") (solder_mask_margin 0.06) (clearance 0.06))
    (pad 1 smd rect (at 0.46 0.93) (size 0.5 1.44) (layers F.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 smd rect (at 0 0) (size 1.414 3.3) (layers B.Cu)
      (net 75 GND1))
    (pad 1 smd rect (at 0.46 -0.93) (size 0.5 1.44) (layers F.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 2 smd rect (at 0 0) (size 0.25 5.5) (layers F.Cu)
      (net 13 "Net-(J103-Pad1)") (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 smd rect (at -0.457 0) (size 0.5 3.3) (layers F.Cu)
      (net 75 GND1) (zone_connect 2))
    (pad 1 smd rect (at 2.21 0.46 270) (size 0.5 4) (layers F.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 smd rect (at 2.22 -0.46 270) (size 0.5 4) (layers F.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 0.57 -0.58 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 smd rect (at 2.88 0.01 270) (size 1.414 6) (layers B.Cu)
      (net 75 GND1))
    (pad 1 thru_hole circle (at 1.23 -0.58 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.89 -0.58 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 2.55 -0.58 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.21 -0.58 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.87 -0.58 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 0.57 0.57 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.23 0.57 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.89 0.57 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 2.55 0.57 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.21 0.58 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.87 0.58 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 0.58 1.23 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at -0.57 1.24 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at -0.57 0.58 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at -0.57 -0.08 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at -0.57 -0.75 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at -0.57 -1.41 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 0.57 -1.24 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 0.57 -1.91 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at -0.57 -2.07 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
  )
  (module Oddities:Waveguide_50_ohms (layer F.Cu) (tedit 60884FCC)
    (at 163.07 113.41 180)
    (fp_text reference WG2 (at 0.06 0.5) (layer F.SilkS) hide)
    (fp_text value Waveguide_50_ohms (at 0.06 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.414 3.3) (layers B.Cu)
      (net 75 GND1) (zone_connect 2))
    (pad 1 smd rect (at 0.457 0 180) (size 0.5 3.3) (layers F.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 2 smd rect (at 0 0 180) (size 0.25 5.5) (layers F.Cu)
      (net 11 "Net-(J101-Pad1)") (solder_mask_margin 0.06) (clearance 0.06))
    (pad 1 smd rect (at -0.457 0 180) (size 0.5 3.3) (layers F.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 0.57 0.14 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 0.57 -0.48 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 0.57 -1.1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 0.57 0.76 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at 0.57 1.38 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at -0.57 1.38 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at -0.57 0.76 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at -0.57 0.14 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at -0.57 -0.48 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
    (pad 1 thru_hole circle (at -0.58 -1.11 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND1) (solder_mask_margin 0.06) (clearance 0.06) (zone_connect 2))
  )
  (module Connect:DB9F_CI (layer F.Cu) (tedit 606862E2)
    (at 160.770999 130.809999 180)
    (descr "DB9 connector female")
    (tags "CONN DB9")
    (fp_text reference J111 (at 0 -9.144 180) (layer F.SilkS))
    (fp_text value DB9_Male (at 0 -3.048 180) (layer F.Fab))
    (pad 6 connect rect (at 4.191 2.127 180) (size 1.778 4) (layers B.Cu B.Mask)
      (net 70 "Net-(J111-Pad6)"))
    (pad 7 connect rect (at 1.397 2.127 180) (size 1.778 4) (layers B.Cu B.Mask)
      (net 71 "Net-(J111-Pad7)"))
    (pad 8 connect rect (at -1.397 2.127 180) (size 1.778 4) (layers B.Cu B.Mask)
      (net 72 "Net-(J111-Pad8)"))
    (pad 9 connect rect (at -4.191 2.127 180) (size 1.778 4) (layers B.Cu B.Mask)
      (net 73 "Net-(J111-Pad9)"))
    (pad 1 connect rect (at 5.588 2.127 180) (size 1.778 4) (layers F.Cu F.Mask)
      (net 68 "Net-(J111-Pad1)"))
    (pad 5 connect rect (at -5.588 2.127 180) (size 1.778 4) (layers F.Cu F.Mask)
      (net 69 "Net-(J111-Pad5)"))
    (pad 4 connect rect (at -2.794 2.127 180) (size 1.778 4) (layers F.Cu F.Mask)
      (net 65 "Net-(J111-Pad4)"))
    (pad 3 connect rect (at 0 2.127 180) (size 1.778 4) (layers F.Cu F.Mask)
      (net 66 "Net-(J111-Pad3)"))
    (pad 2 connect rect (at 2.794 2.127 180) (size 1.778 4) (layers F.Cu F.Mask)
      (net 67 "Net-(J111-Pad2)"))
    (model Connect.3dshapes/DB9M_CI.wrl
      (offset (xyz 0 0 -0.838199987411499))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Oddities:BC501SM_CR1220_BAT_Handsolder (layer B.Cu) (tedit 60685B0A)
    (at 104.56 97.04 90)
    (fp_text reference BT101 (at 0.19 -0.09 180) (layer B.SilkS))
    (fp_text value CR1220 (at 6.5405 5.4229 270) (layer B.Fab))
    (fp_text user + (at 9.2456 -2.3368 270) (layer B.SilkS))
    (fp_text user - (at -8.6614 -2.1209 270) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 4 0 90) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -3.5 0 90) (size 1 1) (drill 1) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 8.23 0 90) (size 3.54 2.6) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(BT101-Pad1)"))
    (pad 2 smd rect (at -7.57 0 90) (size 3.66 2.6) (layers B.Cu B.Paste B.Mask)
      (net 1 EXT_PWR_GROUND))
  )
  (module Pin_Headers:Pin_Header_Angled_1x06 (layer F.Cu) (tedit 60458511)
    (at 154.86 123.15 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J112 (at -1.84 5.96 180) (layer B.SilkS))
    (fp_text value Conn_01x06 (at 0 -3.1 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(J111-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(J111-Pad9)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(J111-Pad8)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(J111-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(J111-Pad6)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(J111-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (offset (xyz 0 -6.349999904632568 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.19 130.38)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.17 129.41)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.19 128.42)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.17 127.51)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 126.57)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 125.65)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.17 124.74)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.17 123.81)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.17 122.9)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.17 121.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer B.Cu) (tedit 60423BE2)
    (at 170.02 110.06)
    (descr "Through hole pin header")
    (tags "pin header")
    (attr smd)
    (fp_text reference J109 (at 1.3 -0.02 90) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 3.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 2.2352 2.2352) (layers B.Cu B.Paste B.Mask)
      (net 45 VDC) (solder_mask_margin 0.07) (clearance 0.07))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer B.Cu) (tedit 60423BA5)
    (at 159.89 104.55)
    (descr "Through hole pin header")
    (tags "pin header")
    (solder_mask_margin 0.06)
    (clearance 0.06)
    (attr smd)
    (fp_text reference J110 (at -1.33 0.27 -90) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 3.1) (layer B.Fab))
    (pad 1 smd rect (at 1 0) (size 2.2352 2.2352) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(FB106-Pad1)") (solder_mask_margin 0.07) (clearance 0.07))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 6042356C)
    (at 103.62 123.09 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q103 (at -2.22 -0.16) (layer B.SilkS))
    (fp_text value PN2222A (at 0 -2.3 90) (layer B.Fab))
    (pad 3 smd rect (at 0 0.99822 270) (size 0.8001 0.8001) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(Q103-Pad3)"))
    (pad 2 smd rect (at 0.95 -1.00076 270) (size 0.8001 0.8001) (layers B.Cu B.Paste B.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 1 smd rect (at -0.95 -1.00076 270) (size 0.8001 0.8001) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(Q103-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 600A0A89)
    (at 97.06 104.85 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D103 (at 0.48 -1.22) (layer F.SilkS))
    (fp_text value CG0603MLC-05LECT-ND (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 RXD) (solder_mask_margin 0.06) (clearance 0.06))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363-0.65 (layer F.Cu) (tedit 5FE40272)
    (at 106.63 123.65 90)
    (attr smd)
    (fp_text reference Q102 (at 1.25 0.01) (layer F.SilkS))
    (fp_text value LMN200 (at -1.28 0.01) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65038 0.71882 90) (size 0.29972 0.55118) (layers F.Cu F.Paste F.Mask)
      (net 49 EXTERNAL_PWR_SOURCE) (solder_mask_margin 0.06) (clearance 0.06))
    (pad 2 smd rect (at 0 0.71882 90) (size 0.29972 0.55118) (layers F.Cu F.Paste F.Mask)
      (net 25 PWDN) (solder_mask_margin 0.06) (clearance 0.06))
    (pad 3 smd rect (at 0.65038 0.71882 90) (size 0.29972 0.55118) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q102-Pad3)") (solder_mask_margin 0.06) (clearance 0.06))
    (pad 4 smd rect (at 0.65038 -0.71882 90) (size 0.29972 0.55118) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 5 smd rect (at 0 -0.71882 90) (size 0.29972 0.55118) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q102-Pad3)") (solder_mask_margin 0.06) (clearance 0.06))
    (pad 6 smd rect (at -0.65038 -0.71882 90) (size 0.29972 0.55118) (layers F.Cu F.Paste F.Mask)
      (net 43 Controlled_Power) (solder_mask_margin 0.06) (clearance 0.06))
    (model ../../../../../Users/Charles/Documents/KiCad/3D/SOT23-6.wrl
      (offset (xyz 0 0 -0.06349999904632568))
      (scale (xyz 0.2 0.2 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:SM_Pin_Header_Straight_2x03 (layer B.Cu) (tedit 5FD14A07)
    (at 122.85 96.05 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (attr smd)
    (fp_text reference P101 (at 1.25 2.26) (layer B.SilkS))
    (fp_text value ISP/PDI (at 0 3.1) (layer B.Fab))
    (pad 1 smd rect (at -2.7 0 180) (size 3.1 1) (layers B.Cu B.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 2 smd oval (at 5.24 0 180) (size 3.1 1) (layers B.Cu B.Mask)
      (net 23 ~RESET~))
    (pad 3 smd oval (at -2.7 -2.54 180) (size 3.1 1) (layers B.Cu B.Mask)
      (net 16 D3))
    (pad 4 smd oval (at 5.24 -2.54 180) (size 3.1 1) (layers B.Cu B.Mask)
      (net 14 D5))
    (pad 5 smd oval (at -2.7 -5.08 180) (size 3.1 1) (layers B.Cu B.Mask)
      (net 6 Vproc))
    (pad 6 smd oval (at 5.24 -5.08 180) (size 3.1 1) (layers B.Cu B.Mask)
      (net 15 D4))
    (model "../../../../../Users/Charles/Documents/KiCad/3D/6-Pin 2x3 Header.wrl"
      (offset (xyz 1.142999982833862 -2.539999961853027 2.539999961853027))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5FCE567A)
    (at 123.35 114 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C109 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /ADC7))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5FCE567A)
    (at 96.77 102.71)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C108 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /ADC6))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /AUDIO_IN))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5FCE567A)
    (at 141.27 99.27)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C101 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 Vproc))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5FCE567A)
    (at 141.39 105.6 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C102 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5FCE567A)
    (at 99.2 115.89)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C103 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C103-Pad2)"))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /AUDIO_OUT))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5FCE567A)
    (at 166.6 112.78)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C110 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 75 GND1))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 45 VDC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 118.34 106.51 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R103 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C104-Pad1)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R103-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 124.24 110.77 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R107 (at 0 0) (layer F.SilkS))
    (fp_text value 162k (at 0 2.1 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 64 Power_In))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /ADC7))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 116.86 109.25 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R105 (at 0 0) (layer F.SilkS))
    (fp_text value 1M (at 0 2.1 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /ADC6))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 Vproc))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 116.88 112.56 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R106 (at 0 0) (layer F.SilkS))
    (fp_text value 100k (at 0 2.1 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /ADC6))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 103.28 110.42 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R104 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(Q101-Pad1)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 PTT_LOGIC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 110.82 113.18 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R101 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100k (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R101-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 TONE_LOGIC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 98.95 113.36 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R102 (at 0 0 90) (layer F.SilkS))
    (fp_text value 2.2k (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /AUDIO_OUT))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R102-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_4mm_Outlined locked (layer F.Cu) (tedit 5FCE4E8B)
    (at 93.3 127)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (zone_connect 2)
    (fp_text reference "4mm thru" (at 0 -5.4991) (layer F.SilkS) hide)
    (fp_text value MountingHole_4mm (at 0 5.99948) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask)
      (net 1 EXT_PWR_GROUND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_4mm_Outlined locked (layer F.Cu) (tedit 5FCE4E8B)
    (at 147.5 127)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (zone_connect 2)
    (fp_text reference "4mm thru" (at 0 -5.4991) (layer F.SilkS) hide)
    (fp_text value MountingHole_4mm (at 0 5.99948) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask)
      (net 1 EXT_PWR_GROUND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_4mm_Outlined locked (layer F.Cu) (tedit 5FCE4E8B)
    (at 147.5 90)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (zone_connect 2)
    (fp_text reference "4mm thru" (at 0 -5.4991) (layer F.SilkS) hide)
    (fp_text value MountingHole_4mm (at 0 5.99948) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask)
      (net 1 EXT_PWR_GROUND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_4mm_Outlined locked (layer F.Cu) (tedit 5FCE4E8B)
    (at 93.3 90)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (zone_connect 2)
    (fp_text reference "4mm thru" (at 0 -5.4991) (layer F.SilkS) hide)
    (fp_text value MountingHole_4mm (at 0 5.99948) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask)
      (net 1 EXT_PWR_GROUND) (zone_connect 2))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 98.05)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 98.96)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 100.12)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 101.04)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 102.21)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 103.14)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 104.08)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 105.31)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 106.22)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 107.4)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 108.34)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 109.27)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 110.47)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 111.4)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 112.57)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 117.7)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 113.49)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 114.41)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 115.63)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 116.55)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 118.6)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CE3527D)
    (at 152.18 119.49)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Connect:DB9F_CI locked (layer F.Cu) (tedit 0)
    (at 89.4 108.5 90)
    (descr "Connecteur DB9 femelle encarte")
    (tags "CONN DB9")
    (fp_text reference J102 (at 0 -9.144 90) (layer F.SilkS))
    (fp_text value "DB9 Female" (at 0 -3.048 90) (layer F.Fab))
    (pad 4 connect rect (at 2.794 2.54 90) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 60 CW_KEY))
    (pad 3 connect rect (at 0 2.54 90) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 12 /PTT_OUT))
    (pad 2 connect rect (at -2.794 2.54 90) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 61 DTR))
    (pad 1 connect rect (at -5.588 2.54 90) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 5 /AUDIO_OUT))
    (pad 5 connect rect (at 5.588 2.54 90) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 8 /AUDIO_IN))
    (pad 6 connect rect (at -4.191 2.54 90) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 77 /GROUND))
    (pad 7 connect rect (at -1.397 2.54 90) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 78 /RADIO_V+))
    (pad 8 connect rect (at 1.397 2.54 90) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 48 RXD))
    (pad 9 connect rect (at 4.191 2.54 90) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 44 TXD))
    (model Connect.3dshapes/DB9F_CI.wrl
      (offset (xyz 0 0 -0.838199987411499))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Wire_Pads:SolderWirePad_2x_1-5mmDrill_Polarized (layer F.Cu) (tedit 5FCAA05C)
    (at 102.04 127.5 180)
    (fp_text reference J108 (at 0.49 2.6) (layer B.SilkS))
    (fp_text value "Controlled Power" (at 0.635 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 1 EXT_PWR_GROUND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 43 Controlled_Power))
  )
  (module Potentiometers:Potentiometer_ST32ET_Handsolder (layer F.Cu) (tedit 5FA20D94)
    (at 105.32 114.73 90)
    (descr "Potentiometer, ST32ET")
    (tags "Potentiometer, ST32ET")
    (attr smd)
    (fp_text reference RV101 (at 1.8 -1.3) (layer F.SilkS))
    (fp_text value 10k (at -2.78 -0.57 90) (layer F.Fab))
    (pad 2 smd rect (at 0 -2.25 90) (size 1.6 2.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C103-Pad2)"))
    (pad 3 smd rect (at -1 2.25 90) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R101-Pad2)"))
    (pad 1 smd rect (at 1 2.25 90) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer F.Cu) (tedit 5FD14B30)
    (at 144.39 102 270)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (attr smd)
    (fp_text reference SJ101 (at 3.15 0.54 270) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 2.54 3.81 270) (layer F.Fab))
    (pad 1 smd trapezoid (at -0.916 0 90) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers F.Cu F.Mask)
      (net 6 Vproc))
    (pad 2 smd trapezoid (at 0.916 0 270) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers F.Cu F.Mask)
      (net 3 +3V3))
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer B.Cu) (tedit 5FD14AD9)
    (at 99.08 111.63 270)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (attr smd)
    (fp_text reference SJ102 (at 0.03 -1.79 90) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 2.54 -3.81 90) (layer B.Fab))
    (pad 2 smd trapezoid (at 0.916 0 270) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 31 "Net-(R102-Pad1)"))
    (pad 1 smd trapezoid (at -0.916 0 90) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 12 /PTT_OUT))
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer B.Cu) (tedit 5FD155CD)
    (at 141.62 106.24)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (attr smd)
    (fp_text reference SJ103 (at -3.46 -0.14) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 2.54 -3.81) (layer B.Fab))
    (pad 1 smd trapezoid (at -0.916 0 180) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 14 D5))
    (pad 2 smd trapezoid (at 0.916 0) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 37 "Net-(J104-Pad3)"))
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer B.Cu) (tedit 5FD14971)
    (at 141.62 108.552)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (attr smd)
    (fp_text reference SJ104 (at -3.62 0.056) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 2.54 -3.81) (layer B.Fab))
    (pad 2 smd trapezoid (at 0.916 0) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 38 "Net-(J104-Pad4)"))
    (pad 1 smd trapezoid (at -0.916 0 180) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 15 D4))
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer B.Cu) (tedit 5FD14985)
    (at 141.62 110.864)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (attr smd)
    (fp_text reference SJ105 (at -3.57 -0.03) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 2.54 -3.81) (layer B.Fab))
    (pad 1 smd trapezoid (at -0.916 0 180) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 16 D3))
    (pad 2 smd trapezoid (at 0.916 0) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 39 "Net-(J104-Pad5)"))
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer B.Cu) (tedit 5FD1499A)
    (at 141.62 113.176)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (attr smd)
    (fp_text reference SJ106 (at -3.674 0.06) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 2.54 -3.81) (layer B.Fab))
    (pad 2 smd trapezoid (at 0.916 0) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 40 "Net-(J104-Pad6)"))
    (pad 1 smd trapezoid (at -0.916 0 180) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 17 D2))
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer B.Cu) (tedit 5FD149AF)
    (at 141.62 115.488)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (attr smd)
    (fp_text reference SJ107 (at -3.5 -0.02) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 2.54 -3.81) (layer B.Fab))
    (pad 1 smd trapezoid (at -0.916 0 180) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 18 D1))
    (pad 2 smd trapezoid (at 0.916 0) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 41 "Net-(J104-Pad7)"))
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer B.Cu) (tedit 5FD149C5)
    (at 141.62 117.8)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (attr smd)
    (fp_text reference SJ108 (at -3.45 -0.04) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 2.54 -3.81) (layer B.Fab))
    (pad 2 smd trapezoid (at 0.916 0) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 42 "Net-(J104-Pad8)"))
    (pad 1 smd trapezoid (at -0.916 0 180) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 19 D0))
  )
  (module Buttons_Switches_SMD:PTS645SL50SMTR92 (layer F.Cu) (tedit 5FC998F7)
    (at 137.51 126.46)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW101 (at 0.12 -4.11) (layer F.SilkS))
    (fp_text value SPST_small (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 3.9 -2.25) (size 1.75 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 /PC3))
    (pad 1 smd rect (at -3.9 -2.25) (size 1.75 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 /PC3))
    (pad 2 smd rect (at -3.9 2.25) (size 1.75 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 2 smd rect (at 3.9 2.25) (size 1.75 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 55360473)
    (at 141.33 102.08 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U101 (at -0.03 2.63 90) (layer F.SilkS))
    (fp_text value MIC5265-3.3YD5-TR (at -0.05 2.35 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 Vproc))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 25 PWDN))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U101-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 149.52 99.64)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J104 (at -2.17 9.12 90) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(FB103-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(FB105-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J104-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J104-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J104-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J104-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(J104-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(J104-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (offset (xyz 0 -8.889999866485596 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 154.71 99.64)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J105 (at 2.2 8.78 90) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 -3.1) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(J104-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(J104-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J104-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J104-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J104-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J104-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(FB105-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(FB103-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (offset (xyz 0 -8.889999866485596 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wire_Pads:SolderWirePad_2x_1-5mmDrill_Polarized (layer F.Cu) (tedit 5FCAA05C)
    (at 111.89 127.45 180)
    (fp_text reference J107 (at 0.39 2.55) (layer B.SilkS))
    (fp_text value "External Power Source" (at 0.635 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 1 EXT_PWR_GROUND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 49 EXTERNAL_PWR_SOURCE))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 113.21 89.66 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R110 (at 0.03 -0.04) (layer F.SilkS))
    (fp_text value 10 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 54 /PD1))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 TXD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 6008587F)
    (at 123.66 103.95 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C104 (at 0 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C104-Pad1)") (solder_mask_margin 0.06) (clearance 0.06))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 126.3 110.77 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R108 (at 0 0) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /ADC7))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 99.75 109.16 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q101 (at 2.1 0.47) (layer F.SilkS))
    (fp_text value PN2222A (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(Q101-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 12 /PTT_OUT))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Connections_Bridges:Solder-Jumperx3-NC_1-2_SMD-Pad_Small (layer B.Cu) (tedit 59D5869A)
    (at 97.09 122.73)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (zone_connect 0)
    (attr smd)
    (fp_text reference SJ110 (at -0.03 1.62) (layer B.SilkS))
    (fp_text value SolderJumper_3_Bridged12 (at 2.54 -3.81) (layer B.Fab))
    (pad 3 smd trapezoid (at 2.159 0) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(Q103-Pad3)") (zone_connect 0))
    (pad 1 smd trapezoid (at -2.159 0 180) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers B.Cu B.Paste B.Mask)
      (net 21 CW_KEY_LOGIC) (zone_connect 0))
    (pad 2 smd rect (at 0 0) (size 2.032 2.032) (layers B.Cu B.Paste B.Mask)
      (net 60 CW_KEY) (zone_connect 0))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 109.78 105.23 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q104 (at 0.01 2.04 90) (layer F.SilkS))
    (fp_text value PN2222A (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(Q104-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 24 RTC_SQW))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5FCE5748)
    (at 107.42 122.51 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R109 (at 0 0 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(Q103-Pad1)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 CW_KEY_LOGIC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 121.22 102.87 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R111 (at 0 0) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R111-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 Vproc))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 107.77 110.24 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R113 (at 0 0 90) (layer F.SilkS))
    (fp_text value 210k (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(Q104-Pad1)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R113-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer B.Cu) (tedit 0)
    (at 91.95 120.01 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J106 (at -0.064999 2.205001 270) (layer B.SilkS))
    (fp_text value "Logic Level" (at 0 3.1 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 EXT_PWR_GROUND))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 20 TONE_LOGIC))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 60 CW_KEY))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 22 PTT_LOGIC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_SMD:SW_SPDT_PCM12 (layer F.Cu) (tedit 55DB5CA3)
    (at 135.94 89.91 180)
    (descr "Ultraminiature Surface Mount Slide Switch")
    (attr smd)
    (fp_text reference SW102 (at -1.5 -3.175) (layer F.SilkS))
    (fp_text value 5V/12V (at 0 0.325) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.5 0.325 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.5 0.325 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -2.25 -1.425 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 Vproc))
    (pad 2 smd rect (at 0.75 -1.425 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 64 Power_In))
    (pad 3 smd rect (at 2.25 -1.425 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 EXT_BATTERY))
    (pad "" smd rect (at -3.65 1.425 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.65 1.425 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.65 -0.775 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.65 -0.775 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 128.45 127.82 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D102 (at 0 -1.75) (layer F.SilkS))
    (fp_text value LED (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(D102-Pad2)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5FCE5748)
    (at 125.45 125.45 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R114 (at 0 0) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 /PC2))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(D102-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 142.64 95.81 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TP101 (at -2.18 3.9) (layer B.SilkS))
    (fp_text value Conn_01x04 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 EXT_PWR_GROUND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 Vproc))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 SDA))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 SCL))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 95.9 112.66 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference FB101 (at -0.34 1.35) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 /GROUND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 95.88 108.93 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference FB102 (at -0.34 1.29) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 /RADIO_V+))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 Power_In))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 149.53 96.47 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference FB103 (at 0.05 -1.32 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(FB103-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 157.88 99.4 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference FB104 (at 0.09 -1.37) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 GND1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(FB103-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 146.74 102.99 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference FB105 (at -2.85 0.73 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(FB105-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 157.83 102.48 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference FB106 (at 0.09 -1.26) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(FB105-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(FB106-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5FCE567A)
    (at 98.14 94.5 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C105 (at 0 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 Vproc))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 115.57 88.7 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D104 (at 0 -1.13) (layer F.SilkS))
    (fp_text value CG0603MLC-05LECT-ND (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 TXD))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 93.65 122.41)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D105 (at 0 1.16) (layer F.SilkS))
    (fp_text value CG0603MLC-05LECT-ND (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 TONE_LOGIC))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 110.63 115.94 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D106 (at 0 -1.15 90) (layer F.SilkS))
    (fp_text value CG0603MLC-05LECT-ND (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 CW_KEY_LOGIC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 100.52 122.43 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D107 (at 0 -1.12) (layer F.SilkS))
    (fp_text value CG0603MLC-05LECT-ND (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 PTT_LOGIC))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 EXT_PWR_GROUND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text TX (at 168.3 117.89 180) (layer B.SilkS))
  (gr_text ANT. (at 169.02 98.81 180) (layer B.SilkS))
  (gr_text TX (at 168.38 117.93) (layer F.SilkS))
  (gr_text ANT. (at 169.14 98.89) (layer F.SilkS))
  (gr_text +12V (at 131.97 87) (layer F.SilkS))
  (gr_text +5V (at 139.09 87.07) (layer F.SilkS))
  (gr_text "FTDI Adapter" (at 163.04 125.08) (layer F.SilkS))
  (gr_text GND (at 154.79 125.24 180) (layer B.SilkS))
  (gr_text GND (at 154.79 125.31) (layer F.SilkS))
  (gr_line (start 169.5 121.5) (end 152 121.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.5 131) (end 169.5 121.5) (layer Edge.Cuts) (width 0.1))
  (gr_text + (at 107.74 125.55 180) (layer B.SilkS))
  (gr_text + (at 97.64 125.68 180) (layer B.SilkS))
  (gr_text + (at 97.64 125.58) (layer F.SilkS))
  (gr_text + (at 107.71 125.48) (layer F.SilkS))
  (gr_text GND (at 157.52 99.51 90) (layer B.SilkS))
  (gr_text D5 (at 156.57 104.67 90) (layer B.SilkS))
  (gr_text D4 (at 156.6 107.27 90) (layer B.SilkS))
  (gr_text D3 (at 156.57 109.75 90) (layer B.SilkS))
  (gr_text D2 (at 156.53 112.29 90) (layer B.SilkS))
  (gr_text D1 (at 156.57 114.9 90) (layer B.SilkS))
  (gr_text D0 (at 156.57 117.34 90) (layer B.SilkS))
  (gr_text GND (at 147.39 99.65 90) (layer B.SilkS))
  (gr_text +3.3 (at 147.39 102.22 90) (layer B.SilkS))
  (gr_text D5 (at 147.39 104.67 90) (layer B.SilkS))
  (gr_text D4 (at 147.45 107.17 90) (layer B.SilkS))
  (gr_text D3 (at 147.39 109.82 90) (layer B.SilkS))
  (gr_text D2 (at 147.39 112.46 90) (layer B.SilkS))
  (gr_text D1 (at 147.42 115.03 90) (layer B.SilkS))
  (gr_text D0 (at 147.35 117.31 90) (layer B.SilkS))
  (gr_text +3.3 (at 157.56 102.09 90) (layer B.SilkS))
  (gr_text TONE (at 94.325 117.925) (layer B.SilkS))
  (gr_text KEY (at 97.05 117.925) (layer B.SilkS))
  (gr_text PTT (at 99.675 117.975) (layer B.SilkS))
  (gr_text "AM Attenuator\nRev 1.2 - Apr 2021" (at 170.496905 110.62 270) (layer F.SilkS))
  (gr_text "EXT BAT." (at 112.05 130.2) (layer B.SilkS))
  (gr_text "SWITCHED BAT." (at 101.925 130.15) (layer B.SilkS))
  (gr_text "LOGIC LEVEL OUT" (at 96.87 116.91) (layer B.SilkS))
  (gr_text TONE (at 94.325 117.925) (layer F.SilkS))
  (gr_text KEY (at 96.95 117.925) (layer F.SilkS))
  (gr_text PTT (at 99.65 117.975) (layer F.SilkS))
  (gr_text "SWITCHED BAT." (at 101.75 130.175) (layer F.SilkS))
  (gr_text "EXT BAT." (at 112.05 130.175) (layer F.SilkS))
  (gr_text VCC (at 125.71 100.1) (layer B.SilkS))
  (gr_text MOSI (at 125.59 97.59) (layer B.SilkS))
  (gr_text GND (at 125.55 94.89) (layer B.SilkS))
  (gr_text MISO (at 117.33 99.86) (layer B.SilkS))
  (gr_text SCK (at 117.29 97.44) (layer B.SilkS))
  (gr_text Reset (at 117.33 94.81) (layer B.SilkS))
  (gr_text https://github.com/OpenARDF/Arducon (at 131.3 128.55) (layer B.SilkS))
  (gr_text CR1220 (at 96.21 96.06 90) (layer B.SilkS))
  (gr_text 6 (at 95.24 112.82) (layer B.SilkS))
  (gr_text 7 (at 95.21 109.82) (layer B.SilkS))
  (gr_text 8 (at 95.24 107) (layer B.SilkS))
  (gr_text 9 (at 95.21 104.38) (layer B.SilkS))
  (gr_text 5 (at 95.02 101.43) (layer F.SilkS))
  (gr_text 1 (at 95.1 115.19) (layer F.SilkS))
  (gr_text "Arducon\nARDF Transmitter Controller\nRev 2.3 - May 2021" (at 143.76 125.33) (layer B.SilkS))
  (gr_line (start 172.5 97) (end 172.5 120) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152 120) (end 172.5 120) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152 97) (end 172.5 97) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152 97) (end 152 86) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152 121.5) (end 152 120) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152 86) (end 89 86) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89 131) (end 169.5 131) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89 86) (end 89 131) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name EXT_PWR_GROUND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.655 86.31) (xy 151.71 130.55) (xy 89.47 130.56) (xy 89.38 86.34)
      )
    )
  )
  (zone (net 75) (net_name GND1) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.2775 97.3) (xy 172.2225 119.72) (xy 152.57 119.58) (xy 152.57 97.36)
      )
    )
  )
  (zone (net 75) (net_name GND1) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.28 97.23) (xy 172.24 119.72) (xy 152.57 119.515) (xy 152.47 97.245)
      )
    )
  )
  (zone (net 1) (net_name EXT_PWR_GROUND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.655 86.51) (xy 151.71 130.73) (xy 89.429957 130.56) (xy 89.339957 86.34)
      )
    )
  )
  (zone (net 75) (net_name GND1) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.27 107.13) (xy 167.27 107.93) (xy 164.95 107.94) (xy 164.98 107.35) (xy 164.99 107.37)
        (xy 164.97 106.04) (xy 167.17 106.03)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.07 123.72) (xy 95.68 123.72) (xy 95.68 121.74) (xy 96.07 121.73)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.48 123.75) (xy 98.11 123.74) (xy 98.11 121.729474) (xy 98.48 121.71)
      )
    )
    (polygon
      (pts
        (xy 98.11 121.729474) (xy 98.1 121.73) (xy 98.11 121.72)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.09 111.78) (xy 98.07 111.78) (xy 98.08 111.47) (xy 98.08 111.46) (xy 100.08 111.46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.75 107.25) (xy 141.44 107.25) (xy 141.45 105.26) (xy 141.45 105.24) (xy 141.76 105.24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.75 109.57) (xy 141.47 109.6) (xy 141.44 107.59) (xy 141.45 107.57) (xy 141.76 107.56)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.78 111.85) (xy 141.44 111.87) (xy 141.42 109.89) (xy 141.41 109.87) (xy 141.78 109.86)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.75 114.17) (xy 141.45 114.17) (xy 141.42 112.19) (xy 141.45 112.19) (xy 141.76 112.17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.76 116.47) (xy 141.44 116.48) (xy 141.45 114.52) (xy 141.42 114.51) (xy 141.78 114.51)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.76 118.81) (xy 141.44 118.81) (xy 141.44 116.82) (xy 141.42 116.8) (xy 141.74 116.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.082))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.32 102.21) (xy 143.37 102.19) (xy 143.37 101.84) (xy 145.3 101.84)
      )
    )
  )
)
