(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 13)
    (zones 0)
    (modules 3)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.1524)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.25)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /A0)
  (net 2 /A1)
  (net 3 /A2)
  (net 4 /A3)
  (net 5 /D0)
  (net 6 /D1)
  (net 7 /D2)
  (net 8 /D3)
  (net 9 /D4)
  (net 10 /D5)
  (net 11 /D6)
  (net 12 /D7)
  (net 13 /D8)
  (net 14 /D9)
  (net 15 /D10)
  (net 16 /D13)
  (net 17 /D12)
  (net 18 /D11)
  (net 19 /A4)
  (net 20 /A5)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
  )
  (module footprints:HarwinM300 (layer F.Cu) (tedit 63407E27)
    (at 113.03 125.73 180)
    (descr "Molex 734 Male header (for PCBs); Straight solder pin 1 x 1 mm, 734-134 , 4 Pins (http://www.farnell.com/datasheets/2157639.pdf), generated with kicad-footprint-generator")
    (tags "connector Wago  side entry")
    (fp_text reference J1 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 4.25) (layer F.Fab))
    (pad 3 thru_hole circle (at -3 0.1 180) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 2 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 /D1))
    (pad 1 thru_hole circle (at 3 0 180) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 /D0))
    (pad "" np_thru_hole circle (at 8 0 180) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -8 0 180) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Wago.3dshapes/Wago_734-134_1x04_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 63331346)
    (at 101.6 120.65 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x10_Male (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /A5))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /A2))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A1))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A0))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /D10))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /D11))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /D12))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /D13))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 63331326)
    (at 101.6 130.81 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x10_Male (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /D9))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /D8))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /D7))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /D6))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /D5))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /D4))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /D3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /D1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /D0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "20 19 18 17 16 15 14 13 12 11" (at 113.03 119.126) (layer B.SilkS))
  (gr_text "10  9  8  7  6  5  4  3  2  1" (at 113.284 132.334) (layer B.SilkS))
  (dimension 10.16 (width 0.15) (layer Dwgs.User)
    (gr_text "0.4000 in" (at 130.84 125.73 270) (layer Dwgs.User))
    (feature1 (pts (xy 124.46 130.81) (xy 130.126421 130.81)))
    (feature2 (pts (xy 124.46 120.65) (xy 130.126421 120.65)))
    (crossbar (pts (xy 129.54 120.65) (xy 129.54 130.81)))
    (arrow1a (pts (xy 129.54 130.81) (xy 128.953579 129.683496)))
    (arrow1b (pts (xy 129.54 130.81) (xy 130.126421 129.683496)))
    (arrow2a (pts (xy 129.54 120.65) (xy 128.953579 121.776504)))
    (arrow2b (pts (xy 129.54 120.65) (xy 130.126421 121.776504)))
  )
  (dimension 25.4 (width 0.15) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 113.03 139.73) (layer Dwgs.User))
    (feature1 (pts (xy 125.73 130.81) (xy 125.73 139.016421)))
    (feature2 (pts (xy 100.33 130.81) (xy 100.33 139.016421)))
    (crossbar (pts (xy 100.33 138.43) (xy 125.73 138.43)))
    (arrow1a (pts (xy 125.73 138.43) (xy 124.603496 139.016421)))
    (arrow1b (pts (xy 125.73 138.43) (xy 124.603496 137.843579)))
    (arrow2a (pts (xy 100.33 138.43) (xy 101.456504 139.016421)))
    (arrow2b (pts (xy 100.33 138.43) (xy 101.456504 137.843579)))
  )
  (dimension 15.24 (width 0.15) (layer Dwgs.User)
    (gr_text "0.6000 in" (at 93.95 125.73 90) (layer Dwgs.User))
    (feature1 (pts (xy 102.87 118.11) (xy 94.663579 118.11)))
    (feature2 (pts (xy 102.87 133.35) (xy 94.663579 133.35)))
    (crossbar (pts (xy 95.25 133.35) (xy 95.25 118.11)))
    (arrow1a (pts (xy 95.25 118.11) (xy 95.836421 119.236504)))
    (arrow1b (pts (xy 95.25 118.11) (xy 94.663579 119.236504)))
    (arrow2a (pts (xy 95.25 133.35) (xy 95.836421 132.223496)))
    (arrow2b (pts (xy 95.25 133.35) (xy 94.663579 132.223496)))
  )
  (gr_line (start 100.33 120.65) (end 100.33 130.81) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 118.11) (end 102.87 118.11) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 130.81) (end 125.73 120.65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.87 133.35) (end 123.19 133.35) (layer Edge.Cuts) (width 0.15))
  (gr_text "Harwin M300 Breakout" (at 113.157 128.778) (layer B.SilkS))
  (gr_text "11 12 13 14 15 16 17 18 19 20" (at 113.03 119.126) (layer F.SilkS))
  (gr_text "1  2  3  4  5  6  7  8  9  10" (at 113.284 132.334) (layer F.SilkS))
  (gr_arc (start 102.87 130.81) (end 100.33 130.81) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 123.19 130.81) (end 123.19 133.35) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 123.19 120.65) (end 125.73 120.65) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102.87 120.65) (end 102.87 118.11) (angle -90) (layer Edge.Cuts) (width 0.15))
)
