(kicad_pcb (version 20171130) (host pcbnew "(5.1.12-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 8)
    (zones 0)
    (modules 2)
    (nets 4)
  )
  (page A4)
  (title_block
    (title "XLR Breakout Board")
    (date 2021-12-10)
    (rev 0.0.1)
    (company NH)
    (comment 2 https://creativecommons.org/licenses/by/4.0/)
    (comment 3 "License: CC BY 4.0")
    (comment 4 "Author: Hieu Minh Nguyen")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.762)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.635)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.6858 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 /XLR-)
  (net 3 /XLR+)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net /XLR+)
    (add_net /XLR-)
    (add_net "Net-(J1-Pad1)")
  )
  (module xlr_breakout_board:Jack_XLR_Amphenol_AC3FAHL-AU-PRE (layer F.Cu) (tedit 61B30392)
    (at 0 -22.86)
    (descr "Includes an extra pad for compatibility with Neutrik NC3FAAH2-0 and related parts")
    (fp_text reference J1 (at -9.144 17.272) (layer F.SilkS))
    (fp_text value XLR3_Amphenol_AC3FAHL (at 11.4 19.4 90) (layer F.Fab))
    (fp_text user %R (at 0 7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 3.81 8.89) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 3.81) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad G thru_hole circle (at -8.25 6.98) (size 2.9 2.9) (drill 1.2) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 17.15) (size 2.9 2.9) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /XLR-))
    (pad 2 thru_hole circle (at 3.81 13.335) (size 3.4 3.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 /XLR+))
    (pad 1 thru_hole circle (at -3.81 12.7) (size 3.4 3.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KIPRJMOD}/docs/amphenol_AC3FAHL-AU-PRE.stp
      (offset (xyz 0 0 12.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 180))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 2.54 0 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.794) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 2.54 2.54) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /XLR-))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /XLR+))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text " (\\__/)\n (•.•)  \nc(“)(“) " (at -3.81 -14.986) (layer F.SilkS))
  (gr_text - (at -2.54 -2.286) (layer F.SilkS))
  (gr_text + (at 0 -2.286) (layer F.SilkS))
  (gr_text v0.0.1 (at 6.858 -14.478) (layer B.SilkS))
  (gr_text "XLR3\nBreakout\nBoard" (at 6.858 -17.78) (layer B.SilkS))
  (gr_circle (center -8 -1.144) (end -6.8 -1.144) (layer Edge.Cuts) (width 0.0254))
  (gr_circle (center 8 -1.144) (end 9.2 -1.144) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start -8.89 -0.254) (end -10.922 -0.254) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start -8.89 -19.05) (end -8.89 -21.082) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 8.89 -19.05) (end 10.922 -19.05) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 8.89 -0.254) (end 8.89 1.778) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 10.922 -19.05) (end 10.922 -0.254) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start -8.89 -21.082) (end 8.89 -21.082) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start -10.922 -0.254) (end -10.922 -19.05) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start -8.89 1.778) (end 8.89 1.778) (layer Edge.Cuts) (width 0.0254))
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.635) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 11.684 2.286) (xy -11.43 2.286) (xy -11.43 -21.59) (xy 11.684 -21.59)
      )
    )
  )
)
