<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="17.78" y1="0" x2="1.27" y2="0" width="0" layer="20"/>
<wire x1="1.27" y1="0" x2="0" y2="1.27" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="1.27" x2="0" y2="17.78" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="1.27" y2="19.05" width="0" layer="20" curve="-90"/>
<wire x1="1.27" y1="19.05" x2="17.78" y2="19.05" width="0" layer="20"/>
<wire x1="17.78" y1="19.05" x2="19.05" y2="17.78" width="0" layer="20" curve="-90"/>
<wire x1="19.05" y1="17.78" x2="19.05" y2="1.27" width="0" layer="20"/>
<wire x1="19.05" y1="1.27" x2="17.78" y2="0" width="0" layer="20" curve="-90"/>
<text>U1</text>
<text>R2</text>
<text>R1</text>
<text>R3</text>
<text>R4</text>
<text>C1</text>
<text>zeruel85</text>
<text>Switch Board</text>
<text>v1.0</text>
</plain>
<libraries>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP18R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="snes_div">
<packages>
<package name="Z0805">
</package>
</packages>
</library>
<library name="74hc4066">
<packages>
<package name="SOIC127P600X175-14N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CE" library="testpad" package="TP18R" value="TPSQTP18R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="CI" library="testpad" package="TP18R" value="TPSQTP18R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="EN" library="testpad" package="TP18R" value="TPSQTP18R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="GND" library="testpad" package="TP18R" value="TPSQTP18R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="PE" library="testpad" package="TP18R" value="TPSQTP18R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="PI" library="testpad" package="TP18R" value="TPSQTP18R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="U$3" library="snes_div" package="Z0805" value="C0805"/>
<element name="U$4" library="snes_div" package="Z0805" value="R0805"/>
<element name="U$5" library="snes_div" package="Z0805" value="R0805"/>
<element name="U$6" library="snes_div" package="Z0805" value="R0805"/>
<element name="U$7" library="snes_div" package="Z0805" value="R0805"/>
<element name="U1" library="74hc4066" package="SOIC127P600X175-14N" value="SN74HC4066D">
<attribute name="OC_NEWARK" value="72K9433"/>
<attribute name="MPN" value="SN74HC4066D"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="1236227"/>
</element>
<element name="VCC" library="testpad" package="TP18R" value="TPSQTP18R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="XE" library="testpad" package="TP18R" value="TPSQTP18R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="XI" library="testpad" package="TP18R" value="TPSQTP18R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U1" pad="14"/>
<contactref element="VCC" pad="TP"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$4" pad="2"/>
<contactref element="U$5" pad="2"/>
<contactref element="U$7" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="4"/>
<contactref element="GND" pad="TP"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="XE">
<contactref element="U1" pad="2"/>
<contactref element="XE" pad="TP"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="3"/>
<contactref element="U$5" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="6"/>
<contactref element="EN" pad="TP"/>
<contactref element="U$6" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="8"/>
<contactref element="PI" pad="TP"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="9"/>
<contactref element="CI" pad="TP"/>
<contactref element="U$7" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="11"/>
<contactref element="XI" pad="TP"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="1"/>
<contactref element="PE" pad="TP"/>
<contactref element="CE" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
