(kicad_pcb (version 20170123) (host pcbnew "(2017-02-21 revision 35a8d78)-master")
  (general
    (links 181)
    (no_connects 0)
    (area 93.402639 43.44533 143.37725 84.911001)
    (thickness 1.6002)
    (drawings 18)
    (tracks 595)
    (zones 0)
    (modules 63)
    (nets 75)
  )
  (page A)
  (title_block
    (title "Portable Impedance Tomography")
    (date 2017-09-16)
    (rev NEW)
    (company "Ashton Johnson")
    (comment 1 "University of Alabama in Huntsville")
  )
  (layers
    (0 Top signal)
    (1 In1.Cu mixed)
    (2 In2.Cu mixed)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (trace_clearance 0.14986)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.508 0.508)
    (mod_text_width 0.0762)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 136.0175 82.821265)
    (visible_elements FFFEEF7F)
    (pcbplotparams
      (layerselection 0x000f0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(C8-Pad1)")
  (net 2 +2V5)
  (net 3 "/AD5933 Front End/VOUT")
  (net 4 "Net-(C13-Pad1)")
  (net 5 "Net-(C15-Pad1)")
  (net 6 "Net-(C15-Pad2)")
  (net 7 "Net-(C16-Pad2)")
  (net 8 "/AD5933 Front End/SHIELD_DRIVE")
  (net 9 "/Receive Mux/SA1")
  (net 10 "/Receive Mux/SA2")
  (net 11 "/Receive Mux/SA3")
  (net 12 "/Receive Mux/SA4")
  (net 13 "Net-(J5-Pad1)")
  (net 14 "Net-(J6-Pad1)")
  (net 15 "Net-(J7-Pad1)")
  (net 16 "Net-(J8-Pad1)")
  (net 17 "/Transmit Mux/SA1")
  (net 18 "/Transmit Mux/SA2")
  (net 19 "/Transmit Mux/SA3")
  (net 20 "/Transmit Mux/SA4")
  (net 21 "Net-(J13-Pad1)")
  (net 22 "Net-(J14-Pad1)")
  (net 23 "Net-(J15-Pad1)")
  (net 24 "Net-(J16-Pad1)")
  (net 25 GND)
  (net 26 "Net-(J17-Pad21)")
  (net 27 "Net-(J17-Pad20)")
  (net 28 "Net-(J17-Pad19)")
  (net 29 "Net-(J17-Pad18)")
  (net 30 "Net-(J17-Pad17)")
  (net 31 "Net-(J17-Pad16)")
  (net 32 "Net-(J17-Pad15)")
  (net 33 "Net-(J17-Pad14)")
  (net 34 "Net-(J17-Pad13)")
  (net 35 "Net-(J17-Pad12)")
  (net 36 "Net-(J17-Pad11)")
  (net 37 /AD5933/SCL)
  (net 38 /AD5933/SDA)
  (net 39 "/Cypress BLE Headers/SEL0")
  (net 40 "Net-(J17-Pad7)")
  (net 41 "/Cypress BLE Headers/SEL1")
  (net 42 "Net-(J17-Pad5)")
  (net 43 "Net-(J17-Pad3)")
  (net 44 "Net-(J19-Pad8)")
  (net 45 "Net-(J19-Pad7)")
  (net 46 "Net-(J19-Pad2)")
  (net 47 "/AD5933 Front End/VIN")
  (net 48 /AD5933/AD5933_RFB)
  (net 49 "Net-(R6-Pad1)")
  (net 50 "Net-(R11-Pad2)")
  (net 51 "Net-(R10-Pad2)")
  (net 52 "Net-(R10-Pad1)")
  (net 53 "/Receive Mux/DRIVE")
  (net 54 "/Transmit Mux/DRIVE")
  (net 55 VCC)
  (net 56 /AD5933/MCLK)
  (net 57 "Net-(U2-Pad7)")
  (net 58 "Net-(U2-Pad3)")
  (net 59 "Net-(U2-Pad2)")
  (net 60 "Net-(U2-Pad1)")
  (net 61 "/Receive Mux/SENSE")
  (net 62 "/Transmit Mux/SENSE")
  (net 63 /AD5933/VOUT)
  (net 64 /AD5933/VIN)
  (net 65 "/AD5933 Front End/DRIVE_P")
  (net 66 "/AD5933 Front End/SENSE_P")
  (net 67 "/AD5933 Front End/DRIVE_N")
  (net 68 "/AD5933 Front End/SENSE_N")
  (net 69 "Net-(RV1-Pad1)")
  (net 70 "/AD5933 Front End/EN")
  (net 71 "Net-(R17-Pad1)")
  (net 72 "Net-(R15-Pad2)")
  (net 73 "Net-(R16-Pad2)")
  (net 74 "/Auxiliary Analog Connector/AIN")
  (net_class Default "This is the default net class."
    (clearance 0.14986)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "/AD5933 Front End/DRIVE_N")
    (add_net "/AD5933 Front End/DRIVE_P")
    (add_net "/AD5933 Front End/EN")
    (add_net "/AD5933 Front End/SENSE_N")
    (add_net "/AD5933 Front End/SENSE_P")
    (add_net "/AD5933 Front End/SHIELD_DRIVE")
    (add_net "/AD5933 Front End/VIN")
    (add_net "/AD5933 Front End/VOUT")
    (add_net /AD5933/AD5933_RFB)
    (add_net /AD5933/VIN)
    (add_net /AD5933/VOUT)
    (add_net "/Auxiliary Analog Connector/AIN")
    (add_net "/Cypress BLE Headers/SEL0")
    (add_net "/Cypress BLE Headers/SEL1")
    (add_net "/Receive Mux/DRIVE")
    (add_net "/Receive Mux/SA1")
    (add_net "/Receive Mux/SA2")
    (add_net "/Receive Mux/SA3")
    (add_net "/Receive Mux/SA4")
    (add_net "/Receive Mux/SENSE")
    (add_net "/Transmit Mux/DRIVE")
    (add_net "/Transmit Mux/SA1")
    (add_net "/Transmit Mux/SA2")
    (add_net "/Transmit Mux/SA3")
    (add_net "/Transmit Mux/SA4")
    (add_net "/Transmit Mux/SENSE")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J17-Pad11)")
    (add_net "Net-(J17-Pad12)")
    (add_net "Net-(J17-Pad13)")
    (add_net "Net-(J17-Pad14)")
    (add_net "Net-(J17-Pad15)")
    (add_net "Net-(J17-Pad16)")
    (add_net "Net-(J17-Pad17)")
    (add_net "Net-(J17-Pad18)")
    (add_net "Net-(J17-Pad19)")
    (add_net "Net-(J17-Pad20)")
    (add_net "Net-(J17-Pad21)")
    (add_net "Net-(J17-Pad3)")
    (add_net "Net-(J17-Pad5)")
    (add_net "Net-(J17-Pad7)")
    (add_net "Net-(J19-Pad2)")
    (add_net "Net-(J19-Pad7)")
    (add_net "Net-(J19-Pad8)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(RV1-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad7)")
  )
  (net_class 10mil ""
    (clearance 0.14986)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /AD5933/MCLK)
    (add_net /AD5933/SCL)
    (add_net /AD5933/SDA)
  )
  (net_class POWER ""
    (clearance 0.14986)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +2V5)
    (add_net GND)
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Bottom) (tedit 58AA848B)
    (at 95.504 50.353 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at -2.093 -1.3716) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06_Pitch2.54mm locked (layer Top) (tedit 58CD5449)
    (at 136.017 82.804 180)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (fp_text reference J19 (at 4.572 4.826 270) (layer F.SilkS))
    (fp_text value Conn_02x06_Odd_Even (at -1.27 15.03 180) (layer F.Fab))
    (fp_text user %R (at -1.27 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/Cypress BLE Headers/SEL1"))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J19-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "/AD5933 Front End/EN"))
    (pad 4 thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/Cypress BLE Headers/SEL0"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 6 thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 VCC))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J19-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J19-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /AD5933/SCL))
    (pad 10 thru_hole oval (at -2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /AD5933/SDA))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 12 thru_hole oval (at -2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 VCC))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x12_Pitch2.54mm locked (layer Bottom) (tedit 58CD5449)
    (at 96.466 75.4296 270)
    (descr "Through hole straight socket strip, 2x12, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x12 2.54mm double row")
    (fp_text reference J17 (at -4.5636 0.962) (layer B.SilkS))
    (fp_text value Conn_02x12_Odd_Even (at -1.27 -30.27 270) (layer B.Fab))
    (fp_text user %R (at -1.27 2.33 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 VCC))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J17-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "/AD5933 Front End/EN"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J17-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/Cypress BLE Headers/SEL1"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J17-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/Cypress BLE Headers/SEL0"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /AD5933/SDA))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /AD5933/SCL))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J17-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J17-Pad12)"))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J17-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J17-Pad14)"))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J17-Pad15)"))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J17-Pad16)"))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J17-Pad17)"))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J17-Pad18)"))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J17-Pad19)"))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J17-Pad20)"))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J17-Pad21)"))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "/Auxiliary Analog Connector/AIN"))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 VCC))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x12_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Bottom) (tedit 58AA848B)
    (at 116.84 67.691 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Bottom) (tedit 58AA848B)
    (at 120.65 67.691)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.1524 1.1938) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Bottom) (tedit 58AA848B)
    (at 116.84 68.961 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -0.0508 -1.143 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 58AA848B)
    (at 111.76 52.451 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 2.032 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 25 GND))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 55 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 58AA848B)
    (at 114.935 54.356 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 25 GND))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 55 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 58AA841A)
    (at 119.761 54.356 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at -2.3368 -0.3302) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 1 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 25 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 58AA848B)
    (at 115.763 51.308 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0.955 0.889 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 2 +2V5))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 25 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 58AA841A)
    (at 117.856 55.711 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at -1.355 -0.508) (layer B.SilkS))
    (fp_text value 33n (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 "/AD5933 Front End/VOUT"))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 4 "Net-(C13-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Bottom) (tedit 58AA848B)
    (at 100.838 47.879)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0.0508 -1.143) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 5 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 6 "Net-(C15-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Bottom) (tedit 58AA848B)
    (at 105.918 51.181 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0.9144 -1.0922 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 7 "Net-(C16-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Bottom) (tedit 58AA848B)
    (at 100.264 55.753 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 2.728 -0.0254 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 58AA848B)
    (at 135.89 52.451 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 2.032 -0.254 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 55 VCC))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 25 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 99.06 47.371)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J1 (at 1.524 -2.032) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302) (layer F.Fab))
    (pad 2 smd rect (at -1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 0 -1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 1 smd rect (at 0 1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 9 "/Receive Mux/SA1"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 104.14 47.371)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J2 (at 1.524 -2.032) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302) (layer F.Fab))
    (pad 2 smd rect (at -1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 0 -1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 1 smd rect (at 0 1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 10 "/Receive Mux/SA2"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 109.22 47.371)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J3 (at 1.524 -2.032) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302) (layer F.Fab))
    (pad 2 smd rect (at -1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 0 -1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 1 smd rect (at 0 1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 11 "/Receive Mux/SA3"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 114.3 47.371)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J4 (at 1.524 -2.032) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302) (layer F.Fab))
    (pad 1 smd rect (at 0 1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 12 "/Receive Mux/SA4"))
    (pad 2 smd rect (at 0 -1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at -1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 99.06 60.071 180)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J5 (at -1.524 2.032 180) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302 180) (layer F.Fab))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 0 -1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 1 smd rect (at 0 1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 13 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 104.14 60.071 180)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J6 (at -1.524 2.032 180) (layer F.SilkS))
    (fp_text value UMC (at 0.432938 -1.098987 180) (layer F.Fab))
    (pad 1 smd rect (at 0 1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 14 "Net-(J6-Pad1)"))
    (pad 2 smd rect (at 0 -1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 109.22 60.071 180)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J7 (at -1.3716 1.9558 180) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302 180) (layer F.Fab))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 0 -1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 1 smd rect (at 0 1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 15 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 114.3 60.071 180)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J8 (at 1.3208 2.032 180) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302 180) (layer F.Fab))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 0 -1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 1 smd rect (at 0 1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 16 "Net-(J8-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 121.92 47.371)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J9 (at 2.032 -2.032) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302) (layer F.Fab))
    (pad 1 smd rect (at 0 1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 17 "/Transmit Mux/SA1"))
    (pad 2 smd rect (at 0 -1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at -1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 127 47.371)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J10 (at 2.032 -2.032) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302) (layer F.Fab))
    (pad 1 smd rect (at 0 1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 18 "/Transmit Mux/SA2"))
    (pad 2 smd rect (at 0 -1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at -1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 132.08 47.282)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J11 (at 2.032 -1.943) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302) (layer F.Fab))
    (pad 1 smd rect (at 0 1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 19 "/Transmit Mux/SA3"))
    (pad 2 smd rect (at 0 -1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at -1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 137.16 47.371)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J12 (at 1.524 -2.032) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302) (layer F.Fab))
    (pad 1 smd rect (at 0 1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 20 "/Transmit Mux/SA4"))
    (pad 2 smd rect (at 0 -1.5) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at -1.475 0) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 121.92 60.071 180)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J13 (at -1.524 2.032 180) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302 180) (layer F.Fab))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 0 -1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 1 smd rect (at 0 1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 21 "Net-(J13-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 127 60.071 180)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J14 (at -1.524 2.032 180) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302 180) (layer F.Fab))
    (pad 1 smd rect (at 0 1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 22 "Net-(J14-Pad1)"))
    (pad 2 smd rect (at 0 -1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 132.08 60.071 180)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J15 (at -1.524 2.032 180) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302 180) (layer F.Fab))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 0 -1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 1 smd rect (at 0 1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 23 "Net-(J15-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microcoaxial_RF (layer Top) (tedit 5884C15F)
    (at 137.16 60.071 180)
    (descr "Molex Microcoaxial RF, mates Hirose U.FL, http://www.molex.com/pdm_docs/sd/734120110_sd.pdf")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J16 (at -1.524 2.032 180) (layer F.SilkS))
    (fp_text value UMC (at 0 -3.302 180) (layer F.Fab))
    (pad 1 smd rect (at 0 1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 24 "Net-(J16-Pad1)"))
    (pad 2 smd rect (at 0 -1.5 180) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers Top F.Paste F.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microcoaxial_RF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Bottom) (tedit 58E0A804)
    (at 141.224 71.374 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.413 0.254) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 38 /AD5933/SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Bottom) (tedit 58E0A804)
    (at 133.223 71.204 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.4208 0.7874) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 37 /AD5933/SCL))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Bottom) (tedit 58E0A804)
    (at 116.078 54.653 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.27) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 64 /AD5933/VIN))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 48 /AD5933/AD5933_RFB))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 58E0A804)
    (at 117.475 57.15 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.397 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 55 VCC))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 49 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Bottom) (tedit 58E0A804)
    (at 117.856 51.7955 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.45) (layer B.SilkS))
    (fp_text value 75k (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 2 +2V5))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 4 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Bottom) (tedit 58E0A804)
    (at 106.172 49.657 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 2.667 180) (layer B.SilkS))
    (fp_text value 1M (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 7 "Net-(C16-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 50 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Bottom) (tedit 58E0A804)
    (at 106.172 48.133 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.778 180) (layer B.SilkS))
    (fp_text value 1M (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 2 +2V5))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 5 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Bottom) (tedit 58E0A804)
    (at 100.16 57.531)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0.932 1.143) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at -0.084 0) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 51 "Net-(R10-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 52 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Bottom) (tedit 58E0A804)
    (at 109.728 49.657 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -0.127 1.143 180) (layer B.SilkS))
    (fp_text value 75 (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 50 "Net-(R11-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Bottom) (tedit 58E0A804)
    (at 109.728 51.181)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0.762 1.143) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 8 "/AD5933 Front End/SHIELD_DRIVE"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Bottom) (tedit 58E0A804)
    (at 98.214 58.547)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -1.44 -1.27) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 65 "/AD5933 Front End/DRIVE_P"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 52 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 58E0A804)
    (at 123.19 56.261 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -2.794 -0.635 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 2 +2V5))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 67 "/AD5933 Front End/DRIVE_N"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-16_5.3x6.2mm_Pitch0.65mm (layer Bottom) (tedit 54130A77)
    (at 116.84 61.341 270)
    (descr "SSOP16: plastic shrink small outline package; 16 leads; body width 5.3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot338-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at -3.3782 3.556) (layer B.SilkS))
    (fp_text value AD5933 (at 0 -4.2 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 16 smd rect (at 3.45 2.275 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 37 /AD5933/SCL))
    (pad 15 smd rect (at 3.45 1.625 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 38 /AD5933/SDA))
    (pad 14 smd rect (at 3.45 0.975 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (pad 13 smd rect (at 3.45 0.325 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (pad 12 smd rect (at 3.45 -0.325 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (pad 11 smd rect (at 3.45 -0.975 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (pad 10 smd rect (at 3.45 -1.625 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (pad 9 smd rect (at 3.45 -2.275 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (pad 8 smd rect (at -3.45 -2.275 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 56 /AD5933/MCLK))
    (pad 7 smd rect (at -3.45 -1.625 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 57 "Net-(U2-Pad7)"))
    (pad 6 smd rect (at -3.45 -0.975 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 63 /AD5933/VOUT))
    (pad 5 smd rect (at -3.45 -0.325 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 64 /AD5933/VIN))
    (pad 4 smd rect (at -3.45 0.325 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 48 /AD5933/AD5933_RFB))
    (pad 3 smd rect (at -3.45 0.975 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 58 "Net-(U2-Pad3)"))
    (pad 2 smd rect (at -3.45 1.625 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 59 "Net-(U2-Pad2)"))
    (pad 1 smd rect (at -3.45 2.275 270) (size 1.2 0.4) (layers Bottom B.Paste B.Mask)
      (net 60 "Net-(U2-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-16_5.3x6.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer Top) (tedit 54130A77)
    (at 106.68 53.721)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at -0.127 3.175) (layer F.SilkS))
    (fp_text value ADG1209 (at 0 3.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.275) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 41 "/Cypress BLE Headers/SEL1"))
    (pad 2 smd rect (at -2.95 -1.625) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 70 "/AD5933 Front End/EN"))
    (pad 3 smd rect (at -2.95 -0.975) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 25 GND))
    (pad 4 smd rect (at -2.95 -0.325) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 9 "/Receive Mux/SA1"))
    (pad 5 smd rect (at -2.95 0.325) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 10 "/Receive Mux/SA2"))
    (pad 6 smd rect (at -2.95 0.975) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 11 "/Receive Mux/SA3"))
    (pad 7 smd rect (at -2.95 1.625) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 12 "/Receive Mux/SA4"))
    (pad 8 smd rect (at -2.95 2.275) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 53 "/Receive Mux/DRIVE"))
    (pad 9 smd rect (at 2.95 2.275) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 61 "/Receive Mux/SENSE"))
    (pad 10 smd rect (at 2.95 1.625) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 16 "Net-(J8-Pad1)"))
    (pad 11 smd rect (at 2.95 0.975) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 15 "Net-(J7-Pad1)"))
    (pad 12 smd rect (at 2.95 0.325) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 14 "Net-(J6-Pad1)"))
    (pad 13 smd rect (at 2.95 -0.325) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 13 "Net-(J5-Pad1)"))
    (pad 14 smd rect (at 2.95 -0.975) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 55 VCC))
    (pad 15 smd rect (at 2.95 -1.625) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 25 GND))
    (pad 16 smd rect (at 2.95 -2.275) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 39 "/Cypress BLE Headers/SEL0"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23-5 (layer Top) (tedit 58CE4E80)
    (at 117.475 54.356 90)
    (descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
    (tags TSOT-23-5)
    (attr smd)
    (fp_text reference U5 (at 2.54 0.889 180) (layer F.SilkS))
    (fp_text value LD3985G25R_TSOT23 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 5 smd rect (at 1.31 -0.95 90) (size 1.22 0.65) (layers Top F.Paste F.Mask)
      (net 2 +2V5))
    (pad 4 smd rect (at 1.31 0.95 90) (size 1.22 0.65) (layers Top F.Paste F.Mask)
      (net 1 "Net-(C8-Pad1)"))
    (pad 3 smd rect (at -1.31 0.95 90) (size 1.22 0.65) (layers Top F.Paste F.Mask)
      (net 49 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at -1.31 0 90) (size 1.22 0.65) (layers Top F.Paste F.Mask)
      (net 25 GND))
    (pad 1 smd rect (at -1.31 -0.95 90) (size 1.22 0.65) (layers Top F.Paste F.Mask)
      (net 55 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-10_3x3mm_Pitch0.5mm (layer Bottom) (tedit 54130A77)
    (at 100.702 50.411 180)
    (descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U6 (at 1.388 -2.167 180) (layer B.SilkS))
    (fp_text value OPA2836 (at 0 -2.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -2.15 1 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 6 "Net-(C15-Pad2)"))
    (pad 2 smd rect (at -2.15 0.5 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 5 "Net-(C15-Pad1)"))
    (pad 3 smd rect (at -2.15 0 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 7 "Net-(C16-Pad2)"))
    (pad 4 smd rect (at -2.15 -0.5 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (pad 5 smd rect (at -2.15 -1 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 70 "/AD5933 Front End/EN"))
    (pad 6 smd rect (at 2.15 -1 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 70 "/AD5933 Front End/EN"))
    (pad 7 smd rect (at 2.15 -0.5 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 52 "Net-(R10-Pad1)"))
    (pad 8 smd rect (at 2.15 0 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 50 "Net-(R11-Pad2)"))
    (pad 9 smd rect (at 2.15 0.5 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 50 "Net-(R11-Pad2)"))
    (pad 10 smd rect (at 2.15 1 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-10_3x3mm_Pitch0.5mm (layer Bottom) (tedit 54130A77)
    (at 129.54 53.721 180)
    (descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U7 (at 0 2.286 180) (layer B.SilkS))
    (fp_text value OPA2836 (at 0 -2.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 10 smd rect (at 2.15 1 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (pad 9 smd rect (at 2.15 0.5 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask))
    (pad 8 smd rect (at 2.15 0 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask))
    (pad 7 smd rect (at 2.15 -0.5 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask))
    (pad 6 smd rect (at 2.15 -1 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask))
    (pad 5 smd rect (at -2.15 -1 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 70 "/AD5933 Front End/EN"))
    (pad 4 smd rect (at -2.15 -0.5 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (pad 3 smd rect (at -2.15 0 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 72 "Net-(R15-Pad2)"))
    (pad 2 smd rect (at -2.15 0.5 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 73 "Net-(R16-Pad2)"))
    (pad 1 smd rect (at -2.15 1 180) (size 1.1 0.25) (layers Bottom B.Paste B.Mask)
      (net 47 "/AD5933 Front End/VIN"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SO-8_5.3x6.2mm_Pitch1.27mm (layer Bottom) (tedit 59920130)
    (at 106.934 56.261 180)
    (descr "8-Lead Plastic Small Outline, 5.3x6.2mm Body (http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U8 (at 0 3.683 180) (layer B.SilkS))
    (fp_text value AD8130 (at 0 -4.13 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 8 smd rect (at 3.7 1.905 180) (size 1.75 0.55) (layers Bottom B.Paste B.Mask)
      (net 6 "Net-(C15-Pad2)"))
    (pad 7 smd rect (at 3.7 0.635 180) (size 1.75 0.55) (layers Bottom B.Paste B.Mask)
      (net 55 VCC))
    (pad 6 smd rect (at 3.7 -0.635 180) (size 1.75 0.55) (layers Bottom B.Paste B.Mask)
      (net 51 "Net-(R10-Pad2)"))
    (pad 5 smd rect (at 3.7 -1.905 180) (size 1.75 0.55) (layers Bottom B.Paste B.Mask)
      (net 51 "Net-(R10-Pad2)"))
    (pad 4 smd rect (at -3.7 -1.905 180) (size 1.75 0.55) (layers Bottom B.Paste B.Mask)
      (net 50 "Net-(R11-Pad2)"))
    (pad 3 smd rect (at -3.7 -0.635 180) (size 1.75 0.55) (layers Bottom B.Paste B.Mask)
      (net 70 "/AD5933 Front End/EN"))
    (pad 2 smd rect (at -3.7 0.635 180) (size 1.75 0.55) (layers Bottom B.Paste B.Mask)
      (net 25 GND))
    (pad 1 smd rect (at -3.7 1.905 180) (size 1.75 0.55) (layers Bottom B.Paste B.Mask)
      (net 4 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SO-8_5.3x6.2mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer Top) (tedit 54130A77)
    (at 129.54 53.721)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U9 (at 0.127 3.175) (layer F.SilkS))
    (fp_text value ADG1209 (at 0 3.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 16 smd rect (at 2.95 -2.275) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 39 "/Cypress BLE Headers/SEL0"))
    (pad 15 smd rect (at 2.95 -1.625) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 25 GND))
    (pad 14 smd rect (at 2.95 -0.975) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 55 VCC))
    (pad 13 smd rect (at 2.95 -0.325) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 21 "Net-(J13-Pad1)"))
    (pad 12 smd rect (at 2.95 0.325) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 22 "Net-(J14-Pad1)"))
    (pad 11 smd rect (at 2.95 0.975) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 23 "Net-(J15-Pad1)"))
    (pad 10 smd rect (at 2.95 1.625) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 24 "Net-(J16-Pad1)"))
    (pad 9 smd rect (at 2.95 2.275) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 62 "/Transmit Mux/SENSE"))
    (pad 8 smd rect (at -2.95 2.275) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 54 "/Transmit Mux/DRIVE"))
    (pad 7 smd rect (at -2.95 1.625) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 20 "/Transmit Mux/SA4"))
    (pad 6 smd rect (at -2.95 0.975) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 19 "/Transmit Mux/SA3"))
    (pad 5 smd rect (at -2.95 0.325) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 18 "/Transmit Mux/SA2"))
    (pad 4 smd rect (at -2.95 -0.325) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 17 "/Transmit Mux/SA1"))
    (pad 3 smd rect (at -2.95 -0.975) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 25 GND))
    (pad 2 smd rect (at -2.95 -1.625) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 70 "/AD5933 Front End/EN"))
    (pad 1 smd rect (at -2.95 -2.275) (size 1.5 0.45) (layers Top F.Paste F.Mask)
      (net 41 "/Cypress BLE Headers/SEL1"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer Top) (tedit 58CD5446)
    (at 128.905 66.421 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J20 (at 2.286 1.143 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/AD5933 Front End/VOUT"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /AD5933/VOUT))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer Top) (tedit 58CD5446)
    (at 135.89 66.421 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J21 (at 2.286 1.27 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 /AD5933/VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/AD5933 Front End/VIN"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer Top) (tedit 58CD5446)
    (at 95.3775 53.6621 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J22 (at -1.778 1.27 -180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.794 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "/Receive Mux/DRIVE"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "/AD5933 Front End/DRIVE_P"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer Top) (tedit 58CD5446)
    (at 118.11 46.101)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J23 (at 1.778 -0.762) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "/AD5933 Front End/SENSE_P"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "/Receive Mux/SENSE"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer Top) (tedit 58CD5446)
    (at 121.92 54.356 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J24 (at -1.778 -1.524 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "/AD5933 Front End/DRIVE_N"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "/Transmit Mux/DRIVE"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer Top) (tedit 58CD5446)
    (at 139.7 51.181)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J25 (at 1.016 -1.778) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "/Transmit Mux/SENSE"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "/AD5933 Front End/SENSE_N"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Bourns_3214W (layer Bottom) (tedit 58826B0B)
    (at 110.236 62.865 270)
    (descr "Spindle Trimmer Potentiometer, Bourns 3214W, https://www.bourns.com/pdfs/3214.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3214W")
    (attr smd)
    (fp_text reference RV1 (at -2.3114 3.2512) (layer B.SilkS))
    (fp_text value 20K (at 0 -3.5 270) (layer B.Fab))
    (pad 3 smd rect (at -1.25 1.45 270) (size 1.3 1.6) (layers Bottom B.Mask)
      (net 48 /AD5933/AD5933_RFB))
    (pad 2 smd rect (at 0 -1.45 270) (size 2 1.6) (layers Bottom B.Mask)
      (net 64 /AD5933/VIN))
    (pad 1 smd rect (at 1.25 1.45 270) (size 1.3 1.6) (layers Bottom B.Mask)
      (net 69 "Net-(RV1-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Bourns_3214W.wrl
      (at (xyz 0 0.02 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer Bottom) (tedit 58E0A804)
    (at 128.27 56.642 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.143 180) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 71 "Net-(R17-Pad1)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 72 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer Top) (tedit 58E0A804)
    (at 136.144 56.515 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.143 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 73 "Net-(R16-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 47 "/AD5933 Front End/VIN"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer Top) (tedit 58E0A804)
    (at 123.063 50.927)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at -2.921 -0.127) (layer F.SilkS))
    (fp_text value 1k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 66 "/AD5933 Front End/SENSE_P"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 72 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer Top) (tedit 58E0A804)
    (at 140.081 56.515 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at -0.762 -1.016 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 73 "Net-(R16-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 68 "/AD5933 Front End/SENSE_N"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering placed (layer Bottom) (tedit 58E0A804)
    (at 124.333 56.642 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 -1.143 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 2 +2V5))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Bottom B.Paste B.Mask)
      (net 71 "Net-(R17-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03_Pitch2.54mm (layer Top) (tedit 58CD5446)
    (at 95.8855 64.4825 90)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J18 (at 3.3528 -1.0668 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "/Auxiliary Analog Connector/AIN"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_text GND (at 128.016 78.486 180) (layer B.SilkS))
  (gr_text "Ashton Johnson\nhttps://github.com/ashtonchase/\nportable_impedance_tomography" (at 96.012 81.534) (layer Bottom))
  (gr_text SEL1 (at 133.731 82.55 90) (layer F.SilkS))
  (gr_text EN (at 133.731 80.264 90) (layer F.SilkS))
  (gr_text SEL0 (at 140.97 80.391 90) (layer F.SilkS))
  (gr_text "SCL\n" (at 133.731 72.771 90) (layer F.SilkS))
  (gr_text SDA (at 140.843 72.644 90) (layer F.SilkS))
  (gr_text PMOD (at 132.715 76.708 90) (layer F.SilkS))
  (gr_text "PSoC BLE MODULE" (at 101.854 78.105) (layer F.SilkS))
  (gr_text DRIVE- (at 130.175 50.165) (layer F.SilkS))
  (gr_text "SENSE-\n" (at 123.952 63.627) (layer F.SilkS))
  (gr_text "SENSE+\n" (at 107.188 63.627) (layer F.SilkS))
  (gr_text DRIVE+ (at 107.188 50.292) (layer F.SilkS))
  (gr_line (start 93.98 84.836) (end 93.98 43.942) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 84.836) (end 93.98 84.836) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 43.942) (end 142.24 84.836) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.98 43.942) (end 142.24 43.942) (layer Edge.Cuts) (width 0.15))
  (zone (net 8) (net_name "/AD5933 Front End/SHIELD_DRIVE") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 5.08))
    (polygon
      (pts
        (xy 93.98 43.942) (xy 142.24 43.942) (xy 142.24 84.582) (xy 93.98 84.582)
      )
    )
  )
  (zone (net 25) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.98 43.942) (xy 142.24 43.942) (xy 142.24 84.582) (xy 93.98 84.582)
      )
    )
  )
  (zone (net 25) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.98 43.942) (xy 142.24 43.942) (xy 142.24 84.582) (xy 93.98 84.582)
      )
    )
  )
  (zone (net 55) (net_name VCC) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.98 43.942) (xy 142.24 43.942) (xy 142.24 84.582) (xy 93.98 84.582)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch full 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.54 83.82) (xy 116.332 83.82) (xy 116.332 79.248) (xy 129.54 79.248)
      )
    )
  )
)
