<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="28.194" y1="0.762" x2="28.194" y2="19.812" width="0.0254" layer="20"/>
<wire x1="28.194" y1="19.812" x2="27.559" y2="20.447" width="0.0254" layer="20" curve="90"/>
<wire x1="27.559" y1="20.447" x2="2.032" y2="20.447" width="0.0254" layer="20"/>
<wire x1="2.032" y1="20.447" x2="1.397" y2="19.812" width="0.0254" layer="20" curve="90"/>
<wire x1="1.397" y1="19.812" x2="0.762" y2="19.177" width="0.0254" layer="20" curve="-90"/>
<wire x1="0.762" y1="19.177" x2="0.127" y2="18.542" width="0.0254" layer="20" curve="90"/>
<wire x1="0.127" y1="18.542" x2="0.127" y2="2.032" width="0.0254" layer="20"/>
<wire x1="0.127" y1="2.032" x2="0.762" y2="1.397" width="0.0254" layer="20" curve="90"/>
<wire x1="0.762" y1="1.397" x2="1.397" y2="0.762" width="0.0254" layer="20" curve="-90"/>
<wire x1="1.397" y1="0.762" x2="1.397" y2="0.761996875" width="0.0254" layer="20"/>
<wire x1="1.397" y1="0.761996875" x2="2.032" y2="0.126996875" width="0.0254" layer="20" curve="90"/>
<wire x1="2.032" y1="0.126996875" x2="27.559" y2="0.127" width="0.0254" layer="20"/>
<wire x1="27.559" y1="0.127" x2="28.194" y2="0.762" width="0.0254" layer="20" curve="90"/>
<hole x="3.048" y="1.778" drill="1.905"/>
<hole x="3.048" y="18.796" drill="1.905"/>
<hole x="26.543" y="18.796" drill="1.905"/>
<hole x="26.543" y="1.778" drill="1.905"/>
<text>Unit:mm</text>
<text>Xadow</text>
<text>Serial</text>
<text>v2.0 15/10/2014</text>
<text>by Tisham Dhar</text>
</plain>
<libraries>
<library name="template">
<packages>
<package name="12P-0.5">
</package>
</packages>
</library>
<library name="nxpsemi">
<packages>
<package name="TSSOP_24">
</package>
</packages>
</library>
<library name="cts_crystal">
<packages>
<package name="CTS_32X25">
</package>
</packages>
</library>
<library name="OPL">
<packages>
<package name="C0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="R0603">
</package>
<package name="AVX-A">
</package>
<package name="LED0603">
</package>
</packages>
</library>
<library name="NXP_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 14:27:46</description>
<packages>
<package name="SOT65P210X110-6N">
</package>
</packages>
</library>
<library name="Discrete">
<packages>
<package name="1206-8-3.3X2.4">
<description>&lt;b&gt;BOURNS&lt;/b&gt; Chip Resistor Array&lt;p&gt;
Source: RS Component / BUORNS</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-2-NO_NO_SILK">
</package>
</packages>
</library>
<library name="Connector">
<packages>
<package name="MINI-B-SMD">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="template" package="12P-0.5" value="12p 0.5mm bottom contact">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="template" package="12P-0.5" value="12p 0.5mm bottom contact">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="nxpsemi" package="TSSOP_24" value="SC16IS750"/>
<element name="X1" library="cts_crystal" package="CTS_32X25" value="CTS_32X25_SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="OPL" package="C0603" value="26pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="OPL" package="C0603" value="26pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="OPL" package="R0603" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="OPL" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="OPL" package="AVX-A" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="OPL" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="OPL" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="OPL" package="LED0603" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="OPL" package="LED0603" value="GRN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="OPL" package="R0603" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="OPL" package="R0603" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="NXP_By_element14_Batch_1" package="SOT65P210X110-6N" value="BSS138PS">
<attribute name="PACKAGE" value="SOT-363-6"/>
<attribute name="OC_NEWARK" value="58T9002"/>
<attribute name="MPN" value="BSS138PS"/>
<attribute name="SUPPLIER" value="NXP"/>
<attribute name="OC_FARNELL" value="1972664"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Discrete" package="1206-8-3.3X2.4" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="GND" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SCL" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SDA" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="3V3" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="A0" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_NO_SILK" value="JUMPER-PAD-2-NO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A1" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_NO_SILK" value="JUMPER-PAD-2-NO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="Connector" package="MINI-B-SMD" value="MINI-USB-5P-3400020P1"/>
<element name="IO0" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IO1" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IO2" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IO3" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IO4" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IO5" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IO6" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IO7" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="3V3">
<contactref element="J2" pad="5"/>
<contactref element="J2" pad="8"/>
<contactref element="J3" pad="8"/>
<contactref element="J3" pad="5"/>
<contactref element="U1" pad="P$7"/>
<contactref element="U1" pad="P$8"/>
<contactref element="C4" pad="+"/>
<contactref element="C3" pad="2"/>
<contactref element="D2" pad="+"/>
<contactref element="D1" pad="+"/>
<contactref element="3V3" pad="1"/>
<contactref element="R7" pad="5"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="2"/>
<contactref element="R7" pad="6"/>
<contactref element="U1" pad="P$4"/>
<contactref element="A0" pad="1"/>
<contactref element="A1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="6"/>
<contactref element="J2" pad="7"/>
<contactref element="J2" pad="P2"/>
<contactref element="J3" pad="6"/>
<contactref element="J3" pad="7"/>
<contactref element="J2" pad="P1"/>
<contactref element="J3" pad="P2"/>
<contactref element="J3" pad="P1"/>
<contactref element="X1" pad="2"/>
<contactref element="X1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="P$19"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="GND" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="-"/>
<contactref element="J5" pad="5"/>
<contactref element="J5" pad="P$1"/>
<contactref element="J5" pad="P$3"/>
<contactref element="J5" pad="P$2"/>
<contactref element="J5" pad="P$4"/>
</signal>
<signal name="PB1/D15/SCK">
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="12"/>
</signal>
<signal name="PB3/D14/MISO">
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="10"/>
</signal>
<signal name="PB2/D16/MOSI">
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="11"/>
</signal>
<signal name="PD3/TXO/D1">
<contactref element="J2" pad="12"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="PF0/A5">
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="PD1/SDA/D2">
<contactref element="J2" pad="10"/>
<contactref element="J3" pad="3"/>
<contactref element="U1" pad="P$13"/>
<contactref element="SDA" pad="1"/>
</signal>
<signal name="PD0/SCL/D3">
<contactref element="J2" pad="9"/>
<contactref element="J3" pad="4"/>
<contactref element="U1" pad="P$12"/>
<contactref element="SCL" pad="1"/>
</signal>
<signal name="PD2/RXI/D0">
<contactref element="J2" pad="11"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$10">
</signal>
<signal name="N$1">
<contactref element="U1" pad="P$5"/>
<contactref element="C1" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="P$6"/>
<contactref element="C2" pad="2"/>
<contactref element="X1" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="P$10"/>
<contactref element="R3" pad="1"/>
<contactref element="A1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="P$9"/>
<contactref element="R2" pad="1"/>
<contactref element="A0" pad="2"/>
</signal>
<signal name="IO0">
<contactref element="U1" pad="P$15"/>
<contactref element="IO0" pad="1"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="IO1">
<contactref element="U1" pad="P$16"/>
<contactref element="IO1" pad="1"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="IO2">
<contactref element="U1" pad="P$17"/>
<contactref element="IO2" pad="1"/>
</signal>
<signal name="IO3">
<contactref element="U1" pad="P$18"/>
<contactref element="IO3" pad="1"/>
</signal>
<signal name="IO4">
<contactref element="U1" pad="P$20"/>
<contactref element="IO4" pad="1"/>
</signal>
<signal name="IO5">
<contactref element="U1" pad="P$21"/>
<contactref element="IO5" pad="1"/>
</signal>
<signal name="IO6">
<contactref element="U1" pad="P$22"/>
<contactref element="IO6" pad="1"/>
</signal>
<signal name="IO7">
<contactref element="U1" pad="P$23"/>
<contactref element="IO7" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="P$3"/>
<contactref element="R5" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="R7" pad="3"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="P$2"/>
<contactref element="R6" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="R7" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="R5" pad="2"/>
<contactref element="D1" pad="-"/>
</signal>
<signal name="N$16">
<contactref element="R6" pad="2"/>
<contactref element="D2" pad="-"/>
</signal>
<signal name="5V">
<contactref element="R7" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="RX_5">
<contactref element="U2" pad="6"/>
<contactref element="R7" pad="8"/>
</signal>
<signal name="TX_5">
<contactref element="U2" pad="3"/>
<contactref element="R7" pad="7"/>
<contactref element="J5" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
