(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 50)
    (zones 0)
    (modules 7)
    (nets 7)
  )
  (page A4)
  (title_block
    (title "DMX Demonstrator - Fixture Temp Sensor (DMX-FXT)")
    (date 2024-07-06)
    (rev 1.0)
    (company "Sparky Bobo Designs")
    (comment 2 "Designed by: SparkyBobo")
    (comment 3 https://creativecommons.org/licenses/by-sa/4.0/)
    (comment 4 "Released under the Creative Commons Attribution Share-Alike 4.0m License")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.95 0.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "grb"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /TEMP)
  (net 4 "Net-(U1-Pad5)")
  (net 5 "Net-(U1-Pad1)")
  (net 6 GNDD)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net +5V)
    (add_net /TEMP)
    (add_net GND)
    (add_net GNDD)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad5)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 1.27)
    (uvia_drill 0.635)
    (diff_pair_width 0.3048)
    (diff_pair_gap 0.3048)
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopOnly (layer B.Cu) (tedit 56D1B4CB)
    (at 140.7414 104.9655)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference H1 (at 0 3.8) (layer B.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 -3.8) (layer B.Fab))
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 6 GNDD))
    (pad 1 connect circle (at 0 0) (size 5.6 5.6) (layers B.Cu B.Mask)
      (net 6 GNDD))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 150.8379 103.251 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-353_SC-70-5 (layer F.Cu) (tedit 5A02FF57)
    (at 148.3995 106.3371 270)
    (descr "SOT-353, SC-70-5")
    (tags "SOT-353 SC-70-5")
    (attr smd)
    (fp_text reference U1 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value MCP9700T-ELT (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.95 -0.65 270) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at 0.95 0.65 270) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -0.95 0 270) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.95 0.65 270) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /TEMP))
    (pad 1 smd rect (at -0.95 -0.65 270) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical_SMD_Pin1Left (layer F.Cu) (tedit 59FED5CC)
    (at 148.2979 104.9782 90)
    (descr "surface-mounted straight pin header, 1x03, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x03 2.54mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J1 (at 0 -4.87 270) (layer F.SilkS) hide)
    (fp_text value "Temp Sensor" (at 0 4.87 -90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 2 smd rect (at 1.655 0 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /TEMP))
    (pad 3 smd rect (at -1.655 2.54 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.655 -2.54 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 145.7452 103.2891 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -2.7178 -0.00508 90) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:OSHW-LOGO-S locked (layer B.Cu) (tedit 200000)
    (at 150.3045 104.7369 180)
    (descr "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (tags "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (attr virtual)
    (fp_text reference "" (at 0 0) (layer B.SilkS))
    (fp_text value "" (at 0 0) (layer B.SilkS))
  )
  (module footprints:logo_cr_5x5 locked (layer B.Cu) (tedit 0)
    (at 146.7358 104.2416 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text DMX-FXT,V1.0 (at 147.4851 107.8103) (layer B.SilkS))
  (gr_arc (start 151.5058 102.22738) (end 152.3238 102.22738) (angle -90.53371786) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 151.51342 107.7162) (end 151.51342 108.5342) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.1125 107.7849) (end 137.3505 107.7849) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.1125 102.1842) (end 138.1125 101.4222) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.3505 107.7849) (end 137.3505 102.1842) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.1125 108.5469) (end 151.51342 108.5342) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.3265 102.2275) (end 152.33142 107.7162) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.1125 101.4222) (end 151.49818 101.409415) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.2349 102.235) (xy 152.2349 107.7087) (xy 151.511 108.4453) (xy 138.0617 108.458) (xy 137.4394 107.7722)
        (xy 137.4394 102.2096) (xy 138.1252 101.4984) (xy 151.4983 101.4984)
      )
    )
  )
  (zone (net 6) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.4028 106.807) (xy 147.4089 106.807) (xy 147.3962 105.8672) (xy 149.4028 105.8672)
      )
    )
  )
)
