(kicad_pcb (version 4) (host pcbnew "(2015-08-15 BZR 6092)-product")
  (general
    (links 17)
    (no_connects 0)
    (area 129.489999 107.899999 154.990001 142.290001)
    (thickness 1.6)
    (drawings 65)
    (tracks 79)
    (zones 0)
    (modules 20)
    (nets 5)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 0.9144)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.254)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.651 1.651)
    (pad_drill 0.9652)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 N-000001)
  (net 3 N-000002)
  (net 4 N-000004)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
    (add_net N-000001)
    (add_net N-000002)
    (add_net N-000004)
  )
  (net_class PWR ""
    (clearance 0.6096)
    (trace_width 0.6096)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module R3-LARGE_PADS (layer F.Cu) (tedit 56F20982)
    (at 133.35 111.76 225)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 0 0 225) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 0 225) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 225) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.81 0 225) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 N-000004))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module R3-LARGE_PADS (layer F.Cu) (tedit 56F2090D)
    (at 151.13 111.76 135)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 0 0 135) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 0 135) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 135) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.81 0 135) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 N-000002))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED-5MM (layer F.Cu) (tedit 56F207B9)
    (at 148.59 114.3 45)
    (descr "LED 5mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 5mm 5MM 100mil 2,54mm")
    (fp_text reference D2 (at 0 -3.81 45) (layer F.SilkS) hide)
    (fp_text value LED (at 0 2.286 45) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 45) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 N-000001))
    (pad 2 thru_hole circle (at 1.27 0 45) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 N-000002))
    (model discret/leds/led5_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 1pin-Sew-thin (layer F.Cu) (tedit 544BB5C8)
    (at 139.065 109.855 270)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference L1_C1 (at 0.127 0 360) (layer F.SilkS) hide)
    (fp_text value " " (at 0 2.54 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 3.048 3.048) (drill 1.984375) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module 1pin-Sew-thin (layer F.Cu) (tedit 544ADA00)
    (at 131.445 117.475 270)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference L1_C2 (at 0 -3.048 270) (layer F.SilkS) hide)
    (fp_text value " " (at 0 2.794 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 3.048 3.048) (drill 1.984375) (layers *.Cu *.Mask F.SilkS)
      (net 2 N-000001))
  )
  (module LED-5MM (layer F.Cu) (tedit 546F57AE)
    (at 135.89 114.3 135)
    (descr "LED 5mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 5mm 5MM 100mil 2,54mm")
    (fp_text reference D1 (at -0.635 1.905 135) (layer F.SilkS) hide)
    (fp_text value LED (at 5.08 -2.54 225) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 135) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 N-000001))
    (pad 2 thru_hole circle (at 1.27 0 135) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 N-000004))
    (model discret/leds/led5_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 3hole_mousebite (layer F.Cu) (tedit 544BCA0D)
    (at 141.605 113.665 90)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference p (at 0 -0.762 90) (layer F.SilkS) hide)
    (fp_text value P (at 0 -0.254 90) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 -0.381 90) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -1.27 -0.381 90) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 1.27 -0.381 90) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
  )
  (module 3hole_mousebite (layer F.Cu) (tedit 544BCA0D)
    (at 134.62 119.38 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference p (at 0 -0.762 180) (layer F.SilkS) hide)
    (fp_text value P (at 0 -0.254 180) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 -0.381 180) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -1.27 -0.381 180) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 1.27 -0.381 180) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
  )
  (module 3hole_mousebite (layer F.Cu) (tedit 544BCA0D)
    (at 142.875 113.665 270)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference p (at 0 -0.762 270) (layer F.SilkS) hide)
    (fp_text value P (at 0 -0.254 270) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 -0.381 270) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -1.27 -0.381 270) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 1.27 -0.381 270) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
  )
  (module BATT_CR2032 (layer F.Cu) (tedit 544BC08C)
    (at 142.24 132.08)
    (tags battery)
    (fp_text reference BT1 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text value BATTERY (at 0 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -10.414 1.524) (size 2.286 2.286) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 N-000001))
    (pad 1 thru_hole circle (at 10.414 1.524) (size 2.286 2.286) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 N-000001))
    (pad 1 thru_hole circle (at -10.414 -1.524) (size 2.286 2.286) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 N-000001))
    (pad 1 thru_hole circle (at 10.414 -1.524) (size 2.286 2.286) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 N-000001))
    (pad 2 smd circle (at 0 0) (size 17.78 17.78) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 1pin-Sew-thin (layer F.Cu) (tedit 546FC1C2)
    (at 153.035 123.825)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference B_N1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value GND (at 1.143 3.048 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.984375) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module 1pin-Sew-thin (layer F.Cu) (tedit 546FC1FF)
    (at 153.035 140.335)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference B_N2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -2.54) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.984375) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module 1pin-Sew-thin (layer F.Cu) (tedit 546FC1B9)
    (at 131.445 123.825)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference B_P2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value PWR (at -1.016 3.175 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.984375) (layers *.Cu *.Mask F.SilkS)
      (net 2 N-000001))
  )
  (module 1pin-Sew-thin (layer F.Cu) (tedit 546FC1F9)
    (at 131.445 140.335)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference B_P1 (at 0.127 -0.381) (layer F.SilkS) hide)
    (fp_text value PWR (at 0 -2.54) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.984375) (layers *.Cu *.Mask F.SilkS)
      (net 2 N-000001))
  )
  (module 3hole_mousebite (layer F.Cu) (tedit 544BCA0D)
    (at 134.62 121.92)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference p (at 0 -0.762) (layer F.SilkS) hide)
    (fp_text value P (at 0 -0.254) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 -0.381) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -1.27 -0.381) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 1.27 -0.381) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
  )
  (module 3hole_mousebite (layer F.Cu) (tedit 544BCA0D)
    (at 149.86 121.285 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference p (at 0 -0.762 180) (layer F.SilkS) hide)
    (fp_text value P (at 0 -0.254 180) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 -0.381 180) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -1.27 -0.381 180) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 1.27 -0.381 180) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
  )
  (module 3hole_mousebite (layer F.Cu) (tedit 544BCA0D)
    (at 149.86 119.38 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference p (at 0 -0.762 180) (layer F.SilkS) hide)
    (fp_text value P (at 0 -0.254 180) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 -0.381 180) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -1.27 -0.381 180) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 1.27 -0.381 180) (size 0.508 0.508) (drill 0.508) (layers *.Cu *.Mask F.SilkS))
  )
  (module 1pin-Sew-thin (layer F.Cu) (tedit 56F2001B)
    (at 145.415 109.855)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference L1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value " " (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.984375) (layers *.Cu *.Mask F.SilkS)
      (net 2 N-000001))
  )
  (module 1pin-Sew-thin (layer F.Cu) (tedit 56F20099)
    (at 153.035 117.475)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference L2 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value " " (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.984375) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module myFootPrints:Frysklab_logo (layer F.Cu) (tedit 576C8D6E)
    (at 142 132)
    (fp_text reference G*** (at -4 3) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text "Rev 0.2\nJune 2016" (at 154.559 111.125) (layer B.SilkS))
  (gr_text - (at 150.495 123.19) (layer F.SilkS))
  (gr_text + (at 133.985 123.19 180) (layer F.SilkS))
  (gr_text + (at 137.795 114.046) (layer B.SilkS))
  (gr_text + (at 148.971 115.951) (layer B.SilkS))
  (gr_text + (at 146.558 113.919) (layer F.SilkS))
  (gr_text + (at 135.89 116.332) (layer F.SilkS))
  (gr_line (start 129.54 139.7) (end 129.54 124.46) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 132.08 139.7) (end 132.08 142.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 154.94 133.35) (end 154.94 138.43) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.51 111.125) (end 143.51 110.49) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.97 111.125) (end 140.97 110.49) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.97 116.84) (end 140.97 116.205) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 146.05 116.84) (end 146.05 119.38) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 142.24 116.205) (end 142.24 114.935) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 142.24 116.205) (end 140.97 116.205) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 142.24 111.125) (end 143.51 111.125) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 142.24 111.125) (end 142.24 112.395) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.51 116.205) (end 143.51 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.16 119.38) (end 138.43 119.38) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.05 119.38) (end 147.32 119.38) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.16 121.92) (end 147.32 121.92) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 152.4 110.49) (end 152.4 107.95) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 154.94 116.84) (end 154.94 110.49) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.05 107.95) (end 152.4 107.95) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.43 107.95) (end 132.08 107.95) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.54 110.49) (end 129.54 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 132.08 110.49) (end 129.54 110.49) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 146.05 110.49) (end 143.51 110.49) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 138.43 110.49) (end 138.43 107.95) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 138.43 116.84) (end 140.97 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 147.32 120.65) (end 148.59 120.65) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 147.32 120.65) (end 147.32 119.38) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 152.4 120.65) (end 152.4 121.92) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 152.4 120.65) (end 151.13 120.65) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 137.16 120.65) (end 137.16 121.92) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 137.16 120.65) (end 135.89 120.65) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 132.08 120.65) (end 132.08 119.38) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 132.08 120.65) (end 133.35 120.65) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 132.08 116.84) (end 132.08 119.38) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text + (at 133.731 118.364 180) (layer F.SilkS))
  (gr_text - (at 139.954 111.633) (layer F.SilkS))
  (gr_text + (at 133.731 118.364 180) (layer B.SilkS))
  (gr_text - (at 139.954 111.633) (layer B.SilkS))
  (gr_text LED (at 137.414 118.364) (layer B.SilkS))
  (gr_arc (start 132.08 124.46) (end 129.54 124.46) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text LED (at 146.431 118.237) (layer B.SilkS))
  (gr_text - (at 150.495 118.745) (layer B.SilkS))
  (gr_text + (at 144.78 112.395 180) (layer B.SilkS))
  (gr_text www.frysklab.nl (at 142.5 127) (layer B.SilkS))
  (gr_text "CR2032 BAT" (at 142.24 135.89) (layer B.SilkS))
  (gr_arc (start 144.78 139.7) (end 144.78 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 149.86 139.7) (end 149.86 142.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 139.7 139.7) (end 137.16 139.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 134.62 139.7) (end 137.16 139.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text - (at 150.495 118.11) (layer F.SilkS))
  (gr_text + (at 144.78 112.395 180) (layer F.SilkS))
  (gr_line (start 132.08 142.24) (end 134.62 142.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.7 137.16) (end 144.78 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.86 142.24) (end 152.4 142.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 154.94 133.35) (end 154.94 124.46) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 154.94 139.7) (end 154.94 138.43) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 152.4 116.84) (end 154.94 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 152.4 124.46) (end 152.4 121.92) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 152.4 139.7) (end 154.94 139.7) (angle 90) (layer Edge.Cuts) (width 0.1))
)
