(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 24)
    (no_connects 0)
    (area 170.104999 82.474999 202.005001 108.025001)
    (thickness 1.6)
    (drawings 11)
    (tracks 295)
    (zones 0)
    (modules 16)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.15)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(R1-Pad1)")
  (net 9 "Net-(R2-Pad1)")
  (net 10 "Net-(R3-Pad1)")
  (net 11 "Net-(RV1-Pad3)")
  (net 12 "Net-(RV1-Pad1)")
  (net 13 "Net-(U1-Pad7)")
  (net 14 "Net-(BT1-Pad1)")
  (net 15 "Net-(SW1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(RV1-Pad1)")
    (add_net "Net-(RV1-Pad3)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(U1-Pad7)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 59605604)
    (at 172.72 93.98)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference BT1 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value Battery (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5_P5 (layer F.Cu) (tedit 596055B9)
    (at 196.215 85.09 180)
    (descr "Capacitor 7.5mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 47nF (at 2.5 3.5 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D7.5_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5_P5 (layer F.Cu) (tedit 59605598)
    (at 186.69 93.345 270)
    (descr "Capacitor 7.5mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 47nF (at 2.5 3.5 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D7.5_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 596055A1)
    (at 180.975 93.98 270)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at 4.445 0 360) (layer F.SilkS))
    (fp_text value 2.2uF (at 1 3.8 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 596055AE)
    (at 192.786 103.378 180)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D1 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value D (at 4.41452 -3.55854 180) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_THT:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 596055BD)
    (at 189.103 88.646)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D2 (at 5.08 0) (layer F.SilkS))
    (fp_text value D (at 4.41452 -3.55854) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 59605A85)
    (at 186.69 85.725 180)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D3 (at 1.27 -1.778 180) (layer F.SilkS))
    (fp_text value LED (at 1.524 -3.937 180) (layer F.Fab) hide)
    (fp_text user K (at -1.905 1.905 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_THT:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 59605A9B)
    (at 172.72 100.965)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.08 0) (layer F.SilkS) hide)
    (fp_text value 1K (at 5.08 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 59605ACA)
    (at 172.72 89.535)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 5.08 0) (layer F.SilkS) hide)
    (fp_text value 1K (at 5.08 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 59605656)
    (at 193.04 106.045 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 5.08 0 180) (layer F.SilkS) hide)
    (fp_text value 470 (at 5.08 3.81 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 59605512)
    (at 173.99 85.725 270)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV1 (at -1.651 -2.54 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.905 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 "Net-(R3-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "Net-(RV1-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 "Net-(RV1-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 5960555F)
    (at 179.07 104.775 90)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV2 (at -1.905 -2.54 180) (layer F.SilkS))
    (fp_text value 10K (at 1.27 5.08 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 "Net-(RV1-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 59605625)
    (at 191.135 98.425 90)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 3.81 90) (layer F.SilkS) hide)
    (fp_text value LM555N (at 3.81 10.01 90) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R3-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_Micro_SPST (layer F.Cu) (tedit 59605B6E)
    (at 176.276 95.25 90)
    (tags "Switch Micro SPST")
    (fp_text reference SW1 (at -2.667 2.032 90) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0.025 2.45 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 "Net-(SW1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 "Net-(BT1-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_Micro_SPST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.33 0.33 0.33))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Radial_D8_L13_P3.8 (layer F.Cu) (tedit 59608440)
    (at 196.342 104.267)
    (descr "Radial Electrolytic Capacitor Diameter 8mm x Length 13mm, Pitch 3.8mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C4 (at -2.667 -3.302) (layer F.SilkS))
    (fp_text value 470uF (at 1.9 5.3) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 3.8 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D8_L13_P3.8.wrl
      (at (xyz 0.0748031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 555_Adjustable_Blinking_LED:MakerLabNW_logo (layer B.Cu) (tedit 0)
    (at 188.214 94.234)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text On (at 173.99 91.567) (layer F.SilkS))
  (gr_text + (at 170.815 91.821 270) (layer F.SilkS))
  (gr_text GND (at 170.815 98.806 270) (layer F.SilkS))
  (gr_text 1K (at 177.165 89.535) (layer F.SilkS))
  (gr_text 1K (at 177.165 100.965) (layer F.SilkS))
  (gr_text 470 (at 187.96 106.045) (layer F.SilkS))
  (gr_text NE555 (at 194.945 94.615) (layer F.SilkS))
  (gr_line (start 201.93 82.55) (end 170.18 82.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 201.93 107.95) (end 201.93 82.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 107.95) (end 201.93 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 82.55) (end 170.18 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.93 107.95) (xy 170.18 107.95) (xy 170.18 82.55) (xy 201.93 82.55)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.93 107.95) (xy 170.18 107.95) (xy 170.18 82.55) (xy 201.93 82.55)
      )
    )
  )
)
