(kicad_pcb (version 20171130) (host pcbnew 5.0.1)
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 94)
    (zones 0)
    (modules 26)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.6 5.2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x310fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../grb"))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GNDREF)
  (net 3 -BATT)
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(C2-Pad2)")
  (net 6 "Net-(C1-Pad2)")
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(J1-PadR)")
  (net 9 "Net-(C3-Pad1)")
  (net 10 "Net-(J1-PadT)")
  (net 11 "Net-(BT1-Pad1)")
  (net 12 AMPLIFIED_RIGHT)
  (net 13 AMPLIFIED_LEFT)
  (net 14 IN_RIGHT)
  (net 15 IN_LEFT)
  (net 16 "Net-(J2-PadRN)")
  (net 17 "Net-(J2-PadTN)")
  (net 18 "Net-(J1-PadTN)")
  (net 19 "Net-(J1-PadRN)")
  (net 20 "Net-(D2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net -BATT)
    (add_net AMPLIFIED_LEFT)
    (add_net AMPLIFIED_RIGHT)
    (add_net GNDREF)
    (add_net IN_LEFT)
    (add_net IN_RIGHT)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-PadR)")
    (add_net "Net-(J1-PadRN)")
    (add_net "Net-(J1-PadT)")
    (add_net "Net-(J1-PadTN)")
    (add_net "Net-(J2-PadRN)")
    (add_net "Net-(J2-PadTN)")
  )
  (module Symbol:Symbol_KiCAD-Logo_CopperAndSilkScreenTop locked (layer B.Cu) (tedit 0)
    (at 195.58 71.12 270)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (attr virtual)
    (fp_text reference REF** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value "KiCAD Logo" (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 177.8 87.67 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C7 (at 4.405 0) (layer F.SilkS))
    (fp_text value 10u (at 1.25 2.05 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 190.5 90.17 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C8 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 10u (at 1.25 2.05 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 -BATT))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 177.8 97.79 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value green (at 1.27 3.96 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 177.8 101.6)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N5818-T (at 3.81 2.47) (layer F.Fab))
    (fp_text user %R (at 4.2 0) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.Fab))
    (fp_text user K (at -2.54 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 2 thru_hole oval (at 7.62 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 187.96 93.98)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1k (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 -BATT))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 176.53 80.01 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 75 (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 IN_LEFT))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 191.77 80.01 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 75 (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 IN_RIGHT))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 173.99 86.36 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 100k (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 AMPLIFIED_LEFT))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 194.31 86.36 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 100k (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 AMPLIFIED_RIGHT))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 180.34 97.79)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1k (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 -BATT))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 172.72 93.98)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1k (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Audio:3F07 (layer F.Cu) (tedit 5BC845A2)
    (at 199.39 105.41 180)
    (fp_text reference J1 (at 6.35 0 90) (layer F.SilkS))
    (fp_text value "Audio Out" (at 6 0 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 8.5 0 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.5 5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1 5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.5 -5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1 -5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad S thru_hole circle (at 3.5 0 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (pad R thru_hole circle (at 8.5 -5 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-PadR)"))
    (pad RN thru_hole circle (at 8.5 -2.5 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-PadRN)"))
    (pad TN thru_hole circle (at 8.5 2.5 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-PadTN)"))
    (pad T thru_hole circle (at 8.5 5 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-PadT)"))
  )
  (module Connector_Audio:3F07 (layer F.Cu) (tedit 5BC845A2)
    (at 184.15 63.5 270)
    (fp_text reference J2 (at 6.35 0) (layer F.SilkS))
    (fp_text value "Audio In" (at 6 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 8.5 0 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.5 5 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1 5 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.5 -5 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1 -5 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad S thru_hole circle (at 3.5 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (pad R thru_hole circle (at 8.5 -5 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 IN_RIGHT))
    (pad RN thru_hole circle (at 8.5 -2.5 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-PadRN)"))
    (pad TN thru_hole circle (at 8.5 2.5 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-PadTN)"))
    (pad T thru_hole circle (at 8.5 5 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 IN_LEFT))
  )
  (module Inductor_THT:L_Radial_D7.0mm_P3.00mm (layer F.Cu) (tedit 5BC844C1)
    (at 172.72 69.85 45)
    (descr "Inductor, Radial series, Radial, pin pitch=3.00mm, , diameter=7mm, http://www.abracon.com/Magnetics/radial/AIUR-16.pdf")
    (tags "Inductor Radial series Radial pin pitch 3.00mm  diameter 7mm")
    (fp_text reference L1 (at 6.286179 -0.898026 180) (layer F.SilkS))
    (fp_text value 10mH (at 1.5 4.75 45) (layer F.Fab))
    (fp_text user %R (at 1.5 0 45) (layer F.Fab))
    (pad 2 connect roundrect (at 3 0 45) (size 2.6 5.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(J2-PadTN)"))
    (pad 1 connect roundrect (at 0 0 45) (size 2.6 5.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDREF))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Radial_D7.0mm_P3.00mm.wrl
      (offset (xyz 0 2.6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Inductor_THT:L_Radial_D7.0mm_P3.00mm (layer F.Cu) (tedit 5BC844A7)
    (at 195.58 69.85 135)
    (descr "Inductor, Radial series, Radial, pin pitch=3.00mm, , diameter=7mm, http://www.abracon.com/Magnetics/radial/AIUR-16.pdf")
    (tags "Inductor Radial series Radial pin pitch 3.00mm  diameter 7mm")
    (fp_text reference L2 (at 6.286179 0.898026 180) (layer F.SilkS))
    (fp_text value 10mH (at 1.5 4.75 135) (layer F.Fab))
    (fp_text user %R (at 1.5 0 135) (layer F.Fab))
    (pad 1 connect roundrect (at 0 0 135) (size 2.6 5.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDREF))
    (pad 2 connect roundrect (at 3 0 135) (size 2.6 5.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(J2-PadRN)"))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Radial_D7.0mm_P3.00mm.wrl
      (offset (xyz 0 -2.6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Battery:BatteryHolder_Eagle_12BH611-GR (layer B.Cu) (tedit 5BC83EA3)
    (at 177.8 114.3 270)
    (descr https://eu.mouser.com/datasheet/2/209/EPD-200766-1274481.pdf)
    (tags "9V Battery Holder")
    (fp_text reference BT1 (at 0 -6.35) (layer B.SilkS))
    (fp_text value Battery (at 0 -6.35 180) (layer B.Fab))
    (fp_text user %R (at -2.95 -6.35 180) (layer B.Fab))
    (fp_text user - (at -7 0 270) (layer B.Fab))
    (fp_text user + (at -7 -12.7 270) (layer B.Fab))
    (pad "" np_thru_hole circle (at -24.15 -17.45 270) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -38.9 4.75 270) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -10.9 4.75 270) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 -12.7 180) (size 3 3) (drill 2.4) (layers *.Cu *.Mask)
      (net 3 -BATT))
    (pad 1 thru_hole circle (at 0 0 270) (size 3 3) (drill 2.4) (layers *.Cu *.Mask)
      (net 11 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Bulgin_Eagle_12BH611-GR.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 176.53 82.55 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at 0 -1.905 90) (layer F.SilkS))
    (fp_text value 10p (at 1.25 2.05 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 AMPLIFIED_LEFT))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 191.77 82.55 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C2 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 10p (at 1.25 2.05 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 AMPLIFIED_RIGHT))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 182.88 90.13 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C3 (at -1.945 0 180) (layer F.SilkS))
    (fp_text value 10u (at 1.25 2.05 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 AMPLIFIED_LEFT))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 185.42 90.13 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C4 (at -1.945 0 180) (layer F.SilkS))
    (fp_text value 10u (at 1.25 2.05 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 AMPLIFIED_RIGHT))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 180.34 87.63 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C5 (at 4.445 0) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.05 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 187.96 90.13 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C6 (at -1.945 0 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.05 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 -BATT))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 187.96 83.82 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U1 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value AS358P-E1 (at 3.81 9.95 180) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 180) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 -BATT))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 AMPLIFIED_LEFT))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 AMPLIFIED_RIGHT))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Alps_RK097_Dual_Horizontal_Switch (layer F.Cu) (tedit 5B1588C6)
    (at 176.57 105.41 180)
    (descr "Potentiometer, horizontal, Alps RK097 Dual, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK097/RK097_list.html")
    (tags "Potentiometer horizontal Alps RK097 Dual")
    (fp_text reference RV1 (at -6.31 -2.54 270) (layer F.SilkS))
    (fp_text value 10k (at 0 3.5 180) (layer F.Fab))
    (fp_text user %R (at 0.225 -2.5 180) (layer F.Fab))
    (pad 4 thru_hole circle (at -2.5 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 5 thru_hole circle (at -2.5 -2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-PadR)"))
    (pad 6 thru_hole circle (at -2.5 -5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-PadT)"))
    (pad 3 thru_hole circle (at 0 -5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDREF))
    (pad 8 thru_hole circle (at -8.75 -5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(BT1-Pad1)"))
    (pad 7 thru_hole circle (at -8.75 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK097_Dual_Horizontal_Switch.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_Copper locked (layer F.Cu) (tedit 0)
    (at 172.085 113.03 90)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_Copper (at 0.75 0 90) (layer F.Fab) hide)
  )
  (gr_text v0.1 (at 197.485 73.66 90) (layer F.Mask))
  (gr_text v0.1 (at 194.31 68.58 270) (layer F.Mask))
  (gr_text MicroFlux (at 197.485 81.915 90) (layer F.SilkS))
  (gr_text github.com/FOSHSolderKits (at 170.5 86.36 90) (layer F.SilkS))
  (gr_line (start 171.45 116.84) (end 196.85 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 171.45 114.3) (end 168.91 114.3) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 66.04) (end 168.91 114.3) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 171.45 66.04) (end 171.45 63.5) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.85 63.5) (end 171.45 63.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 196.85 66.04) (end 199.39 66.04) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.39 114.3) (end 199.39 66.04) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 196.85 114.3) (end 196.85 116.84) (angle -90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 60.96) (xy 200.66 60.96) (xy 200.66 119.38) (xy 167.64 119.38)
      )
    )
  )
  (zone (net 2) (net_name GNDREF) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 62.23) (xy 201.93 62.23) (xy 201.93 118.11) (xy 166.37 118.11)
      )
    )
  )
)
