(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3.3V")
  (net 2 "+5V")
  (net 3 "/ANALOG_IN")
  (net 4 "/FWD_LIM_SW")
  (net 5 "unconnected-(J500-Pad5)")
  (net 6 "/ALT_ENC_A")
  (net 7 "unconnected-(J500-Pad7)")
  (net 8 "/RVS_LIM_SW")
  (net 9 "unconnected-(J500-Pad9)")
  (net 10 "GND")
  (net 11 "Net-(LED3-Pad2)")
  (net 12 "Net-(P1-Pad2)")
  (net 13 "Net-(P2-Pad2)")
  (net 14 "Net-(LED5-Pad1)")
  (footprint "Library Loader:0015912045" locked (layer "F.Cu")
    (tedit 0)
    (at 174.177 103.215 90)
    (descr "0015912045-2")
    (tags "Connector")
    (property "Arrow Part Number" "0015912045")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/0015912045/molex")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "0015912045")
    (property "Mouser Part Number" "N/A")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=N%2FA")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P2" (at 8.015 -7.877 180) (layer "F.SilkS"))
    (fp_text value "0015912045" (at 0 -1.853 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -1.853 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 5.21 3.195 90) (size 3.81 3.81) (drill 3.81) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -5.21 3.195 90) (size 3.81 3.81) (drill 3.81) (layers *.Cu *.Mask))
    (pad "1" smd rect locked (at 3.81 -7.495 90) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.27 -7.495 90) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(P2-Pad2)") (pintype "passive"))
    (pad "3" smd rect locked (at -1.27 -7.495 90) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/FWD_LIM_SW") (pintype "passive"))
    (pad "4" smd rect locked (at -3.81 -7.495 90) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/RVS_LIM_SW") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\0015912045.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 144.347714 90.3)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "MH1" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.7 121.1)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at -3 -0.7) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 2 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 12 "Net-(P1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 140.925 123.2)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Description" "Lite-On LTST-C190KGKT, 571 nm Green LED, 1608 (0603) SMD package")
    (property "Height" "0.8")
    (property "Manufacturer_Name" "Lite-On")
    (property "Manufacturer_Part_Number" "LTST-C190KGKT")
    (property "Mouser Part Number" "859-LTST-C190KGKT")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Lite-On/LTST-C190KGKT?qs=205qCy6M2Q%252BAdcgwUZktqw%3D%3D")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "LED3" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "LTST-C190KGKT" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(LED3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 140.725 97.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Description" "Lite-On LTST-C190KGKT, 571 nm Green LED, 1608 (0603) SMD package")
    (property "Height" "0.8")
    (property "Manufacturer_Name" "Lite-On")
    (property "Manufacturer_Part_Number" "LTST-C190KGKT")
    (property "Mouser Part Number" "859-LTST-C190KGKT")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Lite-On/LTST-C190KGKT?qs=205qCy6M2Q%252BAdcgwUZktqw%3D%3D")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "LED5" (at -0.025 -1.5) (layer "F.SilkS"))
    (fp_text value "LTST-C190KGKT" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(LED5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.7 121.1 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at -1.4 1.7) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 12 "Net-(P1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.9875 97.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 3.0905 0.14) (layer "F.SilkS"))
    (fp_text value "301" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(LED5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:15917050" (layer "F.Cu")
    (tedit 0)
    (at 144.305 110.4 -90)
    (descr "15-91-7050-2")
    (tags "Connector")
    (property "Arrow Part Number" "")
    (property "Arrow Price/Stock" "")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7050")
    (property "Mouser Part Number" "538-15-91-7050")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Molex/15-91-7050?qs=9GkFbIK8PKA0zLwr%2FmKOQQ%3D%3D")
    (property "Mouser Testing Part Number" "")
    (property "Mouser Testing Price/Stock" "")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at -9 -7.995 180) (layer "F.SilkS"))
    (fp_text value "15-91-7050" (at 0 -1.333 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -1.333 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 6.48 3.195 270) (size 3.76 3.76) (drill 3.76) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.48 3.195 270) (size 3.76 3.76) (drill 3.76) (layers *.Cu *.Mask))
    (pad "1" smd rect (at 5.08 -7.495 270) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 2.54 -7.495 270) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(P1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 0 -7.495 270) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/FWD_LIM_SW") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -2.54 -7.495 270) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/ALT_ENC_A") (pinfunction "4") (pintype "passive"))
    (pad "5" smd rect (at -5.08 -7.495 270) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/RVS_LIM_SW") (pinfunction "5") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\15-91-7050.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.9 96.4 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0.9 -1.6 90) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 13 "Net-(P2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 1 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 168.447 130.4)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "MH2" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 144.8125 123.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0.7125 1.5) (layer "F.SilkS"))
    (fp_text value "137" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(LED3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160 101 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -2.3 0.6 180) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/FWD_LIM_SW") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:15912035" (layer "F.Cu")
    (tedit 0)
    (at 177.4 119.24 90)
    (descr "15-91-2035-3")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "P3" (at 6.34 -11.2 180) (layer "F.SilkS"))
    (fp_text value "15912035" (at 0 -4.898 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -4.898 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -3.94 0 90) (size 3.81 3.81) (drill 3.81) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.94 0 90) (size 3.81 3.81) (drill 3.81) (layers *.Cu *.Mask))
    (pad "1" smd rect (at 2.54 -10.69 90) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0 -10.69 90) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "3" smd rect (at -2.54 -10.69 90) (size 1.65 5.33) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/ANALOG_IN") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\15-91-2035.stp"
      (offset (xyz 0 2.229999986 2.950000003))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 157.8 95.4)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at -2.7 -0.7) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 2 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 13 "Net-(P2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 144.347714 90.3 180)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers F&B.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.9 101.8875 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -1.3875 1.5 180) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/RVS_LIM_SW") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:M503110542" (layer "B.Cu")
    (tedit 0)
    (at 157.76 100.0875 -90)
    (descr "M50-3110542-2")
    (tags "Connector")
    (property "Description" "Headers & Wire Housings 5+5 DIL SMT SKT WITH POST")
    (property "Height" "4.85")
    (property "Manufacturer_Name" "Harwin")
    (property "Manufacturer_Part_Number" "M50-3110542")
    (property "Mouser Part Number" "855-M50-3110542")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Harwin/M50-3110542?qs=9fQaSFfsqszB0q9gosr4Mg%3D%3D")
    (property "Sheetfile" "4272SparkMaxBreakout_R2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J500" (at 3.3125 1.06 180) (layer "B.SilkS"))
    (fp_text value "M50-3110542" (at 0.073 0 90) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 11.982 1.36 90) (layer "B.Fab") hide)
    (pad "" np_thru_hole circle (at 6.1125 1.36 90) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 14.3525 1.36 90) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad "1" smd rect (at 12.7725 -1.145 90) (size 0.74 2.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd rect (at 12.7725 3.865 90) (size 0.74 2.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "+5V") (pintype "passive"))
    (pad "3" smd rect (at 11.5025 -1.145 90) (size 0.74 2.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/ANALOG_IN") (pintype "passive"))
    (pad "4" smd rect (at 11.5025 3.865 90) (size 0.74 2.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "/FWD_LIM_SW") (pintype "passive"))
    (pad "5" smd rect (at 10.2325 -1.145 90) (size 0.74 2.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "unconnected-(J500-Pad5)") (pintype "passive"))
    (pad "6" smd rect (at 10.2325 3.865 90) (size 0.74 2.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "/ALT_ENC_A") (pintype "passive"))
    (pad "7" smd rect (at 8.9625 -1.145 90) (size 0.74 2.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "unconnected-(J500-Pad7)") (pintype "passive"))
    (pad "8" smd rect (at 8.9625 3.865 90) (size 0.74 2.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/RVS_LIM_SW") (pintype "passive"))
    (pad "9" smd rect (at 7.6925 -1.145 90) (size 0.74 2.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "unconnected-(J500-Pad9)") (pintype "passive"))
    (pad "10" smd rect (at 7.6925 3.865 90) (size 0.74 2.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "GND") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\M50-3110542.stp"
      (offset (xyz -2.539999924 0 4.599999836))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
  )
  (gr_line (start 171.9 127) (end 180.6 127) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 140.7 93.3) (end 137.8 93.3) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 140.7 90.3) (mid 144.4 86.6) (end 148.1 90.3) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 171.899993 130.4) (end 171.9 127) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 137.8 93.3) (end 138 127) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 180.6 127) (end 180.6 93.3) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 171.899993 130.4) (mid 168.4 133.899993) (end 164.900007 130.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 148.1 90.3) (end 148 93.3) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138 127) (end 164.9 127) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 140.7 90.3) (end 140.7 93.3) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 180.6 93.3) (end 148 93.3) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 164.900007 130.4) (end 164.9 127) (layer "Edge.Cuts") (width 0.1))
  (gr_text "Maverick Robotics \n4272" (at 160.1 113.7 90) (layer "F.SilkS"))
  (gr_text "5V" (at 153 94.8) (layer "F.SilkS"))
  (gr_text "3.3V" (at 154.4 122.9) (layer "F.SilkS"))
  (gr_text "BLD DATE 2023" (at 145.3 125.4) (layer "F.SilkS"))
  (gr_text "5V\n" (at 149.5 122.9) (layer "F.SilkS"))
  (gr_text "3.3V" (at 161.9 96.7 90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "User.2")
    (pts (xy 139.1 96.7) (xy 137.9 96.7))
    (height -2.9)
    (gr_text "0.0472 in" (at 138.5 98.45) (layer "User.2"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.2")
    (pts (xy 139.2 122.2) (xy 138 122.2))
    (height -2.9)
    (gr_text "0.0472 in" (at 138.6 123.95) (layer "User.2"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.2")
    (pts (xy 135 117.6) (xy 137.9 117.6))
    (height 0)
    (gr_text "0.1142 in" (at 136.45 116.45) (layer "User.2"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 1) (net_name "+3.3V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.4 126.7)
        (xy 138.2 126.7)
        (xy 138.2 94)
        (xy 180.4 94)
      )
    )
  )
  (zone (net 10) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.4 126.743)
        (xy 138.194 126.743)
        (xy 138.194 93.977)
        (xy 180.4 93.977)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.5 113.6)
        (xy 155.3 113.584862)
        (xy 155.3 107)
        (xy 157.5 107)
      )
    )
  )
)
