(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu14.04.1)
  (general
    (links 2)
    (no_connects 0)
    (area 85.824287 66.515 173.890715 132.24)
    (thickness 1.6)
    (drawings 24)
    (tracks 4)
    (zones 0)
    (modules 5)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.048 3.048)
    (pad_drill 2.032)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1.27)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P2-Pad1)")
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A12BC52)
    (at 125.222 90.17)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P3 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 3.048 3.048) (drill oval 2.032) (layers *.Cu *.Mask)
      (net 2 "Net-(P2-Pad1)"))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A12BC5B)
    (at 104.775 90.17)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P4 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 4.064 4.064) (drill oval 3.048) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_2.7mm (layer F.Cu) (tedit 5A12BCB1)
    (at 111.76 117.475)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference MH (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 1.6256 4.572) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Connectors:PINTST (layer F.Cu) (tedit 5A12BC41)
    (at 104.775 79.375)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P1 (at 0 -1.26746) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST (layer F.Cu) (tedit 5A12BC4A)
    (at 130.175 104.775)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P2 (at 0 -1.26746) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 2 "Net-(P2-Pad1)"))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 20.447 (width 0.3) (layer Dwgs.User)
    (gr_text "0.8050 in" (at 114.9985 83.867) (layer Dwgs.User))
    (feature1 (pts (xy 125.222 88.646) (xy 125.222 82.517)))
    (feature2 (pts (xy 104.775 88.646) (xy 104.775 82.517)))
    (crossbar (pts (xy 104.775 85.217) (xy 125.222 85.217)))
    (arrow1a (pts (xy 125.222 85.217) (xy 124.095496 85.803421)))
    (arrow1b (pts (xy 125.222 85.217) (xy 124.095496 84.630579)))
    (arrow2a (pts (xy 104.775 85.217) (xy 105.901504 85.803421)))
    (arrow2b (pts (xy 104.775 85.217) (xy 105.901504 84.630579)))
  )
  (gr_text "CDT 2017" (at 121.92 117.475) (layer F.SilkS))
  (gr_text "Harris CPU606\nBattery holder" (at 117.475 111.125) (layer F.SilkS))
  (dimension 6.985 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2750 in" (at 108.2675 107.235) (layer Dwgs.User))
    (feature1 (pts (xy 111.76 111.76) (xy 111.76 105.885)))
    (feature2 (pts (xy 104.775 111.76) (xy 104.775 105.885)))
    (crossbar (pts (xy 104.775 108.585) (xy 111.76 108.585)))
    (arrow1a (pts (xy 111.76 108.585) (xy 110.633496 109.171421)))
    (arrow1b (pts (xy 111.76 108.585) (xy 110.633496 107.998579)))
    (arrow2a (pts (xy 104.775 108.585) (xy 105.901504 109.171421)))
    (arrow2b (pts (xy 104.775 108.585) (xy 105.901504 107.998579)))
  )
  (gr_text - (at 129.159 89.408) (layer F.SilkS))
  (gr_text - (at 130.6322 90.9828) (layer F.SilkS))
  (gr_text + (at 104.775 94.234) (layer F.SilkS))
  (gr_text CR2477 (at 116.713 78.994) (layer F.SilkS))
  (dimension 25.4 (width 0.3) (layer Cmts.User)
    (gr_text "1.0000 in" (at 117.475 101.045) (layer Cmts.User))
    (feature1 (pts (xy 130.175 98.425) (xy 130.175 102.395)))
    (feature2 (pts (xy 104.775 98.425) (xy 104.775 102.395)))
    (crossbar (pts (xy 104.775 99.695) (xy 130.175 99.695)))
    (arrow1a (pts (xy 130.175 99.695) (xy 129.048496 100.281421)))
    (arrow1b (pts (xy 130.175 99.695) (xy 129.048496 99.108579)))
    (arrow2a (pts (xy 104.775 99.695) (xy 105.901504 100.281421)))
    (arrow2b (pts (xy 104.775 99.695) (xy 105.901504 99.108579)))
  )
  (dimension 25.4 (width 0.3) (layer Cmts.User)
    (gr_text "1.0000 in" (at 143.59 92.075 270) (layer Cmts.User))
    (feature1 (pts (xy 133.35 104.775) (xy 144.94 104.775)))
    (feature2 (pts (xy 133.35 79.375) (xy 144.94 79.375)))
    (crossbar (pts (xy 142.24 79.375) (xy 142.24 104.775)))
    (arrow1a (pts (xy 142.24 104.775) (xy 141.653579 103.648496)))
    (arrow1b (pts (xy 142.24 104.775) (xy 142.826421 103.648496)))
    (arrow2a (pts (xy 142.24 79.375) (xy 141.653579 80.501504)))
    (arrow2b (pts (xy 142.24 79.375) (xy 142.826421 80.501504)))
  )
  (dimension 41.275 (width 0.3) (layer Cmts.User)
    (gr_text "1.6250 in" (at 91.36 100.0125 270) (layer Cmts.User))
    (feature1 (pts (xy 101.6 120.65) (xy 90.01 120.65)))
    (feature2 (pts (xy 101.6 79.375) (xy 90.01 79.375)))
    (crossbar (pts (xy 92.71 79.375) (xy 92.71 120.65)))
    (arrow1a (pts (xy 92.71 120.65) (xy 92.123579 119.523496)))
    (arrow1b (pts (xy 92.71 120.65) (xy 93.296421 119.523496)))
    (arrow2a (pts (xy 92.71 79.375) (xy 92.123579 80.501504)))
    (arrow2b (pts (xy 92.71 79.375) (xy 93.296421 80.501504)))
  )
  (dimension 3.175 (width 0.3) (layer Cmts.User)
    (gr_text "0.1250 in" (at 103.1875 130.889999) (layer Cmts.User))
    (feature1 (pts (xy 104.775 107.95) (xy 104.775 132.239999)))
    (feature2 (pts (xy 101.6 107.95) (xy 101.6 132.239999)))
    (crossbar (pts (xy 101.6 129.539999) (xy 104.775 129.539999)))
    (arrow1a (pts (xy 104.775 129.539999) (xy 103.648496 130.12642)))
    (arrow1b (pts (xy 104.775 129.539999) (xy 103.648496 128.953578)))
    (arrow2a (pts (xy 101.6 129.539999) (xy 102.726504 130.12642)))
    (arrow2b (pts (xy 101.6 129.539999) (xy 102.726504 128.953578)))
  )
  (dimension 12.7 (width 0.3) (layer Cmts.User)
    (gr_text "0.5000 in" (at 149.305 114.3 90) (layer Cmts.User))
    (feature1 (pts (xy 130.175 107.95) (xy 150.655 107.95)))
    (feature2 (pts (xy 130.175 120.65) (xy 150.655 120.65)))
    (crossbar (pts (xy 147.955 120.65) (xy 147.955 107.95)))
    (arrow1a (pts (xy 147.955 107.95) (xy 148.541421 109.076504)))
    (arrow1b (pts (xy 147.955 107.95) (xy 147.368579 109.076504)))
    (arrow2a (pts (xy 147.955 120.65) (xy 148.541421 119.523496)))
    (arrow2b (pts (xy 147.955 120.65) (xy 147.368579 119.523496)))
  )
  (dimension 44.45 (width 0.3) (layer Cmts.User)
    (gr_text "1.7500 in" (at 168.355 98.425 90) (layer Cmts.User))
    (feature1 (pts (xy 130.175 76.2) (xy 169.705 76.2)))
    (feature2 (pts (xy 130.175 120.65) (xy 169.705 120.65)))
    (crossbar (pts (xy 167.005 120.65) (xy 167.005 76.2)))
    (arrow1a (pts (xy 167.005 76.2) (xy 167.591421 77.326504)))
    (arrow1b (pts (xy 167.005 76.2) (xy 166.418579 77.326504)))
    (arrow2a (pts (xy 167.005 120.65) (xy 167.591421 119.523496)))
    (arrow2b (pts (xy 167.005 120.65) (xy 166.418579 119.523496)))
  )
  (dimension 31.75 (width 0.3) (layer Cmts.User)
    (gr_text "1.2500 in" (at 117.475 67.865) (layer Cmts.User))
    (feature1 (pts (xy 133.35 76.2) (xy 133.35 66.515)))
    (feature2 (pts (xy 101.6 76.2) (xy 101.6 66.515)))
    (crossbar (pts (xy 101.6 69.215) (xy 133.35 69.215)))
    (arrow1a (pts (xy 133.35 69.215) (xy 132.223496 69.801421)))
    (arrow1b (pts (xy 133.35 69.215) (xy 132.223496 68.628579)))
    (arrow2a (pts (xy 101.6 69.215) (xy 102.726504 69.801421)))
    (arrow2b (pts (xy 101.6 69.215) (xy 102.726504 68.628579)))
  )
  (gr_line (start 101.6 107.95) (end 101.6 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.775 107.95) (end 101.6 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.775 120.65) (end 104.775 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.175 120.65) (end 104.775 120.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.175 107.95) (end 130.175 120.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 107.95) (end 130.175 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 76.2) (end 133.35 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 76.2) (end 133.35 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(P2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 107.95) (xy 101.6 107.95) (xy 101.6 76.2) (xy 133.35 76.2)
      )
    )
  )
  (zone (net 2) (net_name "Net-(P2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 107.95) (xy 101.6 107.95) (xy 101.6 76.2) (xy 133.35 76.2)
      )
    )
  )
)
