(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 329)
    (zones 0)
    (modules 40)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.154)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.635)
    (user_trace_width 1.5)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.15)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.381)
    (user_via 1.27 0.635)
    (uvia_size 0.381)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 4)
    (pad_drill 2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 SDA)
  (net 4 SCL)
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 "Net-(D3-Pad2)")
  (net 10 "Net-(FB1-Pad2)")
  (net 11 "Net-(J1-Pad2)")
  (net 12 "Net-(J2-Pad1)")
  (net 13 "Net-(J2-Pad2)")
  (net 14 "Net-(J2-Pad3)")
  (net 15 "Net-(R3-Pad1)")
  (net 16 "Net-(R6-Pad2)")
  (net 17 "Net-(R7-Pad1)")
  (net 18 +2V8)
  (net 19 "Net-(C6-Pad1)")
  (net 20 SCL_2V8)
  (net 21 SDA_2V8)
  (net 22 "Net-(JP1-Pad2)")
  (net 23 +5V)
  (net 24 GPO)
  (net 25 GPI)
  (net 26 "Net-(JP2-Pad2)")
  (net 27 "Net-(JP3-Pad2)")
  (net 28 "Net-(JP4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.381)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net +2V8)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net GPI)
    (add_net GPO)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(FB1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(JP4-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net SCL)
    (add_net SCL_2V8)
    (add_net SDA)
    (add_net SDA_2V8)
  )
  (net_class Minimum ""
    (clearance 0.154)
    (trace_width 0.154)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
  )
  (net_class Power ""
    (clearance 0.635)
    (trace_width 1.27)
    (via_dia 0.635)
    (via_drill 0.508)
    (uvia_dia 0.381)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x07_P2.54mm_Vertical (layer B.Cu) (tedit 5EC7F998)
    (at 161.29 93.98 180)
    (descr "Through hole straight socket strip, 1x07, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x07 2.54mm single row")
    (fp_text reference S42 (at -0.127 -17.272 180) (layer B.SilkS))
    (fp_text value VL53LnX (at 0 -18.01 180) (layer B.Fab))
    (fp_text user %R (at 0 -7.62 90) (layer B.Fab))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KIPRJMOD}/Adafruit_VL53L0X.step
      (offset (xyz 0 0 2.54))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5EC7F900)
    (at 132.969 97.028)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 3.048 0) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 22 "Net-(JP1-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 2 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5EC7F8E1)
    (at 132.969 100.076 180)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 4.699 0 180) (layer B.SilkS))
    (fp_text value SolderJumper_3_Bridged12 (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd custom (at -1.3 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)) (width 0))
      ))
    (pad 2 smd rect (at 0 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 26 "Net-(JP2-Pad2)"))
    (pad 3 smd custom (at 1.3 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 4 SCL) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy -0.55 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5EC7F8D0)
    (at 133.604 105.791 180)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP4 (at 3.429 -0.889 180) (layer B.SilkS))
    (fp_text value SolderJumper_3_Bridged12 (at 0 -1.9 180) (layer B.Fab) hide)
    (pad 1 smd custom (at -1.3 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)) (width 0))
      ))
    (pad 2 smd rect (at 0 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 28 "Net-(JP4-Pad2)"))
    (pad 3 smd custom (at 1.3 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 3 SDA) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy -0.55 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5EC7F8B8)
    (at 133.604 103.759)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at -3.429 -0.254) (layer B.SilkS))
    (fp_text value SolderJumper_3_Bridged12 (at 0 -1.9) (layer B.Fab) hide)
    (pad 1 smd custom (at -1.3 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 3 SDA) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)) (width 0))
      ))
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 27 "Net-(JP3-Pad2)"))
    (pad 3 smd custom (at 1.3 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy -0.55 -0.75)) (width 0))
      ))
  )
  (module Connector_Phoenix_MC_HighVoltage:PhoenixContact_MC_1,5_2-G-5.08_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5EC7F6A1)
    (at 112.522 108.204)
    (descr "Generic Phoenix Contact connector footprint for: MC_1,5/2-G-5.08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1836189 8A 320V")
    (tags "phoenix_contact connector MC_01x02_G_5.08mm")
    (fp_text reference J1 (at -3.937 2.921) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 2.54 9.2) (layer F.Fab))
    (fp_text user %R (at 2.54 -0.5) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 3.5 4) (drill 2) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 1 thru_hole oval (at 0 0) (size 3.5 4) (drill 2) (layers *.Cu *.Mask)
      (net 10 "Net-(FB1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC_HighVoltage.3dshapes/PhoenixContact_MC_1,5_2-G-5.08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MC_HighVoltage:PhoenixContact_MC_1,5_3-G-5.08_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5EC7F670)
    (at 172.212 108.204)
    (descr "Generic Phoenix Contact connector footprint for: MC_1,5/3-G-5.08; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1836192 8A 320V")
    (tags "phoenix_contact connector MC_01x03_G_5.08mm")
    (fp_text reference J2 (at -4.445 3.175) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 5.08 9.2) (layer F.Fab))
    (fp_text user %R (at 5.08 -0.5) (layer F.Fab))
    (pad 3 thru_hole oval (at 10.16 0) (size 3.5 4) (drill 2) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 3.5 4) (drill 2) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (pad 1 thru_hole oval (at 0 0) (size 3.5 4) (drill 2) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC_HighVoltage.3dshapes/PhoenixContact_MC_1,5_3-G-5.08_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-39-8_Window (layer B.Cu) (tedit 5EC7F1C2)
    (at 140.97 101.6 315)
    (descr "TO-39-8_Window, Window")
    (tags "TO-39-8_Window Window")
    (fp_text reference S1 (at -0.449013 -5.837166) (layer B.SilkS))
    (fp_text value 917-47-208-41-005000 (at 0.000001 -5.82 315) (layer B.Fab))
    (fp_text user %R (at 0.000001 5.82 315) (layer B.Fab))
    (pad 8 thru_hole oval (at -2.064752 2.064752 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 7 thru_hole oval (at 0 2.92 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 "Net-(JP3-Pad2)"))
    (pad 6 thru_hole oval (at 2.064752 2.064752 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 2.92 0 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 "Net-(JP4-Pad2)"))
    (pad 4 thru_hole oval (at 2.064752 -2.064752 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 3 thru_hole oval (at 0 -2.92 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 "Net-(JP1-Pad2)"))
    (pad 2 thru_hole oval (at -2.064752 -2.064752 315) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at -2.92 0 315) (size 1.6 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 26 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-39-8_Window.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/MLX90614ESF-DAA-000-TU--3DModel-STEP-56544.STEP
      (offset (xyz 0 0 4.3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
    (model ${KIPRJMOD}/mill-max-P917-47-208-41-005000.step
      (offset (xyz 0 0 2.8))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module MountingHole:MountingHole_4.3x6.2mm_M4_Pad_Via (layer F.Cu) (tedit 581E29B6)
    (at 191.643 95.25)
    (descr "Mounting Hole 4.3x6.2mm, M4")
    (tags "mounting hole 4.3x6.2mm m4")
    (attr virtual)
    (fp_text reference H1 (at 0 -5.3) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.801 -1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.801 -1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -4.15 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.801 1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 3.801 1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 4.15 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.505 -3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.92 -2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.92 2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.92 2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.92 -2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.505 -3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.505 3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.505 3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0) (size 10.4 8.6) (drill oval 6.2 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_4.3x6.2mm_M4_Pad_Via (layer F.Cu) (tedit 581E29B6)
    (at 102.87 107.95)
    (descr "Mounting Hole 4.3x6.2mm, M4")
    (tags "mounting hole 4.3x6.2mm m4")
    (attr virtual)
    (fp_text reference H3 (at 0 -5.3) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.801 -1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.801 -1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -4.15 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.801 1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 3.801 1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 4.15 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.505 -3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.92 -2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.92 2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.92 2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.92 -2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.505 -3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.505 3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.505 3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0) (size 10.4 8.6) (drill oval 6.2 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_4.3x6.2mm_M4_Pad_Via (layer F.Cu) (tedit 581E29B6)
    (at 191.77 107.95)
    (descr "Mounting Hole 4.3x6.2mm, M4")
    (tags "mounting hole 4.3x6.2mm m4")
    (attr virtual)
    (fp_text reference H2 (at 0 -5.3) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.801 -1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.801 -1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -4.15 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.801 1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 3.801 1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 4.15 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.505 -3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.92 -2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.92 2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.92 2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.92 -2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.505 -3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.505 3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.505 3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0) (size 10.4 8.6) (drill oval 6.2 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_4.3x6.2mm_M4_Pad_Via (layer F.Cu) (tedit 581E29B6)
    (at 102.87 95.25)
    (descr "Mounting Hole 4.3x6.2mm, M4")
    (tags "mounting hole 4.3x6.2mm m4")
    (attr virtual)
    (fp_text reference H6 (at 0 -5.3) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.801 -1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.801 -1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -4.15 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.801 1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 3.801 1.45) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 4.15 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.505 -3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.92 -2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.92 2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.92 2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.92 -2.521) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.505 -3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.505 3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.505 3.151) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0) (size 10.4 8.6) (drill oval 6.2 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer B.Cu) (tedit 58641869)
    (at 176.276 96.647 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at -3.429 0.127) (layer B.SilkS))
    (fp_text value D (at 0.1 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 1.85) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 23 +5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 169.545 93.218)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -3.175 0.127) (layer B.SilkS))
    (fp_text value R (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 24 GPO))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 5A0AB76C)
    (at 176.53 94.107)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 3.81 -0.127) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 24 GPO))
    (pad 1 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module teensy:Teensy30_31_32_LC (layer F.Cu) (tedit 5EC71868)
    (at 141.605 101.6)
    (fp_text reference U1 (at -20.828 -5.588) (layer F.SilkS) hide)
    (fp_text value Teensy-LC (at 0 10.16) (layer F.Fab))
    (fp_text user Vin (at -18.288 -7.62 90) (layer F.SilkS))
    (fp_text user GND (at -13.97 -2.54 90) (layer F.SilkS))
    (fp_text user 3V3 (at -10.668 -5.08 90) (layer F.SilkS))
    (fp_text user 23 (at -9.525 -5.715 90) (layer F.SilkS) hide)
    (fp_text user 20 (at -1.27 -5.08 90) (layer F.SilkS))
    (fp_text user 19 (at 1.27 -5.08 90) (layer F.SilkS))
    (fp_text user 18 (at 3.81 -5.08 90) (layer F.SilkS))
    (fp_text user 17 (at 6.35 -5.08 90) (layer F.SilkS))
    (fp_text user 16 (at 8.89 -5.08 90) (layer F.SilkS) hide)
    (fp_text user 15 (at 11.43 -5.08 90) (layer F.SilkS) hide)
    (fp_text user 14 (at 13.97 -5.08 90) (layer F.SilkS) hide)
    (fp_text user 2 (at -8.89 5.08 90) (layer F.SilkS) hide)
    (fp_text user 7 (at 3.81 5.08 90) (layer F.SilkS))
    (fp_text user 6 (at 1.27 5.08 90) (layer F.SilkS))
    (fp_text user 4 (at -3.81 5.08 90) (layer F.SilkS))
    (fp_text user 5 (at -1.27 5.08 90) (layer F.SilkS))
    (fp_text user 8 (at 6.35 5.08 90) (layer F.SilkS))
    (fp_text user 3 (at -6.35 5.08 270) (layer F.SilkS) hide)
    (fp_text user 9 (at 8.89 5.08 90) (layer F.SilkS))
    (fp_text user 1 (at -11.43 5.08 90) (layer F.SilkS))
    (fp_text user 0 (at -13.97 5.08 90) (layer F.SilkS))
    (fp_text user GND (at -16.51 5.08 90) (layer F.SilkS))
    (pad 1 thru_hole roundrect (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GPI))
    (pad 3 thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 +5V))
    (pad 32 thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 30 thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 29 thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 25 thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 24 thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 GPO))
    (pad 20 thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/Teensy-LC-StdPins.step
      (offset (xyz -18.321 -9.430999999999999 2.54))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module temp_screen_pcb:VL53L0CXV0DH_1 (layer B.Cu) (tedit 5EC716F6)
    (at 153.67 101.6)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/group3/b2/1e/33/77/c6/92/47/6b/DM00279086/files/DM00279086.pdf/jcr:content/translations/en.DM00279086.pdf)
    (attr smd)
    (fp_text reference S41 (at 1.397 -2.286) (layer B.SilkS))
    (fp_text value VL53L0CXV0DH_1 (at 0 -2.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 12 smd rect (at -1.6 0) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.6 0.8) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 18 +2V8))
    (pad 2 smd rect (at -0.8 0.8) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 0.8) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.8 0.8) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.6 0.8) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(R7-Pad1)"))
    (pad 6 smd rect (at 1.6 0) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 1.6 -0.8) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 0.8 -0.8) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 0 -0.8) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 21 SDA_2V8))
    (pad 10 smd rect (at -0.8 -0.8) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 20 SCL_2V8))
    (pad 11 smd rect (at -1.6 -0.8) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 18 +2V8))
    (pad 1 smd rect (at -1.89 0.675) (size 0.08 0.25) (layers B.Cu B.Paste B.Mask)
      (net 18 +2V8))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-14_3x5mm_P0.8mm_LayoutBorder1x6y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Package_SO:SO-4_4.4x3.6mm_P2.54mm (layer B.Cu) (tedit 5B1E4C51)
    (at 120.396 103.632)
    (descr "4-Lead Plastic Small Outline (SO), see https://www.elpro.org/de/index.php?controller=attachment&id_attachment=339")
    (tags "SO SOIC 2.54")
    (attr smd)
    (fp_text reference U3 (at 1.27 2.794) (layer B.SilkS))
    (fp_text value LTV-356T (at 0 -2.8) (layer B.Fab))
    (fp_text user %R (at 0 0.065) (layer B.Fab))
    (pad 4 smd rect (at 3.15 1.27) (size 2 0.64) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(R6-Pad2)"))
    (pad 3 smd rect (at 3.15 -1.27) (size 2 0.64) (layers B.Cu B.Paste B.Mask)
      (net 25 GPI))
    (pad 2 smd rect (at -3.15 -1.27) (size 2 0.64) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(R3-Pad1)"))
    (pad 1 smd rect (at -3.15 1.27) (size 2 0.64) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-4_4.4x3.6mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 149.225 104.14 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 3.048 -1.016) (layer B.SilkS))
    (fp_text value 4.7u (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 18 +2V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5_HandSoldering (layer B.Cu) (tedit 5A0AB76C)
    (at 153.67 105.156 180)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U4 (at 0.127 -2.286) (layer B.SilkS))
    (fp_text value LP2985-2.8 (at 0 -2.9) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 5 smd rect (at 1.35 0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 18 +2V8))
    (pad 4 smd rect (at 1.35 -0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C6-Pad1)"))
    (pad 3 smd rect (at -1.35 -0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -1.35 0 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 149.733 97.536 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at -1.524 -2.032 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 +2V8))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 21 SDA_2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 153.797 96.012 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -2.794 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 +2V8))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 SCL_2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5A02FF57)
    (at 153.797 99.06)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference Q1 (at 0.254 2.54) (layer F.SilkS))
    (fp_text value FDC6506P (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 SCL))
    (pad 6 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 SCL_2V8))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 SDA))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 +2V8))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 SDA_2V8))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 +2V8))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 149.225 106.172 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 3.048 -1.016) (layer B.SilkS))
    (fp_text value 10n (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 19 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 157.48 105.283 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 2.413 -0.127) (layer B.SilkS))
    (fp_text value 2.2u (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 151.257 101.854 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 +2V8))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 149.216 102.108 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 2.023 2.286) (layer B.SilkS))
    (fp_text value "0.1 u" (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 18 +2V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_THT:Relay_SPDT_Omron_G6E (layer F.Cu) (tedit 5A57DE62)
    (at 182.372 96.647 270)
    (descr "Relay SPDT Omron Serie G6E")
    (tags "Relay SPDT Omron Serie G6E 1x um")
    (fp_text reference K1 (at -2.667 13.335) (layer F.SilkS))
    (fp_text value G6E (at 3.6 15.5 270) (layer F.Fab))
    (fp_text user %R (at 3.81 6.35 90) (layer F.Fab))
    (pad 7 thru_hole circle (at 7.62 12.7 180) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad1)"))
    (pad 6 thru_hole circle (at 0 12.7 180) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 10 thru_hole circle (at 7.62 5.08 180) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (pad 12 thru_hole circle (at 7.62 0 180) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 23 +5V))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_Omron_G6E.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 127.626 104.902 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.778) (layer B.SilkS))
    (fp_text value R (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 16 "Net-(R6-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 102.861 101.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 3.184 0) (layer F.SilkS))
    (fp_text value R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 25 GPI))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 192.024 101.6 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 2.794 0) (layer F.SilkS))
    (fp_text value R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 +5V))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 117.348 98.552 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -0.254 2.032) (layer B.SilkS))
    (fp_text value R (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 6 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 111.76 102.108 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference FB1 (at 0 2.54 180) (layer B.SilkS))
    (fp_text value Ferrite_Bead (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 10 "Net-(FB1-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 5 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B4B45C9)
    (at 102.87 101.6 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D3 (at -3.175 0) (layer B.SilkS))
    (fp_text value LED (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B4B45C9)
    (at 192.024 101.6)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at -2.794 0) (layer B.SilkS))
    (fp_text value LED (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer B.Cu) (tedit 58641869)
    (at 112.776 97.028 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 1.85) (layer B.SilkS))
    (fp_text value D (at 0.1 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 1.85) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.159 96.52 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 2.912 0 180) (layer F.SilkS))
    (fp_text value "0.1 u" (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 158.369 97.536 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 2.54 -1.27 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 SCL))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 158.369 97.536 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 2.032 180) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 SDA))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 128.905 97.028 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 3.81 -0.127) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.279999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text NO (at 184.531 104.14) (layer B.SilkS))
  (gr_text NC (at 175.133 104.14) (layer B.SilkS))
  (gr_text COM (at 167.005 104.14) (layer B.SilkS))
  (dimension 6.35 (width 0.15) (layer F.Fab)
    (gr_text "0.2500 in" (at 150.495 82.139) (layer F.Fab))
    (feature1 (pts (xy 153.67 113.03) (xy 153.67 82.852579)))
    (feature2 (pts (xy 147.32 113.03) (xy 147.32 82.852579)))
    (crossbar (pts (xy 147.32 83.439) (xy 153.67 83.439)))
    (arrow1a (pts (xy 153.67 83.439) (xy 152.543496 84.025421)))
    (arrow1b (pts (xy 153.67 83.439) (xy 152.543496 82.852579)))
    (arrow2a (pts (xy 147.32 83.439) (xy 148.446504 84.025421)))
    (arrow2b (pts (xy 147.32 83.439) (xy 148.446504 82.852579)))
  )
  (dimension 6.35 (width 0.15) (layer F.Fab)
    (gr_text "0.2500 in" (at 144.145 82.139) (layer F.Fab))
    (feature1 (pts (xy 147.32 113.03) (xy 147.32 82.852579)))
    (feature2 (pts (xy 140.97 113.03) (xy 140.97 82.852579)))
    (crossbar (pts (xy 140.97 83.439) (xy 147.32 83.439)))
    (arrow1a (pts (xy 147.32 83.439) (xy 146.193496 84.025421)))
    (arrow1b (pts (xy 147.32 83.439) (xy 146.193496 82.852579)))
    (arrow2a (pts (xy 140.97 83.439) (xy 142.096504 84.025421)))
    (arrow2b (pts (xy 140.97 83.439) (xy 142.096504 82.852579)))
  )
  (dimension 50.8 (width 0.15) (layer F.Fab)
    (gr_text "2.0000 in" (at 121.92 76.551) (layer F.Fab))
    (feature1 (pts (xy 147.32 90.043) (xy 147.32 77.264579)))
    (feature2 (pts (xy 96.52 90.043) (xy 96.52 77.264579)))
    (crossbar (pts (xy 96.52 77.851) (xy 147.32 77.851)))
    (arrow1a (pts (xy 147.32 77.851) (xy 146.193496 78.437421)))
    (arrow1b (pts (xy 147.32 77.851) (xy 146.193496 77.264579)))
    (arrow2a (pts (xy 96.52 77.851) (xy 97.646504 78.437421)))
    (arrow2b (pts (xy 96.52 77.851) (xy 97.646504 77.264579)))
  )
  (dimension 88.9 (width 0.15) (layer F.Fab)
    (gr_text "3.5000 in" (at 147.32 72.868001) (layer F.Fab))
    (feature1 (pts (xy 102.87 95.25) (xy 102.87 73.58158)))
    (feature2 (pts (xy 191.77 95.25) (xy 191.77 73.58158)))
    (crossbar (pts (xy 191.77 74.168001) (xy 102.87 74.168001)))
    (arrow1a (pts (xy 102.87 74.168001) (xy 103.996504 73.58158)))
    (arrow1b (pts (xy 102.87 74.168001) (xy 103.996504 74.754422)))
    (arrow2a (pts (xy 191.77 74.168001) (xy 190.643496 73.58158)))
    (arrow2b (pts (xy 191.77 74.168001) (xy 190.643496 74.754422)))
  )
  (dimension 6.35 (width 0.15) (layer F.Fab)
    (gr_text "0.2500 in" (at 194.945 70.582) (layer F.Fab))
    (feature1 (pts (xy 191.77 95.25) (xy 191.77 71.295579)))
    (feature2 (pts (xy 198.12 95.25) (xy 198.12 71.295579)))
    (crossbar (pts (xy 198.12 71.882) (xy 191.77 71.882)))
    (arrow1a (pts (xy 191.77 71.882) (xy 192.896504 71.295579)))
    (arrow1b (pts (xy 191.77 71.882) (xy 192.896504 72.468421)))
    (arrow2a (pts (xy 198.12 71.882) (xy 196.993496 71.295579)))
    (arrow2b (pts (xy 198.12 71.882) (xy 196.993496 72.468421)))
  )
  (dimension 6.35 (width 0.15) (layer F.Fab)
    (gr_text "0.2500 in" (at 99.695 72.868) (layer F.Fab))
    (feature1 (pts (xy 102.87 95.25) (xy 102.87 73.581579)))
    (feature2 (pts (xy 96.52 95.25) (xy 96.52 73.581579)))
    (crossbar (pts (xy 96.52 74.168) (xy 102.87 74.168)))
    (arrow1a (pts (xy 102.87 74.168) (xy 101.743496 74.754421)))
    (arrow1b (pts (xy 102.87 74.168) (xy 101.743496 73.581579)))
    (arrow2a (pts (xy 96.52 74.168) (xy 97.646504 74.754421)))
    (arrow2b (pts (xy 96.52 74.168) (xy 97.646504 73.581579)))
  )
  (dimension 101.6 (width 0.15) (layer F.Fab)
    (gr_text "4.0000 in" (at 147.32 67.026) (layer F.Fab))
    (feature1 (pts (xy 198.12 101.6) (xy 198.12 67.739579)))
    (feature2 (pts (xy 96.52 101.6) (xy 96.52 67.739579)))
    (crossbar (pts (xy 96.52 68.326) (xy 198.12 68.326)))
    (arrow1a (pts (xy 198.12 68.326) (xy 196.993496 68.912421)))
    (arrow1b (pts (xy 198.12 68.326) (xy 196.993496 67.739579)))
    (arrow2a (pts (xy 96.52 68.326) (xy 97.646504 68.912421)))
    (arrow2b (pts (xy 96.52 68.326) (xy 97.646504 67.739579)))
  )
  (gr_arc (start 101.6 95.25) (end 101.6 90.17) (angle -90) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 193.04 95.25) (end 198.12 95.25) (angle -90) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 193.04 107.95) (end 193.04 113.03) (angle -90) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 101.6 107.95) (end 96.52 107.95) (angle -90) (layer Edge.Cuts) (width 0.254))
  (gr_text "WPSA 6915 Temp Screen\nCriterion Manufacturing\n20200522 Rev A" (at 186.436 100.584) (layer B.SilkS))
  (gr_text SDA (at 145.669 91.948) (layer F.SilkS))
  (gr_text SCL (at 142.113 91.948) (layer F.SilkS))
  (gr_line (start 101.6 90.17) (end 193.04 90.17) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 96.52 107.95) (end 96.52 95.25) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 193.04 113.03) (end 101.6 113.03) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 198.12 95.25) (end 198.12 107.95) (layer Edge.Cuts) (width 0.254))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 97.536 91.44) (xy 197.104 91.44) (xy 197.104 111.76) (xy 185.42 111.76) (xy 185.42 101.6)
        (xy 166.116 101.6) (xy 166.116 111.76) (xy 121.412 111.76) (xy 121.412 93.98) (xy 107.95 93.98)
        (xy 107.95 111.76) (xy 97.536 111.76)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 97.536 91.44) (xy 197.104 91.44) (xy 197.104 111.76) (xy 185.42 111.76) (xy 185.42 101.6)
        (xy 166.116 101.6) (xy 166.116 111.76) (xy 121.412 111.76) (xy 121.412 93.98) (xy 107.95 93.98)
        (xy 107.95 111.76) (xy 97.536 111.76)
      )
    )
  )
)
