(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 122)
    (no_connects 0)
    (area 101.524999 25.324999 185.495001 100.151001)
    (thickness 1.6)
    (drawings 110)
    (tracks 294)
    (zones 0)
    (modules 66)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.19812)
    (uvia_min_drill 0.09906)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.4 2.4)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 GND)
  (net 5 VCC)
  (net 6 Earth)
  (net 7 /Channel1/SENS_CH)
  (net 8 /Channel1/OUT_CH)
  (net 9 "Net-(C2-Pad1)")
  (net 10 "Net-(C2-Pad2)")
  (net 11 /Channel2/SENS_CH)
  (net 12 "Net-(D2-Pad2)")
  (net 13 /Channel2/OUT_CH)
  (net 14 "Net-(C3-Pad1)")
  (net 15 "Net-(C3-Pad2)")
  (net 16 "Net-(C4-Pad1)")
  (net 17 "Net-(C4-Pad2)")
  (net 18 "Net-(C5-Pad1)")
  (net 19 "Net-(C5-Pad2)")
  (net 20 "Net-(C6-Pad1)")
  (net 21 "Net-(C6-Pad2)")
  (net 22 "Net-(C7-Pad1)")
  (net 23 "Net-(C7-Pad2)")
  (net 24 "Net-(C8-Pad1)")
  (net 25 "Net-(C8-Pad2)")
  (net 26 /Channel3/SENS_CH)
  (net 27 "Net-(D3-Pad2)")
  (net 28 /Channel4/SENS_CH)
  (net 29 "Net-(D4-Pad2)")
  (net 30 /Channel5/SENS_CH)
  (net 31 "Net-(D5-Pad2)")
  (net 32 /Channel6/SENS_CH)
  (net 33 "Net-(D6-Pad2)")
  (net 34 /Channel7/SENS_CH)
  (net 35 "Net-(D7-Pad2)")
  (net 36 /Channel8/SENS_CH)
  (net 37 "Net-(D8-Pad2)")
  (net 38 /Channel3/OUT_CH)
  (net 39 /Channel4/OUT_CH)
  (net 40 /Channel5/OUT_CH)
  (net 41 /Channel6/OUT_CH)
  (net 42 /Channel7/OUT_CH)
  (net 43 /Channel8/OUT_CH)
  (net 44 "Net-(J87-Pad1)")
  (net 45 "Net-(J89-Pad1)")
  (net 46 "Net-(J91-Pad1)")
  (net 47 "Net-(J93-Pad1)")
  (net 48 "Net-(J88-Pad1)")
  (net 49 "Net-(J90-Pad1)")
  (net 50 "Net-(J92-Pad1)")
  (net 51 "Net-(J94-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.381)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /Channel1/OUT_CH)
    (add_net /Channel1/SENS_CH)
    (add_net /Channel2/OUT_CH)
    (add_net /Channel2/SENS_CH)
    (add_net /Channel3/OUT_CH)
    (add_net /Channel3/SENS_CH)
    (add_net /Channel4/OUT_CH)
    (add_net /Channel4/SENS_CH)
    (add_net /Channel5/OUT_CH)
    (add_net /Channel5/SENS_CH)
    (add_net /Channel6/OUT_CH)
    (add_net /Channel6/SENS_CH)
    (add_net /Channel7/OUT_CH)
    (add_net /Channel7/SENS_CH)
    (add_net /Channel8/OUT_CH)
    (add_net /Channel8/SENS_CH)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(J87-Pad1)")
    (add_net "Net-(J88-Pad1)")
    (add_net "Net-(J89-Pad1)")
    (add_net "Net-(J90-Pad1)")
    (add_net "Net-(J91-Pad1)")
    (add_net "Net-(J92-Pad1)")
    (add_net "Net-(J93-Pad1)")
    (add_net "Net-(J94-Pad1)")
    (add_net VCC)
  )
  (net_class EARTH ""
    (clearance 0.1524)
    (trace_width 0.762)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net Earth)
  )
  (module "Custom Library:Socket_Strip_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5972624E)
    (at 156.21 82.55 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J94 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value R_MEAS (at 0 7.41 270) (layer F.Fab))
    (fp_text user J2 (at 2.54 2.794 360) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J94-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(D8-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /Channel8/SENS_CH))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module "Custom Library:Socket_Strip_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5972624E)
    (at 156.21 66.548 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J93 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value R_MEAS (at 0 7.41 270) (layer F.Fab))
    (fp_text user J2 (at 2.54 2.794 360) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J93-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(D7-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /Channel7/SENS_CH))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module "Custom Library:Socket_Strip_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5972624E)
    (at 156.21 50.546 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J92 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value R_MEAS (at 0 7.41 270) (layer F.Fab))
    (fp_text user J2 (at 2.54 2.794 360) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J92-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /Channel6/SENS_CH))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module "Custom Library:Socket_Strip_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5972624E)
    (at 156.21 34.544 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J91 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value R_MEAS (at 0 7.41 270) (layer F.Fab))
    (fp_text user J2 (at 2.54 2.794 360) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J91-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(D5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /Channel5/SENS_CH))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module "Custom Library:Socket_Strip_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5972624E)
    (at 118.745 82.423 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J90 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value R_MEAS (at 0 7.41 270) (layer F.Fab))
    (fp_text user J2 (at 2.54 2.794 360) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J90-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(D4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /Channel4/SENS_CH))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module "Custom Library:Socket_Strip_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5972624E)
    (at 118.618 66.548 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J89 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value R_MEAS (at 0 7.41 270) (layer F.Fab))
    (fp_text user J2 (at 2.54 2.794 360) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J89-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(D3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /Channel3/SENS_CH))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module "Custom Library:Socket_Strip_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5972624E)
    (at 118.745 50.419 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J88 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value R_MEAS (at 0 7.41 270) (layer F.Fab))
    (fp_text user J2 (at 2.54 2.794 360) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(J88-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /Channel2/SENS_CH))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module "Custom Library:Socket_Strip_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5972624E)
    (at 118.618 34.544 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J87 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value R_MEAS (at 0 7.41 270) (layer F.Fab))
    (fp_text user J2 (at 2.54 2.794 360) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J87-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /Channel1/SENS_CH))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module "Custom Library:Pin_Header_Straight_2x01_Pitch2.54mm" (layer F.Cu) (tedit 597231FC)
    (at 181.102 50.292 90)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference J3 (at 6.096 0 90) (layer B.SilkS) hide)
    (fp_text value "Ground Isolation Switch" (at 1.27 2.33 90) (layer F.Fab))
    (fp_text user %R (at 1.27 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 Earth))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Custom Library:C_0805" (layer F.Cu) (tedit 58AA8463)
    (at 148.844 91.948 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value "10uF GRM219R60J106KE19D" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:C_0805" (layer F.Cu) (tedit 58AA8463)
    (at 148.844 75.946 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value "10uF GRM219R60J106KE19D" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:C_0805" (layer F.Cu) (tedit 58AA8463)
    (at 148.844 59.944 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value "10uF GRM219R60J106KE19D" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:C_0805" (layer F.Cu) (tedit 58AA8463)
    (at 148.844 43.942 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value "10uF GRM219R60J106KE19D" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:C_0805" (layer F.Cu) (tedit 58AA8463)
    (at 111.379 91.821 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value "10uF GRM219R60J106KE19D" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:C_0805" (layer F.Cu) (tedit 58AA8463)
    (at 111.252 75.946 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value "10uF GRM219R60J106KE19D" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:C_0805" (layer F.Cu) (tedit 58AA8463)
    (at 111.379 59.817 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value "10uF GRM219R60J106KE19D" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:C_0805" (layer F.Cu) (tedit 58AA8463)
    (at 111.252 43.942 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value "10uF GRM219R60J106KE19D" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_3pol (layer B.Cu) (tedit 56301605)
    (at 144.78 82.296 270)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J9 (at 3.5 4.3 270) (layer B.SilkS))
    (fp_text value CH8_OUTPUT (at 3.5 -6 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 43 /Channel8/OUT_CH))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 /Channel8/SENS_CH))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_3pol (layer B.Cu) (tedit 56301605)
    (at 107.188 82.042 270)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J8 (at 3.5 4.3 270) (layer B.SilkS))
    (fp_text value CH4_OUTPUT (at 3.5 -6 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 39 /Channel4/OUT_CH))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 /Channel4/SENS_CH))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_3pol (layer B.Cu) (tedit 56301605)
    (at 144.78 66.294 270)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J7 (at 3.5 4.3 270) (layer B.SilkS))
    (fp_text value CH7_OUTPUT (at 3.5 -6 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 42 /Channel7/OUT_CH))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 /Channel7/SENS_CH))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_3pol (layer B.Cu) (tedit 56301605)
    (at 107.188 66.04 270)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J6 (at 3.5 4.3 270) (layer B.SilkS))
    (fp_text value CH3_OUTPUT (at 3.5 -6 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 38 /Channel3/OUT_CH))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 /Channel3/SENS_CH))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_3pol (layer B.Cu) (tedit 56301605)
    (at 107.188 50.038 270)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J5 (at 3.5 4.3 270) (layer B.SilkS))
    (fp_text value CH2_OUTPUT (at 3.5 -6 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 /Channel2/OUT_CH))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 /Channel2/SENS_CH))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_3pol (layer B.Cu) (tedit 56301605)
    (at 144.78 50.292 270)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J4 (at 3.5 4.3 270) (layer B.SilkS))
    (fp_text value CH6_OUTPUT (at 3.5 -6 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 /Channel6/OUT_CH))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 32 /Channel6/SENS_CH))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_3pol (layer B.Cu) (tedit 56301605)
    (at 144.78 34.29 270)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J2 (at 3.5 4.3 270) (layer B.SilkS))
    (fp_text value CH5_OUTPUT (at 3.5 -6 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 40 /Channel5/OUT_CH))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 30 /Channel5/SENS_CH))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_3pol (layer B.Cu) (tedit 56301605)
    (at 107.188 34.29 270)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J1 (at 3.5 4.3 270) (layer B.SilkS))
    (fp_text value CH1_OUTPUT (at 3.5 -6 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 /Channel1/OUT_CH))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /Channel1/SENS_CH))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_3pol (layer B.Cu) (tedit 56301605)
    (at 180.594 55.626 270)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J10 (at 3.5 4.3 270) (layer B.SilkS))
    (fp_text value DC_IN (at 3.5 -6 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 Earth))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Pin_Header_Straight_2x02_Pitch2.54mm" (layer F.Cu) (tedit 59726226)
    (at 115.697 59.563 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J44 (at 2.286 -2.794 90) (layer F.SilkS) hide)
    (fp_text value CAP_ENABLE (at 1.27 4.87 90) (layer F.Fab) hide)
    (fp_text user J3 (at 5.08 1.524 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /Channel2/OUT_CH))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(C2-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /Channel2/SENS_CH))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Custom Library:Pin_Header_Straight_2x02_Pitch2.54mm" (layer F.Cu) (tedit 59726226)
    (at 115.57 75.692 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J61 (at 2.286 -2.794 90) (layer F.SilkS) hide)
    (fp_text value CAP_ENABLE (at 1.27 4.87 90) (layer F.Fab) hide)
    (fp_text user J3 (at 5.08 1.524 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /Channel3/OUT_CH))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C3-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /Channel3/SENS_CH))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Custom Library:Pin_Header_Straight_2x02_Pitch2.54mm" (layer F.Cu) (tedit 59726226)
    (at 115.697 91.567 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J66 (at 2.286 -2.794 90) (layer F.SilkS) hide)
    (fp_text value CAP_ENABLE (at 1.27 4.87 90) (layer F.Fab) hide)
    (fp_text user J3 (at 5.08 1.524 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(C4-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /Channel4/OUT_CH))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C4-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /Channel4/SENS_CH))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Custom Library:Pin_Header_Straight_2x02_Pitch2.54mm" (layer F.Cu) (tedit 59726226)
    (at 153.162 43.688 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J71 (at 2.286 -2.794 90) (layer F.SilkS) hide)
    (fp_text value CAP_ENABLE (at 1.27 4.87 90) (layer F.Fab) hide)
    (fp_text user J3 (at 5.08 1.524 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(C5-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /Channel5/OUT_CH))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(C5-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /Channel5/SENS_CH))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Custom Library:Pin_Header_Straight_2x02_Pitch2.54mm" (layer F.Cu) (tedit 59726226)
    (at 153.162 59.69 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J76 (at 2.286 -2.794 90) (layer F.SilkS) hide)
    (fp_text value CAP_ENABLE (at 1.27 4.87 90) (layer F.Fab) hide)
    (fp_text user J3 (at 5.08 1.524 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(C6-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /Channel6/OUT_CH))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(C6-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /Channel6/SENS_CH))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Custom Library:Pin_Header_Straight_2x02_Pitch2.54mm" (layer F.Cu) (tedit 59726226)
    (at 153.162 75.692 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J81 (at 2.286 -2.794 90) (layer F.SilkS) hide)
    (fp_text value CAP_ENABLE (at 1.27 4.87 90) (layer F.Fab) hide)
    (fp_text user J3 (at 5.08 1.524 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(C7-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /Channel7/OUT_CH))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(C7-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /Channel7/SENS_CH))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Custom Library:Pin_Header_Straight_2x02_Pitch2.54mm" (layer F.Cu) (tedit 59726226)
    (at 153.162 91.694 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J86 (at 2.286 -2.794 90) (layer F.SilkS) hide)
    (fp_text value CAP_ENABLE (at 1.27 4.87 90) (layer F.Fab) hide)
    (fp_text user J3 (at 5.08 1.524 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /Channel8/OUT_CH))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(C8-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /Channel8/SENS_CH))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Custom Library:TI_TO92_LM334" (layer F.Cu) (tedit 5972450D)
    (at 173.736 82.804 90)
    (fp_text reference U8 (at 0 -2.794 90) (layer F.SilkS) hide)
    (fp_text value LM334 (at 0 -3.302 90) (layer F.Fab))
    (fp_text user U1 (at 0 -2.794 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 "Net-(J94-Pad1)"))
    (pad 3 thru_hole circle (at 2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 "Net-(D8-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "Custom Library:TI_TO92_LM334" (layer F.Cu) (tedit 5972450D)
    (at 173.736 66.802 90)
    (fp_text reference U7 (at 0 -2.794 90) (layer F.SilkS) hide)
    (fp_text value LM334 (at 0 -3.302 90) (layer F.Fab))
    (fp_text user U1 (at 0 -2.794 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 "Net-(J93-Pad1)"))
    (pad 3 thru_hole circle (at 2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(D7-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "Custom Library:TI_TO92_LM334" (layer F.Cu) (tedit 5972450D)
    (at 173.736 50.8 90)
    (fp_text reference U6 (at 0 -2.794 90) (layer F.SilkS) hide)
    (fp_text value LM334 (at 0 -3.302 90) (layer F.Fab))
    (fp_text user U1 (at 0 -2.794 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "Net-(J92-Pad1)"))
    (pad 3 thru_hole circle (at 2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "Net-(D6-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "Custom Library:TI_TO92_LM334" (layer F.Cu) (tedit 5972450D)
    (at 173.736 34.798 90)
    (fp_text reference U5 (at 0 -2.794 90) (layer F.SilkS) hide)
    (fp_text value LM334 (at 0 -3.302 90) (layer F.Fab))
    (fp_text user U1 (at 0 -2.794 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "Net-(J91-Pad1)"))
    (pad 3 thru_hole circle (at 2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "Net-(D5-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "Custom Library:TI_TO92_LM334" (layer F.Cu) (tedit 5972450D)
    (at 136.144 82.55 90)
    (fp_text reference U4 (at 0 -2.794 90) (layer F.SilkS) hide)
    (fp_text value LM334 (at 0 -3.302 90) (layer F.Fab))
    (fp_text user U1 (at 0 -2.794 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 "Net-(J90-Pad1)"))
    (pad 3 thru_hole circle (at 2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "Net-(D4-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "Custom Library:TI_TO92_LM334" (layer F.Cu) (tedit 5972450D)
    (at 136.144 66.802 90)
    (fp_text reference U3 (at 0 -2.794 90) (layer F.SilkS) hide)
    (fp_text value LM334 (at 0 -3.302 90) (layer F.Fab))
    (fp_text user U1 (at 0 -2.794 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 "Net-(J89-Pad1)"))
    (pad 3 thru_hole circle (at 2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 "Net-(D3-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "Custom Library:TI_TO92_LM334" (layer F.Cu) (tedit 5972450D)
    (at 136.144 50.546 90)
    (fp_text reference U2 (at 0 -2.794 90) (layer F.SilkS) hide)
    (fp_text value LM334 (at 0 -3.302 90) (layer F.Fab))
    (fp_text user U1 (at 0 -2.794 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 "Net-(J88-Pad1)"))
    (pad 3 thru_hole circle (at 2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "Custom Library:TI_TO92_LM334" (layer F.Cu) (tedit 5972450D)
    (at 136.144 34.798 90)
    (fp_text reference U1 (at 0 -2.794 90) (layer F.SilkS) hide)
    (fp_text value LM334 (at 0 -3.302 90) (layer F.Fab))
    (fp_text user U1 (at 0 -2.794 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Net-(J87-Pad1)"))
    (pad 3 thru_hole circle (at 2.6 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "Custom Library:Pin_Header_Straight_2x02_Pitch2.54mm" (layer F.Cu) (tedit 59726226)
    (at 115.57 43.688 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J39 (at 2.286 -2.794 90) (layer F.SilkS) hide)
    (fp_text value CAP_ENABLE (at 1.27 4.87 90) (layer F.Fab) hide)
    (fp_text user J3 (at 5.08 1.524 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /Channel1/OUT_CH))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /Channel1/SENS_CH))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_1" (layer F.Cu) (tedit 597246AD)
    (at 124.968 34.544 90)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value "33 3299Y-1-500LF" (at 0 5.06 90) (layer F.Fab))
    (fp_text user R1 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at -2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 44 "Net-(J87-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_1" (layer F.Cu) (tedit 597246AD)
    (at 125.222 50.546 90)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV3 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value "33 3299Y-1-500LF" (at 0 5.06 90) (layer F.Fab))
    (fp_text user R1 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at -2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 48 "Net-(J88-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_1" (layer F.Cu) (tedit 597246AD)
    (at 124.968 66.548 90)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV5 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value "33 3299Y-1-500LF" (at 0 5.06 90) (layer F.Fab))
    (fp_text user R1 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 27 "Net-(D3-Pad2)"))
    (pad 3 smd rect (at -2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 45 "Net-(J89-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_1" (layer F.Cu) (tedit 597246AD)
    (at 125.095 82.423 90)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV7 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value "33 3299Y-1-500LF" (at 0 5.06 90) (layer F.Fab))
    (fp_text user R1 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 29 "Net-(D4-Pad2)"))
    (pad 3 smd rect (at -2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 49 "Net-(J90-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_1" (layer F.Cu) (tedit 597246AD)
    (at 162.56 34.544 90)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV9 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value "33 3299Y-1-500LF" (at 0 5.06 90) (layer F.Fab))
    (fp_text user R1 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 31 "Net-(D5-Pad2)"))
    (pad 3 smd rect (at -2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 46 "Net-(J91-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_1" (layer F.Cu) (tedit 597246AD)
    (at 162.56 50.546 90)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV11 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value "33 3299Y-1-500LF" (at 0 5.06 90) (layer F.Fab))
    (fp_text user R1 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 33 "Net-(D6-Pad2)"))
    (pad 3 smd rect (at -2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 50 "Net-(J92-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_1" (layer F.Cu) (tedit 597246AD)
    (at 162.56 66.548 90)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV13 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value "33 3299Y-1-500LF" (at 0 5.06 90) (layer F.Fab))
    (fp_text user R1 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 35 "Net-(D7-Pad2)"))
    (pad 3 smd rect (at -2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 47 "Net-(J93-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_1" (layer F.Cu) (tedit 597246AD)
    (at 162.56 82.55 90)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV15 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value "33 3299Y-1-500LF" (at 0 5.06 90) (layer F.Fab))
    (fp_text user R1 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 37 "Net-(D8-Pad2)"))
    (pad 3 smd rect (at -2.54 -2.42 90) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 51 "Net-(J94-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_2" (layer F.Cu) (tedit 597246CB)
    (at 124.968 42.418 270)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV2 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value "330 3296W-1-501LF" (at 0 5.06 270) (layer F.Fab))
    (fp_text user R2 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 7 /Channel1/SENS_CH))
    (pad 3 smd rect (at -2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 44 "Net-(J87-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_2" (layer F.Cu) (tedit 597246CB)
    (at 125.095 58.293 270)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV4 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value "330 3296W-1-501LF" (at 0 5.06 270) (layer F.Fab))
    (fp_text user R2 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 11 /Channel2/SENS_CH))
    (pad 3 smd rect (at -2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 48 "Net-(J88-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_2" (layer F.Cu) (tedit 597246CB)
    (at 124.968 74.422 270)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV6 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value "330 3296W-1-501LF" (at 0 5.06 270) (layer F.Fab))
    (fp_text user R2 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 26 /Channel3/SENS_CH))
    (pad 3 smd rect (at -2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 45 "Net-(J89-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_2" (layer F.Cu) (tedit 597246CB)
    (at 125.095 90.297 270)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV8 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value "330 3296W-1-501LF" (at 0 5.06 270) (layer F.Fab))
    (fp_text user R2 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 28 /Channel4/SENS_CH))
    (pad 3 smd rect (at -2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 49 "Net-(J90-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_2" (layer F.Cu) (tedit 597246CB)
    (at 162.56 42.418 270)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV10 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value "330 3296W-1-501LF" (at 0 5.06 270) (layer F.Fab))
    (fp_text user R2 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 30 /Channel5/SENS_CH))
    (pad 3 smd rect (at -2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 46 "Net-(J91-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_2" (layer F.Cu) (tedit 597246CB)
    (at 162.56 58.42 270)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV12 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value "330 3296W-1-501LF" (at 0 5.06 270) (layer F.Fab))
    (fp_text user R2 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 32 /Channel6/SENS_CH))
    (pad 3 smd rect (at -2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 50 "Net-(J92-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_2" (layer F.Cu) (tedit 597246CB)
    (at 162.56 74.422 270)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV14 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value "330 3296W-1-501LF" (at 0 5.06 270) (layer F.Fab))
    (fp_text user R2 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 34 /Channel7/SENS_CH))
    (pad 3 smd rect (at -2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 47 "Net-(J93-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Potentiometer_Trimmer_Bourns_3269W_2" (layer F.Cu) (tedit 597246CB)
    (at 162.56 90.424 270)
    (descr "Spindle Trimmer Potentiometer, Bourns 3269W, https://www.bourns.com/pdfs/3269.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3269W")
    (attr smd)
    (fp_text reference RV16 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value "330 3296W-1-501LF" (at 0 5.06 270) (layer F.Fab))
    (fp_text user R2 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at 2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 0 2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 36 /Channel8/SENS_CH))
    (pad 3 smd rect (at -2.54 -2.42 270) (size 1.19 2.79) (layers F.Cu F.Mask)
      (net 51 "Net-(J94-Pad1)"))
    (model ../../../../../../Users/tjames/Documents/KiCad/ICPSignalConditioner/3269W001XXX.wrl
      (at (xyz 0.1 -0.1 0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:D_DO-35_SOD27_P10.16mm_Horizontal" (layer F.Cu) (tedit 59724522)
    (at 130.81 43.434 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 5.08 0 90) (layer F.SilkS) hide)
    (fp_text value "1N457TR - Fairchild" (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user D1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /Channel1/SENS_CH))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:D_DO-35_SOD27_P10.16mm_Horizontal" (layer F.Cu) (tedit 59724522)
    (at 131.064 59.436 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 5.08 0 90) (layer F.SilkS) hide)
    (fp_text value "1N457TR - Fairchild" (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user D1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /Channel2/SENS_CH))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:D_DO-35_SOD27_P10.16mm_Horizontal" (layer F.Cu) (tedit 59724522)
    (at 130.81 75.438 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 5.08 0 90) (layer F.SilkS) hide)
    (fp_text value "1N457TR - Fairchild" (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user D1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /Channel3/SENS_CH))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(D3-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:D_DO-35_SOD27_P10.16mm_Horizontal" (layer F.Cu) (tedit 59724522)
    (at 130.937 91.313 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D4 (at 5.08 0 90) (layer F.SilkS) hide)
    (fp_text value "1N457TR - Fairchild" (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user D1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /Channel4/SENS_CH))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(D4-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:D_DO-35_SOD27_P10.16mm_Horizontal" (layer F.Cu) (tedit 59724522)
    (at 168.402 43.434 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D5 (at 5.08 0 90) (layer F.SilkS) hide)
    (fp_text value "1N457TR - Fairchild" (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user D1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /Channel5/SENS_CH))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(D5-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:D_DO-35_SOD27_P10.16mm_Horizontal" (layer F.Cu) (tedit 59724522)
    (at 168.402 59.436 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D6 (at 5.08 0 90) (layer F.SilkS) hide)
    (fp_text value "1N457TR - Fairchild" (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user D1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /Channel6/SENS_CH))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(D6-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:D_DO-35_SOD27_P10.16mm_Horizontal" (layer F.Cu) (tedit 59724522)
    (at 168.402 75.438 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D7 (at 5.08 0 90) (layer F.SilkS) hide)
    (fp_text value "1N457TR - Fairchild" (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user D1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /Channel7/SENS_CH))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(D7-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:D_DO-35_SOD27_P10.16mm_Horizontal" (layer F.Cu) (tedit 59724522)
    (at 168.402 91.44 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D8 (at 5.08 0 90) (layer F.SilkS) hide)
    (fp_text value "1N457TR - Fairchild" (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user D1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /Channel8/SENS_CH))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(D8-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "GND\nJumper" (at 180.975 41.91 90) (layer F.SilkS))
  (gr_text "R2 R1 COM" (at 153.67 31.75) (layer F.SilkS))
  (gr_text "R2 R1 COM" (at 153.67 47.752) (layer F.SilkS))
  (gr_text "R2 R1 COM" (at 153.67 63.754) (layer F.SilkS))
  (gr_text "R2 R1 COM" (at 153.67 79.756) (layer F.SilkS))
  (gr_text "R2 R1 COM" (at 116.078 79.502) (layer F.SilkS))
  (gr_text "R2 R1 COM" (at 116.078 63.5) (layer F.SilkS))
  (gr_text "R2 R1 COM" (at 116.078 47.498) (layer F.SilkS))
  (gr_text "R2 R1 COM" (at 116.078 31.496) (layer F.SilkS))
  (gr_line (start 101.6 25.4) (end 101.6 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text CH8 (at 173.736 90.424) (layer F.SilkS))
  (gr_text CH7 (at 173.736 74.422) (layer F.SilkS))
  (gr_text CH6 (at 173.736 58.42) (layer F.SilkS))
  (gr_text CH5 (at 173.736 42.418) (layer F.SilkS))
  (gr_text CH4 (at 136.144 90.17) (layer F.SilkS))
  (gr_text CH3 (at 136.144 74.422) (layer F.SilkS))
  (gr_text CH2 (at 136.144 58.166) (layer F.SilkS))
  (gr_text CH1 (at 136.144 42.418) (layer F.SilkS))
  (gr_line (start 185.42 100.076) (end 101.6 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.42 25.4) (end 185.42 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 25.4) (end 185.42 25.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.42 100.076) (xy 101.6 100.076) (xy 101.6 25.4) (xy 185.42 25.4)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.42 100.076) (xy 101.6 100.076) (xy 101.6 25.4) (xy 185.42 25.4)
      )
    )
  )
)
