<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<text>OpenEnergyMonitor.org</text>
<text>OpenEnergyMonitor.org</text>
<text>433Mhz</text>
<text>868Mhz</text>
<text>915Mhz</text>
<text>165mm ant</text>
<text>82mm ant</text>
<text>78mm ant</text>
<text>433Mhz</text>
<text>868Mhz</text>
<text>915Mhz</text>
<text>165mm ant</text>
<text>82mm ant</text>
<text>78mm ant</text>
<text>433Mhz</text>
<text>868Mhz</text>
<text>915Mhz</text>
<text>165mm ant</text>
<text>82mm ant</text>
<text>78mm ant</text>
<text>433Mhz</text>
<text>868Mhz</text>
<text>915Mhz</text>
<text>165mm ant</text>
<text>82mm ant</text>
<text>78mm ant</text>
<text>433Mhz</text>
<text>868Mhz</text>
<text></text>
<text>87mm ant</text>
<text>175mm ant</text>
<text>V3.4 Oct 2014</text>
<text>emonTx</text>
<text>Open-Hardware</text>
<text>Designed in </text>
<text>North Wales </text>
<text>Made in UK</text>
<text>Designed in </text>
<text>North Wales </text>
<text>Made in UK</text>
<wire x1="0" y1="79.9066" x2="0" y2="0.0066" width="0.1" layer="20"/>
<wire x1="0" y1="0.0066" x2="82.1" y2="0" width="0.1" layer="20"/>
<wire x1="82.1" y1="0" x2="82.1" y2="2" width="0.1" layer="20"/>
<wire x1="82.1" y1="2" x2="92.2" y2="2" width="0.1" layer="20"/>
<wire x1="92.2" y1="2" x2="92.2" y2="0.0066" width="0.1" layer="20"/>
<wire x1="92.2" y1="0.0066" x2="99.9" y2="0.0066" width="0.1" layer="20"/>
<wire x1="99.9" y1="0.0066" x2="99.9" y2="79.9066" width="0.1" layer="20"/>
<wire x1="99.9" y1="79.9066" x2="0" y2="79.9066" width="0.1" layer="20"/>
<text>5V </text>
<text>3.3V</text>
<text>IRQ1 Dig2</text>
<text>ADC5 / Dig19 /DS18B20 PWR</text>
<text>GND</text>
<text>Dig 5 / DS18B20 Data / PWM</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>Wireless Energy 
Monitoring Node</text>
<text>UART</text>
<text>Reset</text>
<text>CT 1-3
23kW MAX
</text>
<text>SMT V0.6 rev3</text>
<text>emonTx</text>
<text>wireless energy monitoring node</text>
<text>Technology that helps us live within ecological limits</text>
<text>Designed in North Wales UK by Glyn Hudson &amp; Trystan Lea</text>
<text>SMT V0.6 rev3</text>
<text>emonTx</text>
<text>wireless energy monitoring node</text>
<text>Technology that helps us live within ecological limits</text>
<text>Designed in North Wales UK by Glyn Hudson &amp; Trystan Lea</text>
<text>SMT V0.6 rev3</text>
<text>emonTx</text>
<text>wireless energy monitoring node</text>
<text>Technology that helps us live within ecological limits</text>
<text>Designed in North Wales UK by Glyn Hudson &amp; Trystan Lea</text>
<text>V3.4</text>
<text>emonTx</text>
<text>wireless energy monitoring node</text>
<text>Technology that helps us live within ecological limits</text>
<text>Designed in North Wales UK by Glyn Hudson &amp; Trystan Lea</text>
<text>Lead free PCB - RoHS components</text>
<text>@240V</text>
<text>4.5kW 
MAX
@240V</text>
<text>4.5kW MAX</text>
<text>9V AC</text>
<text>5V USB</text>
<text>JP2 AC-DC Power Supply 
Enable - 20mA  MAX</text>
<text>Front Act LED
Dig 6 PWM</text>
<text>GND</text>
<text>3 x AA
Battery</text>
<text>Programming Header</text>
<text>5V
</text>
<text>3.3V</text>
<text>GND</text>
<text>Dig3
IRQ1</text>
<text>ADC5/Dig19
DS18B20 PWR</text>
<text>Dig 5 PWM
DS18B20 Data</text>
<text>915Mhz</text>
<text>78mm ant</text>
<text>Node:</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>Rx</text>
<text>Tx</text>
<text>5V</text>
<text>RST</text>
<text>LED</text>
<text>2.1MM</text>
<text>Red Socket</text>
<text>2

1</text>
<text>RFM12B
RFM69CW</text>
<text>D9</text>
<text>D8</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="STX3100">
<description>&lt;b&gt;MIC/HEADPHONE JACK&lt;/b&gt;&lt;p&gt;
KS-S stereo microphone/headphone jack&lt;p&gt;
 PG203JN (Schukat) &lt;p&gt;
 TruConnect K-PJ-317 http://www.rapidonline.com/Cables-Connectors/Stereo-Socket-3-5mm-Switched-20-5108</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="1X2-3.5MM">
</package>
<package name="B3F-31XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="FTDI_BASIC">
</package>
<package name="1X02_LOCK">
</package>
<package name="SOD-323">
</package>
<package name="0603">
</package>
<package name="2X3">
</package>
</packages>
</library>
<library name="OpenEnergyMonitor">
<packages>
<package name="SOT89">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;</description>
</package>
<package name="DIP_SWITCH_SMT">
</package>
</packages>
</library>
<library name="Battery Holders">
<packages>
<package name="AAA_PCB_HOLDER">
<description>3x AAA PCB Battery Holder</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_6X200_NOTEXT">
</package>
</packages>
</library>
<library name="Ciseco USB miniB">
<packages>
<package name="USB-MINIB-CISECO">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Farnell_MCP1700">
<packages>
<package name="SOT95P237X112-3N">
</package>
</packages>
</library>
<library name="con-jack">
<description>&lt;b&gt;Jacks&lt;/b&gt;&lt;p&gt;
Power Connectors&lt;br&gt;
Phone Connectors&lt;br&gt;
Cinch Connectors&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SPC4077">
<description>&lt;b&gt;DC POWER JACK 2mm&lt;/b&gt;&lt;br&gt; Right Angle, Through Hole, Rated 5A at 16VDC, PC Terminals&lt;p&gt;
Source: www.spctechnology.com .. 84N1161.pdf&lt;br&gt;
Distributor: &lt;b&gt;Farnell (www.Farnell.de)&lt;/b&gt;&lt;br&gt;
Created by Robert Siegler</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
</packages>
</library>
<library name="discrete">
<description>Discrete devices (Antenna, Arrrester, Thermistor)</description>
<packages>
<package name="PAD-01">
<description>&lt;b&gt;PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-EDGE">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;&lt;p&gt;
This is a footprint for an edge mount RF antenna. Works pretty well with SMA type connectors but may also work with other edge mount RF connectors. Keep in mind, these edge mount connectors assume you are using a 0.062" PCB thickness.</description>
</package>
<package name="RJ45-8">
</package>
</packages>
</library>
<library name="JeeParts">
<packages>
<package name="RFM12B">
<description>RFM12B radio module by HopeRF</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="SOD-523">
<description>SOD-523 (0.8x1.2mm)

&lt;p&gt;Source: http://www.rohm.com/products/databook/di/pdf/rb751s-40.pdf&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CT4" library="adafruit" package="STX3100" value="STEREOJACK">
<attribute name="NAME"/>
</element>
<element name="CT3" library="adafruit" package="STX3100" value="STEREOJACK">
<attribute name="NAME"/>
</element>
<element name="CT2" library="adafruit" package="STX3100" value="STEREOJACK">
<attribute name="NAME"/>
</element>
<element name="R2" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="0204/7" value="22R">
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0603" value="120K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="0204/7" value="120R">
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="0204/7" value="22R">
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CT1" library="adafruit" package="STX3100" value="STEREOJACK">
<attribute name="NAME"/>
</element>
<element name="R21" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="0204/7" value="22R">
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="Battery Holders" package="AAA_PCB_HOLDER" value="4.5V">
<attribute name="RAPID_OC" value="18-2967"/>
</element>
<element name="H1" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H2" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H3" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H4" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="U$4" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$5" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="JP1" library="SparkFun" package="FTDI_BASIC" value="FTDI">
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R1206" value="22R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R1206" value="22R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R1206" value="22R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R1206" value="120R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="Farnell_MCP1700" package="SOT95P237X112-3N" value="MCP1702T-3302E/CB">
<attribute name="PACKAGE" value="SOT23-3"/>
<attribute name="OC_NEWARK" value="88H9817"/>
<attribute name="MPN" value="MCP1700T-3302E/TT"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="OC_FARNELL" value="1296592"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="resistor" package="C0603" value="1uF 6V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="resistor" package="C0603" value="1uF 6V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="linear" package="TO220V" value="7805">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="resistor" package="C0603" value="10uF 6V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="resistor" package="C0603" value="10uF 6V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="resistor" package="C0603" value="10uF 6V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="resistor" package="C0603" value="10uF 6V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="resistor" package="C0603" value="10uF 6V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="resistor" package="C0603" value="1uF 25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rcl" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun" package="SOD-323" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="resistor" package="R1206" value="56R 0.25W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="resistor" package="PANASONIC_D" value="47uF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="adafruit" package="B3F-31XX" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="ohw-logo" package="OSHW_6X200_NOTEXT" value="OSHW_LOGO_6MILX0200-NT"/>
<element name="U$1" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$7" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="LED1" library="adafruit" package="CHIP-LED0805" value="Red 1.85V">
<attribute name="VALUE"/>
</element>
<element name="U$10" library="Ciseco USB miniB" package="USB-MINIB-CISECO" value="USB-MINIB-5PIN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$11" library="OpenEnergyMonitor" package="SOT89" value="MCP1754">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN1" library="con-jack" package="SPC4077" value="2.1MM">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="adafruit" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="adafruit" package="HC49UP" value="16Mhz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="resistor" package="C0603" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="resistor" package="C0603" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1_TQFP" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P">
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-DigitalIC" package="MLF32" value="ATMEGA168MLF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ANT1" library="discrete" package="PAD-01" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J$1" library="SparkFun-Connectors" package="SMA-EDGE" value="SMA_EDGE"/>
<element name="C16" library="rcl" package="C0603" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0603" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$14" library="JeeParts" package="RFM12B" value="RFM12B"/>
<element name="ISP1" library="SparkFun" package="2X3" value="2x3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="rcl" package="R0603" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$13" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="J3" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="NAME"/>
</element>
<element name="J5" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="NAME"/>
</element>
<element name="J6" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="NAME"/>
</element>
<element name="R24" library="rcl" package="R0603" value="120K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="S3" library="OpenEnergyMonitor" package="DIP_SWITCH_SMT" value="2_SMT_DIP_SWITCH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R0603" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="C0603" value="ant tune?">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="microbuilder" package="SOD-523" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="microbuilder" package="SOD-523" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="microbuilder" package="SOD-523" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="microbuilder" package="SOD-523" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="microbuilder" package="SOD-523" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+5V">
<contactref element="U$3" pad="+"/>
<contactref element="C5" pad="2"/>
<contactref element="U$6" pad="3"/>
<contactref element="IC2" pad="1"/>
<contactref element="U$10" pad="VBUS"/>
<contactref element="JP1" pad="VCC"/>
<contactref element="J6" pad="2"/>
<contactref element="TP5" pad="TP"/>
<contactref element="R27" pad="2"/>
<contactref element="U$13" pad="7"/>
</signal>
<signal name="GND">
<contactref element="U$6" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="L1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C18" pad="-"/>
<contactref element="LED1" pad="C"/>
<contactref element="U$3" pad="-"/>
<contactref element="U$10" pad="GND"/>
<contactref element="U$10" pad="MTN1"/>
<contactref element="U$10" pad="MTN3"/>
<contactref element="U$10" pad="MTN2"/>
<contactref element="U$10" pad="MTN4"/>
<contactref element="U$11" pad="2.1"/>
<contactref element="U$11" pad="2"/>
<contactref element="CN1" pad="2"/>
<contactref element="CN1" pad="1"/>
<contactref element="U1_TQFP" pad="3"/>
<contactref element="U1_TQFP" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="C4" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="ISP1" pad="6"/>
<contactref element="JP1" pad="GND"/>
<contactref element="U$14" pad="P$12"/>
<contactref element="U$14" pad="GND"/>
<contactref element="C10" pad="2"/>
<contactref element="U$13" pad="1"/>
<contactref element="U$13" pad="3"/>
<contactref element="U$13" pad="5"/>
<contactref element="J5" pad="2"/>
<contactref element="TP3" pad="TP"/>
<contactref element="S3" pad="1"/>
<contactref element="S3" pad="2"/>
<contactref element="R30" pad="1"/>
<contactref element="C20" pad="2"/>
<contactref element="J$1" pad="GND@2"/>
<contactref element="J$1" pad="GND@3"/>
<contactref element="J$1" pad="GND@1"/>
<contactref element="J$1" pad="GND@0"/>
<contactref element="D4" pad="A"/>
<contactref element="D5" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="ADC0">
<contactref element="R28" pad="1"/>
<contactref element="U1_TQFP" pad="23"/>
<contactref element="U1" pad="23"/>
<contactref element="D6" pad="K"/>
</signal>
<signal name="ADC1">
<contactref element="U1_TQFP" pad="24"/>
<contactref element="U1" pad="24"/>
<contactref element="D2" pad="K"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="ADC2">
<contactref element="U1_TQFP" pad="25"/>
<contactref element="U1" pad="25"/>
<contactref element="R20" pad="2"/>
<contactref element="D3" pad="K"/>
</signal>
<signal name="ADC3">
<contactref element="U1_TQFP" pad="26"/>
<contactref element="U1" pad="26"/>
<contactref element="R25" pad="2"/>
<contactref element="D4" pad="K"/>
</signal>
<signal name="ADC4">
<contactref element="U1_TQFP" pad="27"/>
<contactref element="U1" pad="27"/>
<contactref element="R26" pad="2"/>
<contactref element="D5" pad="K"/>
</signal>
<signal name="N$33">
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="CT2" pad="5"/>
<contactref element="R8" pad="1"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="R15" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="CT4" pad="5"/>
<contactref element="R18" pad="1"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="R5" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="CT1" pad="5"/>
<contactref element="R7" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="R10" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R22" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="CT3" pad="5"/>
<contactref element="R9" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="CT4" pad="4"/>
<contactref element="CT3" pad="4"/>
<contactref element="CT2" pad="4"/>
<contactref element="CT1" pad="4"/>
<contactref element="U1_TQFP" pad="21"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="3.3V">
<contactref element="U$6" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="C7" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="U1_TQFP" pad="4"/>
<contactref element="U1_TQFP" pad="18"/>
<contactref element="C3" pad="1"/>
<contactref element="U1_TQFP" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="18"/>
<contactref element="U$14" pad="VDD"/>
<contactref element="C10" pad="1"/>
<contactref element="ISP1" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="J6" pad="1"/>
<contactref element="TP4" pad="TP"/>
<contactref element="U$13" pad="2"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="AC">
<contactref element="C17" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="CN1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R14" pad="1"/>
<contactref element="R28" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R13" pad="1"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R16" pad="2"/>
<contactref element="R26" pad="1"/>
<contactref element="CT4" pad="1"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R29" pad="2"/>
<contactref element="C18" pad="+"/>
<contactref element="U$11" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="D1" pad="1"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R5" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="CT1" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="CT2" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R22" pad="2"/>
<contactref element="R25" pad="1"/>
<contactref element="CT3" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U$11" pad="3"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$14">
</signal>
<signal name="RESET">
<contactref element="R32" pad="1"/>
<contactref element="U1_TQFP" pad="29"/>
<contactref element="U1" pad="29"/>
<contactref element="ISP1" pad="5"/>
<contactref element="S1" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="D5">
<contactref element="U1_TQFP" pad="9"/>
<contactref element="U1" pad="9"/>
<contactref element="U$13" pad="4"/>
<contactref element="R33" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="D4">
<contactref element="U1_TQFP" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="D3">
<contactref element="U1_TQFP" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="TP2" pad="TP"/>
<contactref element="J5" pad="1"/>
<contactref element="U$13" pad="6"/>
</signal>
<signal name="D2">
<contactref element="U1_TQFP" pad="32"/>
<contactref element="U1" pad="32"/>
<contactref element="U$14" pad="IRQ"/>
</signal>
<signal name="D1/TX">
<contactref element="U1_TQFP" pad="31"/>
<contactref element="U1" pad="31"/>
<contactref element="JP1" pad="RXI"/>
</signal>
<signal name="D6">
<contactref element="U1_TQFP" pad="10"/>
<contactref element="U1" pad="10"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="D7">
<contactref element="U1_TQFP" pad="11"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="D8">
<contactref element="U1_TQFP" pad="12"/>
<contactref element="U1" pad="12"/>
<contactref element="S3" pad="4"/>
</signal>
<signal name="D9">
<contactref element="U1_TQFP" pad="13"/>
<contactref element="U1" pad="13"/>
<contactref element="S3" pad="3"/>
</signal>
<signal name="D10">
<contactref element="U1_TQFP" pad="14"/>
<contactref element="U1" pad="14"/>
<contactref element="U$14" pad="SEL"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="D11/MOSI">
<contactref element="U1_TQFP" pad="15"/>
<contactref element="U1" pad="15"/>
<contactref element="U$14" pad="SDI"/>
<contactref element="ISP1" pad="4"/>
</signal>
<signal name="D12/MISO">
<contactref element="U1_TQFP" pad="16"/>
<contactref element="U1" pad="16"/>
<contactref element="U$14" pad="SDO"/>
<contactref element="ISP1" pad="1"/>
</signal>
<signal name="A6">
<contactref element="U1_TQFP" pad="19"/>
<contactref element="U1" pad="19"/>
<contactref element="U$13" pad="8"/>
</signal>
<signal name="A7">
<contactref element="U1_TQFP" pad="22"/>
<contactref element="U1" pad="22"/>
<contactref element="R27" pad="1"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="D13/SCK">
<contactref element="U1_TQFP" pad="17"/>
<contactref element="U1" pad="17"/>
<contactref element="U$14" pad="SCK"/>
<contactref element="ISP1" pad="3"/>
</signal>
<signal name="D0/RX">
<contactref element="U1_TQFP" pad="30"/>
<contactref element="U1" pad="30"/>
<contactref element="JP1" pad="TXO"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U1_TQFP" pad="7"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="Q1" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="U1_TQFP" pad="8"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$20">
<contactref element="C8" pad="1"/>
<contactref element="U1_TQFP" pad="20"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="DIG1">
<contactref element="C19" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="U$14" pad="ANT"/>
<contactref element="C20" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="J$1" pad="SIG"/>
<contactref element="C19" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="ANT1" pad="1"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="ADC5">
<contactref element="U1_TQFP" pad="28"/>
<contactref element="U1" pad="28"/>
<contactref element="J3" pad="2"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="N$19">
<contactref element="JP1" pad="CTS"/>
</signal>
<signal name="N$23">
<contactref element="JP1" pad="DTR"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$16">
</signal>
</signals>
</board>
</drawing>
</eagle>
