(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 18)
    (no_connects 0)
    (area 101.77465 65.499216 124.37425 82.831)
    (thickness 1.6)
    (drawings 13)
    (tracks 51)
    (zones 0)
    (modules 9)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(D1-Pad1)")
  (net 4 /RXD)
  (net 5 /TXD)
  (net 6 /RS)
  (net 7 /CANH)
  (net 8 /CANL)
  (net 9 "Net-(R1-Pad1)")
  (net 10 "Net-(U1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CANH)
    (add_net /CANL)
    (add_net /RS)
    (add_net /RXD)
    (add_net /TXD)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57981D59)
    (at 109.474 69.342)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.778) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57981D12)
    (at 113.538 79.756)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -1.75) (layer F.SilkS))
    (fp_text value LED (at 0 1.75) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun:SparkFun-1X05 (layer F.Cu) (tedit 5798205E)
    (at 105.537 69.342 270)
    (attr virtual)
    (fp_text reference P1 (at 9.3218 2.67716 270) (layer B.SilkS) hide)
    (fp_text value CONN_01X05 (at 2.54 2.54 270) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.Paste)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.Paste)
      (net 4 /RXD))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.Paste)
      (net 5 /TXD))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.Paste)
      (net 6 /RS))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.Paste)
      (net 2 GND))
  )
  (module SparkFun:SparkFun-1X03 (layer F.Cu) (tedit 57981D24)
    (at 120.777 69.342 270)
    (attr virtual)
    (fp_text reference P2 (at 1.8288 -2.4638 270) (layer B.SilkS) hide)
    (fp_text value CONN_01X03 (at 2.54 2.54 270) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.Paste)
      (net 7 /CANH))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.Paste)
      (net 8 /CANL))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.Paste)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57981D54)
    (at 116.84 69.342)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.905) (layer F.SilkS))
    (fp_text value 0R (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /RS))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57981D4E)
    (at 113.284 69.342 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57981E37)
    (at 117.729 74.422 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 2.54 0.127 360) (layer F.SilkS))
    (fp_text value 120R (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /CANH))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /CANL))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57981D64)
    (at 109.601 79.756)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun:SparkFun-SO08 (layer F.Cu) (tedit 57981D1E)
    (at 112.014 74.422 270)
    (descr "SMALL OUTLINE PACKAGE FITS JEDEC PACKAGES (NARROW SOIC-8)")
    (tags "SMALL OUTLINE PACKAGE FITS JEDEC PACKAGES (NARROW SOIC-8)")
    (attr smd)
    (fp_text reference U1 (at -0.0508 0.4318 270) (layer B.SilkS))
    (fp_text value MCP2551-I/SN (at -0.254 -0.2032 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.905 2.6162 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 5 /TXD))
    (pad 2 smd rect (at -0.635 2.6162 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.635 2.6162 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 4 smd rect (at 1.905 2.6162 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 4 /RXD))
    (pad 5 smd rect (at 1.905 -2.6162 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 0.635 -2.6162 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 8 /CANL))
    (pad 7 smd rect (at -0.635 -2.6162 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 7 /CANH))
    (pad 8 smd rect (at -1.905 -2.6162 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
  )
  (gr_line (start 103.886 81.153) (end 116.967 81.153) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.428 67.691) (end 122.428 75.692) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.428 75.692) (end 116.967 81.153) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.886 67.691) (end 122.428 67.691) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.886 81.153) (end 103.886 67.691) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 109.347 79.756) (layer B.SilkS))
  (gr_text RS (at 108.585 77.089) (layer B.SilkS))
  (gr_text TX (at 108.458 74.549) (layer B.SilkS))
  (gr_text RX (at 108.712 72.009) (layer B.SilkS))
  (gr_text VCC (at 109.347 69.469) (layer B.SilkS))
  (gr_text GND (at 116.967 74.676) (layer B.SilkS))
  (gr_text "CANL\n" (at 116.459 72.009) (layer B.SilkS))
  (gr_text CANH (at 116.332 69.342) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.428 75.692) (xy 116.967 81.153) (xy 103.886 81.153) (xy 103.886 67.691) (xy 122.428 67.691)
        (xy 122.428 75.692)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.428 75.692) (xy 116.967 81.153) (xy 103.886 81.153) (xy 103.886 67.691) (xy 122.428 67.691)
        (xy 122.428 75.692)
      )
    )
  )
)
