(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 104)
    (zones 0)
    (modules 2)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.127)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.6096)
    (via_min_drill 0.3048)
    (user_via 0.6096 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J?1-Pad2)")
  (net 2 "Net-(J?1-Pad1)")
  (net 3 "Net-(J?1-Pad4)")
  (net 4 "Net-(J?1-Pad3)")
  (net 5 "Net-(J?1-Pad6)")
  (net 6 "Net-(J?1-Pad5)")
  (net 7 "Net-(J?1-Pad8)")
  (net 8 "Net-(J?1-Pad7)")
  (net 9 "Net-(J?1-Pad10)")
  (net 10 "Net-(J?1-Pad9)")
  (net 11 "Net-(J?1-Pad12)")
  (net 12 "Net-(J?1-Pad11)")
  (net 13 "Net-(J?1-Pad14)")
  (net 14 "Net-(J?1-Pad13)")
  (net 15 "Net-(J?1-Pad16)")
  (net 16 "Net-(J?1-Pad15)")
  (net 17 "Net-(J?1-Pad18)")
  (net 18 "Net-(J?1-Pad17)")
  (net 19 "Net-(J?1-Pad20)")
  (net 20 "Net-(J?1-Pad19)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J?1-Pad1)")
    (add_net "Net-(J?1-Pad10)")
    (add_net "Net-(J?1-Pad11)")
    (add_net "Net-(J?1-Pad12)")
    (add_net "Net-(J?1-Pad13)")
    (add_net "Net-(J?1-Pad14)")
    (add_net "Net-(J?1-Pad15)")
    (add_net "Net-(J?1-Pad16)")
    (add_net "Net-(J?1-Pad17)")
    (add_net "Net-(J?1-Pad18)")
    (add_net "Net-(J?1-Pad19)")
    (add_net "Net-(J?1-Pad2)")
    (add_net "Net-(J?1-Pad20)")
    (add_net "Net-(J?1-Pad3)")
    (add_net "Net-(J?1-Pad4)")
    (add_net "Net-(J?1-Pad5)")
    (add_net "Net-(J?1-Pad6)")
    (add_net "Net-(J?1-Pad7)")
    (add_net "Net-(J?1-Pad8)")
    (add_net "Net-(J?1-Pad9)")
  )
  (module t_connectors:AXK5S20047Y_socket (layer F.Cu) (tedit 5FEC5EF5)
    (at 150.39 79.982491)
    (attr smd)
    (fp_text reference J2 (at -4.1495 -4.163491) (layer F.SilkS))
    (fp_text value AXK520147YG_socket (at 0 0) (layer F.Fab))
    (pad 20 smd oval (at 2.54 2) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J?1-Pad20)"))
    (pad 19 smd oval (at 2.5146 -1.9812) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J?1-Pad19)"))
    (pad 18 smd oval (at 1.75 2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J?1-Pad18)"))
    (pad 17 smd oval (at 1.75 -2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J?1-Pad17)"))
    (pad 16 smd oval (at 1.25 2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J?1-Pad16)"))
    (pad 15 smd oval (at 1.25 -2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J?1-Pad15)"))
    (pad 14 smd oval (at 0.75 2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J?1-Pad14)"))
    (pad 13 smd oval (at 0.75 -2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J?1-Pad13)"))
    (pad 12 smd oval (at 0.25 2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J?1-Pad12)"))
    (pad 11 smd oval (at 0.25 -2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J?1-Pad11)"))
    (pad 10 smd oval (at -0.25 2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J?1-Pad10)"))
    (pad 9 smd oval (at -0.25 -2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J?1-Pad9)"))
    (pad 8 smd oval (at -0.75 2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J?1-Pad8)"))
    (pad 7 smd oval (at -0.75 -2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J?1-Pad7)"))
    (pad 6 smd oval (at -1.25 2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J?1-Pad6)"))
    (pad 5 smd oval (at -1.25 -2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J?1-Pad5)"))
    (pad 4 smd oval (at -1.75 2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J?1-Pad4)"))
    (pad 3 smd oval (at -1.75 -2) (size 0.25 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J?1-Pad3)"))
    (pad 2 smd oval (at -2.5146 2.032) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J?1-Pad2)"))
    (pad 1 smd rect (at -2.5146 -1.9812) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J?1-Pad1)"))
  )
  (module t_connectors:AXK6S20447Y_header (layer B.Cu) (tedit 5FEC6F0C)
    (at 150.3934 79.9846 180)
    (attr smd)
    (fp_text reference J1 (at 3.7084 4.1656) (layer B.SilkS))
    (fp_text value AXK6S20447Y_header (at 0 0) (layer B.Fab))
    (pad 2 smd oval (at 2.54 -2 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J?1-Pad2)"))
    (pad 1 smd rect (at 2.5146 1.9812 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J?1-Pad1)"))
    (pad 4 smd oval (at 1.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J?1-Pad4)"))
    (pad 3 smd oval (at 1.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J?1-Pad3)"))
    (pad 6 smd oval (at 1.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J?1-Pad6)"))
    (pad 5 smd oval (at 1.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J?1-Pad5)"))
    (pad 8 smd oval (at 0.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J?1-Pad8)"))
    (pad 7 smd oval (at 0.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J?1-Pad7)"))
    (pad 10 smd oval (at 0.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J?1-Pad10)"))
    (pad 9 smd oval (at 0.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J?1-Pad9)"))
    (pad 12 smd oval (at -0.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J?1-Pad12)"))
    (pad 11 smd oval (at -0.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J?1-Pad11)"))
    (pad 14 smd oval (at -0.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J?1-Pad14)"))
    (pad 13 smd oval (at -0.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J?1-Pad13)"))
    (pad 16 smd oval (at -1.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J?1-Pad16)"))
    (pad 15 smd oval (at -1.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J?1-Pad15)"))
    (pad 18 smd oval (at -1.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J?1-Pad18)"))
    (pad 17 smd oval (at -1.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J?1-Pad17)"))
    (pad 20 smd oval (at -2.5146 -2.032 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J?1-Pad20)"))
    (pad 19 smd oval (at -2.5146 1.9812 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J?1-Pad19)"))
  )
  (gr_text SK1600 (at 150.8125 75.692) (layer F.SilkS))
  (gr_line (start 154.94 74.93) (end 156.21 76.2) (layer Edge.Cuts) (width 0.100076))
  (gr_line (start 144.78 76.2) (end 146.05 74.93) (layer Edge.Cuts) (width 0.100076))
  (gr_line (start 156.21 76.2) (end 156.21 84.455) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.05 74.93) (end 154.94 74.93) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.78 84.455) (end 144.78 76.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.21 84.455) (end 144.78 84.455) (layer Edge.Cuts) (width 0.1))
)
