(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6002)
    (drawings 6)
    (tracks 124)
    (zones 0)
    (modules 10)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 "Net-(M1-Pad1)")
  (net 2 "Net-(M1-Pad2)")
  (net 3 "Net-(M1-Pad3)")
  (net 4 "Net-(M1-Pad4)")
  (net 5 "Net-(M1-Pad6)")
  (net 6 "Net-(M1-Pad7)")
  (net 7 "Net-(M1-Pad8)")
  (net 8 "Net-(M1-Pad9)")
  (net 9 "Net-(M1-Pad10)")
  (net 10 "Net-(M1-Pad11)")
  (net 11 "Net-(M1-Pad13)")
  (net 12 "Net-(M1-Pad14)")
  (net 13 "Net-(M1-Pad15)")
  (net 14 "Net-(M1-Pad16)")
  (net 15 "Net-(M2-Pad1)")
  (net 16 "Net-(M2-Pad12)")
  (net 17 "Net-(M2-Pad13)")
  (net 18 "Net-(M2-Pad14)")
  (net 19 "Net-(M2-Pad15)")
  (net 20 "Net-(M2-Pad16)")
  (net 21 "Net-(M2-Pad20)")
  (net 22 GND)
  (net 23 VCC)
  (net 24 "Net-(NX1-PadA)")
  (net 25 "Net-(J1-Pad1)")
  (net 26 "Net-(J1-Pad2)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M1-Pad10)")
    (add_net "Net-(M1-Pad11)")
    (add_net "Net-(M1-Pad13)")
    (add_net "Net-(M1-Pad14)")
    (add_net "Net-(M1-Pad15)")
    (add_net "Net-(M1-Pad16)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M1-Pad3)")
    (add_net "Net-(M1-Pad4)")
    (add_net "Net-(M1-Pad6)")
    (add_net "Net-(M1-Pad7)")
    (add_net "Net-(M1-Pad8)")
    (add_net "Net-(M1-Pad9)")
    (add_net "Net-(M2-Pad1)")
    (add_net "Net-(M2-Pad12)")
    (add_net "Net-(M2-Pad13)")
    (add_net "Net-(M2-Pad14)")
    (add_net "Net-(M2-Pad15)")
    (add_net "Net-(M2-Pad16)")
    (add_net "Net-(M2-Pad20)")
    (add_net "Net-(NX1-PadA)")
    (add_net VCC)
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module nixiemisc:nixiemisc-SOIC16-5.3MM (layer F.Cu) (tedit 5BBFF1F5)
    (at 140 100)
    (attr smd)
    (fp_text reference M1 (at 0.6731 -6.0325) (layer F.SilkS))
    (fp_text value 74141SOIC16 (at 0 0) (layer F.SilkS) hide)
    (pad 16 smd rect (at 3.29946 -4.445 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(M1-Pad16)"))
    (pad 15 smd rect (at 3.29946 -3.175 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(M1-Pad15)"))
    (pad 14 smd rect (at 3.29946 -1.905 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(M1-Pad14)"))
    (pad 13 smd rect (at 3.29946 -0.635 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(M1-Pad13)"))
    (pad 12 smd rect (at 3.29946 0.635 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 11 smd rect (at 3.29946 1.905 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(M1-Pad11)"))
    (pad 10 smd rect (at 3.29946 3.175 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(M1-Pad10)"))
    (pad 9 smd rect (at 3.29946 4.445 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(M1-Pad9)"))
    (pad 8 smd rect (at -3.29946 4.445 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(M1-Pad8)"))
    (pad 7 smd rect (at -3.29946 3.175 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(M1-Pad7)"))
    (pad 6 smd rect (at -3.29946 1.905 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(M1-Pad6)"))
    (pad 5 smd rect (at -3.29946 0.635 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 23 VCC))
    (pad 4 smd rect (at -3.29946 -0.635 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(M1-Pad4)"))
    (pad 3 smd rect (at -3.29946 -1.905 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(M1-Pad3)"))
    (pad 2 smd rect (at -3.29946 -3.175 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(M1-Pad2)"))
    (pad 1 smd rect (at -3.29946 -4.445 270) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(M1-Pad1)"))
  )
  (module nixiemisc:nixiemisc-QFN20 (layer B.Cu) (tedit 5BC00B59)
    (at 141.25 97.75)
    (attr smd)
    (fp_text reference M2 (at -0.05 3.45) (layer B.SilkS))
    (fp_text value ATTINY84 (at 1.3081 -5.16382) (layer B.SilkS) hide)
    (pad EXP smd rect (at 0 0) (size 2.49936 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 22 GND))
    (pad 20 smd rect (at -0.99822 1.99898 90) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(M2-Pad20)"))
    (pad 19 smd rect (at -0.49784 1.99898 90) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd rect (at 0 1.99898 90) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd rect (at 0.49784 1.99898 90) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd rect (at 0.99822 1.99898 90) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(M2-Pad16)"))
    (pad 15 smd rect (at 1.99898 0.99822 180) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(M2-Pad15)"))
    (pad 14 smd rect (at 1.99898 0.49784 180) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(M2-Pad14)"))
    (pad 13 smd rect (at 1.99898 0 180) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(M2-Pad13)"))
    (pad 12 smd rect (at 1.99898 -0.49784 180) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(M2-Pad12)"))
    (pad 11 smd rect (at 1.99898 -0.99822 180) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J1-Pad2)"))
    (pad 10 smd rect (at 0.99822 -1.99898 270) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 0.49784 -1.99898 270) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 23 VCC))
    (pad 8 smd rect (at 0 -1.99898 270) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 22 GND))
    (pad 7 smd rect (at -0.49784 -1.99898 270) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -0.99822 -1.99898 270) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -1.99898 -0.99822) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(M1-Pad3)"))
    (pad 4 smd rect (at -1.99898 -0.49784) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(M1-Pad4)"))
    (pad 3 smd rect (at -1.99898 0) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(M1-Pad6)"))
    (pad 2 smd rect (at -1.99898 0.49784) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(M1-Pad7)"))
    (pad 1 smd rect (at -1.99898 0.99822) (size 0.7493 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(M2-Pad1)"))
  )
  (module mynixies:mynixies-ZM1232SPECIAL (layer F.Cu) (tedit 5BC0076E)
    (at 139.9991 99.99872)
    (attr virtual)
    (fp_text reference NX1 (at 0 -7.99846) (layer F.SilkS) hide)
    (fp_text value ZM1232SPECIAL (at 0 7.99846) (layer F.SilkS) hide)
    (pad 0 thru_hole circle (at 5.4991 -4.99872) (size 1.2065 1.2065) (drill 0.6985) (layers *.Cu *.Paste *.Mask)
      (net 14 "Net-(M1-Pad16)"))
    (pad 1 thru_hole circle (at -5.4991 -2.99974) (size 1.2065 1.2065) (drill 0.6985) (layers *.Cu *.Paste *.Mask)
      (net 1 "Net-(M1-Pad1)"))
    (pad 2 thru_hole circle (at -5.4991 -0.99822) (size 1.2065 1.2065) (drill 0.6985) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(M1-Pad2)"))
    (pad 3 thru_hole circle (at -5.4991 0.99822) (size 1.2065 1.2065) (drill 0.6985) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(M1-Pad8)"))
    (pad 4 thru_hole circle (at -5.4991 2.99974) (size 1.2065 1.2065) (drill 0.6985) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(M1-Pad9)"))
    (pad 5 thru_hole circle (at 5.4991 4.99872) (size 1.2065 1.2065) (drill 0.6985) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(M1-Pad10)"))
    (pad 6 thru_hole circle (at 5.4991 2.99974) (size 1.2065 1.2065) (drill 0.6985) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(M1-Pad11)"))
    (pad 7 thru_hole circle (at 5.4991 0.99822) (size 1.2065 1.2065) (drill 0.6985) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(M1-Pad13)"))
    (pad 8 thru_hole circle (at 5.4991 -0.99822) (size 1.2065 1.2065) (drill 0.6985) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(M1-Pad14)"))
    (pad 9 thru_hole circle (at 5.4991 -2.99974) (size 1.2065 1.2065) (drill 0.6985) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(M1-Pad15)"))
    (pad A thru_hole circle (at -5.4991 -4.99872) (size 1.2065 1.2065) (drill 0.6985) (layers *.Cu *.Paste *.Mask)
      (net 24 "Net-(NX1-PadA)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 139.75 93 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.2 180) (layer B.SilkS))
    (fp_text value R_Small10K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(NX1-PadA)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nixiemisc:nixiemisc-PAD (layer F.Cu) (tedit 5BC00B4C)
    (at 143 107)
    (attr virtual)
    (fp_text reference T5 (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value SS (at 0 -1.3) (layer F.SilkS))
    (pad P$1 thru_hole circle (at 0 0) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 17 "Net-(M2-Pad13)"))
  )
  (module nixiemisc:nixiemisc-PAD (layer F.Cu) (tedit 5BC00B44)
    (at 141 107)
    (attr virtual)
    (fp_text reference T6 (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value MOSI (at 0.5 1.3) (layer F.SilkS))
    (pad P$1 thru_hole circle (at 0 0) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 20 "Net-(M2-Pad16)"))
  )
  (module nixiemisc:nixiemisc-PAD (layer F.Cu) (tedit 5BC00B3C)
    (at 139 107)
    (attr virtual)
    (fp_text reference T7 (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value MISO (at -0.3 1.3) (layer F.SilkS))
    (pad P$1 thru_hole circle (at 0 0) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 21 "Net-(M2-Pad20)"))
  )
  (module nixiemisc:nixiemisc-PAD (layer F.Cu) (tedit 5BC00B33)
    (at 137 107)
    (attr virtual)
    (fp_text reference T8 (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value SCK (at 0 -1.3) (layer F.SilkS))
    (pad P$1 thru_hole circle (at 0 0) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 15 "Net-(M2-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 5BBFF1E8)
    (at 147.5 99 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 -4.87 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 5BBFF1C9)
    (at 132.5 99 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 -4.87 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer B.Fab))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 VCC))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Ven (at 147.3 103.5) (layer F.SilkS))
  (gr_text HV (at 147.4 97) (layer F.SilkS))
  (gr_text VIN (at 132.7 103.5) (layer F.SilkS))
  (gr_text GND (at 132.5 97.1) (layer F.SilkS))
  (gr_circle (center 140 100) (end 149.5 100) (layer Edge.Cuts) (width 0.127))
  (zone (net 22) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130 90) (xy 150 90) (xy 150 110) (xy 130 110)
      )
    )
  )
)
