(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 53)
    (tracks 766)
    (zones 0)
    (modules 117)
    (nets 88)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (user_trace_width 4)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D2-Pad1)")
  (net 3 "Net-(D3-Pad1)")
  (net 4 "Net-(D4-Pad2)")
  (net 5 "Net-(D5-Pad1)")
  (net 6 "Net-(D6-Pad1)")
  (net 7 "Net-(D7-Pad1)")
  (net 8 "Net-(D8-Pad1)")
  (net 9 "Net-(D9-Pad1)")
  (net 10 "Net-(D10-Pad1)")
  (net 11 "Net-(D11-Pad1)")
  (net 12 "Net-(D12-Pad1)")
  (net 13 "Net-(D13-Pad2)")
  (net 14 "Net-(D14-Pad2)")
  (net 15 "Net-(D15-Pad2)")
  (net 16 "Net-(C1-Pad1)")
  (net 17 "Net-(L1-Pad1)")
  (net 18 /GND)
  (net 19 /+5V)
  (net 20 "Net-(U2-Pad26)")
  (net 21 "Net-(U2-PadPRG)")
  (net 22 "Net-(U2-PadGNDb)")
  (net 23 "Net-(U2-Pad33Vb)")
  (net 24 "Net-(U2-Pad17_5V)")
  (net 25 "Net-(U2-Pad4)")
  (net 26 "Net-(U2-Pad33Va)")
  (net 27 "Net-(U2-PadGNDc)")
  (net 28 "Net-(J2-PadB8)")
  (net 29 "Net-(J2-PadB7)")
  (net 30 "Net-(J2-PadB6)")
  (net 31 "Net-(J2-PadB5)")
  (net 32 "Net-(J2-PadS1)")
  (net 33 "Net-(J2-PadA8)")
  (net 34 "Net-(J2-PadA7)")
  (net 35 "Net-(J2-PadA6)")
  (net 36 "Net-(J2-PadA5)")
  (net 37 /LED_SEL8)
  (net 38 /LED_SEL4)
  (net 39 /LED_SEL2)
  (net 40 /LED_SEL1)
  (net 41 /PWM_D3_280nm)
  (net 42 /BRIGHT8)
  (net 43 /BRIGHT4)
  (net 44 /BRIGHT2)
  (net 45 /BRIGHT1)
  (net 46 "Net-(C4-Pad1)")
  (net 47 "Net-(L2-Pad1)")
  (net 48 /PWM_D5_367nm)
  (net 49 "Net-(C6-Pad1)")
  (net 50 "Net-(L3-Pad1)")
  (net 51 /PWM_D4_405nm)
  (net 52 "Net-(C8-Pad1)")
  (net 53 "Net-(L4-Pad1)")
  (net 54 /PWM_D2_448nm)
  (net 55 "Net-(C10-Pad1)")
  (net 56 "Net-(L5-Pad1)")
  (net 57 /PWM_D1_470nm)
  (net 58 "Net-(C12-Pad1)")
  (net 59 "Net-(L6-Pad1)")
  (net 60 /PWM_D6_505nm)
  (net 61 "Net-(C14-Pad1)")
  (net 62 "Net-(L7-Pad1)")
  (net 63 /PWM_D7_530nm)
  (net 64 "Net-(C16-Pad1)")
  (net 65 "Net-(L8-Pad1)")
  (net 66 /PWM_D8_568nm)
  (net 67 "Net-(C18-Pad1)")
  (net 68 "Net-(L9-Pad1)")
  (net 69 /PWM_D10_617nm)
  (net 70 "Net-(C20-Pad1)")
  (net 71 "Net-(L10-Pad1)")
  (net 72 /PWM_D9_591nm)
  (net 73 "Net-(C22-Pad1)")
  (net 74 "Net-(L11-Pad1)")
  (net 75 /PWM_D11_627nm)
  (net 76 "Net-(C24-Pad1)")
  (net 77 "Net-(L12-Pad1)")
  (net 78 /PWM_D12_655nm)
  (net 79 "Net-(C26-Pad1)")
  (net 80 "Net-(L13-Pad1)")
  (net 81 /PWM_D13_740nm)
  (net 82 "Net-(C28-Pad1)")
  (net 83 "Net-(L14-Pad1)")
  (net 84 /PWM_D14_850nm)
  (net 85 "Net-(C30-Pad1)")
  (net 86 "Net-(L15-Pad1)")
  (net 87 /PWM_D15_940nm)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+5V)
    (add_net /BRIGHT1)
    (add_net /BRIGHT2)
    (add_net /BRIGHT4)
    (add_net /BRIGHT8)
    (add_net /GND)
    (add_net /LED_SEL1)
    (add_net /LED_SEL2)
    (add_net /LED_SEL4)
    (add_net /LED_SEL8)
    (add_net /PWM_D10_617nm)
    (add_net /PWM_D11_627nm)
    (add_net /PWM_D12_655nm)
    (add_net /PWM_D13_740nm)
    (add_net /PWM_D14_850nm)
    (add_net /PWM_D15_940nm)
    (add_net /PWM_D1_470nm)
    (add_net /PWM_D2_448nm)
    (add_net /PWM_D3_280nm)
    (add_net /PWM_D4_405nm)
    (add_net /PWM_D5_367nm)
    (add_net /PWM_D6_505nm)
    (add_net /PWM_D7_530nm)
    (add_net /PWM_D8_568nm)
    (add_net /PWM_D9_591nm)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(J2-PadA5)")
    (add_net "Net-(J2-PadA6)")
    (add_net "Net-(J2-PadA7)")
    (add_net "Net-(J2-PadA8)")
    (add_net "Net-(J2-PadB5)")
    (add_net "Net-(J2-PadB6)")
    (add_net "Net-(J2-PadB7)")
    (add_net "Net-(J2-PadB8)")
    (add_net "Net-(J2-PadS1)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L10-Pad1)")
    (add_net "Net-(L11-Pad1)")
    (add_net "Net-(L12-Pad1)")
    (add_net "Net-(L13-Pad1)")
    (add_net "Net-(L14-Pad1)")
    (add_net "Net-(L15-Pad1)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(L3-Pad1)")
    (add_net "Net-(L4-Pad1)")
    (add_net "Net-(L5-Pad1)")
    (add_net "Net-(L6-Pad1)")
    (add_net "Net-(L7-Pad1)")
    (add_net "Net-(L8-Pad1)")
    (add_net "Net-(L9-Pad1)")
    (add_net "Net-(U2-Pad17_5V)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad33Va)")
    (add_net "Net-(U2-Pad33Vb)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-PadGNDb)")
    (add_net "Net-(U2-PadGNDc)")
    (add_net "Net-(U2-PadPRG)")
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 170.65 69.75)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at 0.15 -1) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 /PWM_D15_940nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 178.45 72.95 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at 2.25 -0.15 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 /PWM_D14_850nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 191.5 72.385 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 0.4 -1 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /PWM_D13_740nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 203 72.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at 0.4 -1 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 /PWM_D12_655nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 211.115 69.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 0.4 -1) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /PWM_D11_627nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 223.45 72.15 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0.4 -1 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 /PWM_D10_617nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 230.65 71.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 0.4 -1 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 /PWM_D9_591nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 224.95 113.95 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0.4 -1 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /PWM_D8_568nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 219.1 114.15 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at -1.5 -1.05 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /PWM_D7_530nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 206.4 113.4 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0.4 -1 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /PWM_D6_505nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 197.5 113.8 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0.4 -1 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /PWM_D1_470nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 192.3 113.6 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0.4 -1 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /PWM_D2_448nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 186.8 114.3 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -2.2 -0.2 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /PWM_D4_405nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 171.8 113.9 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0.4 -1 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /PWM_D5_367nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0402_1005Metric (layer F.Cu) (tedit 6211C127)
    (at 162.2 112.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0.1 -1) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /PWM_D3_280nm) (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:QT_Brightek_QBHP684 (layer F.Cu) (tedit 61F8C343)
    (at 169 84.6)
    (fp_text reference D15 (at 3.7 1.2) (layer F.SilkS))
    (fp_text value 940nm (at 0.4 -5.2) (layer F.Fab))
    (fp_text user + (at -2.5 -1.1) (layer F.SilkS))
    (fp_text user - (at 2.6 -1.2) (layer F.SilkS))
    (pad 3 thru_hole circle (at 2.5 -3.8 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 2.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 2.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.1 -2.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.4 -3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 -2.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.2 -3.8 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.6 2.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.2 3.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.2 -3.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.5 -3.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.8 -2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.1 2.3) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.6 -2.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.4 -2.9 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.7 -2.9 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.4 3.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at 0.1 0.1) (size 1.75 6) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -3 4.25) (xy 3.05 4.25) (xy 3.05 1.75) (xy -3 1.75)) (width 0.1))
        (gr_poly (pts
           (xy -3 -1.75) (xy 3.05 -1.75) (xy 3.05 -4.25) (xy -3 -4.25)) (width 0.1))
      ))
    (pad 2 smd rect (at 2.13 0.1) (size 2 3) (layers F.Cu)
      (net 15 "Net-(D15-Pad2)") (zone_connect 0))
    (pad 3 thru_hole circle (at 2.8 2.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.5 4) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.6 3.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.7 3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.5 3.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.2 4) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.4 3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.6 -3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 1 smd rect (at -1.93 0.1 180) (size 2 3) (layers F.Cu)
      (net 85 "Net-(C30-Pad1)") (zone_connect 0))
  )
  (module MultiSpectLED:QT_Brightek_QBHP684 (layer F.Cu) (tedit 61F8C343)
    (at 178 84.6)
    (fp_text reference D14 (at 3.7 1.2) (layer F.SilkS))
    (fp_text value 850nm (at 0.4 -5.2) (layer F.Fab))
    (fp_text user + (at -2.5 -1.1) (layer F.SilkS))
    (fp_text user - (at 2.6 -1.2) (layer F.SilkS))
    (pad 3 thru_hole circle (at 2.5 -3.8 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 2.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 2.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.1 -2.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.4 -3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 -2.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.2 -3.8 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.6 2.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.2 3.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.2 -3.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.5 -3.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.8 -2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.1 2.3) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.6 -2.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.4 -2.9 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.7 -2.9 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.4 3.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at 0.1 0.1) (size 1.75 6) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -3 4.25) (xy 3.05 4.25) (xy 3.05 1.75) (xy -3 1.75)) (width 0.1))
        (gr_poly (pts
           (xy -3 -1.75) (xy 3.05 -1.75) (xy 3.05 -4.25) (xy -3 -4.25)) (width 0.1))
      ))
    (pad 2 smd rect (at 2.13 0.1) (size 2 3) (layers F.Cu)
      (net 14 "Net-(D14-Pad2)") (zone_connect 0))
    (pad 3 thru_hole circle (at 2.8 2.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.5 4) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.6 3.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.7 3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.5 3.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.2 4) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.4 3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.6 -3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 1 smd rect (at -1.93 0.1 180) (size 2 3) (layers F.Cu)
      (net 82 "Net-(C28-Pad1)") (zone_connect 0))
  )
  (module MultiSpectLED:FAN_PADS (layer B.Cu) (tedit 61FE2082)
    (at 140 116.8)
    (fp_text reference J1 (at 4.8 5.8) (layer B.SilkS) hide)
    (fp_text value Conn_01x02_Female (at -8 6.2) (layer B.Fab))
    (fp_text user +5V (at 2 2.8 -90) (layer B.SilkS))
    (fp_text user GND (at -2 2.8 -90) (layer B.SilkS))
    (pad 2 smd roundrect (at 2 0) (size 2 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -2 0) (size 2 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 168.4 74.3 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U16 (at 0 -2.4 90) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D15-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(L15-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 87 /PWM_D15_940nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 170.8 78.6 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -0.7 -1.6 90) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D15-Pad2)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 165.5 78.7 270)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L15 (at -2.3 0.7 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(C30-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(L15-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 168.65 78.6 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at -0.7 1.35 90) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(C30-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 172.1 73.3 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 176.1 73.6 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U15 (at -2.4 -2.4 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D14-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(L14-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 84 /PWM_D14_850nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 178.7 78.5 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -0.1 -2.6 90) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D14-Pad2)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 174.4 78.8 270)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L14 (at -2 0.1 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C28-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(L14-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 176.6 78.5 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at -0.1 -3.6 90) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C28-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 174.9 70.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at -1 1.55) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 189 73 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U14 (at -2.2 -2.9 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D13-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(L13-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 81 /PWM_D13_740nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 190.8 78 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -0.5 -2.8 90) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D13-Pad2)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 185.7 78.7 270)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L13 (at -2 -0.7 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(C26-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(L13-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 188.5 77.9 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at -0.4 -3.9 90) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(C26-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 188.1 70.1 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at -2.8 0.8) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 200.3 73.3 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U13 (at 1.15 -2.85 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D12-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(L12-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 78 /PWM_D12_655nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 202.1 79.2)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 3 1.1) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D12-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 198.7 78 270)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L12 (at -2.1 0.4 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(C24-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(L12-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 202.1 77.1)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 2.4 -1.5) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(C24-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 199 70.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at -1.2 1.5) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 208.7 73.3 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U12 (at -2.2 -2.7 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D11-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(L11-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 75 /PWM_D11_627nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 210.8 79.3)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 2.8 0.1) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D11-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 207.3 78.2 270)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L11 (at -2 0.1 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C22-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(L11-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 210.5 77.4)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 2.9 0.3) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C22-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 207.6 70.2 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at -0.65 1.5) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 228.3 73.4 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U11 (at 2.3 -2.9 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D9-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(L10-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 72 /PWM_D9_591nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 230.7 79.1)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 2.8 0.5) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D9-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 227.1 77.5 270)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L10 (at 2.2 -0.1 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(C20-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(L10-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 230.7 77.1)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 2.8 0.3) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(C20-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 227.4 70.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at -1 1.55) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 221 73.1 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U10 (at 1.9 -2.9 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D10-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(L9-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 69 /PWM_D10_617nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 221.6 79.3)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 2.5 0.5) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D10-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 218.3 78.6 270)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L9 (at -2 -0.5 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C18-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(L9-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 221.6 77.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 2.8 0.4) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C18-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 220.1 70 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at -0.8 1.6) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 227.275 112.85 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U9 (at 1.65 -2.4 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D8-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(L8-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 66 /PWM_D8_568nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 227.225 109.45 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.475 -0.75) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D8-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 230.2 108.05 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L8 (at -0.05 1.8 90) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C16-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(L8-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 227.225 107.475 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 2.325 1.375) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C16-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 228.5 115.85)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -0.9 1.65) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 221.4 112.775 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U8 (at 1.775 -2.5 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D7-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(L7-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 63 /PWM_D7_530nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 220.35 109.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 3.325 1.35) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D7-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 223.275 108.025 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L7 (at -2.025 0.925 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C14-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(L7-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 220.325 107.425 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 2.875 0.7) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C14-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 222.475 115.725)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -1.125 1.725) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 208.8 112.975 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U7 (at 1.775 -2.5 180) (layer F.SilkS))
    (fp_text value PAM2804 (at -1.825 -2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D6-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(L6-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 60 /PWM_D6_505nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 207.75 109.45 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 2.45 -0.225) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D6-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 210.8 107.925 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L6 (at 0.875 1.95 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(C12-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(L6-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 207.75 107.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0.375 1.45) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(C12-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 209.9625 115.925)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -1.0125 1.575) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 199.8 112.75 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U6 (at 1.45 -2.4 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(L5-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 57 /PWM_D1_470nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 199.7125 109.35 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -0.0875 -1.3) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(D1-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 202.6 108.35 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L5 (at 1.975 0.1 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(C10-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(L5-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 199.7 107.225 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0.075 1.425) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(C10-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 200.775 115.85)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -0.775 1.6) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 189.075 112.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at 1.775 -2.275 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D4-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(L3-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 51 /PWM_D4_405nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 194.65 112.325 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U5 (at 1.125 -2.575 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D2-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(L4-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 54 /PWM_D2_448nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 193.725 108.7 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 1.55 -1.6) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D2-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 196.65 108.275 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L4 (at -2.025 0.125 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(C8-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(L4-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 193.725 106.7 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 1.775 1.175) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(C8-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 195.65 115.7)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -1.1 1.6) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 186.7 107.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.3 -0.1 180) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D4-Pad2)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 190.825 108.025 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L3 (at -2.05 -0.35 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(L3-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 188.65 107.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.325 0.075 180) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(C6-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 189.975 115.85)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -1.1 1.6) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 174.2 113.4 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 2.4 -2.1 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D5-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 48 /PWM_D5_367nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 173.9 109.7 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 1 -1.8 180) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(D5-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 177.3 113.9 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at -0.9 2.1 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(C4-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(L2-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 177.9 109.7 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.5 0.2 180) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(C4-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 175.9 109.7 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.4 0 180) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:USB_C_Receptacle_Amphenol_12401610E4-2A (layer F.Cu) (tedit 61FB7344)
    (at 129.3 113.6 270)
    (descr "USB TYPE C, RA RCPT PCB, SMT, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401610E4%7e2A")
    (tags "USB C Type-C Receptacle SMD")
    (attr smd)
    (fp_text reference J2 (at 0 -6.36 90) (layer F.SilkS))
    (fp_text value USB_C_Receptacle_USB2.0 (at 0 6.14 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad B12 smd rect (at -3 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad B11 smd rect (at -2.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad B10 smd rect (at -2 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad B9 smd rect (at -1.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad B8 smd rect (at -1 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J2-PadB8)"))
    (pad B7 smd rect (at -0.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J2-PadB7)"))
    (pad B6 smd rect (at 0 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J2-PadB6)"))
    (pad B5 smd rect (at 0.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J2-PadB5)"))
    (pad B4 smd rect (at 1 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad B3 smd rect (at 1.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad B2 smd rect (at 2 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole circle (at -3.6 -4.36 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 3.6 -4.36 270) (size 0.95 0.65) (drill oval 0.95 0.65) (layers *.Cu *.Mask))
    (pad S1 thru_hole oval (at -4.49 2.84 270) (size 0.8 1.4) (drill oval 0.5 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-PadS1)"))
    (pad S1 thru_hole oval (at 4.49 2.84 270) (size 0.8 1.4) (drill oval 0.5 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-PadS1)"))
    (pad S1 thru_hole oval (at 4.13 -3.11 270) (size 0.8 1.4) (drill oval 0.5 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-PadS1)"))
    (pad B1 smd rect (at 2.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad A11 smd rect (at 2.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad A8 smd rect (at 0.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J2-PadA8)"))
    (pad A9 smd rect (at 1.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad A10 smd rect (at 1.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad A12 smd rect (at 2.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad A7 smd rect (at 0.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J2-PadA7)"))
    (pad A6 smd rect (at -0.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-PadA6)"))
    (pad A5 smd rect (at -0.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J2-PadA5)"))
    (pad A4 smd rect (at -1.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad A3 smd rect (at -1.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad A2 smd rect (at -2.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad A1 smd rect (at -2.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad S1 thru_hole oval (at -4.13 -3.11 270) (size 0.8 1.4) (drill oval 0.5 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-PadS1)"))
    (model ${KIPRJMOD}/M-12401610E42A-REVT2.stp
      (offset (xyz 0 -5.25 1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module MultiSpectLED:LuxeonRebelColor (layer F.Cu) (tedit 61FA1CA8)
    (at 200 84.6 90)
    (fp_text reference D12 (at 2.7 -4.3) (layer F.SilkS))
    (fp_text value 655nm (at -4.4 0.6 180) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user - (at 2.4 3.4) (layer F.SilkS))
    (fp_text user + (at 2.4 -3 90) (layer F.SilkS))
    (fp_text user 3.05 (at -2.38376 0.019224) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user 4.50 (at 1.038115 -3.370011 90) (layer F.Fab))
    (fp_text user 1.525 (at -0.313518 -2.848821 90) (layer F.Fab))
    (fp_text user 2.25 (at 1.575482 -2.297609 90) (layer F.Fab))
    (pad 2 smd custom (at 3.4 -1.5 90) (size 0.5 0.5) (layers F.Cu)
      (net 76 "Net-(C24-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.74 -0.375) (xy -0.74 1.325) (xy 0.51 1.325) (xy 0.51 -0.375)) (width 0.1))
      ))
    (pad 1 smd custom (at 3.45 1.55 90) (size 0.5 0.5) (layers F.Cu)
      (net 12 "Net-(D12-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.78 -1.35) (xy -0.78 0.35) (xy 0.47 0.35) (xy 0.47 -1.35)) (width 0.1))
      ))
    (pad 3 thru_hole circle (at 0.55 0 90) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 0 90) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.9 1.85 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 1.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.65 0.9 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 0.5 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.45 0.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 -1.3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.7 -0.85 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.95 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.15 -2.75 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 -2.45 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 -3.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 -2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 -2.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.65 -2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 -2.95 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2 -2.95 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 -2.15 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 -1.25 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 0.45 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 1.3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 2.2 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.05 3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.7 2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 2.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 2.9 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.7 3.15 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 2.5 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at -3.4 -3.45 90) (size 0.3 0.3) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 0) (xy 0 7) (xy 5.75 7) (xy 5.75 6.15) (xy 5.25 5.65)
           (xy 5.25 1.5) (xy 5.75 1) (xy 5.75 0)) (width 0.5))
      ))
    (pad 3 thru_hole circle (at -2.11 2.795 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (model ${KIPRJMOD}/LuxeonRebel.stp
      (offset (xyz 0.45 0 0.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module MultiSpectLED:LuxeonRebelColor (layer F.Cu) (tedit 61FA1CA8)
    (at 209.6 84.6 90)
    (fp_text reference D11 (at 2.8 -4) (layer F.SilkS))
    (fp_text value 627nm (at -4.4 0.4 180) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user - (at 2.4 3.4) (layer F.SilkS))
    (fp_text user + (at 2.4 -3 90) (layer F.SilkS))
    (fp_text user 3.05 (at -2.38376 0.019224) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user 4.50 (at 1.038115 -3.370011 90) (layer F.Fab))
    (fp_text user 1.525 (at -0.313518 -2.848821 90) (layer F.Fab))
    (fp_text user 2.25 (at 1.575482 -2.297609 90) (layer F.Fab))
    (pad 2 smd custom (at 3.4 -1.5 90) (size 0.5 0.5) (layers F.Cu)
      (net 73 "Net-(C22-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.74 -0.375) (xy -0.74 1.325) (xy 0.51 1.325) (xy 0.51 -0.375)) (width 0.1))
      ))
    (pad 1 smd custom (at 3.45 1.55 90) (size 0.5 0.5) (layers F.Cu)
      (net 11 "Net-(D11-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.78 -1.35) (xy -0.78 0.35) (xy 0.47 0.35) (xy 0.47 -1.35)) (width 0.1))
      ))
    (pad 3 thru_hole circle (at 0.55 0 90) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 0 90) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.9 1.85 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 1.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.65 0.9 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 0.5 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.45 0.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 -1.3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.7 -0.85 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.95 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.15 -2.75 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 -2.45 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 -3.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 -2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 -2.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.65 -2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 -2.95 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2 -2.95 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 -2.15 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 -1.25 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 0.45 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 1.3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 2.2 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.05 3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.7 2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 2.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 2.9 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.7 3.15 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 2.5 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at -3.4 -3.45 90) (size 0.3 0.3) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 0) (xy 0 7) (xy 5.75 7) (xy 5.75 6.15) (xy 5.25 5.65)
           (xy 5.25 1.5) (xy 5.75 1) (xy 5.75 0)) (width 0.5))
      ))
    (pad 3 thru_hole circle (at -2.11 2.795 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (model ${KIPRJMOD}/LuxeonRebel.stp
      (offset (xyz 0.45 0 0.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module MultiSpectLED:LuxeonRebelColor (layer F.Cu) (tedit 61FA1CA8)
    (at 218.9 84.6 90)
    (fp_text reference D10 (at 2.7 -4.1) (layer F.SilkS))
    (fp_text value 617nm (at -4.4 1.9 180) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user - (at 2.4 3.4) (layer F.SilkS))
    (fp_text user + (at 2.4 -3 90) (layer F.SilkS))
    (fp_text user 3.05 (at -2.38376 0.019224) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user 4.50 (at 1.038115 -3.370011 90) (layer F.Fab))
    (fp_text user 1.525 (at -0.313518 -2.848821 90) (layer F.Fab))
    (fp_text user 2.25 (at 1.575482 -2.297609 90) (layer F.Fab))
    (pad 2 smd custom (at 3.4 -1.5 90) (size 0.5 0.5) (layers F.Cu)
      (net 67 "Net-(C18-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.74 -0.375) (xy -0.74 1.325) (xy 0.51 1.325) (xy 0.51 -0.375)) (width 0.1))
      ))
    (pad 1 smd custom (at 3.45 1.55 90) (size 0.5 0.5) (layers F.Cu)
      (net 10 "Net-(D10-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.78 -1.35) (xy -0.78 0.35) (xy 0.47 0.35) (xy 0.47 -1.35)) (width 0.1))
      ))
    (pad 3 thru_hole circle (at 0.55 0 90) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 0 90) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.9 1.85 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 1.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.65 0.9 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 0.5 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.45 0.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 -1.3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.7 -0.85 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.95 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.15 -2.75 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 -2.45 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 -3.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 -2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 -2.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.65 -2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 -2.95 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2 -2.95 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 -2.15 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 -1.25 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 0.45 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 1.3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 2.2 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.05 3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.7 2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 2.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 2.9 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.7 3.15 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 2.5 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at -3.4 -3.45 90) (size 0.3 0.3) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 0) (xy 0 7) (xy 5.75 7) (xy 5.75 6.15) (xy 5.25 5.65)
           (xy 5.25 1.5) (xy 5.75 1) (xy 5.75 0)) (width 0.5))
      ))
    (pad 3 thru_hole circle (at -2.11 2.795 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (model ${KIPRJMOD}/LuxeonRebel.stp
      (offset (xyz 0.45 0 0.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module MultiSpectLED:LuxeonRebelColor (layer F.Cu) (tedit 61FA1CA8)
    (at 228.2 84.5 90)
    (fp_text reference D9 (at 2.7 -3.9) (layer F.SilkS))
    (fp_text value 591nm (at -4.5 1.3 180) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user - (at 2.4 3.4) (layer F.SilkS))
    (fp_text user + (at 2.4 -3 90) (layer F.SilkS))
    (fp_text user 3.05 (at -2.38376 0.019224) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user 4.50 (at 1.038115 -3.370011 90) (layer F.Fab))
    (fp_text user 1.525 (at -0.313518 -2.848821 90) (layer F.Fab))
    (fp_text user 2.25 (at 1.575482 -2.297609 90) (layer F.Fab))
    (pad 2 smd custom (at 3.4 -1.5 90) (size 0.5 0.5) (layers F.Cu)
      (net 70 "Net-(C20-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.74 -0.375) (xy -0.74 1.325) (xy 0.51 1.325) (xy 0.51 -0.375)) (width 0.1))
      ))
    (pad 1 smd custom (at 3.45 1.55 90) (size 0.5 0.5) (layers F.Cu)
      (net 9 "Net-(D9-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.78 -1.35) (xy -0.78 0.35) (xy 0.47 0.35) (xy 0.47 -1.35)) (width 0.1))
      ))
    (pad 3 thru_hole circle (at 0.55 0 90) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 0 90) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.9 1.85 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 1.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.65 0.9 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 0.5 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.45 0.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 -1.3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.7 -0.85 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.95 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.15 -2.75 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 -2.45 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 -3.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 -2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 -2.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.65 -2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 -2.95 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2 -2.95 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 -2.15 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 -1.25 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 0.45 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 1.3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 2.2 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.05 3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 3 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.7 2.05 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 2.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 2.9 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.7 3.15 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 2.5 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at -3.4 -3.45 90) (size 0.3 0.3) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 0) (xy 0 7) (xy 5.75 7) (xy 5.75 6.15) (xy 5.25 5.65)
           (xy 5.25 1.5) (xy 5.75 1) (xy 5.75 0)) (width 0.5))
      ))
    (pad 3 thru_hole circle (at -2.11 2.795 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (model ${KIPRJMOD}/LuxeonRebel.stp
      (offset (xyz 0.45 0 0.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module MultiSpectLED:LuxeonRebelColor (layer F.Cu) (tedit 61FA1CA8)
    (at 227.7 101.8 270)
    (fp_text reference D8 (at -3.125 2.925) (layer F.SilkS))
    (fp_text value 568nm (at -4.4 0.325 180) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user - (at 2.4 3.4) (layer F.SilkS))
    (fp_text user + (at 2.4 -2.1 90) (layer F.SilkS))
    (fp_text user 3.05 (at -2.38376 0.019224) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user 4.50 (at 1.038115 -3.370011 90) (layer F.Fab))
    (fp_text user 1.525 (at -0.313518 -2.848821 90) (layer F.Fab))
    (fp_text user 2.25 (at 1.575482 -2.297609 90) (layer F.Fab))
    (pad 2 smd custom (at 3.4 -1.5 270) (size 0.5 0.5) (layers F.Cu)
      (net 64 "Net-(C16-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.74 -0.375) (xy -0.74 1.325) (xy 0.51 1.325) (xy 0.51 -0.375)) (width 0.1))
      ))
    (pad 1 smd custom (at 3.45 1.55 270) (size 0.5 0.5) (layers F.Cu)
      (net 8 "Net-(D8-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.78 -1.35) (xy -0.78 0.35) (xy 0.47 0.35) (xy 0.47 -1.35)) (width 0.1))
      ))
    (pad 3 thru_hole circle (at 0.55 0 270) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 0 270) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.9 1.85 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 1.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.65 0.9 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 0.5 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.45 0.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 -1.3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.7 -0.85 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.95 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.15 -2.75 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 -2.45 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 -3.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 -2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 -2.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.65 -2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 -2.95 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2 -2.95 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 -2.15 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 -1.25 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 0.45 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 1.3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 2.2 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.05 3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.7 2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 2.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 2.9 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.7 3.15 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 2.5 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at -3.4 -3.45 270) (size 0.3 0.3) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 0) (xy 0 7) (xy 5.75 7) (xy 5.75 6.15) (xy 5.25 5.65)
           (xy 5.25 1.5) (xy 5.75 1) (xy 5.75 0)) (width 0.5))
      ))
    (pad 3 thru_hole circle (at -2.11 2.795 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (model ${KIPRJMOD}/LuxeonRebel.stp
      (offset (xyz 0.45 0 0.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module MultiSpectLED:LuxeonRebelColor (layer F.Cu) (tedit 61FA1CA8)
    (at 219.7 101.85 270)
    (fp_text reference D7 (at -3.075 2.9) (layer F.SilkS))
    (fp_text value 530nm (at -4.375 0.45 180) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user - (at 2.4 3.4) (layer F.SilkS))
    (fp_text user + (at 2.35 -2.1 90) (layer F.SilkS))
    (fp_text user 3.05 (at -2.38376 0.019224) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user 4.50 (at 1.038115 -3.370011 90) (layer F.Fab))
    (fp_text user 1.525 (at -0.313518 -2.848821 90) (layer F.Fab))
    (fp_text user 2.25 (at 1.575482 -2.297609 90) (layer F.Fab))
    (pad 2 smd custom (at 3.4 -1.5 270) (size 0.5 0.5) (layers F.Cu)
      (net 61 "Net-(C14-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.74 -0.375) (xy -0.74 1.325) (xy 0.51 1.325) (xy 0.51 -0.375)) (width 0.1))
      ))
    (pad 1 smd custom (at 3.45 1.55 270) (size 0.5 0.5) (layers F.Cu)
      (net 7 "Net-(D7-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.78 -1.35) (xy -0.78 0.35) (xy 0.47 0.35) (xy 0.47 -1.35)) (width 0.1))
      ))
    (pad 3 thru_hole circle (at 0.55 0 270) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 0 270) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.9 1.85 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 1.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.65 0.9 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 0.5 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.45 0.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 -1.3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.7 -0.85 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.95 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.15 -2.75 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 -2.45 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 -3.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 -2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 -2.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.65 -2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 -2.95 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2 -2.95 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 -2.15 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 -1.25 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 0.45 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 1.3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 2.2 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.05 3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.7 2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 2.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 2.9 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.7 3.15 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 2.5 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at -3.4 -3.45 270) (size 0.3 0.3) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 0) (xy 0 7) (xy 5.75 7) (xy 5.75 6.15) (xy 5.25 5.65)
           (xy 5.25 1.5) (xy 5.75 1) (xy 5.75 0)) (width 0.5))
      ))
    (pad 3 thru_hole circle (at -2.11 2.795 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (model ${KIPRJMOD}/LuxeonRebel.stp
      (offset (xyz 0.45 0 0.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module MultiSpectLED:LuxeonRebelColor (layer F.Cu) (tedit 61FA1CA8)
    (at 211.7 101.8 270)
    (fp_text reference D6 (at -3.05 2.95) (layer F.SilkS))
    (fp_text value 505nm (at -4.6 0.075 180) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user - (at 2.4 3.4) (layer F.SilkS))
    (fp_text user + (at 2.3 -2 90) (layer F.SilkS))
    (fp_text user 3.05 (at -2.38376 0.019224) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user 4.50 (at 1.038115 -3.370011 90) (layer F.Fab))
    (fp_text user 1.525 (at -0.313518 -2.848821 90) (layer F.Fab))
    (fp_text user 2.25 (at 1.575482 -2.297609 90) (layer F.Fab))
    (pad 2 smd custom (at 3.4 -1.5 270) (size 0.5 0.5) (layers F.Cu)
      (net 58 "Net-(C12-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.74 -0.375) (xy -0.74 1.325) (xy 0.51 1.325) (xy 0.51 -0.375)) (width 0.1))
      ))
    (pad 1 smd custom (at 3.45 1.55 270) (size 0.5 0.5) (layers F.Cu)
      (net 6 "Net-(D6-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.78 -1.35) (xy -0.78 0.35) (xy 0.47 0.35) (xy 0.47 -1.35)) (width 0.1))
      ))
    (pad 3 thru_hole circle (at 0.55 0 270) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 0 270) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.9 1.85 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 1.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.65 0.9 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 0.5 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.45 0.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 -1.3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.7 -0.85 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.95 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.15 -2.75 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 -2.45 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 -3.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 -2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 -2.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.65 -2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 -2.95 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2 -2.95 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 -2.15 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 -1.25 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 0.45 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 1.3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 2.2 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.05 3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.7 2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 2.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 2.9 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.7 3.15 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 2.5 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at -3.4 -3.45 270) (size 0.3 0.3) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 0) (xy 0 7) (xy 5.75 7) (xy 5.75 6.15) (xy 5.25 5.65)
           (xy 5.25 1.5) (xy 5.75 1) (xy 5.75 0)) (width 0.5))
      ))
    (pad 3 thru_hole circle (at -2.11 2.795 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (model ${KIPRJMOD}/LuxeonRebel.stp
      (offset (xyz 0.45 0 0.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module MultiSpectLED:LuxeonRebelColor (layer F.Cu) (tedit 61FA1CA8)
    (at 195.5 101.8 270)
    (fp_text reference D2 (at -3.1 3.2) (layer F.SilkS))
    (fp_text value 448nm (at -4.3 1.4 180) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user - (at 2.4 3.1) (layer F.SilkS))
    (fp_text user + (at 2.425 -1.9 90) (layer F.SilkS))
    (fp_text user 3.05 (at -2.38376 0.019224) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user 4.50 (at 1.038115 -3.370011 90) (layer F.Fab))
    (fp_text user 1.525 (at -0.313518 -2.848821 90) (layer F.Fab))
    (fp_text user 2.25 (at 1.575482 -2.297609 90) (layer F.Fab))
    (pad 2 smd custom (at 3.4 -1.5 270) (size 0.5 0.5) (layers F.Cu)
      (net 52 "Net-(C8-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.74 -0.375) (xy -0.74 1.325) (xy 0.51 1.325) (xy 0.51 -0.375)) (width 0.1))
      ))
    (pad 1 smd custom (at 3.45 1.55 270) (size 0.5 0.5) (layers F.Cu)
      (net 2 "Net-(D2-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.78 -1.35) (xy -0.78 0.35) (xy 0.47 0.35) (xy 0.47 -1.35)) (width 0.1))
      ))
    (pad 3 thru_hole circle (at 0.55 0 270) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 0 270) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.9 1.85 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 1.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.65 0.9 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 0.5 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.45 0.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 -1.3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.7 -0.85 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.95 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.15 -2.75 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 -2.45 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 -3.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 -2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 -2.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.65 -2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 -2.95 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2 -2.95 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 -2.15 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 -1.25 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 0.45 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 1.3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 2.2 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.05 3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.7 2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 2.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 2.9 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.7 3.15 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 2.5 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at -3.4 -3.45 270) (size 0.3 0.3) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 0) (xy 0 7) (xy 5.75 7) (xy 5.75 6.15) (xy 5.25 5.65)
           (xy 5.25 1.5) (xy 5.75 1) (xy 5.75 0)) (width 0.5))
      ))
    (pad 3 thru_hole circle (at -2.11 2.795 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (model ${KIPRJMOD}/LuxeonRebel.stp
      (offset (xyz 0.45 0 0.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module MultiSpectLED:LuxeonRebelColor (layer F.Cu) (tedit 61FA1CA8)
    (at 203.9 101.8 270)
    (fp_text reference D1 (at -3.05 2.875) (layer F.SilkS))
    (fp_text value 470nm (at -4.525 0.25 180) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user - (at 2.4 3.1) (layer F.SilkS))
    (fp_text user + (at 2.4 -2 90) (layer F.SilkS))
    (fp_text user 3.05 (at -2.38376 0.019224) (layer F.Fab))
    (fp_text user 1.25 (at -1.813303 -0.605776) (layer F.Fab))
    (fp_text user 4.50 (at 1.038115 -3.370011 90) (layer F.Fab))
    (fp_text user 1.525 (at -0.313518 -2.848821 90) (layer F.Fab))
    (fp_text user 2.25 (at 1.575482 -2.297609 90) (layer F.Fab))
    (pad 2 smd custom (at 3.4 -1.5 270) (size 0.5 0.5) (layers F.Cu)
      (net 55 "Net-(C10-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.74 -0.375) (xy -0.74 1.325) (xy 0.51 1.325) (xy 0.51 -0.375)) (width 0.1))
      ))
    (pad 1 smd custom (at 3.45 1.55 270) (size 0.5 0.5) (layers F.Cu)
      (net 1 "Net-(D1-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.78 -1.35) (xy -0.78 0.35) (xy 0.47 0.35) (xy 0.47 -1.35)) (width 0.1))
      ))
    (pad 3 thru_hole circle (at 0.55 0 270) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 0 270) (size 0.3 0.3) (drill 0.12) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.9 1.85 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 1.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.65 0.9 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 0.5 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.45 0.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.75 -1.3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.7 -0.85 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.95 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.15 -2.75 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 -2.45 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.65 -3.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 -2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 -2.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.65 -2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 -2.95 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2 -2.95 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 -2.15 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 -1.25 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 0.45 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.45 1.3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.55 2.2 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.05 3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.1 3 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.7 2.05 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.25 2.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.2 2.9 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.7 3.15 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.25 2.5 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at -3.4 -3.45 270) (size 0.3 0.3) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 0) (xy 0 7) (xy 5.75 7) (xy 5.75 6.15) (xy 5.25 5.65)
           (xy 5.25 1.5) (xy 5.75 1) (xy 5.75 0)) (width 0.5))
      ))
    (pad 3 thru_hole circle (at -2.11 2.795 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (model ${KIPRJMOD}/LuxeonRebel.stp
      (offset (xyz 0.45 0 0.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module MultiSpectLED:NKK_FR02 (layer B.Cu) (tedit 61FA1CC4)
    (at 131.2 73.8 270)
    (fp_text reference SW2 (at -6.7 5.5 270) (layer B.SilkS))
    (fp_text value NKK_HEXADEC (at -7.6 8 90) (layer B.Fab))
    (pad C smd rect (at -1.27 -6.125 270) (size 1 1.75) (layers B.Cu B.Paste B.Mask)
      (net 18 /GND))
    (pad 8 smd rect (at 3.81 6.125 270) (size 1 1.75) (layers B.Cu B.Paste B.Mask)
      (net 42 /BRIGHT8))
    (pad 4 smd rect (at 1.27 6.125 270) (size 1 1.75) (layers B.Cu B.Paste B.Mask)
      (net 43 /BRIGHT4))
    (pad 2 smd rect (at -1.27 6.125 270) (size 1 1.75) (layers B.Cu B.Paste B.Mask)
      (net 44 /BRIGHT2))
    (pad 1 smd rect (at -3.81 6.125 270) (size 1 1.75) (layers B.Cu B.Paste B.Mask)
      (net 45 /BRIGHT1))
    (model ${KIPRJMOD}/FR02KR16P.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module MultiSpectLED:3mm_PTH (layer F.Cu) (tedit 61FA1C55)
    (at 214.8 112)
    (fp_text reference H7 (at 5 -3.5) (layer F.SilkS) hide)
    (fp_text value 3mm_PTH (at -4.3 -5.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3) (layers *.Cu *.Mask)
      (net 18 /GND) (zone_connect 2))
  )
  (module MultiSpectLED:3mm_PTH (layer F.Cu) (tedit 61FA1C55)
    (at 198 93)
    (fp_text reference H6 (at 5 -3.5) (layer F.SilkS) hide)
    (fp_text value 3mm_PTH (at -6.9 0.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3) (layers *.Cu *.Mask)
      (net 18 /GND) (zone_connect 2))
  )
  (module MultiSpectLED:3mm_PTH (layer F.Cu) (tedit 61FA1C55)
    (at 168 93)
    (fp_text reference H5 (at 5 -3.5) (layer F.SilkS) hide)
    (fp_text value 3mm_PTH (at -4.3 -5.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3) (layers *.Cu *.Mask)
      (net 18 /GND) (zone_connect 2))
  )
  (module MultiSpectLED:3mm_PTH (layer F.Cu) (tedit 61FA1C55)
    (at 182.8 112)
    (fp_text reference H4 (at 5 -3.5) (layer F.SilkS) hide)
    (fp_text value 3mm_PTH (at -4.3 -5.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3) (layers *.Cu *.Mask)
      (net 18 /GND) (zone_connect 2))
  )
  (module MultiSpectLED:3mm_PTH (layer F.Cu) (tedit 61FA1C55)
    (at 214.8 74)
    (fp_text reference H3 (at 5 -3.5) (layer F.SilkS) hide)
    (fp_text value 3mm_PTH (at -4.3 -5.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3) (layers *.Cu *.Mask)
      (net 18 /GND) (zone_connect 2))
  )
  (module MultiSpectLED:3mm_PTH (layer F.Cu) (tedit 61FA1C55)
    (at 182.8 74)
    (fp_text reference H2 (at 5 -3.5) (layer F.SilkS) hide)
    (fp_text value 3mm_PTH (at -4.3 -5.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3) (layers *.Cu *.Mask)
      (net 18 /GND) (zone_connect 2))
  )
  (module MultiSpectLED:NKK_FR02 (layer B.Cu) (tedit 61FA1CC4)
    (at 131.2 100.8 270)
    (fp_text reference SW1 (at 5.9 5.9 270) (layer B.SilkS))
    (fp_text value NKK_HEXADEC (at -7.6 8 90) (layer B.Fab))
    (pad C smd rect (at -1.27 -6.125 270) (size 1 1.75) (layers B.Cu B.Paste B.Mask)
      (net 18 /GND))
    (pad 8 smd rect (at 3.81 6.125 270) (size 1 1.75) (layers B.Cu B.Paste B.Mask)
      (net 37 /LED_SEL8))
    (pad 4 smd rect (at 1.27 6.125 270) (size 1 1.75) (layers B.Cu B.Paste B.Mask)
      (net 38 /LED_SEL4))
    (pad 2 smd rect (at -1.27 6.125 270) (size 1 1.75) (layers B.Cu B.Paste B.Mask)
      (net 39 /LED_SEL2))
    (pad 1 smd rect (at -3.81 6.125 270) (size 1 1.75) (layers B.Cu B.Paste B.Mask)
      (net 40 /LED_SEL1))
    (model ${KIPRJMOD}/FR02KR16P.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module MultiSpectLED:TeensyLC (layer F.Cu) (tedit 61FA1C4C)
    (at 141.6 87.2)
    (attr smd)
    (fp_text reference U2 (at 18.5 -11 270) (layer F.SilkS))
    (fp_text value TeensyLC (at 0 0) (layer F.Fab))
    (pad 26 smd rect (at 18 -4.91 90) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad26)"))
    (pad PRG smd rect (at 18 -2.37 90) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-PadPRG)"))
    (pad GNDb smd rect (at 18 0.17 90) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-PadGNDb)"))
    (pad 33Vb smd rect (at 18 2.71 90) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad33Vb)"))
    (pad 17_5V smd rect (at 18 5.25 90) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad17_5V)"))
    (pad 12 smd rect (at 16.51 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 41 /PWM_D3_280nm))
    (pad 13 smd rect (at 16.51 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 87 /PWM_D15_940nm))
    (pad 11 smd rect (at 13.97 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 48 /PWM_D5_367nm))
    (pad 14 smd rect (at 13.97 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 84 /PWM_D14_850nm))
    (pad 10 smd rect (at 11.43 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 51 /PWM_D4_405nm))
    (pad 15 smd rect (at 11.43 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 81 /PWM_D13_740nm))
    (pad 9 smd rect (at 8.89 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 54 /PWM_D2_448nm))
    (pad 16 smd rect (at 8.89 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 78 /PWM_D12_655nm))
    (pad 8 smd rect (at 6.35 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 57 /PWM_D1_470nm))
    (pad 17 smd rect (at 6.35 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 75 /PWM_D11_627nm))
    (pad 7 smd rect (at 3.81 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 60 /PWM_D6_505nm))
    (pad 18 smd rect (at 3.81 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 69 /PWM_D10_617nm))
    (pad 6 smd rect (at 1.27 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 63 /PWM_D7_530nm))
    (pad 19 smd rect (at 1.27 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 72 /PWM_D9_591nm))
    (pad 5 smd rect (at -1.27 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 66 /PWM_D8_568nm))
    (pad 20 smd rect (at -1.27 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 45 /BRIGHT1))
    (pad 4 smd rect (at -3.81 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad4)"))
    (pad 21 smd rect (at -3.81 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 44 /BRIGHT2))
    (pad 3 smd rect (at -6.35 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 37 /LED_SEL8))
    (pad 22 smd rect (at -6.35 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 43 /BRIGHT4))
    (pad 2 smd rect (at -8.89 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 38 /LED_SEL4))
    (pad 23 smd rect (at -8.89 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 42 /BRIGHT8))
    (pad 1 smd rect (at -11.43 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 39 /LED_SEL2))
    (pad 33Va smd rect (at -11.43 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad33Va)"))
    (pad 0 smd rect (at -13.97 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 40 /LED_SEL1))
    (pad GNDc smd rect (at -13.97 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U2-PadGNDc)"))
    (pad GNDa smd rect (at -16.51 9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad VIN smd rect (at -16.51 -9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (model ${KIPRJMOD}/Teensy_lc.stp
      (offset (xyz -17.75 9 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 167.8 114.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -0.2 1.6) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /+5V) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:SOT-23-5 (layer F.Cu) (tedit 61FA1C32)
    (at 165.3 111.5 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 1.6 -2.6 180) (layer F.SilkS))
    (fp_text value PAM2804 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D3-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /+5V))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 41 /PWM_D3_280nm))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:R_0805_2012Metric (layer F.Cu) (tedit 61FA20BD)
    (at 165.4 107.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 1 -1.6 180) (layer F.SilkS))
    (fp_text value 0.2 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D3-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:L_1007_2518Metric (layer F.Cu) (tedit 61FA1C19)
    (at 168.4 112 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 0.9 2 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.1 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C1-Pad1)"))
    (pad 1 smd roundrect (at -1.05 0 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(L1-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:C_0805_2012Metric (layer F.Cu) (tedit 61FA1E25)
    (at 168.6 107.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 1.1 1.9 180) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /GND) (zone_connect 1))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C1-Pad1)") (zone_connect 1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MultiSpectLED:3mm_PTH (layer F.Cu) (tedit 61FA1C55)
    (at 228 93.1)
    (fp_text reference H1 (at 5 -3.5) (layer F.SilkS) hide)
    (fp_text value 3mm_PTH (at -4.3 -5.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3) (layers *.Cu *.Mask)
      (net 18 /GND) (zone_connect 2))
  )
  (module MultiSpectLED:QT_Brightek_QBHP684 (layer F.Cu) (tedit 61F8C343)
    (at 187 84.6)
    (fp_text reference D13 (at 3.7 1.2) (layer F.SilkS))
    (fp_text value 740nm (at 0.3 5.2) (layer F.Fab))
    (fp_text user + (at -2.5 -1.1) (layer F.SilkS))
    (fp_text user - (at 2.6 -1.2) (layer F.SilkS))
    (pad 3 thru_hole circle (at 2.5 -3.8 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 2.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 2.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.1 -2.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.4 -3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 -2.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.2 -3.8 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.6 2.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.2 3.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.2 -3.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.5 -3.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.8 -2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.1 2.3) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.6 -2.5 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.4 -2.9 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.7 -2.9 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.4 3.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at 0.1 0.1) (size 1.75 6) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -3 4.25) (xy 3.05 4.25) (xy 3.05 1.75) (xy -3 1.75)) (width 0.1))
        (gr_poly (pts
           (xy -3 -1.75) (xy 3.05 -1.75) (xy 3.05 -4.25) (xy -3 -4.25)) (width 0.1))
      ))
    (pad 2 smd rect (at 2.13 0.1) (size 2 3) (layers F.Cu)
      (net 13 "Net-(D13-Pad2)") (zone_connect 0))
    (pad 3 thru_hole circle (at 2.8 2.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.5 4) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.6 3.2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.7 3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.5 3.7) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.2 4) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.4 3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.6 -3.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 1 smd rect (at -1.93 0.1 180) (size 2 3) (layers F.Cu)
      (net 79 "Net-(C26-Pad1)") (zone_connect 0))
  )
  (module MultiSpectLED:SeoulViosys_CUN6GF1A (layer F.Cu) (tedit 61F8C093)
    (at 178.1 101.5 180)
    (fp_text reference D5 (at 2.7 1.3) (layer F.SilkS))
    (fp_text value 367nm (at -0.6 -5.1) (layer F.Fab))
    (fp_text user - (at 2.5 -1.2) (layer F.SilkS))
    (fp_text user + (at -2.6 -1.1) (layer F.SilkS))
    (pad 3 thru_hole circle (at 2.4 4 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.4 2.7 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.5 -2.5) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.5 -3.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -3.5) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.6 -2.9) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 3.7 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.6 -2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.6 2.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 -3.5) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.7 -2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -2.9) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.5 3.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.5 3.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 2 smd rect (at -2.03 0.1) (size 2 3) (layers F.Cu)
      (net 46 "Net-(C4-Pad1)") (zone_connect 0))
    (pad 1 smd rect (at 2.03 0.1 180) (size 2 3) (layers F.Cu)
      (net 5 "Net-(D5-Pad1)") (zone_connect 0))
    (pad 3 thru_hole circle (at 2.7 2.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.6 3.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at 0 0.1 180) (size 1.75 6) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -3 4.25) (xy 3.05 4.25) (xy 3.05 1.75) (xy -3 1.75)) (width 0.1))
        (gr_poly (pts
           (xy -3 -1.75) (xy 3.05 -1.75) (xy 3.05 -4.25) (xy -3 -4.25)) (width 0.1))
      ))
    (pad 3 thru_hole circle (at -1.4 -2.5) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.5 2.7 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.3 4 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.5 -3.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.3 -3.8) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 3.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.4 -3.8) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 3.7 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0 -2.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0 2.3 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
  )
  (module MultiSpectLED:Everlight_ELUA3535 (layer F.Cu) (tedit 61FA1C72)
    (at 186.9 101.5 180)
    (fp_text reference D4 (at 2.6 1.3) (layer F.SilkS))
    (fp_text value 405nm (at -13.3 -13.6) (layer F.Fab))
    (fp_text user + (at -2.6 -1.1) (layer F.SilkS))
    (fp_text user - (at 2.5 -1.2) (layer F.SilkS))
    (pad 3 thru_hole circle (at 1.4 3.7 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.5 -3.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.4 4 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.7 2.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 1 smd rect (at -2.03 0.1) (size 2 3) (layers F.Cu)
      (net 49 "Net-(C6-Pad1)") (zone_connect 0))
    (pad 3 thru_hole circle (at -2.6 2.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.5 3.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.6 -2.9) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.6 -2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.7 -2) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.4 2.7 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.5 3.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -2.9) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -3.5) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 2 smd rect (at 2.03 0.1 180) (size 2 3) (layers F.Cu)
      (net 4 "Net-(D4-Pad2)") (zone_connect 0))
    (pad 3 thru_hole circle (at 1.5 -2.5) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 -3.5) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 3.7 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 3.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.3 -3.8) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.5 -3.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.5 2.7 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.4 -2.5) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.4 -3.8) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at 0 0.1 180) (size 1.75 6) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -3 4.25) (xy 3.05 4.25) (xy 3.05 1.75) (xy -3 1.75)) (width 0.1))
        (gr_poly (pts
           (xy -3 -1.75) (xy 3.05 -1.75) (xy 3.05 -4.25) (xy -3 -4.25)) (width 0.1))
      ))
    (pad 3 thru_hole circle (at -2.3 4 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.6 3.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0 -2.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0 2.3 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
  )
  (module MultiSpectLED:Luminus_XBT3535 (layer F.Cu) (tedit 61FA1C78)
    (at 169.6 101.5 180)
    (fp_text reference D3 (at 2.9 1) (layer F.SilkS))
    (fp_text value 280nm (at -2.2 5) (layer F.Fab))
    (fp_text user + (at -2.6 -1.2) (layer F.SilkS))
    (fp_text user - (at 2.5 -1.3) (layer F.SilkS))
    (pad 3 thru_hole circle (at 0 2.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0 -2.3 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.5 -3.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.5 -3.2 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.4 -2.6) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 -3) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.6 -2.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.3 -3.9) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 -3.6) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.7 2.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.5 2.6 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 3.6 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.6 3 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.4 3.9 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.7 -2.1) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.5 -2.6) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 1.4 -3.6) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.6 -3) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.4 -3.9) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.4 2.6 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -1.3 3.6 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.3 3.9 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0.5 3.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -0.5 3.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.5 3 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 thru_hole circle (at -2.6 2.1 180) (size 0.75 0.75) (drill 0.5) (layers *.Cu)
      (net 18 /GND) (zone_connect 2))
    (pad 3 smd custom (at 0 0 180) (size 1.75 6) (layers F.Cu)
      (net 18 /GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -3 4.25) (xy 3.05 4.25) (xy 3.05 1.75) (xy -3 1.75)) (width 0.1))
        (gr_poly (pts
           (xy -3 -1.75) (xy 3.05 -1.75) (xy 3.05 -4.25) (xy -3 -4.25)) (width 0.1))
      ))
    (pad 2 smd rect (at -2.03 0) (size 2 3) (layers F.Cu)
      (net 16 "Net-(C1-Pad1)") (zone_connect 0))
    (pad 1 smd rect (at 2.03 0 180) (size 2 3) (layers F.Cu)
      (net 3 "Net-(D3-Pad1)") (zone_connect 0))
    (model "${KIPRJMOD}/Luminus XBT-3535_DF_102620.STEP"
      (offset (xyz 0 0 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 125.1 100.6 90) (layer F.SilkS))
  (gr_text VIN (at 125.1 74.1 90) (layer F.SilkS))
  (gr_text Teensy-LC (at 160.2 98.5 90) (layer F.SilkS))
  (gr_text "USB\nprogramming" (at 126.7 86.5 270) (layer B.SilkS))
  (gr_text "USB-C\npower only\n5V  >3A" (at 128.1 113.7 270) (layer B.SilkS))
  (gr_text "multispectral LED\nilluminator\n@benkrasnow\nFeb 4 2022" (at 135.9 87.4 270) (layer B.SilkS))
  (gr_text "0 - OFF\n1 - 100mW\n2 - 200mW\n3 - 300mW\n4 - 400mW\n5 - 500mW\n6 - 600mW\n7 - 700mW\n8 - 800mW" (at 146.6 83.5 270) (layer B.SilkS))
  (gr_text "9 - 900mW\nA - 1.0W\nB - 1.1W\nC - 1.2W\nD - 1.3W\nE - 1.4W\nF - 1.5W" (at 147.8 74.4 270) (layer B.SilkS))
  (gr_text "9 - 591nm\nA - 617nm\nB - 627nm\nC - 655nm\nD - 740nm\nE - 850nm\nF - 940nm" (at 148.1 100.4 270) (layer B.SilkS))
  (gr_text "0 - PROG\n1 - 280nm\n2 - 367nm\n3 - 405nm\n4 - 448nm\n5 - 470nm\n6 - 505nm\n7 - 530nm\n8 - 568nm" (at 146.9 109.5 270) (layer B.SilkS))
  (gr_text 940nm (at 172 89.6) (layer F.SilkS))
  (gr_text 850nm (at 178.2 89.6) (layer F.SilkS))
  (gr_text 740nm (at 187.3 89.6) (layer F.SilkS))
  (gr_text 655nm (at 200.5 88.7) (layer F.SilkS))
  (gr_text 627nm (at 209.9 88.7) (layer F.SilkS))
  (gr_text 617nm (at 219.3 88.8) (layer F.SilkS))
  (gr_text 591nm (at 228.5 88.7) (layer F.SilkS))
  (dimension 9 (width 0.15) (layer F.Fab)
    (gr_text "9.000 mm" (at 232.5 61.2) (layer F.Fab))
    (feature1 (pts (xy 228 93.1) (xy 228 61.913579)))
    (feature2 (pts (xy 237 93.1) (xy 237 61.913579)))
    (crossbar (pts (xy 237 62.5) (xy 228 62.5)))
    (arrow1a (pts (xy 228 62.5) (xy 229.126504 61.913579)))
    (arrow1b (pts (xy 228 62.5) (xy 229.126504 63.086421)))
    (arrow2a (pts (xy 237 62.5) (xy 235.873496 61.913579)))
    (arrow2b (pts (xy 237 62.5) (xy 235.873496 63.086421)))
  )
  (gr_text 568nm (at 227.9 97.6) (layer F.SilkS))
  (gr_text 530nm (at 219.8 97.7) (layer F.SilkS))
  (gr_text 505nm (at 211.7 97.6) (layer F.SilkS))
  (gr_text 470nm (at 203.85 97.6) (layer F.SilkS))
  (gr_text 448nm (at 195.6 97.6) (layer F.SilkS))
  (gr_text 405nm (at 186.9 96.6) (layer F.SilkS))
  (gr_text 367nm (at 178.4 96.6) (layer F.SilkS))
  (gr_text 280nm (at 171.7 96.7) (layer F.SilkS))
  (dimension 83 (width 0.12) (layer F.Fab)
    (gr_text "83.000 mm" (at 195.5 52.93) (layer F.Fab))
    (feature1 (pts (xy 154 63.4) (xy 154 53.613579)))
    (feature2 (pts (xy 237 63.4) (xy 237 53.613579)))
    (crossbar (pts (xy 237 54.2) (xy 154 54.2)))
    (arrow1a (pts (xy 154 54.2) (xy 155.126504 53.613579)))
    (arrow1b (pts (xy 154 54.2) (xy 155.126504 54.786421)))
    (arrow2a (pts (xy 237 54.2) (xy 235.873496 53.613579)))
    (arrow2b (pts (xy 237 54.2) (xy 235.873496 54.786421)))
  )
  (dimension 45.000111 (width 0.12) (layer F.Fab)
    (gr_text "45.000 mm" (at 242.743954 92.978014 270.1) (layer F.Fab))
    (feature1 (pts (xy 232.9 115.5) (xy 242.110376 115.479532)))
    (feature2 (pts (xy 232.8 70.5) (xy 242.010376 70.479532)))
    (crossbar (pts (xy 241.423957 70.480836) (xy 241.523957 115.480836)))
    (arrow1a (pts (xy 241.523957 115.480836) (xy 240.935034 114.355638)))
    (arrow1b (pts (xy 241.523957 115.480836) (xy 242.107873 114.353032)))
    (arrow2a (pts (xy 241.423957 70.480836) (xy 240.840041 71.60864)))
    (arrow2b (pts (xy 241.423957 70.480836) (xy 242.01288 71.606034)))
  )
  (dimension 5.5 (width 0.12) (layer F.Fab)
    (gr_text "5.500 mm" (at 244.57 118.25 90) (layer F.Fab))
    (feature1 (pts (xy 237 115.5) (xy 243.886421 115.5)))
    (feature2 (pts (xy 237 121) (xy 243.886421 121)))
    (crossbar (pts (xy 243.3 121) (xy 243.3 115.5)))
    (arrow1a (pts (xy 243.3 115.5) (xy 243.886421 116.626504)))
    (arrow1b (pts (xy 243.3 115.5) (xy 242.713579 116.626504)))
    (arrow2a (pts (xy 243.3 121) (xy 243.886421 119.873496)))
    (arrow2b (pts (xy 243.3 121) (xy 242.713579 119.873496)))
  )
  (dimension 5.5 (width 0.12) (layer F.Fab)
    (gr_text "5.500 mm" (at 244.77 67.75 270) (layer F.Fab))
    (feature1 (pts (xy 237 70.5) (xy 244.086421 70.5)))
    (feature2 (pts (xy 237 65) (xy 244.086421 65)))
    (crossbar (pts (xy 243.5 65) (xy 243.5 70.5)))
    (arrow1a (pts (xy 243.5 70.5) (xy 242.913579 69.373496)))
    (arrow1b (pts (xy 243.5 70.5) (xy 244.086421 69.373496)))
    (arrow2a (pts (xy 243.5 65) (xy 242.913579 66.126504)))
    (arrow2b (pts (xy 243.5 65) (xy 244.086421 66.126504)))
  )
  (dimension 28 (width 0.12) (layer F.Fab)
    (gr_text "28.000 mm" (at 252.07 79 270) (layer F.Fab))
    (feature1 (pts (xy 237 93) (xy 251.386421 93)))
    (feature2 (pts (xy 237 65) (xy 251.386421 65)))
    (crossbar (pts (xy 250.8 65) (xy 250.8 93)))
    (arrow1a (pts (xy 250.8 93) (xy 250.213579 91.873496)))
    (arrow1b (pts (xy 250.8 93) (xy 251.386421 91.873496)))
    (arrow2a (pts (xy 250.8 65) (xy 250.213579 66.126504)))
    (arrow2b (pts (xy 250.8 65) (xy 251.386421 66.126504)))
  )
  (gr_line (start 237 121) (end 123.6 121) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 237 65) (end 237 121) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.6 65) (end 237 65) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.6 121) (end 123.6 65) (layer Edge.Cuts) (width 0.05))
  (zone (net 18) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 232.7 115.5) (xy 232.7 70.5) (xy 163.1 70.5) (xy 163.1 115.5)
      )
    )
  )
  (zone (net 18) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 231.95 70.55) (xy 232.05 115.45) (xy 163.2 115.4) (xy 163.1 70.5)
      )
    )
  )
)
