(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(BT1-+)")
  (net 2 "GND")
  (net 3 "VCC")
  (net 4 "Net-(D1-A)")
  (net 5 "Net-(D2-A)")
  (net 6 "Reset")
  (net 7 "Net-(J2-Pad4)")
  (net 8 "PB1-SCK")
  (net 9 "PB0-Miso")
  (net 10 "Net-(U1-PB2)")
  (net 11 "Net-(R4-Pad1)")
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 126.25 46.75 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0.275 1.55) (layer "F.SilkS"))
    (fp_text value ".1uf" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_1206_3216Metric" (layer "F.Cu")
    (at 114.6 50.4)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D1" (at -1.7 -1.675) (layer "F.SilkS"))
    (fp_text value "Green LED" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 4 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_1206_3216Metric" (layer "F.Cu")
    (at 108 50.4 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D2" (at 3 0.1) (layer "F.SilkS"))
    (fp_text value "RedLED" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 5 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 122.75 45.5 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 1.2 1.625 180) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 9 "PB0-Miso") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 108 47.75)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -2.9 -0.15) (layer "F.SilkS"))
    (fp_text value "2k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 5 "Net-(D2-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 8 "PB1-SCK") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 119.75 50.5)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -1.85 -1.6) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 4 "Net-(D1-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 10 "Net-(U1-PB2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 134.1 42.4375 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 1.6125 -1.65 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 11 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 6 "Reset") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 124 41.6)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 1.55 -1.225) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 9 "PB0-Miso") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 7 "Net-(J2-Pad4)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "F.Cu")
    (at 126.25 50)
    (descr "6-pin SOT-23 package")
    (tags "SOT-23-6")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "ki_description" "12MHz, 1kB Flash, 32B SRAM, No EEPROM, ADC, SOT-23-6")
    (property "ki_keywords" "AVR 8bit Microcontroller tinyAVR")
    (attr smd)
    (fp_text reference "AT10" (at -2.75 -0.8) (layer "F.SilkS"))
    (fp_text value "ATtiny10-TS" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "PB0-Miso") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "2" smd rect (at -1.1 0) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.1 0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "PB1-SCK") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "4" smd rect (at 1.1 0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(U1-PB2)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "5" smd rect (at 1.1 0) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "6" smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Reset") (pinfunction "~{RESET}/PB3") (pintype "bidirectional"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "++Sherms-Custom-Libs:Button_4mm-4pad" (layer "F.Cu")
    (at 134.7 48.7 90)
    (property "Category" "Switches")
    (property "DK_Datasheet_Link" "http://spec_sheets.e-switch.com/specs/29-KS01Q01.pdf")
    (property "DK_Detail_Page" "/product-detail/en/e-switch/KS-01Q-01/EG4791-ND/2116270")
    (property "Description" "SWITCH PUSH SPST-NO 0.01A 35V")
    (property "Digi-Key_PN" "EG4791-ND")
    (property "Family" "Pushbutton Switches")
    (property "MPN" "KS-01Q-01")
    (property "Manufacturer" "E-Switch")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "Status" "Obsolete NonStock")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "S1" (at 0 0 180) (layer "F.SilkS"))
    (fp_text value "Push Button" (at 0.5 4.25 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(R4-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 -5 90) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd roundrect (at -2 -5 90) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "4" smd roundrect (at 2 0 90) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x03_P1.27mm_Vertical" (layer "F.Cu")
    (at 130.77 41.83 -90)
    (descr "Through hole straight pin header, 2x03, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 1.27mm double row")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0.17 -1.23 180) (layer "F.SilkS"))
    (fp_text value "CONN-2x3" (at 0.635 4.235 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.635 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 9 "PB0-Miso") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 270) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 3 "VCC") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 8 "PB1-SCK") (pintype "passive"))
    (pad "4" thru_hole oval (at 1.27 1.27 270) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J2-Pad4)") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 6 "Reset") (pintype "passive"))
    (pad "6" thru_hole oval (at 1.27 2.54 270) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x03_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "++Sherms-Custom-Libs:Rectangle-Pad_4mmx10mm" (layer "F.Cu")
    (at 137.8 51.7)
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H1" (at 0.3 -10.85) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 2) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 -5) (size 4 10) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VCC") (pinfunction "1") (pintype "input"))
  )
  (footprint "++Sherms-Custom-Libs:Rectangle-Pad_4mmx10mm" (layer "F.Cu")
    (at 102.3 51.6)
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H2" (at 0.05 -10.75) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 2) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 -5) (size 4 10) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "PB0-Miso") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 119.7 41.9)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.425 -0.4) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(BT1-+)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "+++Sherms-kicad5-libs:CR2032-Battery-sidemnt_10.5x5.5x4mm-k5" (layer "F.Cu")
    (at 111.15 38.9 180)
    (property "Sheetfile" "C:/Users/sherm/Google Drive/Schematics/ATtiny/ATtiny10/Attiny10-moisture-water-sensor-kicad5-v2/Attiny10-moisture-water-sensor.sch")
    (property "Sheetname" "")
    (property "ki_description" "Single-cell battery")
    (property "ki_keywords" "battery cell")
    (attr through_hole)
    (fp_text reference "BT1" (at 0.1 -2.45) (layer "F.SilkS"))
    (fp_text value "Battery_Cell" (at 0 -0.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5.2 -2.45 180) (size 1.75 1.75) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(BT1-+)") (pinfunction "+") (pintype "passive"))
    (pad "1" thru_hole circle (at 5.3 -2.45 180) (size 1.75 1.75) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(BT1-+)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -6.5 180) (size 1.75 1.75) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
  )
  (gr_line (start 140 52) (end 100 52)
    (layer "Edge.Cuts"))
  (gr_line (start 140 40) (end 140 52)
    (layer "Edge.Cuts"))
  (gr_line (start 100 52) (end 100 40)
    (layer "Edge.Cuts"))
  (gr_line (start 100 40) (end 140 40)
    (layer "Edge.Cuts"))
  (gr_text "-" (at 127 43) (layer "B.SilkS"))
  (gr_text "+\n" (at 107.125 41.8) (layer "B.SilkS"))
  (gr_text "R" (at 127 41.9) (layer "B.SilkS"))
  (gr_text "+" (at 114.775 41.375) (layer "B.SilkS"))
  (gr_text "Attiny10 Moisture Sensor v4\nSherman Stebbins" (at 112.8 47.9) (layer "B.SilkS"))
  (gr_text "GND" (at 113.6 44.8) (layer "B.SilkS"))
  (gr_text "+" (at 132.2 43.1) (layer "B.SilkS"))
  (gr_text "GND" (at 111.4 50.55) (layer "F.SilkS"))
  (gr_text "GND" (at 120.6 46.975) (layer "F.SilkS"))
  (gr_text "Grn" (at 114.55 50.4) (layer "F.SilkS"))
  (gr_text "1k" (at 119.75 50.55) (layer "F.SilkS"))
  (gr_text "1k" (at 134.3 42.45) (layer "F.SilkS"))
  (gr_text "1k" (at 123.85 41.925) (layer "F.SilkS"))
  (gr_text "Red" (at 107.95 50.35) (layer "F.SilkS"))
  (gr_text "+" (at 115.15 42.175) (layer "F.SilkS"))
  (gr_text "+" (at 132.2 43.2) (layer "F.SilkS"))
  (gr_text "+" (at 128.45 49.95) (layer "F.SilkS"))
  (gr_text "GND" (at 113.6 44.8) (layer "F.SilkS"))
  (gr_text "-" (at 127 43.1) (layer "F.SilkS"))
  (gr_text "+" (at 107 42.1) (layer "F.SilkS"))
  (gr_text "2k" (at 107.95 47.7) (layer "F.SilkS"))
  (gr_text "-" (at 124.05 50) (layer "F.SilkS"))
  (gr_text "R" (at 127 41.9) (layer "F.SilkS"))
  (gr_text "1m" (at 122.75 45.75) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 116.45 41.2) (xy 111.25 45.25))
    (height -0.390298)
    (gr_text "6.5911 mm" (at 113.383189 42.625638 37.91310459) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 100 53) (xy 100 41.8))
    (height -1.4)
    (gr_text "11.2000 mm" (at 97.45 47.4 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 116.45 41.2) (xy 106 41.25))
    (height 0.79999)
    (gr_text "10.4501 mm" (at 111.21567 39.275032 0.2741403937) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 140 40) (xy 99.9 40))
    (height 1.2)
    (gr_text "40.1000 mm" (at 119.95 37.65) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 111.25 45.25) (xy 111.25 41.25))
    (height -1.4)
    (gr_text "4.0000 mm" (at 108.75 43.25 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 116.5 41.65) (xy 116.5 40.85))
    (height 1.7)
    (gr_text "0.8000 mm" (at 117.05 41.25 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
)
