(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 38)
    (no_connects 0)
    (area 145.692999 72.814347 182.947001 109.424516)
    (thickness 1.6)
    (drawings 15)
    (tracks 134)
    (zones 0)
    (modules 26)
    (nets 22)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 2.032)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.254)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 1 0.5)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 210.82 95.25)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000000)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +BATT)
  (net 3 "Net-(CON1-Pad1)")
  (net 4 "Net-(CON1-Pad3)")
  (net 5 "Net-(CON1-Pad4)")
  (net 6 "Net-(CON1-Pad5)")
  (net 7 "Net-(D1-Pad1)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 "Net-(D3-Pad1)")
  (net 10 "Net-(D0-Pad1)")
  (net 11 "Net-(D3-Pad2)")
  (net 12 "Net-(D4-Pad2)")
  (net 13 "Net-(D4-Pad1)")
  (net 14 "Net-(P5-Pad1)")
  (net 15 "Net-(PG0-Pad1)")
  (net 16 "Net-(U1-Pad14)")
  (net 17 "Net-(U1-Pad15)")
  (net 18 "Net-(D1-Pad2)")
  (net 19 "Net-(D2-Pad2)")
  (net 20 "Net-(BT1-Pad1)")
  (net 21 "Net-(SW1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(CON1-Pad4)")
    (add_net "Net-(CON1-Pad5)")
    (add_net "Net-(D0-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(PG0-Pad1)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
  )
  (module footprints:BATT_CR2032_SMD (layer B.Cu) (tedit 56CFB5D2)
    (at 162.82 98.25 180)
    (tags battery)
    (fp_text reference BT1 (at 0 -5.08 180) (layer B.SilkS) hide)
    (fp_text value Battery (at 0 2.54 180) (layer B.SilkS) hide)
    (pad 2 smd circle (at 0 0 180) (size 17.78 17.78) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -11.43 0 180) (size 2.54 5.08) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at 11.43 0 180) (size 2.54 5.08) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(BT1-Pad1)"))
  )
  (module footprints:AVR-ISP-6 (layer F.Cu) (tedit 5860A6AE)
    (at 169.82 91.25 90)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference CON1 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 0 -3.72 90) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(CON1-Pad1)"))
    (pad 2 smd rect (at 2.54 0 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (pad 3 smd oval (at 0 2.54 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(CON1-Pad3)"))
    (pad 4 smd oval (at 2.54 2.54 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CON1-Pad4)"))
    (pad 5 smd oval (at 0 5.08 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CON1-Pad5)"))
    (pad 6 smd oval (at 2.54 5.08 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module footprints:testPad (layer F.Cu) (tedit 5A71576D)
    (at 165.82 93.25)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P0 (at -1.27 0.175) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(CON1-Pad3)"))
  )
  (module footprints:testPad (layer F.Cu) (tedit 5902BD57)
    (at 165.82 97.25)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P1 (at -0.0635 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D1-Pad2)"))
  )
  (module footprints:testPad (layer F.Cu) (tedit 5A715F16)
    (at 165.57 100.25)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P2 (at -0.25 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D2-Pad2)"))
  )
  (module footprints:testPad (layer F.Cu) (tedit 5A71575C)
    (at 165.32 103.25)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P3 (at 0 0.65) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D3-Pad2)"))
  )
  (module footprints:testPad (layer F.Cu) (tedit 5902BD57)
    (at 165.07 106.25)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P4 (at -0.0635 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad2)"))
  )
  (module footprints:testPad (layer F.Cu) (tedit 5902BD57)
    (at 150.32 93.25)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference PG0 (at -0.0635 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
  )
  (module footprints:testPad (layer F.Cu) (tedit 5A715734)
    (at 152.07 97.25)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference PG1 (at 2 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
  )
  (module footprints:testPad (layer F.Cu) (tedit 5A715739)
    (at 153.57 100.25)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference PG2 (at -1.078 0.19) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
  )
  (module footprints:testPad (layer F.Cu) (tedit 5902BD57)
    (at 154.82 103.25)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference PG3 (at -0.0635 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
  )
  (module footprints:testPad (layer F.Cu) (tedit 5A715723)
    (at 156.07 106.25)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference PG4 (at -2.3325 1.745) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
  )
  (module footprints:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A2CB1FD)
    (at 162.82 80.25)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -0.6 -0.5) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 14 "Net-(P5-Pad1)"))
  )
  (module footprints:LED-0805 (layer F.Cu) (tedit 5A716011)
    (at 162.82 93.25)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D0 (at 2.2225 1.4605) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.143 0 180) (size 1.3 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(CON1-Pad3)"))
    (pad 1 smd rect (at -1.27 0 180) (size 1.3 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D0-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED-0603 (layer F.Cu) (tedit 5A716017)
    (at 162.82 97.25)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 1.778 1.0795) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.889 0 180) (size 1 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.889 0 180) (size 1 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0402 (layer F.Cu) (tedit 5A71601D)
    (at 162.82 100.25)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference D2 (at 1.3 1) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0) (size 0.7 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.5 0) (size 0.7 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0201 (layer F.Cu) (tedit 5A716024)
    (at 162.82 103.25)
    (descr "Resistor SMD 0201, reflow soldering, Vishay (see crcw0201e3.pdf)")
    (tags "resistor 0201")
    (attr smd)
    (fp_text reference D3 (at 1.016 0.889) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.3 0) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.3 0) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0201.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0201 (layer F.Cu) (tedit 5A71602F)
    (at 162.82 106.25)
    (descr "Resistor SMD 0201, reflow soldering, Vishay (see crcw0201e3.pdf)")
    (tags "resistor 0201")
    (attr smd)
    (fp_text reference D4 (at 1.016 0.889) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.3 0) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.3 0) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0201.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805 (layer F.Cu) (tedit 58DFDC5C)
    (at 153.82 93.25 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R0 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.143 0 180) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D0-Pad1)"))
    (pad 2 smd rect (at 1.143 0 180) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 5902A5F6)
    (at 155.57 97.25 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.889 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.016 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0402 (layer F.Cu) (tedit 58DFDC4A)
    (at 156.07 100.25 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 0 180) (layer Dwgs.User) hide)
    (fp_text value 330 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.4 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.5 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0201 (layer F.Cu) (tedit 5A2C7C82)
    (at 156.82 103.25 180)
    (descr "Resistor SMD 0201, reflow soldering, Vishay (see crcw0201e3.pdf)")
    (tags "resistor 0201")
    (attr smd)
    (fp_text reference R3 (at 1.397 0.762 180) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.4 0 180) (size 0.45 0.43) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.4 0 180) (size 0.45 0.43) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0201.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 171.82 100.25 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SPST_SMD (layer B.Cu) (tedit 5860A656)
    (at 157.82 86.25 45)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference SW1 (at 0 -3 45) (layer B.SilkS))
    (fp_text value SW_SPDT (at 0.1 0 45) (layer B.Fab))
    (fp_text user JS102011SAQN (at 0 -1.7 45) (layer B.Fab))
    (pad "" np_thru_hole circle (at 3.4 -2.75 45) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -2.5 0 45) (size 1.2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(SW1-Pad1)"))
    (pad 2 smd rect (at 0.04 0 45) (size 1.2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(BT1-Pad1)"))
    (pad 3 smd rect (at 2.5 0 45) (size 1.2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
    (pad "" np_thru_hole circle (at -3.4 -2.75 45) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x06.wrl
      (at (xyz 0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module footprints:QFN-20-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 5A715A5E)
    (at 171.82 95.25)
    (descr "20-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 3.75 0) (layer F.SilkS))
    (fp_text value ATTINY84-20MU (at 0 3.33) (layer F.Fab))
    (pad 1 smd rect (at -1.965 -1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(CON1-Pad3)"))
    (pad 2 smd rect (at -1.965 -0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at -1.965 0) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D2-Pad2)"))
    (pad 4 smd rect (at -1.965 0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (pad 5 smd rect (at -1.965 1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad2)"))
    (pad 6 smd rect (at -1 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -0.5 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 0 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0.5 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (pad 10 smd rect (at 1 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 1.965 1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
    (pad 12 smd rect (at 1.965 0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
    (pad 13 smd rect (at 1.965 0) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CON1-Pad5)"))
    (pad 14 smd rect (at 1.965 -0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 1.965 -1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at 1 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CON1-Pad4)"))
    (pad 17 smd rect (at 0.5 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 0 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at -0.5 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at -1 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(CON1-Pad1)"))
    (pad 21 smd rect (at 0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at 0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at -0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at -0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_01005 (layer F.Cu) (tedit 5A716555)
    (at 157.57 106.25 180)
    (descr "Resistor SMD 0201, reflow soldering, Vishay (see crcw0201e3.pdf)")
    (tags "resistor 0201")
    (attr smd)
    (fp_text reference R4 (at 1.397 0.762 180) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.2 0 180) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.2 0 180) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(PG0-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0201.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 01005 (at 160.32 106.25) (layer F.SilkS))
  (gr_text "Misery\nEdition" (at 161.12 84.85) (layer F.SilkS))
  (gr_circle (center 162.82 93.25) (end 148.82 85.25) (layer Edge.Cuts) (width 0.1))
  (dimension 16 (width 0.3) (layer Dwgs.User)
    (gr_text "16.000 mm" (at 154.82 75.9) (layer Dwgs.User))
    (feature1 (pts (xy 146.82 93.25) (xy 146.82 74.55)))
    (feature2 (pts (xy 162.82 93.25) (xy 162.82 74.55)))
    (crossbar (pts (xy 162.82 77.25) (xy 146.82 77.25)))
    (arrow1a (pts (xy 146.82 77.25) (xy 147.946504 76.663579)))
    (arrow1b (pts (xy 146.82 77.25) (xy 147.946504 77.836421)))
    (arrow2a (pts (xy 162.82 77.25) (xy 161.693496 76.663579)))
    (arrow2b (pts (xy 162.82 77.25) (xy 161.693496 77.836421)))
  )
  (gr_text www.MakersBox.us (at 168.32 87.25) (layer B.SilkS))
  (gr_text 0201 (at 159.82 103.25) (layer F.SilkS))
  (gr_text Challenge (at 158.07 89.5) (layer F.SilkS))
  (gr_text SMD (at 155.62 84.85) (layer F.SilkS))
  (gr_text CR2032 (at 150.82 91.25) (layer B.SilkS))
  (gr_text 0402 (at 159.32 100.25) (layer F.SilkS))
  (gr_text 0603 (at 159.07 97.25) (layer F.SilkS))
  (gr_text 0805 (at 158.07 93.25) (layer F.SilkS))
)
