(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 46)
    (tracks 977)
    (zones 0)
    (modules 41)
    (nets 73)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 Gnd.Cu power)
    (2 Pow.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.127)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.1)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.457)
    (via_min_drill 0.254)
    (user_via 0.4572 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.1)
    (segment_width 0.15)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 1.00076)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 124.90984 100.36984)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x030f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/gerber-v0.7/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VDD)
  (net 3 /RTC_OSC_IN)
  (net 4 /RTC_OSC_OUT)
  (net 5 /SDMMC_D2)
  (net 6 /SDMMC_D3)
  (net 7 /SDMMC_CMD)
  (net 8 /SDMMC_D0)
  (net 9 /SDMMC_D1)
  (net 10 /D1)
  (net 11 "Net-(D1-Pad1)")
  (net 12 /BOOT0)
  (net 13 /OTG_FS_D+)
  (net 14 /OTG_FS_D-)
  (net 15 /JTMS/SWDIO)
  (net 16 /JTCK/SWCLK)
  (net 17 /D16)
  (net 18 /D15)
  (net 19 /D14)
  (net 20 /D13)
  (net 21 /D12)
  (net 22 /D11)
  (net 23 /D10)
  (net 24 /D9)
  (net 25 /D8)
  (net 26 /D7)
  (net 27 /D6)
  (net 28 /D5)
  (net 29 /D4)
  (net 30 /D3)
  (net 31 /D2)
  (net 32 /A1)
  (net 33 /A2)
  (net 34 /A3)
  (net 35 /A4)
  (net 36 /A5)
  (net 37 /A6)
  (net 38 /A7)
  (net 39 /A8)
  (net 40 /A9)
  (net 41 /A10)
  (net 42 /A11)
  (net 43 /A12)
  (net 44 /A13)
  (net 45 /A14)
  (net 46 /A15)
  (net 47 /A16)
  (net 48 /JTDI)
  (net 49 /JTDO/SWO)
  (net 50 /~RST)
  (net 51 /VBAT)
  (net 52 /OSC_IN)
  (net 53 /OSC_OUT)
  (net 54 /RTC)
  (net 55 /VBAT_IN)
  (net 56 /BOOT_SEL)
  (net 57 /SDMMC_CLK)
  (net 58 /VIN)
  (net 59 VDDA)
  (net 60 "Net-(D2-Pad1)")
  (net 61 "Net-(P3-Pad7)")
  (net 62 "Net-(U1-Pad4)")
  (net 63 "Net-(U3-Pad4)")
  (net 64 /VBUS)
  (net 65 "Net-(J1-Pad6)")
  (net 66 "Net-(J1-Pad4)")
  (net 67 /D+)
  (net 68 /D-)
  (net 69 /~JTRST)
  (net 70 "Net-(SW2-Pad2)")
  (net 71 /SDMMC_DET)
  (net 72 VSSA)
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /BOOT0)
    (add_net /BOOT_SEL)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D14)
    (add_net /D15)
    (add_net /D16)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /JTCK/SWCLK)
    (add_net /JTDI)
    (add_net /JTDO/SWO)
    (add_net /JTMS/SWDIO)
    (add_net /OSC_IN)
    (add_net /OSC_OUT)
    (add_net /RTC)
    (add_net /RTC_OSC_IN)
    (add_net /RTC_OSC_OUT)
    (add_net /SDMMC_CLK)
    (add_net /SDMMC_CMD)
    (add_net /SDMMC_D0)
    (add_net /SDMMC_D1)
    (add_net /SDMMC_D2)
    (add_net /SDMMC_D3)
    (add_net /SDMMC_DET)
    (add_net /VBAT)
    (add_net /VBAT_IN)
    (add_net /VBUS)
    (add_net /~JTRST)
    (add_net /~RST)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(SW2-Pad2)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U3-Pad4)")
    (add_net VSSA)
  )
  (net_class PowerMain ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /VIN)
    (add_net VDD)
    (add_net VDDA)
  )
  (net_class USB ""
    (clearance 0.1524)
    (trace_width 0.381)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D+)
    (add_net /D-)
    (add_net /OTG_FS_D+)
    (add_net /OTG_FS_D-)
  )
  (module NetTie:NetTie-2_SMD_Pad0.5mm (layer F.Cu) (tedit 5A1CF6D3)
    (at 115.18 72.43 270)
    (descr "Net tie, 2 pin, 0.5mm square SMD pads")
    (tags "net tie")
    (attr virtual)
    (fp_text reference NT1 (at 0 -1.2 90) (layer F.SilkS) hide)
    (fp_text value Net-Tie_2 (at 0 1.2 90) (layer F.Fab))
    (pad 2 smd circle (at 0.5 0 270) (size 0.5 0.5) (layers F.Cu)
      (net 72 VSSA))
    (pad 1 smd circle (at -0.5 0 270) (size 0.5 0.5) (layers F.Cu)
      (net 1 GND))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 115.97 65.72 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -2.48 -0.07 180) (layer B.SilkS))
    (fp_text value LP5907MFX-3.3 (at 0 -2.9 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 VDD))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 58 /VIN))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 58 /VIN))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module engstad:usb-micro-b-amphenol-fci-10118194 (layer F.Cu) (tedit 5F690FEC)
    (at 115.8748 59.9694 180)
    (fp_text reference J1 (at 0 -4.5 180) (layer F.SilkS) hide)
    (fp_text value USB_B_Micro (at 0 4 180) (layer F.Fab))
    (pad 6 thru_hole circle (at -2.65 -2.7 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at -2.35 -2.7 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at 2.35 -2.7 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at 2.65 -2.7 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at 3.5 0 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at 3.5 0.275 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at 3.5 -0.275 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at -3.5 0.275 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at -3.5 0 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at -3.5 -0.275 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 2.9 0 180) (size 1.2 1.55) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 1 0 270) (size 1.5 1.55) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at -1 0 180) (size 1.5 1.55) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at -2.9 0 180) (size 1.2 1.55) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at 1.3 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 67 /D+))
    (pad 2 smd rect (at -0.65 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 68 /D-))
    (pad 1 smd rect (at -1.3 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 64 /VBUS))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.step
      (offset (xyz 0 1.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 119.84 96.8748)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 0.06 -2.2748) (layer F.SilkS))
    (fp_text value APX823 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U3-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(SW2-Pad2)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 50 /~RST))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3215-2Pin_3.2x1.5mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 117.51 69.79 180)
    (descr "SMD Crystal FC-135 https://support.epson.biz/td/api/doc_check.php?dl=brief_FC-135R_en.pdf")
    (tags "SMD SMT Crystal")
    (attr smd)
    (fp_text reference Y1 (at -2.79 -0.01) (layer F.SilkS))
    (fp_text value Crystal (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at -1.25 0 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 /RTC_OSC_OUT))
    (pad 1 smd rect (at 1.25 0 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /RTC_OSC_IN))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3215-2Pin_3.2x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module engstad:cstce-v-c (layer F.Cu) (tedit 5F68EE8D)
    (at 117.5 72.1 180)
    (attr smd)
    (fp_text reference X1 (at -2.9 0 180) (layer F.SilkS))
    (fp_text value XTAL (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at -1.2 0 180) (size 0.4 1.9) (layers F.Cu F.Paste F.Mask)
      (net 52 /OSC_IN))
    (pad 2 smd rect (at 0 0 180) (size 0.4 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.2 0 180) (size 0.4 1.9) (layers F.Cu F.Paste F.Mask)
      (net 53 /OSC_OUT))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Resonator_SMD_muRata_CSTxExxV-3Pin_3.0x1.1mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module engstad:conn-jtag-0.05 (layer F.Cu) (tedit 5F68EE30)
    (at 116.03 90.728)
    (fp_text reference P3 (at -0.08 -0.058) (layer F.SilkS) hide)
    (fp_text value CORTEX-JTAG (at 0.02 -3.678 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.54 -1.95) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 15 /JTMS/SWDIO))
    (pad 4 smd rect (at -1.27 -1.95) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 16 /JTCK/SWCLK))
    (pad 6 smd rect (at 0 -1.95) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 49 /JTDO/SWO))
    (pad 8 smd rect (at 1.27 -1.95) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 48 /JTDI))
    (pad 10 smd rect (at 2.54 -1.95) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 69 /~JTRST))
    (pad 1 smd rect (at -2.54 1.95) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 3 smd rect (at -1.27 1.95) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0 1.95) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 1.27 1.95) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(P3-Pad7)"))
    (pad 9 smd rect (at 2.54 1.95) (size 0.74 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module engstad:slide-switch-smd-cas-220-d20 (layer F.Cu) (tedit 5F68ED41)
    (at 111.1504 70.5 270)
    (fp_text reference SW1 (at 0.05 3.65 90) (layer F.Fab))
    (fp_text value DIPSW (at 0.03 -9.26 270) (layer F.Fab))
    (pad 1 smd rect (at -1.75 1.85 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 0 1.85 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 56 /BOOT_SEL))
    (pad 3 smd rect (at 1.75 1.85 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.75 -1.85 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 /VBAT_IN))
    (pad 5 smd rect (at 0 -1.85 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 51 /VBAT))
    (pad 6 smd rect (at 1.75 -1.85 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 120.45 73.25 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 51 /VBAT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 112.1 65.6)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U2 (at -2.7 1.3) (layer F.SilkS))
    (fp_text value USBLC6-2SC6 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 64 /VBUS))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 67 /D+))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 68 /D-))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 /OTG_FS_D-))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 /OTG_FS_D+))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module engstad:Molex_PS_105162_001 (layer B.Cu) (tedit 5F5C0497)
    (at 116.205 97.155 180)
    (fp_text reference J2 (at -0.06008 0.27134) (layer B.SilkS))
    (fp_text value Micro_SD_Card (at 0.1 5.3) (layer B.Fab))
    (pad "" smd rect (at 2.095 3.69 90) (size 0.55 2.91) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 5.325 3.01) (size 1.05 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 5.325 0.4 180) (size 1.05 1.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 5.3 -0.87) (size 0.72 0.78) (layers B.Cu B.Paste B.Mask)
      (net 71 /SDMMC_DET))
    (pad "" smd rect (at -1.92 3.69 90) (size 0.55 2.91) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at -5.325 2.44 90) (size 1.2 1.05) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -5.325 -0.75 270) (size 2.39 1.05) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -4.15 -3.55 90) (size 1 0.5) (layers B.Cu B.Paste B.Mask)
      (net 9 /SDMMC_D1))
    (pad 7 smd rect (at -3.05 -3.55 90) (size 1 0.5) (layers B.Cu B.Paste B.Mask)
      (net 8 /SDMMC_D0))
    (pad 6 smd rect (at -1.95 -3.55 90) (size 1 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -0.85 -3.55 90) (size 1 0.5) (layers B.Cu B.Paste B.Mask)
      (net 57 /SDMMC_CLK))
    (pad 4 smd rect (at 0.25 -3.55 90) (size 1 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VDD))
    (pad 3 smd rect (at 1.35 -3.55 90) (size 1 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 /SDMMC_CMD))
    (pad 2 smd rect (at 2.45 -3.55 90) (size 1 0.5) (layers B.Cu B.Paste B.Mask)
      (net 6 /SDMMC_D3))
    (pad 1 smd rect (at 3.55 -3.55 90) (size 1 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 /SDMMC_D2))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 110.236 100.33 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -0.014 1.43) (layer F.SilkS))
    (fp_text value 470 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.9 100.35 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0.0514 1.15) (layer F.SilkS))
    (fp_text value 470 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 119.8 69.85)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.45 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 /BOOT0))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 56 /BOOT_SEL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.284 100.33)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at -0.134 -1.43) (layer F.SilkS))
    (fp_text value GREEN (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.9708 100.3554)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at -0.0708 -1.3554) (layer F.SilkS))
    (fp_text value RED (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /D1))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.5324 96.8494 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at -2.7494 0.0324 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 111.2 83.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -3.1 -0.1) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 115.7 91.9 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 1.43) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 119.05 67.614 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0.08 1.464) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /RTC_OSC_OUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.05 67.614)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RTC_OSC_IN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.95 92.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 110.9 77.2 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -2.2 -0.9 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 120.9 88.3 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.25 0.05 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 118.8 65.6 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.6 -0.05) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 118.5 77.35 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 3.12 0 90) (layer B.SilkS))
    (fp_text value 1.0uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 120.5 77.35 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 3.14 0.03 270) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 111.42 71.812 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at -0.712 -2.23 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 114.75 74.85)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.45 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 VDDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 114.75 73.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.45 0.05) (layer B.SilkS))
    (fp_text value 1.0uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 VDDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module engstad:QFP-64_10x10_Pitch0.5mm (layer F.Cu) (tedit 5F57CB32)
    (at 116.03 80.06 270)
    (attr smd)
    (fp_text reference U4 (at -0.06 0.33 180) (layer F.SilkS))
    (fp_text value STM32L486Rx-LQFP64 (at 0 7.95 90) (layer F.Fab))
    (pad 64 smd rect (at -3.7 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 63 smd rect (at -3.2 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 62 smd rect (at -2.7 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 /D16))
    (pad 61 smd rect (at -2.2 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 /D15))
    (pad 60 smd rect (at -1.7 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 /BOOT0))
    (pad 59 smd rect (at -1.2 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 /D14))
    (pad 58 smd rect (at -0.7 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 /D13))
    (pad 57 smd rect (at -0.2 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 /D12))
    (pad 56 smd rect (at 0.3 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 69 /~JTRST))
    (pad 55 smd rect (at 0.8 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 49 /JTDO/SWO))
    (pad 54 smd rect (at 1.3 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /SDMMC_CMD))
    (pad 53 smd rect (at 1.8 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 57 /SDMMC_CLK))
    (pad 52 smd rect (at 2.3 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDMMC_D3))
    (pad 51 smd rect (at 2.8 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /SDMMC_D2))
    (pad 50 smd rect (at 3.3 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 /JTDI))
    (pad 49 smd rect (at 3.8 -5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 /JTCK/SWCLK))
    (pad 48 smd rect (at 5.75 -3.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 47 smd rect (at 5.75 -3.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 46 smd rect (at 5.75 -2.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 /JTMS/SWDIO))
    (pad 45 smd rect (at 5.75 -2.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 /OTG_FS_D+))
    (pad 44 smd rect (at 5.75 -1.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 /OTG_FS_D-))
    (pad 43 smd rect (at 5.75 -1.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 /D11))
    (pad 42 smd rect (at 5.75 -0.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 /D10))
    (pad 41 smd rect (at 5.75 -0.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 71 /SDMMC_DET))
    (pad 40 smd rect (at 5.75 0.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 /SDMMC_D1))
    (pad 39 smd rect (at 5.75 0.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 /SDMMC_D0))
    (pad 38 smd rect (at 5.75 1.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 /D9))
    (pad 37 smd rect (at 5.75 1.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 /D8))
    (pad 36 smd rect (at 5.75 2.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 /D7))
    (pad 35 smd rect (at 5.75 2.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 /D6))
    (pad 34 smd rect (at 5.75 3.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 /D5))
    (pad 33 smd rect (at 5.75 3.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 /D4))
    (pad 32 smd rect (at 3.75 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 31 smd rect (at 3.25 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd rect (at 2.75 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 /D3))
    (pad 29 smd rect (at 2.25 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 /D2))
    (pad 28 smd rect (at 1.75 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 /D1))
    (pad 27 smd rect (at 1.25 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 /A16))
    (pad 26 smd rect (at 0.75 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 /A15))
    (pad 25 smd rect (at 0.25 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 /A14))
    (pad 24 smd rect (at -0.25 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 /A13))
    (pad 23 smd rect (at -0.75 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 /A12))
    (pad 22 smd rect (at -1.25 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 /A11))
    (pad 21 smd rect (at -1.75 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 /A10))
    (pad 20 smd rect (at -2.25 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 /A9))
    (pad 19 smd rect (at -2.75 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 18 smd rect (at -3.25 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at -3.75 5.75 270) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 /A8))
    (pad 16 smd rect (at -5.75 3.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 /A7))
    (pad 15 smd rect (at -5.75 3.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 /A6))
    (pad 14 smd rect (at -5.75 2.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 /A5))
    (pad 13 smd rect (at -5.75 2.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 59 VDDA))
    (pad 12 smd rect (at -5.75 1.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 72 VSSA))
    (pad 11 smd rect (at -5.75 1.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 /A4))
    (pad 10 smd rect (at -5.75 0.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 /A3))
    (pad 9 smd rect (at -5.75 0.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 /A2))
    (pad 8 smd rect (at -5.75 -0.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 /A1))
    (pad 7 smd rect (at -5.75 -0.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 50 /~RST))
    (pad 6 smd rect (at -5.75 -1.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 53 /OSC_OUT))
    (pad 5 smd rect (at -5.75 -1.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 52 /OSC_IN))
    (pad 4 smd rect (at -5.75 -2.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /RTC_OSC_OUT))
    (pad 3 smd rect (at -5.75 -2.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 /RTC_OSC_IN))
    (pad 2 smd rect (at -5.75 -3.25) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 54 /RTC))
    (pad 1 smd rect (at -5.75 -3.75) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 51 /VBAT))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-64_10x10mm_P0.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 114.7 76.75)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB2 (at 0 1.65) (layer B.SilkS))
    (fp_text value 220Ω@100MHz (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 VDD))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 VDDA))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 111.2 65.575 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB1 (at 3.025 0.05 270) (layer B.SilkS))
    (fp_text value 220Ω@100MHz (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 64 /VBUS))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 58 /VIN))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 113.15 65.57 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.58 0 180) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 58 /VIN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module engstad:pin-strip-16 (layer B.Cu) (tedit 56DD5D79)
    (at 107.14 81.33 270)
    (descr "Pin strip 16pin")
    (tags "CONN DEV")
    (fp_text reference P4 (at 0 2.159 270) (layer B.SilkS) hide)
    (fp_text value Analog (at 0.254 3.556 270) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at -19.05 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 32 /A1))
    (pad 2 thru_hole circle (at -16.51 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 33 /A2))
    (pad 3 thru_hole circle (at -13.97 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 34 /A3))
    (pad 4 thru_hole circle (at -11.43 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 35 /A4))
    (pad 5 thru_hole circle (at -8.89 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 36 /A5))
    (pad 6 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 37 /A6))
    (pad 7 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 38 /A7))
    (pad 8 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 39 /A8))
    (pad 9 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 40 /A9))
    (pad 10 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 41 /A10))
    (pad 11 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 42 /A11))
    (pad 12 thru_hole circle (at 8.89 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 43 /A12))
    (pad 13 thru_hole circle (at 11.43 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 44 /A13))
    (pad 14 thru_hole circle (at 13.97 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 45 /A14))
    (pad 15 thru_hole circle (at 16.51 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 46 /A15))
    (pad 16 thru_hole circle (at 19.05 0 270) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 47 /A16))
    (model ${KIWALTER3DMOD}/walter/pin_strip/pin_strip_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module engstad:pin-strip-16 (layer B.Cu) (tedit 56DD5D92)
    (at 124.92 81.33 90)
    (descr "Pin strip 16pin")
    (tags "CONN DEV")
    (fp_text reference P5 (at 0 2.159 90) (layer B.SilkS) hide)
    (fp_text value Digital (at 0.254 3.556 90) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at -19.05 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 10 /D1))
    (pad 2 thru_hole circle (at -16.51 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 31 /D2))
    (pad 3 thru_hole circle (at -13.97 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 30 /D3))
    (pad 4 thru_hole circle (at -11.43 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 29 /D4))
    (pad 5 thru_hole circle (at -8.89 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 28 /D5))
    (pad 6 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 27 /D6))
    (pad 7 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 26 /D7))
    (pad 8 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 25 /D8))
    (pad 9 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 24 /D9))
    (pad 10 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 23 /D10))
    (pad 11 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 22 /D11))
    (pad 12 thru_hole circle (at 8.89 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 21 /D12))
    (pad 13 thru_hole circle (at 11.43 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 20 /D13))
    (pad 14 thru_hole circle (at 13.97 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 19 /D14))
    (pad 15 thru_hole circle (at 16.51 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 18 /D15))
    (pad 16 thru_hole circle (at 19.05 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 17 /D16))
    (model ${KIWALTER3DMOD}/walter/pin_strip/pin_strip_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module engstad:pin-socket-2 (layer F.Cu) (tedit 56DD5D83)
    (at 123.65 59.74)
    (descr "Pin socket 2pin")
    (tags "CONN DEV")
    (fp_text reference P6 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value BATT (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 55 /VBAT_IN))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIWALTER3DMOD}/walter/pin_strip/pin_socket_2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module engstad:pin-strip-1 (layer F.Cu) (tedit 56772AEA)
    (at 109.68 59.74)
    (descr "Pin strip 1pin")
    (tags "CONN DEV")
    (fp_text reference P1 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value VDD (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD))
    (model ${KIWALTER3DMOD}/walter/pin_strip/pin_strip_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module engstad:pin-socket-1 (layer F.Cu) (tedit 567A653D)
    (at 122.37 67.36)
    (descr "Pin socket 2pin")
    (tags "CONN DEV")
    (fp_text reference P7 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value RTC (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 54 /RTC))
  )
  (module engstad:tactile-switch-evpay-34x29mm (layer F.Cu) (tedit 56DE6B1F)
    (at 116.03 96.87)
    (fp_text reference SW2 (at 0.0254 2.1638) (layer F.SilkS) hide)
    (fp_text value RST (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 1.475 -0.9) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.001))
    (pad 1 smd rect (at -1.475 -0.9) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.001))
    (pad 2 smd rect (at 1.475 0.9) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(SW2-Pad2)") (solder_mask_margin 0.001))
    (pad 2 smd rect (at -1.475 0.9) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(SW2-Pad2)") (solder_mask_margin 0.001))
  )
  (module engstad:pin-strip-1 (layer F.Cu) (tedit 56772AEA)
    (at 107.14 59.74 90)
    (descr "Pin strip 1pin")
    (tags "CONN DEV")
    (fp_text reference P2 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value VBUS (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 64 /VBUS))
    (model ${KIWALTER3DMOD}/walter/pin_strip/pin_strip_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 14 (at 109.15 95.35) (layer B.SilkS))
  (gr_text 16 (at 109.1 100.35) (layer B.SilkS))
  (gr_text A11 (at 109.35 87.65) (layer B.SilkS))
  (gr_text RTC (at 122.4 68.8) (layer F.SilkS))
  (gr_text Gnd (at 123.15 61.25 45) (layer F.SilkS))
  (gr_text Bat (at 120.856 61.264 45) (layer F.SilkS))
  (gr_text 3.3 (at 111.1 61.6 315) (layer F.SilkS))
  (gr_text 5.0 (at 108.8 61.55 315) (layer F.SilkS))
  (gr_text A7 (at 109 77.5) (layer B.SilkS))
  (gr_text D12 (at 122.7 72.5) (layer B.SilkS))
  (gr_text D6 (at 123 87.65) (layer B.SilkS))
  (gr_text D3 (at 123.2 95.4) (layer B.SilkS))
  (gr_text D11 (at 122.682 75) (layer B.SilkS))
  (gr_text D13 (at 122.65 69.9) (layer B.SilkS))
  (gr_text GND (at 123.65 59.74 90) (layer B.SilkS))
  (gr_text D15 (at 122.65 64.85) (layer B.SilkS))
  (gr_text D16 (at 122.6 62.3) (layer B.SilkS))
  (gr_text + (at 121.11 59.74) (layer B.SilkS))
  (gr_text D10 (at 122.75 77.5) (layer B.SilkS))
  (gr_text D1 (at 123.15 100.35) (layer B.SilkS))
  (gr_text D2 (at 123.2 97.85) (layer B.SilkS))
  (gr_text D4 (at 123.2 92.75) (layer B.SilkS))
  (gr_text D5 (at 123.15 90.25) (layer B.SilkS))
  (gr_text D7 (at 123 85.15) (layer B.SilkS))
  (gr_text D8 (at 123 82.6) (layer B.SilkS))
  (gr_text D9 (at 122.95 80.06) (layer B.SilkS))
  (gr_text 15 (at 109.1 98) (layer B.SilkS))
  (gr_text A10 (at 109.35 85.2) (layer B.SilkS))
  (gr_text A13 (at 109.4 92.76) (layer B.SilkS))
  (gr_text A12 (at 109.4 90.25) (layer B.SilkS))
  (gr_text "A9\n" (at 108.918 82.6) (layer B.SilkS))
  (gr_text A8 (at 108.95 80.1) (layer B.SilkS))
  (gr_text A6 (at 109.045 74.98) (layer B.SilkS))
  (gr_text A5 (at 109.045 72.44) (layer B.SilkS))
  (gr_text A4 (at 109.045 69.9) (layer B.SilkS))
  (gr_text A3 (at 109.045 67.36) (layer B.SilkS))
  (gr_text "A2\n" (at 109.045 64.82) (layer B.SilkS))
  (gr_text A1 (at 109.045 62.28) (layer B.SilkS))
  (gr_text "BetsyBoard\nV0.9\n\n" (at 110.8 88.15 90) (layer F.SilkS))
  (dimension 43.18 (width 0.3) (layer Eco1.User)
    (gr_text "43.180 mm" (at 132.166165 80.06 90) (layer Eco1.User))
    (feature1 (pts (xy 127.46 58.47) (xy 133.516165 58.47)))
    (feature2 (pts (xy 127.46 101.65) (xy 133.516165 101.65)))
    (crossbar (pts (xy 130.816165 101.65) (xy 130.816165 58.47)))
    (arrow1a (pts (xy 130.816165 58.47) (xy 131.402586 59.596504)))
    (arrow1b (pts (xy 130.816165 58.47) (xy 130.229744 59.596504)))
    (arrow2a (pts (xy 130.816165 101.65) (xy 131.402586 100.523496)))
    (arrow2b (pts (xy 130.816165 101.65) (xy 130.229744 100.523496)))
  )
  (dimension 20.32 (width 0.3) (layer Eco1.User)
    (gr_text "20.320 mm" (at 116.03 107.318) (layer Eco1.User))
    (feature1 (pts (xy 126.19 102.92) (xy 126.19 108.668)))
    (feature2 (pts (xy 105.87 102.92) (xy 105.87 108.668)))
    (crossbar (pts (xy 105.87 105.968) (xy 126.19 105.968)))
    (arrow1a (pts (xy 126.19 105.968) (xy 125.063496 106.554421)))
    (arrow1b (pts (xy 126.19 105.968) (xy 125.063496 105.381579)))
    (arrow2a (pts (xy 105.87 105.968) (xy 106.996504 106.554421)))
    (arrow2b (pts (xy 105.87 105.968) (xy 106.996504 105.381579)))
  )
  (gr_text "Engstad \nDesign " (at 108.8 96.35) (layer F.SilkS))
  (gr_line (start 105.87 101.65) (end 105.87 58.47) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.19 101.65) (end 105.87 101.65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.19 58.47) (end 126.19 101.65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.87 58.47) (end 126.19 58.47) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name VDD) (layer Pow.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109 99.2) (xy 111.47 97.1) (xy 111.45 80.3) (xy 114.17 77.2) (xy 114.17 73.6)
        (xy 121 73.6) (xy 121 68.5) (xy 126.18 68.47) (xy 126.17 101.67) (xy 109 101.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Gnd.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.19 58.47) (xy 126.19 101.65) (xy 105.87 101.65) (xy 105.87 58.47)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Pow.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.5 66.9) (xy 114.5 73.3) (xy 120.5 73.3) (xy 120.5 66.9)
      )
    )
  )
  (zone (net 2) (net_name VDD) (layer Pow.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 105.87 58.47) (xy 105.87 60.87) (xy 108.62 60.87) (xy 111.5 63.7) (xy 111.5 65)
        (xy 112.6 66.1) (xy 121 66.1) (xy 121 68) (xy 126.2 68) (xy 126.2 58.5)
      )
    )
  )
  (zone (net 2) (net_name VDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.32 64.15) (xy 116.32 65.05) (xy 116.45 65.2) (xy 119.6 65.2) (xy 120.4 66)
        (xy 120.8 66) (xy 120.8 64.6) (xy 120.35 64.15)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.17 58.44) (xy 126.27 65.74) (xy 126.19 101.65) (xy 105.87 101.65) (xy 105.87 58.47)
        (xy 116.77 58.47) (xy 118.67 58.47)
      )
    )
    (polygon
      (pts
        (xy 116 65.25) (xy 116.17 65.47) (xy 118.87 65.47) (xy 120 66.6) (xy 120 68.15)
        (xy 120.85 69.1) (xy 121.1 69.1) (xy 121.1 64.5) (xy 120.5 63.9) (xy 116.25 63.9)
        (xy 116 64.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Pow.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 111.07 63.87) (xy 111.0742 65.34658) (xy 113.36782 67.24396) (xy 113.45 77.3) (xy 110.95 80.3)
        (xy 110.97 96.87) (xy 108.47 98.97) (xy 108.47 101.67) (xy 105.87 101.67) (xy 105.87 61.27)
        (xy 108.47 61.27)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.87 58.5) (xy 126.2 58.45) (xy 126.17 63.67) (xy 126.19 101.65) (xy 105.87 101.65)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.1) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 120.5 73.3) (xy 114.5 73.3) (xy 114.5 66.9) (xy 120.5 66.9)
      )
    )
  )
)
