(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 53)
    (zones 0)
    (modules 6)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x10_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 121.0945 79.502)
    (descr "Through hole straight pin header, 1x10, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.00mm single row")
    (fp_text reference REF** (at 0 -2.06) (layer F.SilkS))
    (fp_text value PinHeader_1x10_P2.00mm_Vertical (at 0 20.06) (layer F.Fab))
    (fp_text user %R (at 0 9 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 18) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 16) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 14) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x10_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module spakecdk:LM301B (layer F.Cu) (tedit 6074991E)
    (at 116.275 96.6945)
    (fp_text reference REF** (at 0.1 3.3) (layer F.SilkS) hide)
    (fp_text value LM301B (at 0.1 -3.3) (layer F.Fab))
    (pad 1 smd custom (at 1.2 -1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 2.3 0.1) (xy 1.9 0.1) (xy 1.9 0.8) (xy -0.8 0.8) (xy -0.8 0.1)
           (xy -1.2 0.1) (xy -1.2 -0.7) (xy 2.3 -0.7)) (width 0.01))
      ))
    (pad 2 smd custom (at 1.8 0.9) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -1.8 -0.1) (xy -1.4 -0.1) (xy -1.4 -0.8) (xy 1.3 -0.8) (xy 1.3 -0.1)
           (xy 1.7 -0.1) (xy 1.7 0.7) (xy -1.8 0.7)) (width 0.01))
      ))
  )
  (module spakecdk:LM301B (layer F.Cu) (tedit 6074991E)
    (at 116.1415 84.5185)
    (fp_text reference REF** (at 0.1 3.3) (layer F.SilkS) hide)
    (fp_text value LM301B (at 0.1 -3.3) (layer F.Fab))
    (pad 1 smd custom (at 1.2 -1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 2.3 0.1) (xy 1.9 0.1) (xy 1.9 0.8) (xy -0.8 0.8) (xy -0.8 0.1)
           (xy -1.2 0.1) (xy -1.2 -0.7) (xy 2.3 -0.7)) (width 0.01))
      ))
    (pad 2 smd custom (at 1.8 0.9) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -1.8 -0.1) (xy -1.4 -0.1) (xy -1.4 -0.8) (xy 1.3 -0.8) (xy 1.3 -0.1)
           (xy 1.7 -0.1) (xy 1.7 0.7) (xy -1.8 0.7)) (width 0.01))
      ))
  )
  (module spakecdk:LM301B (layer F.Cu) (tedit 6074991E)
    (at 116.183 88.5715)
    (fp_text reference REF** (at 0.1 3.3) (layer F.SilkS) hide)
    (fp_text value LM301B (at 0.1 -3.3) (layer F.Fab))
    (pad 1 smd custom (at 1.2 -1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 2.3 0.1) (xy 1.9 0.1) (xy 1.9 0.8) (xy -0.8 0.8) (xy -0.8 0.1)
           (xy -1.2 0.1) (xy -1.2 -0.7) (xy 2.3 -0.7)) (width 0.01))
      ))
    (pad 2 smd custom (at 1.8 0.9) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -1.8 -0.1) (xy -1.4 -0.1) (xy -1.4 -0.8) (xy 1.3 -0.8) (xy 1.3 -0.1)
           (xy 1.7 -0.1) (xy 1.7 0.7) (xy -1.8 0.7)) (width 0.01))
      ))
  )
  (module spakecdk:LM301B (layer F.Cu) (tedit 6074991E)
    (at 116.2115 92.6305)
    (fp_text reference REF** (at 0.1 3.3) (layer F.SilkS) hide)
    (fp_text value LM301B (at 0.1 -3.3) (layer F.Fab))
    (pad 1 smd custom (at 1.2 -1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 2.3 0.1) (xy 1.9 0.1) (xy 1.9 0.8) (xy -0.8 0.8) (xy -0.8 0.1)
           (xy -1.2 0.1) (xy -1.2 -0.7) (xy 2.3 -0.7)) (width 0.01))
      ))
    (pad 2 smd custom (at 1.8 0.9) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -1.8 -0.1) (xy -1.4 -0.1) (xy -1.4 -0.8) (xy 1.3 -0.8) (xy 1.3 -0.1)
           (xy 1.7 -0.1) (xy 1.7 0.7) (xy -1.8 0.7)) (width 0.01))
      ))
  )
  (module spakecdk:LM301B (layer F.Cu) (tedit 6074991E)
    (at 116.1415 80.391)
    (fp_text reference REF** (at 0.1 3.3) (layer F.SilkS) hide)
    (fp_text value LM301B (at 0.1 -3.3) (layer F.Fab))
    (pad 1 smd custom (at 1.2 -1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 2.3 0.1) (xy 1.9 0.1) (xy 1.9 0.8) (xy -0.8 0.8) (xy -0.8 0.1)
           (xy -1.2 0.1) (xy -1.2 -0.7) (xy 2.3 -0.7)) (width 0.01))
      ))
    (pad 2 smd custom (at 1.8 0.9) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -1.8 -0.1) (xy -1.4 -0.1) (xy -1.4 -0.8) (xy 1.3 -0.8) (xy 1.3 -0.1)
           (xy 1.7 -0.1) (xy 1.7 0.7) (xy -1.8 0.7)) (width 0.01))
      ))
  )
  (gr_line (start 122.047 78.232) (end 115.6335 78.232) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115.6335 98.679) (end 122.047 98.679) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.047 98.679) (end 122.047 78.232) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115.6335 78.232) (end 115.6335 98.679) (layer Edge.Cuts) (width 0.05))
)
