<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="35.56" x2="0" y2="0.56" width="0" layer="20"/>
<wire x1="0" y1="0.56" x2="42" y2="0.56" width="0" layer="20"/>
<wire x1="42" y1="0.56" x2="42" y2="35.56" width="0" layer="20"/>
<wire x1="42" y1="35.56" x2="0" y2="35.56" width="0" layer="20"/>
<text>SDO</text>
<text>nIRQ</text>
<text>nFFS</text>
<text>FFIT</text>
<text>CLK</text>
<text>nRES</text>
<text>GND</text>
<text>GND</text>
<text>VDD</text>
<text>nINT</text>
<text>SDI</text>
<text>SCK</text>
<text>nSEL</text>
<text>RFM-12B S2</text>
<text>ANT</text>
</plain>
<libraries>
<library name="MF_Connectors">
<packages>
<package name="PTH_2.54MM_01X07">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for 2.54MM Pitch Header 7 Position. Based on 4UCON 00834.&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="Eagle-JeeLabs">
<packages>
<package name="RFM12B/69CW">
<description>RFM12B radio module by HopeRF</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="MF_Connectors" package="PTH_2.54MM_01X07" value="MF-CON-2.54mm-01x07">
<attribute name="URL" value="https://factory.macrofab.com/part/MF-CON-2.54mm-01x07"/>
<attribute name="MPN" value="MF-CON-2.54mm-01x07"/>
<attribute name="LABEL03" value=""/>
<attribute name="LABEL07" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="LABEL01" value=""/>
<attribute name="LABEL04" value=""/>
<attribute name="HOUSEPART" value="YES"/>
<attribute name="LABEL05" value=""/>
<attribute name="LABEL06" value=""/>
<attribute name="LABEL02" value=""/>
</element>
<element name="J2" library="MF_Connectors" package="PTH_2.54MM_01X07" value="MF-CON-2.54mm-01x07">
<attribute name="URL" value="https://factory.macrofab.com/part/MF-CON-2.54mm-01x07"/>
<attribute name="MPN" value="MF-CON-2.54mm-01x07"/>
<attribute name="LABEL03" value=""/>
<attribute name="LABEL07" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="LABEL01" value=""/>
<attribute name="LABEL04" value=""/>
<attribute name="HOUSEPART" value="YES"/>
<attribute name="LABEL05" value=""/>
<attribute name="LABEL06" value=""/>
<attribute name="LABEL02" value=""/>
</element>
<element name="U$1" library="Eagle-JeeLabs" package="RFM12B/69CW" value="RFM12B/69CW"/>
<element name="SJ1" library="jumper" package="SJ" value=""/>
</elements>
<signals>
<signal name="SDO">
<contactref element="J1" pad="P$7"/>
<contactref element="U$1" pad="SDO"/>
</signal>
<signal name="IRQ">
<contactref element="J1" pad="P$6"/>
<contactref element="U$1" pad="IRQ"/>
</signal>
<signal name="FFS">
<contactref element="J1" pad="P$5"/>
<contactref element="U$1" pad="FFS"/>
</signal>
<signal name="FFIT">
<contactref element="J1" pad="P$4"/>
<contactref element="U$1" pad="FFIT"/>
</signal>
<signal name="CLK">
<contactref element="J1" pad="P$3"/>
<contactref element="U$1" pad="CLK"/>
</signal>
<signal name="RST">
<contactref element="J1" pad="P$2"/>
<contactref element="U$1" pad="RST"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="P$1"/>
<contactref element="J2" pad="P$5"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
</signal>
<signal name="SEL">
<contactref element="J2" pad="P$1"/>
<contactref element="U$1" pad="SEL"/>
</signal>
<signal name="SCK">
<contactref element="J2" pad="P$2"/>
<contactref element="U$1" pad="SCK"/>
</signal>
<signal name="SDI">
<contactref element="J2" pad="P$3"/>
<contactref element="U$1" pad="SDI"/>
</signal>
<signal name="INT">
<contactref element="J2" pad="P$4"/>
<contactref element="U$1" pad="NINT"/>
</signal>
<signal name="VCC">
<contactref element="J2" pad="P$6"/>
<contactref element="U$1" pad="VDD"/>
</signal>
<signal name="ANT">
<contactref element="J2" pad="P$7"/>
<contactref element="U$1" pad="ANT"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
