<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="104" y1="35" x2="6" y2="35" width="0" layer="20"/>
<wire x1="6" y1="35" x2="5" y2="34" width="0" layer="20" curve="90"/>
<wire x1="5" y1="34" x2="5" y2="1" width="0" layer="20"/>
<wire x1="5" y1="1" x2="6" y2="0" width="0" layer="20" curve="90"/>
<wire x1="6" y1="0" x2="104" y2="0" width="0" layer="20"/>
<wire x1="104" y1="0" x2="105" y2="1" width="0" layer="20" curve="90"/>
<wire x1="105" y1="1" x2="105" y2="34" width="0" layer="20"/>
<wire x1="105" y1="34" x2="104" y2="35" width="0" layer="20" curve="90"/>
<text>RST</text>
<text>BT0</text>
<text>FAN +</text>
<text>JAW 2015-07</text>
<text>www.A791RL.com</text>
<text>LEDCTL Rev. 1</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>L0</text>
<text>L1</text>
<text>Vcc</text>
<text>Gnd</text>
<text>Tx</text>
<text>Rx</text>
<text>BT0</text>
<text>nRST</text>
<text>PROG</text>
<text>USERINT</text>
<text>DO NOT
TOUCH</text>
<text>HIGH VOLTAGE</text>
<text>INPUT: 12V MAX</text>
<text>3V3</text>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>Pb</text>
<text>JAW 2015-07</text>
<text>JAW 2015-07</text>
</plain>
<libraries>
<library name="jaw">
<packages>
<package name="SMD0805">
</package>
<package name="SMD0603">
</package>
<package name="CAPKE0">
</package>
<package name="SMD1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="HEADER-6X2-PTH">
</package>
<package name="SOD-323">
<description>&lt;b&gt;SOD323&lt;/b&gt; (2.5x1.2mm)</description>
</package>
<package name="DO-214AC">
</package>
<package name="HEADER-4X1-PTH">
</package>
<package name="BOURNS2303">
</package>
<package name="SMD0603D">
</package>
<package name="SOT-23-3">
</package>
<package name="SOT-23-3@1">
</package>
<package name="DFN5X6-8LEP1">
</package>
<package name="SMD1206">
</package>
<package name="PUI-0540">
</package>
<package name="KMR211">
</package>
<package name="UQPFN48">
</package>
<package name="SOT-23-6">
</package>
<package name="SOT-23-5">
</package>
<package name="HEADER-3X2-PTH">
</package>
<package name="HEADER-1X2-THM">
</package>
<package name="SRR1260">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="JST-PH-2-THM-RA">
<description>&lt;b&gt;S2B-PH-K-S&lt;/b&gt; 
&lt;p&gt;
JST PH 2-pin thru-home side entry</description>
</package>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
<package name="MICRO-FIDUCIAL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="jaw" package="SMD0603" value=".1u, 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="jaw" package="SMD0603" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="jaw" package="SMD0603" value=".002u,100V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="jaw" package="CAPKE0" value="100u,100v">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="jaw" package="SMD0805" value=".1u, 100v">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="jaw" package="SMD0603" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="jaw" package="SMD1210" value="100u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="jaw" package="SMD0603" value=".002u,100V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="jaw" package="CAPKE0" value="100u,100v">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="jaw" package="SMD0805" value=".1u, 100v">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CONN1" library="jaw" package="HEADER-6X2-PTH" value="HEADER-6X2-PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="jaw" package="SOD-323" value="any">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="jaw" package="SOD-323" value="DIODESOD-323">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="jaw" package="DO-214AC" value="ss3p6">
<attribute name="NAME"/>
</element>
<element name="D4" library="jaw" package="DO-214AC" value="ss3p6">
<attribute name="NAME"/>
</element>
<element name="J1" library="jaw" package="HEADER-4X1-PTH" value="HEADER-4X1-PTH"/>
<element name="J2" library="jaw" package="HEADER-4X1-PTH" value="HEADER-4X1-PTH"/>
<element name="L1" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="jaw" package="BOURNS2303" value="22u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="jaw" package="BOURNS2303" value="22u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="jaw" package="SMD0603D" value="white">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="jaw" package="SOT-23-3" value="IRLML6344TRPBF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="jaw" package="SOT-23-3@1" value="MOSFET-P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="jaw" package="SOT-23-3" value="MOSFETSOT-23">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="jaw" package="DFN5X6-8LEP1" value="AON6246">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="jaw" package="DFN5X6-8LEP1" value="AON6246">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="jaw" package="SMD0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="jaw" package="SMD0603" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="jaw" package="SMD0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="jaw" package="SMD0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="jaw" package="SMD0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="jaw" package="SMD1206" value=".01">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="jaw" package="SMD0603" value="88k7, .1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="jaw" package="SMD0603" value="3k3, .1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="jaw" package="SMD0603" value="14k7, .1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="jaw" package="SMD0603" value="3k3, .1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="jaw" package="SMD0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="jaw" package="SMD0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="jaw" package="SMD0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="jaw" package="SMD0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="jaw" package="SMD1206" value=".01">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="jaw" package="SMD0603" value="88k7, .1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="jaw" package="SMD0603" value="3k3, .1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="jaw" package="SMD0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="jaw" package="SMD0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="jaw" package="SMD0603" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPKR1" library="jaw" package="PUI-0540" value="PUI-5040">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="jaw" package="KMR211" value="SWITCHKMR211">
<attribute name="NAME"/>
</element>
<element name="SW3" library="jaw" package="KMR211" value="SWITCHKMR211">
<attribute name="NAME"/>
</element>
<element name="U1" library="jaw" package="UQPFN48" value="STM32F411/48">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="jaw" package="SOT-23-6" value="LMP8640-H">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="jaw" package="SOT-23-6" value="LMP8640">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VREG1" library="jaw" package="SOT-23-5" value="MCP1754">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN2" library="adafruit" package="JST-PH-2-THM-RA" value="">
<attribute name="NAME"/>
</element>
<element name="CN1" library="jaw" package="HEADER-3X2-PTH" value="HEADER-3X2-PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="C16" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="jaw" package="SMD0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="jaw" package="SMD0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="jaw" package="SOD-323" value="any">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="jaw" package="SOT-23-3" value="IRLML6344TRPBF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="jaw" package="SMD0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="jaw" package="SMD0603" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN3" library="jaw" package="HEADER-1X2-THM" value="HEADER-1X2-THM">
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="C24" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="jaw" package="SOT-23-6" value="TMP100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="jaw" package="SMD0603" value="10u,16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="jaw" package="SMD0603" value="10u,16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="jaw" package="SMD0603" value=".1u,16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="jaw" package="SOD-323" value="DIODESOD-323"/>
<element name="C28" library="jaw" package="SMD0603" value="10u,16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="jaw" package="SMD0603" value="10u,16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="jaw" package="SRR1260" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L5" library="jaw" package="SRR1260" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FID1" library="SparkFun-Aesthetics" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
</elements>
<signals>
<signal name="GND">
<contactref element="R4" pad="1"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="3"/>
<contactref element="C15" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="U1" pad="P23"/>
<contactref element="U1" pad="P35"/>
<contactref element="U1" pad="P47"/>
<contactref element="U1" pad="PAD"/>
<contactref element="U1" pad="P8"/>
<contactref element="U1" pad="P20"/>
<contactref element="Q1" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="CONN1" pad="8"/>
<contactref element="R1" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="VREG1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="R16" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="U3" pad="4"/>
<contactref element="R24" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="CN2" pad="2"/>
<contactref element="CN1" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="U5" pad="5"/>
<contactref element="C25" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="J2" pad="P$1"/>
<contactref element="C28" pad="2"/>
<contactref element="C29" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R5" pad="2"/>
<contactref element="SW3" pad="1"/>
<contactref element="SW3" pad="3"/>
<contactref element="C20" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="U1" pad="P24"/>
<contactref element="U1" pad="P36"/>
<contactref element="U1" pad="P48"/>
<contactref element="R3" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="SPKR1" pad="P1"/>
<contactref element="D1" pad="C"/>
<contactref element="VREG1" pad="5"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="C8" pad="1"/>
<contactref element="U3" pad="6"/>
<contactref element="C13" pad="1"/>
<contactref element="CN1" pad="1"/>
<contactref element="CONN1" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="U5" pad="4"/>
<contactref element="U5" pad="3"/>
<contactref element="J2" pad="P$4"/>
</signal>
<signal name="BOOT0">
<contactref element="SW3" pad="2"/>
<contactref element="SW3" pad="4"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="P44"/>
<contactref element="U1" pad="P2"/>
<contactref element="CN1" pad="5"/>
</signal>
<signal name="VCCA">
<contactref element="C23" pad="1"/>
<contactref element="U1" pad="P9"/>
<contactref element="L1" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="NRST">
<contactref element="C15" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="SW2" pad="2"/>
<contactref element="SW2" pad="4"/>
<contactref element="U1" pad="P7"/>
<contactref element="CN1" pad="6"/>
<contactref element="CONN1" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="P22"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="P1"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="SPISCK">
<contactref element="U1" pad="P26"/>
<contactref element="CONN1" pad="4"/>
</signal>
<signal name="SPIMISO">
<contactref element="U1" pad="P27"/>
<contactref element="CONN1" pad="3"/>
</signal>
<signal name="SPIMOSI">
<contactref element="U1" pad="P28"/>
<contactref element="CONN1" pad="5"/>
</signal>
<signal name="I2CCL">
<contactref element="U1" pad="P42"/>
<contactref element="R3" pad="1"/>
<contactref element="CONN1" pad="9"/>
<contactref element="J2" pad="P$3"/>
<contactref element="U5" pad="1"/>
</signal>
<signal name="I2CDA">
<contactref element="U1" pad="P43"/>
<contactref element="R9" pad="1"/>
<contactref element="CONN1" pad="10"/>
<contactref element="J2" pad="P$2"/>
<contactref element="U5" pad="6"/>
</signal>
<signal name="DPYDC">
<contactref element="U1" pad="P21"/>
<contactref element="CONN1" pad="6"/>
</signal>
<signal name="DPYCS">
<contactref element="U1" pad="P25"/>
<contactref element="CONN1" pad="7"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="P30"/>
<contactref element="CN1" pad="4"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="P31"/>
<contactref element="CN1" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="Q1" pad="3"/>
<contactref element="SPKR1" pad="P2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="R8" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="Q1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="VCCM">
<contactref element="L2" pad="P$2"/>
<contactref element="R17" pad="2"/>
<contactref element="L3" pad="P$2"/>
<contactref element="CN2" pad="1"/>
<contactref element="CONN1" pad="12"/>
<contactref element="C26" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="D5" pad="C"/>
<contactref element="CN3" pad="P$1"/>
<contactref element="D6" pad="A"/>
<contactref element="C29" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="L5" pad="P$2"/>
<contactref element="L4" pad="P$2"/>
</signal>
<signal name="PWRSW">
<contactref element="R6" pad="2"/>
<contactref element="Q3" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="CONN1" pad="11"/>
</signal>
<signal name="PWREN">
<contactref element="Q2" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="VREG1" pad="3"/>
</signal>
<signal name="IOPEN">
<contactref element="Q2" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="U1" pad="P41"/>
</signal>
<signal name="IOPSW">
<contactref element="Q3" pad="3"/>
<contactref element="U1" pad="P40"/>
</signal>
<signal name="N$2">
<contactref element="Q4" pad="P$5"/>
<contactref element="Q4" pad="P$6"/>
<contactref element="L2" pad="P$1"/>
<contactref element="D3" pad="A"/>
<contactref element="R13" pad="1"/>
<contactref element="Q4" pad="P$7"/>
<contactref element="Q4" pad="P$8"/>
<contactref element="Q4" pad="P$9"/>
<contactref element="L4" pad="P$1"/>
</signal>
<signal name="L1P">
<contactref element="D4" pad="C"/>
<contactref element="C12" pad="P"/>
<contactref element="R23" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="J1" pad="P$3"/>
</signal>
<signal name="N$4">
<contactref element="R13" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="L1M">
<contactref element="Q5" pad="P$1"/>
<contactref element="R20" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="N"/>
<contactref element="R22" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="C14" pad="2"/>
<contactref element="J1" pad="P$4"/>
<contactref element="Q5" pad="P$2"/>
<contactref element="Q5" pad="P$3"/>
</signal>
<signal name="N$6">
<contactref element="R7" pad="1"/>
<contactref element="Q4" pad="P$4"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="PWMB1">
<contactref element="R19" pad="2"/>
<contactref element="U1" pad="P16"/>
</signal>
<signal name="ADCBV1">
<contactref element="R23" pad="1"/>
<contactref element="R24" pad="2"/>
<contactref element="U1" pad="P14"/>
</signal>
<signal name="ADCBI0">
<contactref element="U1" pad="P12"/>
<contactref element="R25" pad="1"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="ADCVBAT">
<contactref element="R17" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="U1" pad="P10"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="Q5" pad="P$5"/>
<contactref element="Q5" pad="P$6"/>
<contactref element="L3" pad="P$1"/>
<contactref element="D4" pad="A"/>
<contactref element="R21" pad="1"/>
<contactref element="Q5" pad="P$7"/>
<contactref element="Q5" pad="P$8"/>
<contactref element="Q5" pad="P$9"/>
<contactref element="L5" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="R21" pad="2"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R19" pad="1"/>
<contactref element="Q5" pad="P$4"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="L0P">
<contactref element="D3" pad="C"/>
<contactref element="C6" pad="P"/>
<contactref element="R15" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="J1" pad="P$2"/>
</signal>
<signal name="L0M">
<contactref element="Q4" pad="P$1"/>
<contactref element="R12" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="N"/>
<contactref element="R14" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="C9" pad="2"/>
<contactref element="J1" pad="P$1"/>
<contactref element="Q4" pad="P$2"/>
<contactref element="Q4" pad="P$3"/>
</signal>
<signal name="ADCBV0">
<contactref element="R16" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="U1" pad="P13"/>
</signal>
<signal name="ADCBI1">
<contactref element="U1" pad="P15"/>
<contactref element="C18" pad="1"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="PWMB0">
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="P11"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$5">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="IOLED">
<contactref element="U1" pad="P45"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="IOSPKR">
<contactref element="U1" pad="P46"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$10">
</signal>
<signal name="N$16">
<contactref element="U2" pad="1"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U3" pad="1"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="Q6" pad="3"/>
<contactref element="D5" pad="A"/>
<contactref element="CN3" pad="P$2"/>
</signal>
<signal name="N$20">
<contactref element="Q6" pad="1"/>
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="IOFAN">
<contactref element="U1" pad="P29"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$22">
</signal>
<signal name="N$23">
</signal>
<signal name="VIN">
<contactref element="VREG1" pad="1"/>
<contactref element="D6" pad="C"/>
<contactref element="C1" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="Q2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
