(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 146)
    (no_connects 0)
    (area 32.701238 38.024999 89.065001 81.010858)
    (thickness 1.6)
    (drawings 16)
    (tracks 153)
    (zones 0)
    (modules 121)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VBUS)
  (net 3 /+5VDC)
  (net 4 "Net-(C5-Pad1)")
  (net 5 "Net-(C6-Pad1)")
  (net 6 "Net-(C7-Pad1)")
  (net 7 "Net-(C8-Pad1)")
  (net 8 "Net-(J3-Pad1)")
  (net 9 "Net-(J3-Pad2)")
  (net 10 "Net-(R4-Pad1)")
  (net 11 /SDA)
  (net 12 /SCL)
  (net 13 "Net-(J1-Pad2)")
  (net 14 "Net-(J1-Pad3)")
  (net 15 "Net-(J1-Pad4)")
  (net 16 "Net-(J2-Pad1)")
  (net 17 /RES/)
  (net 18 /RX)
  (net 19 /TX)
  (net 20 /TimeStamp)
  (net 21 /1PPS)
  (net 22 "Net-(R1-Pad1)")
  (net 23 "Net-(R1-Pad2)")
  (net 24 "Net-(R2-Pad1)")
  (net 25 "Net-(R2-Pad2)")
  (net 26 "Net-(U4-Pad21)")
  (net 27 "Net-(U4-Pad9)")
  (net 28 "Net-(U4-Pad5)")
  (net 29 "Net-(U4-Pad8)")
  (net 30 +BATT)
  (net 31 "Net-(U4-Pad12)")
  (net 32 "Net-(U4-Pad20)")
  (net 33 "Net-(U4-Pad22)")
  (net 34 "Net-(U4-Pad23)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /1PPS)
    (add_net /RES/)
    (add_net /RX)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
    (add_net /TimeStamp)
    (add_net GND)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad20)")
    (add_net "Net-(U4-Pad21)")
    (add_net "Net-(U4-Pad22)")
    (add_net "Net-(U4-Pad23)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U4-Pad9)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.635)
    (via_drill 0.50038)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net /+5VDC)
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net VBUS)
  )
  (net_class StripLine ""
    (clearance 0.19812)
    (trace_width 1.09982)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J2-Pad1)")
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 68.588469 55.205987 270)
    (fp_text reference "" (at -0.025 3.1 270) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 68.588469 56.475987 270)
    (fp_text reference "" (at -0.025 3.1 270) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 68.58 57.531 180)
    (fp_text reference "" (at -0.025 3.1 180) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 64.905469 55.840987 270)
    (fp_text reference "" (at -0.025 3.1 270) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 64.905469 57.110987 270)
    (fp_text reference "" (at -0.025 3.1 270) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 64.897 58.166 180)
    (fp_text reference "" (at -0.025 3.1 180) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 67.984013 45.474469 180)
    (fp_text reference "" (at -0.025 3.1 180) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 66.714013 45.474469 180)
    (fp_text reference "" (at -0.025 3.1 180) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 65.659 45.466 90)
    (fp_text reference "" (at -0.025 3.1 90) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 68.571531 48.553013 90)
    (fp_text reference "" (at -0.025 3.1 90) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 68.571531 47.283013 90)
    (fp_text reference "" (at -0.025 3.1 90) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 68.58 46.228)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 64.888531 48.553013 90)
    (fp_text reference "" (at -0.025 3.1 90) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 64.888531 47.283013 90)
    (fp_text reference "" (at -0.025 3.1 90) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 64.897 46.228)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 41.021 50.292)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 45.339 50.292)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 45.339 45.593)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 44.45 44.958)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -4.064 0.127) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 43.18 44.958)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -4.826 -0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 41.91 44.958)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -4.826 -0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 44.45 50.8)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -4.826 -0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 43.18 50.8)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -4.826 -0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 41.012531 46.648013 90)
    (fp_text reference "" (at -0.025 3.1 90) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 41.012531 47.918013 90)
    (fp_text reference "" (at -0.025 3.1 90) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 41.012531 49.188013 90)
    (fp_text reference "" (at -0.025 3.1 90) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 51.943 49.149)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 51.435 45.339)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 50.165 45.339)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 48.895 45.339)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 51.943 47.879)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 48.006 49.149)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 46.736 49.149)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 45.466 49.149)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -10.16 -0.635) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 51.943 46.609)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 48.006 46.609)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 46.736 46.609)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 45.466 46.609)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 39.116 69.85)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 39.751 68.072)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 40.894 66.929)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 41.021 65.024)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 42.418 60.325)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 42.418 62.611)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 69.723 70.612)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 77.343 68.834)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 74.803 66.294)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 45.72 69.469)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 45.72 68.58)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 71.12 60.706)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 71.12 51.308)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 71.12 55.88)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 71.12 45.72)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 60.96 60.96)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 55.88 55.88)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 60.96 55.88)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 55.88 50.8)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 60.96 50.8)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 55.88 45.72)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 60.96 45.72)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 40.64 55.88)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 41.91 50.8)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -4.826 -0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 41.021 45.593)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A348C4A)
    (at 40.64 40.64)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 45.72 40.64)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 50.8 40.64)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 55.88 40.64)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 60.96 40.64)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 66.04 40.64)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 71.12 40.64)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 76.2 40.64)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 81.28 40.64)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 86.36 71.12)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 86.36 66.04)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 86.36 60.96)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 86.36 55.88)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 86.36 50.8)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 86.36 45.72)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 60.96 73.66)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 71.12 65.913)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 39.37 74.93)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 60.96 71.12)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 40.386 71.247)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 60.96 68.58)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 71.12 68.58)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 60.96 66.04)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 71.12 63.627)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 57.15 71.12)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 54.102 71.12)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 50.8 71.12)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 72.898 68.326)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 57.15 66.04)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 50.8 66.04)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 55.88 60.96)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 86.36 40.64)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58CE4E7E)
    (at 45.72 66.04 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at -2.667 -1.27 180) (layer F.SilkS))
    (fp_text value USBLC6-2 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R2-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R1-Pad2)"))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 41.656 68.072 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.413 -0.508 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 76.2 69.596 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /+5VDC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 41.402 69.85 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -2.794 -0.127 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 74.168 69.342 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /+5VDC))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 41.656 61.468)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 73.66 65.532 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.651 360) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 44.196 58.166 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 2.667 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 70.104 62.23)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -1.651) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A3449B4)
    (at 47.498 53.848)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J3 (at -2.032 0 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J3-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 47.244 58.42 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.159 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 47.498 50.8 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.635 1.778 360) (layer F.SilkS))
    (fp_text value 10R (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 68.58 68.834 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.032 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /SDA))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 66.04 68.072)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.651) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /SCL))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:USB_Micro-B (layer F.Cu) (tedit 5543E447)
    (at 45.720787 73.399421)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J1 (at -5.461787 0.006579) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 5.01) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS))
    (pad 2 smd rect (at -0.65 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 0 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 0.65 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -2.5 -1.35 90) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.5 -1.35 90) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -3.5 1.35 90) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 3.5 1.35 90) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 597BEF84)
    (at 43.18 47.879 90)
    (fp_text reference J2 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 90) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 90) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.475 0 90) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 1.525 90) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 62.992 74.168 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J4 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /RES/))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /RX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /TX))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SCL))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SDA))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 52.832 74.168 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /TimeStamp))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /1PPS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 80.772 74.168 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /+5VDC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 44.704 62.23 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.635 1.651 360) (layer F.SilkS))
    (fp_text value 27R (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 46.736 62.242 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.917 0 360) (layer F.SilkS))
    (fp_text value 27R (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23-5 (layer F.Cu) (tedit 58CE4E80)
    (at 41.148 65.024 180)
    (descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
    (tags TSOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 1.905 -2.413 180) (layer F.SilkS))
    (fp_text value MIC5265-3.3YD5 (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.31 -0.95 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS))
    (pad 2 smd rect (at -1.31 0 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.31 0.95 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS))
    (pad 4 smd rect (at 1.31 0.95 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C5-Pad1)"))
    (pad 5 smd rect (at 1.31 -0.95 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23-5 (layer F.Cu) (tedit 58CE4E80)
    (at 71.12 66.04 90)
    (descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
    (tags TSOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -3.048 -0.635 180) (layer F.SilkS))
    (fp_text value MIC5265-3.3YD5 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.31 -0.95 90) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 /+5VDC))
    (pad 2 smd rect (at -1.31 0 90) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.31 0.95 90) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 /+5VDC))
    (pad 4 smd rect (at 1.31 0.95 90) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 5 smd rect (at 1.31 -0.95 90) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module GPS:LEA-5 (layer F.Cu) (tedit 5A340895)
    (at 58.42 55.118)
    (fp_text reference U4 (at 0 13.5) (layer F.SilkS))
    (fp_text value LEA-5 (at 0 -13.5) (layer F.Fab))
    (pad 21 smd rect (at -8.5 0.95) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U4-Pad21)"))
    (pad 9 smd rect (at 8.5 -2.85) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U4-Pad9)"))
    (pad 1 smd rect (at 8.5 8.65) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 /SDA))
    (pad 2 smd rect (at 8.5 7.55) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 12 /SCL))
    (pad 3 smd rect (at 8.5 6.45) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 19 /TX))
    (pad 4 smd rect (at 8.5 5.35) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 18 /RX))
    (pad 5 smd rect (at 8.5 4.25) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at 8.5 3.15) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 7 smd rect (at 8.5 2.05) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 8.5 0.95) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U4-Pad8)"))
    (pad 10 smd rect (at 8.5 -3.95) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 17 /RES/))
    (pad 11 smd rect (at 8.5 -5.05) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 30 +BATT))
    (pad 12 smd rect (at 8.5 -6.15) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U4-Pad12)"))
    (pad 13 smd rect (at 8.5 -7.25) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 8.5 -8.35) (size 1.8 0.8) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -8.5 -8.35) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -8.5 -7.25) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad1)"))
    (pad 17 smd rect (at -8.5 -6.15) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd rect (at -8.5 -5.05) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R4-Pad1)"))
    (pad 19 smd rect (at -8.5 -3.95) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J3-Pad2)"))
    (pad 20 smd rect (at -8.5 -2.85) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U4-Pad20)"))
    (pad 22 smd rect (at -8.5 2.05) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U4-Pad22)"))
    (pad 23 smd rect (at -8.5 3.15) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U4-Pad23)"))
    (pad 24 smd rect (at -8.5 4.25) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 25 smd rect (at -8.5 5.35) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R1-Pad1)"))
    (pad 26 smd rect (at -8.5 6.45) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R2-Pad1)"))
    (pad 27 smd rect (at -8.5 7.55) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 21 /1PPS))
    (pad 28 smd rect (at -8.5 8.65) (size 1.8 0.8) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 20 /TimeStamp))
  )
  (module Battery:CR-2032-HFN (layer F.Cu) (tedit 5A341214)
    (at 78.74 53.34 90)
    (fp_text reference BT1 (at 10.668 5.207 180) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 -4.55 90) (layer F.Fab))
    (fp_text user + (at 7 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at -10.05 0 90) (size 4 4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 10.45 0 90) (size 4 4) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 +BATT))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08F5)
    (at 54.102 66.04)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (gr_text V1.0 (at 62.865 50.546) (layer B.SilkS))
  (gr_text KD5SSJ (at 63.373 42.799) (layer B.SilkS))
  (gr_text "uBlox LEA-5T Timing GPS Breakout" (at 63.373 48.006) (layer B.SilkS))
  (gr_text +5VDC (at 80.899 69.088 90) (layer B.SilkS))
  (gr_text RES/ (at 62.992 69.85 90) (layer B.SilkS))
  (gr_text SDA (at 73.279 70.739 90) (layer B.SilkS))
  (gr_text SCL (at 70.612 70.739 90) (layer B.SilkS))
  (gr_text Tx (at 68.072 71.628 90) (layer B.SilkS))
  (gr_text Rx (at 65.659 71.501 90) (layer B.SilkS))
  (gr_text 1PPS (at 55.626 69.977 90) (layer B.SilkS))
  (gr_text TS (at 52.959 71.628 90) (layer B.SilkS))
  (gr_text $ (at 58.42 53.594) (layer F.SilkS))
  (gr_line (start 38.1 38.1) (end 88.9 38.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 38.1 38.1) (end 38.1 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 76.2) (end 88.9 38.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 38.1 76.2) (end 88.9 76.2) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.1 38.1) (xy 88.9 38.1) (xy 88.9 76.2) (xy 38.1 76.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.1 38.1) (xy 88.9 38.1) (xy 88.9 76.2) (xy 38.1 76.2)
      )
    )
  )
)
