<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="15.24" y1="33.02" x2="1.27" y2="33.02" width="0.0254" layer="20"/>
<wire x1="1.27" y1="33.02" x2="0" y2="34.29" width="0.0254" layer="20" curve="-90"/>
<wire x1="0" y1="34.29" x2="0" y2="58.42" width="0.0254" layer="20"/>
<wire x1="0" y1="58.42" x2="1.27" y2="59.69" width="0.0254" layer="20" curve="-90"/>
<wire x1="1.27" y1="59.69" x2="13.97" y2="59.69" width="0.0254" layer="20"/>
<wire x1="13.97" y1="59.69" x2="15.24" y2="59.69" width="0.0254" layer="20"/>
<wire x1="15.24" y1="59.69" x2="26.67" y2="72.39" width="0.0254" layer="20" curve="-90"/>
<wire x1="26.67" y1="72.39" x2="49.53" y2="72.39" width="0.0254" layer="20"/>
<wire x1="49.53" y1="72.39" x2="73.66" y2="48.26" width="0.0254" layer="20" curve="-90"/>
<wire x1="73.66" y1="48.26" x2="73.66" y2="45.72" width="0.0254" layer="20"/>
<wire x1="73.66" y1="45.72" x2="49.53" y2="21.59" width="0.0254" layer="20" curve="-90"/>
<wire x1="49.53" y1="21.59" x2="26.67" y2="21.59" width="0.0254" layer="20"/>
<wire x1="26.67" y1="21.59" x2="15.24" y2="33.02" width="0.0254" layer="20" curve="-90"/>
<text>FLASH-O-TRON</text>
<text>By Lauren and Tom Whitwell
Herne Hill, London, January 2014</text>
</plain>
<libraries>
<library name="40xx">
<description>&lt;b&gt;CMOS Logic Devices, 4000 Series&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola &lt;i&gt;CMOS LOGIC DATA&lt;/i&gt;; book, 02/88, DL131 REV 1
&lt;li&gt;http://www.elexp.com
&lt;li&gt;http://www.intersil.com
&lt;li&gt;http://www.ls3c.com.tw/product/1/COMOS.html
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-AnalogIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of analog ICs- DACs, ADCs, video chips, op-amps, and others.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL-08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="TomW">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="EVUF">
<description>&lt;b&gt;9 mm Square Rotary Potentiometers&lt;/b&gt; Vertical, Snap-in&lt;p&gt;
Source: Panasonic</description>
</package>
<package name="LONG_PAD_1">
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="40xx" package="DIL16" value="4017N"/>
<element name="IC2" library="SparkFun-AnalogIC" package="DIL-08" value="">
<attribute name="OC_NEWARK" value="89K1486"/>
<attribute name="MPN" value="NE555N"/>
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="OC_FARNELL" value="1467742"/>
</element>
<element name="LED1" library="TomW" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="TomW" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="TomW" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="TomW" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED5" library="TomW" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED6" library="TomW" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED7" library="TomW" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED8" library="TomW" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED9" library="TomW" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED10" library="TomW" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="TomW" package="0207/10" value="1k"/>
<element name="R2" library="TomW" package="0207/10" value="1k"/>
<element name="R3" library="TomW" package="0207/10" value="1k"/>
<element name="R4" library="TomW" package="0207/10" value="1k"/>
<element name="R5" library="TomW" package="0207/10" value="1k"/>
<element name="R6" library="TomW" package="0207/10" value="1k"/>
<element name="R7" library="TomW" package="0207/10" value="1k"/>
<element name="R8" library="TomW" package="0207/10" value="1k"/>
<element name="R9" library="TomW" package="0207/10" value="1k"/>
<element name="R10" library="TomW" package="0207/10" value="1k"/>
<element name="R11" library="TomW" package="EVUF" value=""/>
<element name="C1" library="gm-caps-electro-pol" package="050_020" value="4.7uf"/>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH"/>
<element name="RED" library="TomW" package="LONG_PAD_1" value="RED">
<attribute name="VALUE"/>
</element>
<element name="BLACK" library="TomW" package="LONG_PAD_1" value="BLACK">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC2" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC2" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="BLACK" pad="P$1"/>
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="K"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="K"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LED3" pad="K"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="LED4" pad="K"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="LED5" pad="K"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="LED6" pad="K"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="LED7" pad="K"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="LED8" pad="K"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="LED9" pad="K"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="3"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="4"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="7"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="10"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="1"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="5"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="6"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="9"/>
<contactref element="LED9" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="LED10" pad="K"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="11"/>
<contactref element="LED10" pad="A"/>
</signal>
<signal name="+9V">
<contactref element="IC1" pad="16"/>
<contactref element="S1" pad="3"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="S1" pad="1"/>
<contactref element="RED" pad="P$1"/>
</signal>
<signal name="N$22">
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="R11" pad="3"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="CLOCK">
<contactref element="IC2" pad="3"/>
<contactref element="IC1" pad="14"/>
<contactref element="R11" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
