(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 50)
    (no_connects 0)
    (area 91.724999 76.624999 155.775001 122.275001)
    (thickness 1.6)
    (drawings 50)
    (tracks 287)
    (zones 0)
    (modules 18)
    (nets 24)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.203)
    (user_trace_width 0.254)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.5 0.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 140 100)
    (grid_origin 140 100)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /D6)
  (net 4 /D5)
  (net 5 /D4)
  (net 6 /D3)
  (net 7 /D2)
  (net 8 /D1)
  (net 9 /readChSel)
  (net 10 /D0)
  (net 11 /CLK)
  (net 12 /D7)
  (net 13 /RSTCh2)
  (net 14 /RSTCH1)
  (net 15 /ch2B)
  (net 16 /ch1B)
  (net 17 /ch1A)
  (net 18 /ch2A)
  (net 19 /readSel1)
  (net 20 /readReset)
  (net 21 /readSel2)
  (net 22 /ch2I)
  (net 23 /ch1I)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /CLK)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /RSTCH1)
    (add_net /RSTCh2)
    (add_net /ch1A)
    (add_net /ch1B)
    (add_net /ch1I)
    (add_net /ch2A)
    (add_net /ch2B)
    (add_net /ch2I)
    (add_net /readChSel)
    (add_net /readReset)
    (add_net /readSel1)
    (add_net /readSel2)
    (add_net GND)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 56CCE8F6)
    (at 126.85 110.6 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0.05 1.65 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 56CCE6EE)
    (at 101.65 93.6 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 4.5 0.1 270) (layer F.SilkS) hide)
    (fp_text value 0.01uF (at -4.75 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 56CCE703)
    (at 100.4 112.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /ch1A))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /ch1B))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /ch1I))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 56CCE6FC)
    (at 100.45 107.45 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /ch2A))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /ch2B))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /ch2I))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 56DE1A50)
    (at 130 80)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X15 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /readSel1))
    (pad 2 smd circle (at 0 2.54) (size 0.5 0.5) (layers Dwgs.User))
    (pad 3 smd circle (at 0 5.08) (size 0.5 0.5) (layers Dwgs.User))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D0))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D1))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D2))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D3))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /D4))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /D5))
    (pad 10 smd circle (at 0 22.86) (size 0.5 0.5) (layers Dwgs.User))
    (pad 11 smd circle (at 0 25.4) (size 0.5 0.5) (layers Dwgs.User))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 13 smd circle (at 0 30.48) (size 0.5 0.5) (layers Dwgs.User))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 smd circle (at 0 35.56) (size 0.5 0.5) (layers Dwgs.User))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 56DE1A45)
    (at 145 80)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X15 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /readReset))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /RSTCh2))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /RSTCH1))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /readSel2))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /readChSel))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /D7))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /D6))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 smd circle (at 0 20.32) (size 0.5 0.5) (layers Dwgs.User))
    (pad 10 smd circle (at 0 22.86) (size 0.5 0.5) (layers Dwgs.User))
    (pad 11 smd circle (at 0 25.4) (size 0.5 0.5) (layers Dwgs.User))
    (pad 12 smd circle (at 0 27.94) (size 0.5 0.5) (layers Dwgs.User))
    (pad 13 smd circle (at 0 30.48) (size 0.5 0.5) (layers Dwgs.User))
    (pad 14 smd circle (at 0 33.02) (size 0.5 0.5) (layers Dwgs.User))
    (pad 15 smd circle (at 0 35.56) (size 0.5 0.5) (layers Dwgs.User))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 56CCE76C)
    (at 150 107.35)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 56CCE771)
    (at 150.05 114.15)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module additional_ics:oscillator_3.2x5mm (layer F.Cu) (tedit 56CCE6D5)
    (at 105.65 93.75 270)
    (fp_text reference OSC1 (at -2.15 -3.45 270) (layer F.SilkS) hide)
    (fp_text value 30MHz (at 3.5 -0.1 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 1.1 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 1.1 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.25 -1.1 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /CLK))
    (pad 4 smd rect (at -1.25 -1.1 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 56DE17F0)
    (at 105.6 118)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.9) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.9) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 23 /ch1I))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 56DE17E4)
    (at 108.35 110.7)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.9) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 22 /ch2I))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 56DE08C8)
    (at 96.4 96.65 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 56DE08BF)
    (at 96.4 87.3)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56DE1802)
    (at 96.6 112.7 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 100K (at 0.2 -1.9 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /ch1A))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56DE17F6)
    (at 96.6 117.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.9 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /ch1B))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56DE1807)
    (at 96.6 107.8 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.85 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /ch2A))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56DE180E)
    (at 96.6 103.1 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 -1.85 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /ch2B))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module additional_ics:SOJ-32_hand_soldering (layer F.Cu) (tedit 56DEF1E2)
    (at 116.05 99.45 270)
    (descr "Module CMS SOJ 32 pins")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference HC1 (at 0 1.905 270) (layer F.SilkS) hide)
    (fp_text value HCTL2032 (at -0.3 0.1 270) (layer F.SilkS))
    (pad 20 smd rect (at 5.715 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 3 /D6))
    (pad 21 smd rect (at 4.445 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 4 /D5))
    (pad 22 smd rect (at 3.175 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 5 /D4))
    (pad 23 smd rect (at 1.905 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 0.635 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at -4.445 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at -5.715 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 6 /D3))
    (pad 30 smd rect (at -6.985 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 7 /D2))
    (pad 31 smd rect (at -8.255 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 8 /D1))
    (pad 32 smd rect (at -9.525 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 9 /readChSel))
    (pad 1 smd rect (at -9.525 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -8.255 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -6.985 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -5.715 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 10 /D0))
    (pad 5 smd rect (at -4.445 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /CLK))
    (pad 9 smd rect (at 0.635 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 1.905 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 12 /D7))
    (pad 11 smd rect (at 3.175 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 13 /RSTCh2))
    (pad 12 smd rect (at 4.445 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 14 /RSTCH1))
    (pad 13 smd rect (at 5.715 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 15 /ch2B))
    (pad 14 smd rect (at 6.985 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 16 /ch1B))
    (pad 15 smd rect (at 8.255 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 17 /ch1A))
    (pad 16 smd rect (at 9.525 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 18 /ch2A))
    (pad 6 smd rect (at -3.175 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 19 /readSel1))
    (pad 7 smd rect (at -1.905 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 20 /readReset))
    (pad 8 smd rect (at -0.635 4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at -3.175 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at -1.905 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 21 /readSel2))
    (pad 25 smd rect (at -0.635 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 6.985 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 22 /ch2I))
    (pad 18 smd rect (at 8.255 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 9.525 -4.699 270) (size 0.4572 2) (layers F.Cu F.Paste F.Mask)
      (net 23 /ch1I))
    (model SMD_Packages.3dshapes/SOJ-32.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.55 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text S1 (at 126.95 80) (layer F.SilkS))
  (gr_text D5 (at 126.9 100.3) (layer F.SilkS))
  (gr_text D4 (at 126.8 97.85) (layer F.SilkS))
  (gr_text D3 (at 126.9 95.4) (layer F.SilkS))
  (gr_text D2 (at 126.9 92.85) (layer F.SilkS))
  (gr_text D1 (at 126.9 90.2) (layer F.SilkS))
  (gr_text D0 (at 126.9 87.6) (layer F.SilkS))
  (gr_text RR (at 148.1 80.15) (layer F.SilkS))
  (gr_text R2 (at 148.05 82.7) (layer F.SilkS))
  (gr_text R1 (at 148.05 85.2) (layer F.SilkS))
  (gr_text S2 (at 148.05 87.7) (layer F.SilkS))
  (gr_text CS (at 148.1 90.25) (layer F.SilkS))
  (gr_text D7 (at 148.05 92.85) (layer F.SilkS))
  (gr_text D6 (at 148.05 95.35) (layer F.SilkS))
  (gr_circle (center 121.2 119.05) (end 121.2 120.55) (layer Edge.Cuts) (width 0.15))
  (gr_text "Arduino\nNano" (at 137.6 96.25) (layer F.SilkS))
  (gr_text uUSB (at 137.4 82.55) (layer F.SilkS))
  (gr_line (start 91.8 80.45) (end 95.55 76.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.85 76.7) (end 95.55 76.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.8 81.45) (end 91.8 80.45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.8 82.65) (end 91.8 81.45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.8 83.55) (end 91.8 82.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.8 117.8) (end 91.8 83.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.2 122.2) (end 91.8 117.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.2 122.2) (end 96.2 122.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text +5V (at 96.2 84.3) (layer F.SilkS))
  (gr_text +5V (at 96.1 99.85) (layer F.SilkS))
  (gr_text GND (at 99.3 91.75 270) (layer F.SilkS))
  (gr_circle (center 151.35 87.75) (end 151.35 89.25) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 103.9 80.6) (end 103.9 82.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.6 122.2) (end 99.2 122.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.7 117.1) (end 150.6 122.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.7 82.4) (end 155.7 117.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150 76.7) (end 155.7 82.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.85 76.7) (end 150 76.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 150.05 117.1) (layer F.SilkS))
  (gr_text GND (at 133.95 112.95) (layer F.SilkS))
  (gr_text +5V (at 133.85 107.8) (layer F.SilkS))
  (gr_text +5V (at 150.1 104.4) (layer F.SilkS))
  (gr_text I (at 104 118.4) (layer F.SilkS))
  (gr_text A (at 104.15 112.9) (layer F.SilkS))
  (gr_text B (at 104.15 104.95) (layer F.SilkS))
  (gr_text B (at 104.1 115.5) (layer F.SilkS))
  (gr_text A (at 104.2 107.9) (layer F.SilkS))
  (gr_text I (at 104.2 102.05) (layer F.SilkS))
  (gr_text EC1 (at 106.5 114.9 90) (layer F.SilkS))
  (gr_text EC2 (at 106.5 105 90) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.203)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.205))
    (polygon
      (pts
        (xy 102.1 88.25) (xy 100.05 90.3) (xy 100.05 93.75) (xy 100.2 93.9) (xy 105.6 93.9)
        (xy 105.6 96.2) (xy 108.7 99.3) (xy 108.7 102.55) (xy 105.95 102.55) (xy 103 99.6)
        (xy 100 99.6) (xy 98.3 101.3) (xy 98.3 103.25) (xy 95.6 103.25) (xy 95.6 107.8)
        (xy 98.3 107.8) (xy 98.3 112.7) (xy 95.65 112.7) (xy 95.65 117.5) (xy 98.3 117.5)
        (xy 98.3 120.1) (xy 95.4 120.1) (xy 92.75 117.45) (xy 92.75 84.85) (xy 102.1 84.85)
        (xy 102.1 88.25)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.203)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.205))
    (polygon
      (pts
        (xy 110.4 88.95) (xy 112.7 88.95) (xy 112.7 91.9) (xy 109.6 91.9) (xy 108.15 93.35)
        (xy 103 93.35) (xy 102.95 93.3) (xy 100.6 93.3) (xy 100.6 90.75) (xy 102.85 88.5)
        (xy 102.85 87.25) (xy 108.7 87.25) (xy 110.4 88.95)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.203)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.205))
    (polygon
      (pts
        (xy 108.5 106.75) (xy 106.9 105.15) (xy 106.9 102.55) (xy 104.2 99.85) (xy 102.2 99.85)
        (xy 102.2 96.6) (xy 105.5 96.6) (xy 116.2 107.3) (xy 122.7 107.3) (xy 126.2 110.8)
        (xy 153.1 110.8) (xy 153.1 116.75) (xy 151.25 118.6) (xy 125.45 118.6) (xy 117.65 110.8)
        (xy 112.95 110.8) (xy 112.55 110.8) (xy 108.5 106.75)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.203)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.205))
    (polygon
      (pts
        (xy 111.15 89.7) (xy 111.15 94.85) (xy 112.2 95.9) (xy 121.85 95.9) (xy 128.35 102.4)
        (xy 153.1 102.4) (xy 153.1 110.2) (xy 126.5 110.2) (xy 124.55 108.25) (xy 124.55 105.6)
        (xy 118.45 99.5) (xy 110.85 99.5) (xy 107.05 95.7) (xy 101.65 95.7) (xy 100.75 96.6)
        (xy 100.75 99.2) (xy 100.25 99.7) (xy 93.5 99.7) (xy 93.5 84.85) (xy 106.3 84.85)
        (xy 111.15 89.7)
      )
    )
  )
)
