(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 57)
    (no_connects 0)
    (area 128.380286 47.730999 177.166191 87.900857)
    (thickness 1.6)
    (drawings 13)
    (tracks 203)
    (zones 0)
    (modules 26)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 SDA)
  (net 2 SCL)
  (net 3 +5V)
  (net 4 OLED_GND)
  (net 5 GND)
  (net 6 TEST_GND)
  (net 7 +9V)
  (net 8 R1HIGH)
  (net 9 VTEST_H)
  (net 10 VTEST_L)
  (net 11 R1GATE)
  (net 12 R1LOW)
  (net 13 OLED_ON)
  (net 14 R2GATE)
  (net 15 R2LOW)
  (net 16 "Net-(uC1-Pad2)")
  (net 17 "Net-(uC1-Pad28)")
  (net 18 "Net-(uC1-Pad3)")
  (net 19 "Net-(uC1-Pad27)")
  (net 20 "Net-(uC1-Pad26)")
  (net 21 "Net-(uC1-Pad25)")
  (net 22 "Net-(uC1-Pad24)")
  (net 23 "Net-(uC1-Pad23)")
  (net 24 "Net-(uC1-Pad22)")
  (net 25 "Net-(uC1-Pad21)")
  (net 26 "Net-(uC1-Pad20)")
  (net 27 "Net-(uC1-Pad18)")
  (net 28 "Net-(uC1-Pad13)")
  (net 29 "Net-(uC1-Pad17)")
  (net 30 "Net-(uC1-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net +9V)
    (add_net GND)
    (add_net "Net-(uC1-Pad13)")
    (add_net "Net-(uC1-Pad16)")
    (add_net "Net-(uC1-Pad17)")
    (add_net "Net-(uC1-Pad18)")
    (add_net "Net-(uC1-Pad2)")
    (add_net "Net-(uC1-Pad20)")
    (add_net "Net-(uC1-Pad21)")
    (add_net "Net-(uC1-Pad22)")
    (add_net "Net-(uC1-Pad23)")
    (add_net "Net-(uC1-Pad24)")
    (add_net "Net-(uC1-Pad25)")
    (add_net "Net-(uC1-Pad26)")
    (add_net "Net-(uC1-Pad27)")
    (add_net "Net-(uC1-Pad28)")
    (add_net "Net-(uC1-Pad3)")
    (add_net OLED_GND)
    (add_net OLED_ON)
    (add_net R1GATE)
    (add_net R1HIGH)
    (add_net R1LOW)
    (add_net R2GATE)
    (add_net R2LOW)
    (add_net SCL)
    (add_net SDA)
    (add_net TEST_GND)
    (add_net VTEST_H)
    (add_net VTEST_L)
  )
  (module FootPrints:OLED_32X128-GVCD (layer F.Cu) (tedit 5B5B6FAC)
    (at 137.16 57.15 270)
    (fp_text reference D1 (at 0 2.7 270) (layer F.SilkS))
    (fp_text value I2C_OLED_GVCD (at 0 -14.986 270) (layer F.Fab))
    (fp_text user SDA (at -3.81 -2.54 360) (layer F.SilkS))
    (fp_text user SCL (at -1.27 -2.54 360) (layer F.SilkS))
    (fp_text user VCC (at 1.27 -2.54 360) (layer F.SilkS))
    (fp_text user GND (at 3.81 -2.794 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.81 0 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 SDA))
    (pad 2 thru_hole oval (at -1.27 0 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 SCL))
    (pad 3 thru_hole oval (at 1.27 0 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 3.81 0 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 OLED_GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 134.366 60.96 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference D2 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value I2C_OLED_VGCD (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 OLED_GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 SCL))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA-SMB_Universal_Handsoldering (layer F.Cu) (tedit 5B8FCFCA)
    (at 153.67 76.454 270)
    (descr "Diode, Universal, SMA (DO-214AC) or SMB (DO-214AA), Handsoldering,")
    (tags "Diode Universal SMA (DO-214AC) SMB (DO-214AA) Handsoldering ")
    (attr smd)
    (fp_text reference D3 (at -5.842 1.524 360) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -3 270) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.9 0 270) (size 3.6 1.7) (rect_delta 0.6 0 ) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd trapezoid (at 2.9 0 90) (size 3.6 1.7) (rect_delta 0.6 0 ) (layers F.Cu F.Paste F.Mask)
      (net 6 TEST_GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5B8FC811)
    (at 142.748 79.502)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -4.064 0) (layer F.SilkS))
    (fp_text value AO3400 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 R1GATE))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 R1LOW))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 TEST_GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 144.526 59.944)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value AO3400 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 OLED_ON))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 OLED_GND))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5B8FC80F)
    (at 165.608 79.502 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value AO3400 (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 R2GATE))
    (pad 2 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 R2LOW))
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 TEST_GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC6AD)
    (at 137.922 68.834)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -4.318 0) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 R1LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC6B0)
    (at 137.922 71.374)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -4.318 0) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 R1LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC6B3)
    (at 137.922 73.914)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -4.318 0) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 R1LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC6B6)
    (at 137.922 76.454)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at -4.318 0) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 R1LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC6AB)
    (at 144.78 68.834 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -4.318 0 180) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 R1LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC6A8)
    (at 144.78 71.374 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at -4.318 -0.254 180) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 R1LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC6A3)
    (at 144.78 73.914 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at -4.318 0 180) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 R1LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC69D)
    (at 144.78 76.454 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at -4.318 0 180) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 R1LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC688)
    (at 162.306 68.834)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -4.572 0) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 R2LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC69A)
    (at 162.306 71.374)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at -4.572 0) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 R2LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC694)
    (at 162.306 73.914)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at -4.572 0) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 R2LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC699)
    (at 162.306 76.454)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at -4.572 -0.254) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 R2LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC686)
    (at 169.164 68.834 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at -4.826 -0.254 180) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 R2LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC682)
    (at 169.164 71.374 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at -4.826 0 180) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 R2LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC680)
    (at 169.164 73.914 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at -4.826 0 180) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 R2LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B8FC676)
    (at 169.164 76.454 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R16 (at -4.826 0 180) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 R1HIGH))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 R2LOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FootPrints:ARDUINO_NANO (layer B.Cu) (tedit 5B5B6DDB)
    (at 154.178 57.15)
    (fp_text reference uC1 (at -12.954 0 270) (layer B.SilkS))
    (fp_text value NANO (at 0 0) (layer B.Fab))
    (fp_text user GND (at 17.78 -5.08 270) (layer B.SilkS))
    (fp_text user VIN (at 15.24 -5.08 270) (layer B.SilkS))
    (fp_text user RX (at 15.24 5.334 270) (layer B.SilkS))
    (fp_text user TX (at 17.78 5.334 270) (layer B.SilkS))
    (fp_text user D13 (at -17.78 -5.842) (layer B.SilkS))
    (fp_text user D12 (at -17.78 5.842 180) (layer B.SilkS))
    (fp_text user USB (at -19.304 0 180) (layer B.SilkS))
    (pad 30 thru_hole oval (at -17.78 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 R1GATE))
    (pad 1 thru_hole oval (at -17.78 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 OLED_ON))
    (pad 29 thru_hole oval (at -15.24 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 R2GATE))
    (pad 2 thru_hole oval (at -15.24 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(uC1-Pad2)"))
    (pad 28 thru_hole oval (at -12.7 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(uC1-Pad28)"))
    (pad 3 thru_hole oval (at -12.7 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(uC1-Pad3)"))
    (pad 27 thru_hole oval (at -10.16 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(uC1-Pad27)"))
    (pad 4 thru_hole oval (at -10.16 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 VTEST_L))
    (pad 26 thru_hole oval (at -7.62 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(uC1-Pad26)"))
    (pad 5 thru_hole oval (at -7.62 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 VTEST_H))
    (pad 25 thru_hole oval (at -5.08 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(uC1-Pad25)"))
    (pad 6 thru_hole oval (at -5.08 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 R1LOW))
    (pad 24 thru_hole oval (at -2.54 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(uC1-Pad24)"))
    (pad 7 thru_hole oval (at -2.54 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 R1HIGH))
    (pad 23 thru_hole oval (at 0 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(uC1-Pad23)"))
    (pad 8 thru_hole oval (at 0 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 SDA))
    (pad 22 thru_hole oval (at 2.54 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(uC1-Pad22)"))
    (pad 9 thru_hole oval (at 2.54 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 SCL))
    (pad 21 thru_hole oval (at 5.08 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(uC1-Pad21)"))
    (pad 10 thru_hole oval (at 5.08 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 R2LOW))
    (pad 20 thru_hole oval (at 7.62 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(uC1-Pad20)"))
    (pad 11 thru_hole oval (at 7.62 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 R1HIGH))
    (pad 19 thru_hole oval (at 10.16 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 12 thru_hole oval (at 10.16 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 18 thru_hole oval (at 12.7 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(uC1-Pad18)"))
    (pad 13 thru_hole oval (at 12.7 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(uC1-Pad13)"))
    (pad 17 thru_hole oval (at 15.24 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(uC1-Pad17)"))
    (pad 14 thru_hole oval (at 15.24 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 16 thru_hole oval (at 17.78 7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(uC1-Pad16)"))
    (pad 15 thru_hole oval (at 17.78 -7.62) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 +9V))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 173.99 58.166 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value 9V_BATT (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +9V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B8FCECA)
    (at 160.782 83.058 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at -2.286 1.27 360) (layer F.SilkS))
    (fp_text value PROBE_HIGH (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 R1HIGH))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 VTEST_H))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B8FCECD)
    (at 149.098 83.058 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at -2.286 1.27 360) (layer F.SilkS))
    (fp_text value PROBE_LOW (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 VTEST_L))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text NANO (at 157.734 56.896) (layer B.SilkS))
  (gr_text OLED (at 157.734 56.896) (layer F.SilkS))
  (gr_text 9V- (at 170.18 58.166) (layer F.SilkS))
  (gr_text 9V+ (at 170.18 55.372) (layer F.SilkS))
  (gr_text v (at 144.272 82.804) (layer F.SilkS))
  (gr_text v (at 155.956 82.804) (layer F.SilkS))
  (gr_text - (at 151.638 82.804) (layer F.SilkS))
  (gr_text + (at 163.576 82.804) (layer F.SilkS))
  (gr_line (start 132.588 84.582) (end 132.588 48.006) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.842 84.582) (end 132.588 84.582) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.768 84.582) (end 132.842 84.582) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.768 48.006) (end 175.768 84.582) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.588 48.006) (end 175.768 48.006) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.514 84.328) (xy 132.842 84.328) (xy 132.842 48.26) (xy 175.514 48.26)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.514 84.328) (xy 132.842 84.328) (xy 132.842 48.26) (xy 175.514 48.26)
      )
    )
  )
)
