(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "3B")
	(net 2 "1B")
	(net 3 "2B")
	(net 4 "2A")
	(net 5 "3A")
	(net 6 "1A")
	(footprint "Potentiometer_THT:Potentiometer_Bourns_PTV112-4_Dual_Vertical"
		(layer "F.Cu")
		(at 181.8325 98.6)
		(descr "2 Gang dual Through Hole, Snap In potentiometer, https://www.bourns.com/docs/Product-Datasheets/PTVPTT.pdf")
		(tags "PTV112-4 Dual gang")
		(property "Reference" "RV1"
			(at 8.5 -6.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PTV112"
			(at 1.6825 12.525 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Bourns_PTV112-4_Dual_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual potentiometer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "Dual-Gang Pot Adapter.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "1A")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -2 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "2A")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 8 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "3A")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 2 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "1B")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 4 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "2B")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 6 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "3B")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "SH" thru_hole oval
			(at 11 -2.8 270)
			(size 3 3.9)
			(drill oval 2 2.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "SH" thru_hole oval
			(at 11 8.8 270)
			(size 3 3.9)
			(drill oval 2 2.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 199.1825 94.8) (xy 199.1825 96.6) (xy 185.7825 96.6) (xy 185.7825 94.8)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 199.1825 106.6) (xy 199.1825 108.4) (xy 185.7825 108.4) (xy 185.7825 106.6)
				)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTV112-4_Dual_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 190.515 91.44 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J1"
			(at 0 2.33 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x03"
			(at 0 -7.41 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Dual-Gang Pot Adapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -2.54 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "1B")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "2B")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "3B")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 190.515 111.76 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J2"
			(at 0 2.33 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x03"
			(at 0 -7.41 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Dual-Gang Pot Adapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -2.54 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "1A")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "2A")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "3A")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 177.8 91.44)
		(mid 178.543949 89.643949)
		(end 180.34 88.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 201.93 111.76)
		(end 201.93 91.44)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 180.34 114.3)
		(mid 178.543949 113.556051)
		(end 177.8 111.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.39 114.3)
		(end 180.34 114.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.39 88.9)
		(end 180.34 88.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.8 91.44)
		(end 177.8 111.76)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 201.93 111.76)
		(mid 201.186051 113.556051)
		(end 199.39 114.3)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 199.39 88.9)
		(mid 201.186051 89.643949)
		(end 201.93 91.44)
		(layer "Edge.Cuts")
	)
)
