<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="12.68" y2="0" width="0" layer="20"/>
<wire x1="12.68" y1="0" x2="12.68" y2="19.99" width="0" layer="20"/>
<wire x1="12.68" y1="19.99" x2="0" y2="19.9644" width="0" layer="20"/>
<wire x1="0" y1="19.9644" x2="0" y2="0" width="0" layer="20"/>
<text>By TinLethax</text>
<text>By TinLethax</text>
<text>By TinLethax</text>
<text>By TinLethax</text>
<text>By TinLethax</text>
<text>By TinLethax</text>
</plain>
<libraries>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SCDV554x">
<packages>
<package name="SCDV554X">
</package>
</packages>
</library>
<library name="STM8L151F3">
<packages>
<package name="UFQFPN-20">
<description>UFQFPN20 Package 3x3mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TP1" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SCDV554x" package="SCDV554X" value="SCDV554X"/>
<element name="U$2" library="STM8L151F3" package="UFQFPN-20" value="STM8L151F3"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="U$1" pad="RST"/>
<contactref element="U$1" pad="VCC3"/>
<contactref element="U$1" pad="VCC2"/>
<contactref element="U$1" pad="VCC1"/>
<contactref element="U$1" pad="CLKSEL"/>
<contactref element="U$2" pad="VDD"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="GND2"/>
<contactref element="U$2" pad="VSS"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="SDCLK"/>
<contactref element="U$2" pad="PA2"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="DATA"/>
<contactref element="U$2" pad="PD0"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="LOAD"/>
<contactref element="U$2" pad="PA3"/>
</signal>
<signal name="N$7">
<contactref element="U$2" pad="NRST/PA1"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="N$8">
<contactref element="TP3" pad="TP"/>
<contactref element="U$2" pad="PA0"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
