(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 30)
    (zones 0)
    (modules 7)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GNDPWR)
  (net 2 "Net-(60ohm1-Pad2)")
  (net 3 "Net-(60ohm1-Pad1)")
  (net 4 "Net-(80ohm1-Pad2)")
  (net 5 "Net-(80ohm1-Pad1)")
  (net 6 "Net-(BT1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDPWR)
    (add_net "Net-(60ohm1-Pad1)")
    (add_net "Net-(60ohm1-Pad2)")
    (add_net "Net-(80ohm1-Pad1)")
    (add_net "Net-(80ohm1-Pad2)")
    (add_net "Net-(BT1-Pad1)")
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x01_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 116.84 120.65)
    (descr "Through hole straight pin header, 1x01, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.00mm single row")
    (fp_text reference GND (at 0 -2.06) (layer F.SilkS))
    (fp_text value "GND Pin" (at 0 2.06) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x01_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EndConnectors:KingbrightTesting (layer F.Cu) (tedit 5DBDF776)
    (at 116.205 105.41 90)
    (descr "Kingbright, dual LED, 3.5 x 2.8 mm Surface Mount LED Lamp (http://www.kingbrightusa.com/images/catalog/SPEC/AAA3528ESGCT.pdf)")
    (tags "dual led smd")
    (attr smd)
    (fp_text reference KingBright (at -1.27 -2.5 90) (layer F.SilkS))
    (fp_text value DualLed (at 0 2.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.4 -0.725 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(60ohm1-Pad2)"))
    (pad 4 smd rect (at 1.4 0.725 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (pad 3 smd rect (at -1.4 0.725 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(80ohm1-Pad2)"))
    (pad 2 smd rect (at 1.4 -0.725 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Kingbright_AAA3528ESGCT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EndConnectors:DualLed (layer F.Cu) (tedit 5DBDB68F)
    (at 114.3 111.76)
    (fp_text reference MyLayout (at 1.27 0.5) (layer F.SilkS))
    (fp_text value DualLed (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 2.54) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(60ohm1-Pad2)"))
    (pad 2 smd rect (at 2.7 2.54) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (pad 3 smd rect (at 0 4.14) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(80ohm1-Pad2)"))
    (pad 4 smd rect (at 2.7 4.14) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
  )
  (module Resistor_SMD:R_2010_5025Metric_Pad1.52x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 110.9225 119.38)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference 80ohm (at 0 -2.28) (layer F.SilkS) hide)
    (fp_text value "80 ohm" (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at -1.1945 -16.256 180) (layer F.SilkS))
    (pad 1 smd roundrect (at -2.3375 0) (size 1.525 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 5 "Net-(80ohm1-Pad1)"))
    (pad 2 smd roundrect (at 2.3375 0) (size 1.525 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 4 "Net-(80ohm1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2010_5025Metric_Pad1.52x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 109.855 105.156)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference 60ohm (at 0 -2.28) (layer F.SilkS) hide)
    (fp_text value 60ohm (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0.889 16.256) (layer F.SilkS))
    (pad 1 smd roundrect (at -2.3375 0) (size 1.525 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 3 "Net-(60ohm1-Pad1)"))
    (pad 2 smd roundrect (at 2.3375 0) (size 1.525 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 2 "Net-(60ohm1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 110.744 110.744)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (fp_text reference SW1 (at 0 -2.06) (layer F.SilkS) hide)
    (fp_text value SW_SPDT (at 0 6.06) (layer F.Fab) hide)
    (pad 3 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(80ohm1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(60ohm1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Battery:BatteryHolder_LINX_BAT-HLD-012-SMT (layer F.Cu) (tedit 5B256044)
    (at 101.6 112.776 270)
    (descr "SMT battery holder for CR1216/1220/1225, https://linxtechnologies.com/wp/wp-content/uploads/bat-hld-012-smt.pdf")
    (tags "battery holder coin cell cr1216 cr1220 cr1225")
    (attr smd)
    (fp_text reference BT1 (at 0 6 90) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 -7 90) (layer F.Fab) hide)
    (fp_text user %R (at -2.54 0.508 90) (layer F.Fab))
    (pad 2 smd circle (at 0 0 270) (size 10.2 10.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (pad 1 smd rect (at 7.6 0 270) (size 2.5 5.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at -7.6 0 270) (size 2.5 5.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_LINX_BAT-HLD-012-SMT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 119.38 122.428) (end 119.38 102.108) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.98 122.428) (end 119.38 122.428) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.98 102.108) (end 93.98 122.428) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.38 102.108) (end 93.98 102.108) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.488 102.616) (xy 118.872 102.616) (xy 118.872 121.92) (xy 94.488 121.92)
      )
    )
  )
)
