<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="149.84" y2="0" width="0" layer="20"/>
<wire x1="149.84" y1="0" x2="149.84" y2="36.8175" width="0" layer="20"/>
<wire x1="149.84" y1="36.8175" x2="0" y2="36.8175" width="0" layer="20"/>
<wire x1="0" y1="36.8175" x2="0" y2="0" width="0" layer="20"/>
<hole x="147.32" y="2.54" drill="1.524"/>
<hole x="147.32" y="34.29" drill="1.524"/>
<hole x="2.54" y="34.29" drill="1.524"/>
<hole x="2.54" y="2.54" drill="1.524"/>
</plain>
<libraries>
<library name="TP4056">
<packages>
<package name="SOP-8">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="CR12&amp;20">
<packages>
<package name="CR1225">
</package>
<package name="CR1620">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector PTH&lt;/h3&gt;
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Barrel-Connector-PJ-202A.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC3" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="C5" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R9" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R10" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R11" library="adafruit" package="R0805" value="122">
<attribute name="NAME"/>
</element>
<element name="CHRG2" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="STDBY2" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R12" library="adafruit" package="R1206" value="0.4">
<attribute name="NAME"/>
</element>
<element name="U$3" library="CR12&amp;20" package="CR1225" value="CR1225"/>
<element name="U$4" library="CR12&amp;20" package="CR1620" value="CR1620"/>
<element name="IC4" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="C7" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C8" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R13" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R14" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R15" library="adafruit" package="R0805" value="122">
<attribute name="NAME"/>
</element>
<element name="CHRG3" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="STDBY3" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R16" library="adafruit" package="R1206" value="0.4">
<attribute name="NAME"/>
</element>
<element name="IC7" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="C13" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C14" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R25" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R26" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R27" library="adafruit" package="R0805" value="122">
<attribute name="NAME"/>
</element>
<element name="CHRG6" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="STDBY6" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R28" library="adafruit" package="R1206" value="0.4">
<attribute name="NAME"/>
</element>
<element name="U$7" library="CR12&amp;20" package="CR1225" value="CR1225"/>
<element name="U$8" library="CR12&amp;20" package="CR1620" value="CR1620"/>
<element name="IC8" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="C15" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C16" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R29" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R30" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R31" library="adafruit" package="R0805" value="122">
<attribute name="NAME"/>
</element>
<element name="CHRG7" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="STDBY7" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R32" library="adafruit" package="R1206" value="0.4">
<attribute name="NAME"/>
</element>
<element name="IC11" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="C21" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C22" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R41" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R42" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R43" library="adafruit" package="R0805" value="122">
<attribute name="NAME"/>
</element>
<element name="CHRG10" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="STDBY10" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R44" library="adafruit" package="R1206" value="0.4">
<attribute name="NAME"/>
</element>
<element name="U$11" library="CR12&amp;20" package="CR1225" value="CR1225"/>
<element name="U$12" library="CR12&amp;20" package="CR1620" value="CR1620"/>
<element name="IC12" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="C23" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C24" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R45" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R46" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R47" library="adafruit" package="R0805" value="122">
<attribute name="NAME"/>
</element>
<element name="CHRG11" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="STDBY11" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R48" library="adafruit" package="R1206" value="0.4">
<attribute name="NAME"/>
</element>
<element name="IC15" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="C29" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C30" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R57" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R58" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R59" library="adafruit" package="R0805" value="122">
<attribute name="NAME"/>
</element>
<element name="CHRG14" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="STDBY14" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R60" library="adafruit" package="R1206" value="0.4">
<attribute name="NAME"/>
</element>
<element name="U$15" library="CR12&amp;20" package="CR1225" value="CR1225"/>
<element name="U$16" library="CR12&amp;20" package="CR1620" value="CR1620"/>
<element name="IC16" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="C31" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C32" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R61" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R62" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R63" library="adafruit" package="R0805" value="122">
<attribute name="NAME"/>
</element>
<element name="CHRG15" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="STDBY15" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R64" library="adafruit" package="R1206" value="0.4">
<attribute name="NAME"/>
</element>
<element name="IC19" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="C37" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C38" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R73" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R74" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R75" library="adafruit" package="R0805" value="122">
<attribute name="NAME"/>
</element>
<element name="CHRG18" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="STDBY18" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R76" library="adafruit" package="R1206" value="0.4">
<attribute name="NAME"/>
</element>
<element name="U$19" library="CR12&amp;20" package="CR1225" value="CR1225"/>
<element name="U$20" library="CR12&amp;20" package="CR1620" value="CR1620"/>
<element name="IC20" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="C39" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C40" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R77" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R78" library="adafruit" package="R0805" value="102">
<attribute name="NAME"/>
</element>
<element name="R79" library="adafruit" package="R0805" value="122">
<attribute name="NAME"/>
</element>
<element name="CHRG19" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="STDBY19" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R80" library="adafruit" package="R1206" value="0.4">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACK">
<attribute name="PROD_ID" value="CONN-08197"/>
</element>
</elements>
<signals>
<signal name="N$6">
<contactref element="R9" pad="1"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="IC3" pad="6"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="CHRG2" pad="C"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R10" pad="2"/>
<contactref element="STDBY2" pad="C"/>
</signal>
<signal name="N$17">
<contactref element="IC3" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC3" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC4" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="IC4" pad="3"/>
<contactref element="U$3" pad="P$2"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="IC7" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="IC7" pad="3"/>
<contactref element="IC8" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="IC8" pad="3"/>
<contactref element="U$7" pad="P$2"/>
<contactref element="U$8" pad="P$2"/>
<contactref element="IC11" pad="1"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="R43" pad="1"/>
<contactref element="IC11" pad="3"/>
<contactref element="IC12" pad="1"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="R47" pad="1"/>
<contactref element="IC12" pad="3"/>
<contactref element="U$11" pad="P$2"/>
<contactref element="U$12" pad="P$2"/>
<contactref element="IC15" pad="1"/>
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="R59" pad="1"/>
<contactref element="IC15" pad="3"/>
<contactref element="IC16" pad="1"/>
<contactref element="C31" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="R63" pad="1"/>
<contactref element="IC16" pad="3"/>
<contactref element="U$15" pad="P$2"/>
<contactref element="U$16" pad="P$2"/>
<contactref element="IC19" pad="1"/>
<contactref element="C37" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="R75" pad="1"/>
<contactref element="IC19" pad="3"/>
<contactref element="IC20" pad="1"/>
<contactref element="C39" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="R79" pad="1"/>
<contactref element="IC20" pad="3"/>
<contactref element="U$19" pad="P$2"/>
<contactref element="U$20" pad="P$2"/>
<contactref element="J2" pad="GNDBREAK"/>
<contactref element="J2" pad="GND"/>
</signal>
<signal name="N$18">
<contactref element="IC3" pad="8"/>
<contactref element="STDBY2" pad="A"/>
<contactref element="CHRG2" pad="A"/>
<contactref element="C5" pad="1"/>
<contactref element="IC3" pad="4"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R13" pad="1"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="N$20">
<contactref element="IC4" pad="6"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="CHRG3" pad="C"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="R14" pad="2"/>
<contactref element="STDBY3" pad="C"/>
</signal>
<signal name="N$23">
<contactref element="IC4" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="IC4" pad="8"/>
<contactref element="STDBY3" pad="A"/>
<contactref element="CHRG3" pad="A"/>
<contactref element="C7" pad="1"/>
<contactref element="IC4" pad="4"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="R12" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R32" pad="2"/>
<contactref element="R44" pad="2"/>
<contactref element="R48" pad="2"/>
<contactref element="R60" pad="2"/>
<contactref element="R64" pad="2"/>
<contactref element="R76" pad="2"/>
<contactref element="R80" pad="2"/>
<contactref element="J2" pad="PWR"/>
</signal>
<signal name="N$37">
<contactref element="R25" pad="1"/>
<contactref element="IC7" pad="7"/>
</signal>
<signal name="N$38">
<contactref element="IC7" pad="6"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="CHRG6" pad="C"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="R26" pad="2"/>
<contactref element="STDBY6" pad="C"/>
</signal>
<signal name="N$41">
<contactref element="IC7" pad="2"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="IC7" pad="8"/>
<contactref element="STDBY6" pad="A"/>
<contactref element="CHRG6" pad="A"/>
<contactref element="C13" pad="1"/>
<contactref element="IC7" pad="4"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="R29" pad="1"/>
<contactref element="IC8" pad="7"/>
</signal>
<signal name="N$44">
<contactref element="IC8" pad="6"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="CHRG7" pad="C"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="R30" pad="2"/>
<contactref element="STDBY7" pad="C"/>
</signal>
<signal name="N$47">
<contactref element="IC8" pad="2"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="IC8" pad="8"/>
<contactref element="STDBY7" pad="A"/>
<contactref element="CHRG7" pad="A"/>
<contactref element="C15" pad="1"/>
<contactref element="IC8" pad="4"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="N$61">
<contactref element="R41" pad="1"/>
<contactref element="IC11" pad="7"/>
</signal>
<signal name="N$62">
<contactref element="IC11" pad="6"/>
<contactref element="R42" pad="1"/>
</signal>
<signal name="N$63">
<contactref element="CHRG10" pad="C"/>
<contactref element="R41" pad="2"/>
</signal>
<signal name="N$64">
<contactref element="R42" pad="2"/>
<contactref element="STDBY10" pad="C"/>
</signal>
<signal name="N$65">
<contactref element="IC11" pad="2"/>
<contactref element="R43" pad="2"/>
</signal>
<signal name="N$66">
<contactref element="IC11" pad="8"/>
<contactref element="STDBY10" pad="A"/>
<contactref element="CHRG10" pad="A"/>
<contactref element="C21" pad="1"/>
<contactref element="IC11" pad="4"/>
<contactref element="R44" pad="1"/>
</signal>
<signal name="N$67">
<contactref element="R45" pad="1"/>
<contactref element="IC12" pad="7"/>
</signal>
<signal name="N$68">
<contactref element="IC12" pad="6"/>
<contactref element="R46" pad="1"/>
</signal>
<signal name="N$69">
<contactref element="CHRG11" pad="C"/>
<contactref element="R45" pad="2"/>
</signal>
<signal name="N$70">
<contactref element="R46" pad="2"/>
<contactref element="STDBY11" pad="C"/>
</signal>
<signal name="N$71">
<contactref element="IC12" pad="2"/>
<contactref element="R47" pad="2"/>
</signal>
<signal name="N$72">
<contactref element="IC12" pad="8"/>
<contactref element="STDBY11" pad="A"/>
<contactref element="CHRG11" pad="A"/>
<contactref element="C23" pad="1"/>
<contactref element="IC12" pad="4"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="N$85">
<contactref element="R57" pad="1"/>
<contactref element="IC15" pad="7"/>
</signal>
<signal name="N$86">
<contactref element="IC15" pad="6"/>
<contactref element="R58" pad="1"/>
</signal>
<signal name="N$87">
<contactref element="CHRG14" pad="C"/>
<contactref element="R57" pad="2"/>
</signal>
<signal name="N$88">
<contactref element="R58" pad="2"/>
<contactref element="STDBY14" pad="C"/>
</signal>
<signal name="N$89">
<contactref element="IC15" pad="2"/>
<contactref element="R59" pad="2"/>
</signal>
<signal name="N$90">
<contactref element="IC15" pad="8"/>
<contactref element="STDBY14" pad="A"/>
<contactref element="CHRG14" pad="A"/>
<contactref element="C29" pad="1"/>
<contactref element="IC15" pad="4"/>
<contactref element="R60" pad="1"/>
</signal>
<signal name="N$91">
<contactref element="R61" pad="1"/>
<contactref element="IC16" pad="7"/>
</signal>
<signal name="N$92">
<contactref element="IC16" pad="6"/>
<contactref element="R62" pad="1"/>
</signal>
<signal name="N$93">
<contactref element="CHRG15" pad="C"/>
<contactref element="R61" pad="2"/>
</signal>
<signal name="N$94">
<contactref element="R62" pad="2"/>
<contactref element="STDBY15" pad="C"/>
</signal>
<signal name="N$95">
<contactref element="IC16" pad="2"/>
<contactref element="R63" pad="2"/>
</signal>
<signal name="N$96">
<contactref element="IC16" pad="8"/>
<contactref element="STDBY15" pad="A"/>
<contactref element="CHRG15" pad="A"/>
<contactref element="C31" pad="1"/>
<contactref element="IC16" pad="4"/>
<contactref element="R64" pad="1"/>
</signal>
<signal name="N$109">
<contactref element="R73" pad="1"/>
<contactref element="IC19" pad="7"/>
</signal>
<signal name="N$110">
<contactref element="IC19" pad="6"/>
<contactref element="R74" pad="1"/>
</signal>
<signal name="N$111">
<contactref element="CHRG18" pad="C"/>
<contactref element="R73" pad="2"/>
</signal>
<signal name="N$112">
<contactref element="R74" pad="2"/>
<contactref element="STDBY18" pad="C"/>
</signal>
<signal name="N$113">
<contactref element="IC19" pad="2"/>
<contactref element="R75" pad="2"/>
</signal>
<signal name="N$114">
<contactref element="IC19" pad="8"/>
<contactref element="STDBY18" pad="A"/>
<contactref element="CHRG18" pad="A"/>
<contactref element="C37" pad="1"/>
<contactref element="IC19" pad="4"/>
<contactref element="R76" pad="1"/>
</signal>
<signal name="N$115">
<contactref element="R77" pad="1"/>
<contactref element="IC20" pad="7"/>
</signal>
<signal name="N$116">
<contactref element="IC20" pad="6"/>
<contactref element="R78" pad="1"/>
</signal>
<signal name="N$117">
<contactref element="CHRG19" pad="C"/>
<contactref element="R77" pad="2"/>
</signal>
<signal name="N$118">
<contactref element="R78" pad="2"/>
<contactref element="STDBY19" pad="C"/>
</signal>
<signal name="N$119">
<contactref element="IC20" pad="2"/>
<contactref element="R79" pad="2"/>
</signal>
<signal name="N$120">
<contactref element="IC20" pad="8"/>
<contactref element="STDBY19" pad="A"/>
<contactref element="CHRG19" pad="A"/>
<contactref element="C39" pad="1"/>
<contactref element="IC20" pad="4"/>
<contactref element="R80" pad="1"/>
</signal>
<signal name="BAT1">
<contactref element="IC4" pad="5"/>
<contactref element="C8" pad="1"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="BAT2">
<contactref element="IC3" pad="5"/>
<contactref element="C6" pad="1"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="BAT3">
<contactref element="IC8" pad="5"/>
<contactref element="C16" pad="1"/>
<contactref element="U$7" pad="P$1"/>
</signal>
<signal name="BAT4">
<contactref element="IC7" pad="5"/>
<contactref element="C14" pad="1"/>
<contactref element="U$8" pad="P$1"/>
</signal>
<signal name="BAT5">
<contactref element="IC12" pad="5"/>
<contactref element="C24" pad="1"/>
<contactref element="U$11" pad="P$1"/>
</signal>
<signal name="BAT6">
<contactref element="IC11" pad="5"/>
<contactref element="C22" pad="1"/>
<contactref element="U$12" pad="P$1"/>
</signal>
<signal name="BAT7">
<contactref element="IC16" pad="5"/>
<contactref element="C32" pad="1"/>
<contactref element="U$15" pad="P$1"/>
</signal>
<signal name="BAT8">
<contactref element="IC15" pad="5"/>
<contactref element="C30" pad="1"/>
<contactref element="U$16" pad="P$1"/>
</signal>
<signal name="BAT9">
<contactref element="IC20" pad="5"/>
<contactref element="C40" pad="1"/>
<contactref element="U$19" pad="P$1"/>
</signal>
<signal name="BAT10">
<contactref element="IC19" pad="5"/>
<contactref element="C38" pad="1"/>
<contactref element="U$20" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
