(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 6)
    (no_connects 0)
    (area 136.576999 100.254999 146.887001 116.661001)
    (thickness 1.6)
    (drawings 11)
    (tracks 12)
    (zones 0)
    (modules 2)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5AAB618A)
    (at 138.43 102.108)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 17.272) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SH_BM06B-SRSS-TB_1x06_P1.00mm_Vertical (layer F.Cu) (tedit 5AAB6188)
    (at 144.145 108.585 270)
    (descr "JST SH series connector, BM06B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH side entry")
    (attr smd)
    (fp_text reference J2 (at -5.715 0 360) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 -6.35 270) (layer F.Fab))
    (fp_text user %R (at 0 -0.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2.5 1.325 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -1.5 1.325 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -0.5 1.325 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 0.5 1.325 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 1.5 1.325 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 2.5 1.325 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad "" smd rect (at -3.8 -1.2 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.8 -1.2 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_BM06B-SRSS-TB_1x06_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "JST SH" (at 144.018 115.697) (layer F.SilkS))
  (gr_line (start 146.812 100.33) (end 136.652 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.812 116.586) (end 146.812 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.652 116.586) (end 146.812 116.586) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.652 100.33) (end 136.652 116.586) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 6 (at 140.335 114.935) (layer F.SilkS))
  (gr_text 5 (at 140.335 112.395) (layer F.SilkS))
  (gr_text 4 (at 140.335 109.855) (layer F.SilkS))
  (gr_text 3 (at 140.335 107.315) (layer F.SilkS))
  (gr_text 2 (at 140.335 104.775) (layer F.SilkS))
  (gr_text 1 (at 140.335 102.235) (layer F.SilkS))
)
