<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.2">
<drawing>
<board>
<plain>
<hole x="3.175" y="3.175" drill="3.556"/>
<hole x="3.175" y="47.625" drill="3.556"/>
<hole x="34.925" y="47.625" drill="3.556"/>
<hole x="34.925" y="3.175" drill="3.556"/>
<wire x1="2.54" y1="50.7492" x2="35.56" y2="50.7492" width="0.0508" layer="20"/>
<wire x1="38.0492" y1="48.26" x2="38.0492" y2="2.54" width="0.0508" layer="20"/>
<wire x1="35.56" y1="0.0508" x2="2.54" y2="0.0508" width="0.0508" layer="20"/>
<wire x1="0.0508" y1="2.54" x2="0.0508" y2="48.26" width="0.0508" layer="20"/>
<wire x1="2.54" y1="0.0508" x2="0.0508" y2="2.54" width="0.0508" layer="20" curve="-90"/>
<wire x1="0.0508" y1="48.26" x2="2.54" y2="50.7492" width="0.0508" layer="20" curve="-90"/>
<wire x1="35.56" y1="50.7492" x2="38.0492" y2="48.26" width="0.0508" layer="20" curve="-90"/>
<wire x1="38.0492" y1="2.54" x2="35.56" y2="0.0508" width="0.0508" layer="20" curve="-90"/>
<text>RA0
RA1
RB0
RB1
RB2
RB3
RA2
RA3
RB4
RA4
GND</text>
<text>VDD</text>
<text>VDD</text>
<text>GND
RB15
RB14
RB13
RB12
RB11
RB10
RB9
RB8
RB7
RB6
RB5
GND</text>
<text>RST</text>
<text>VIN</text>
<text>RA0
RA1
RB0
RB1
RB2
RB3
RA2
RA3
RB4
RA4
GND
VDD</text>
<text>GND
RB15
RB14
RB13
RB12
RB11
RB10
RB9
RB8
RB7
RB6
RB5
GND
VDD</text>
<text>VIN</text>
<text>RST</text>
<text>dsPIC-28 DEV
JC 2017</text>
<text>PWR</text>
<text>RB4</text>
</plain>
<libraries>
<library name="library1">
<packages>
<package name="CAP-6.3MM">
</package>
<package name="1206">
</package>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="DIL28-3-ROUND">
<description>28-pin 0.300" DIP package</description>
</package>
<package name="SOT223-H">
</package>
<package name="PRQC">
</package>
<package name="SPST-6MM">
</package>
<package name="DO-15-V">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint with Long Pads&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X14">
<description>&lt;h3&gt;Plated Through Hole -14 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:14&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_14&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_2_NC_TRACE_NO-SILK">
</package>
</packages>
</library>
<library name="library1">
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="library1" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="library1" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="library1" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="library1" package="0805" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06_LOCK_LONGPADS" value="ICSP">
<attribute name="VALUE"/>
</element>
<element name="L1" library="library1" package="0805" value="FB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="library1" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="library1" package="DIL28-3-ROUND" value="MCU">
<attribute name="VALUE"/>
</element>
<element name="R5" library="library1" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="library1" package="0805" value="FB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="library1" package="SOT223-H" value="LDL1117S50R">
<attribute name="NAME"/>
</element>
<element name="C4" library="library1" package="CAP-6.3MM" value="47uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="library1" package="CAP-6.3MM" value="47uF">
<attribute name="NAME"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X14" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X14" value="">
<attribute name="VALUE"/>
</element>
<element name="Y1" library="library1" package="PRQC" value="PRQC-8MHZ"/>
<element name="SW1" library="library1" package="SPST-6MM" value="RESET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_TRACE_NO-SILK" value="JUMPER-SMT_2_NC_TRACE_NO-SILK">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_TRACE_NO-SILK" value="JUMPER-SMT_2_NC_TRACE_NO-SILK">
<attribute name="NAME"/>
</element>
<element name="LED1" library="library1" package="0805" value="PWR"/>
<element name="R2" library="library1" package="0805" value="150"/>
<element name="LED2" library="library1" package="0805" value="RB4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="library1" package="0805" value="150"/>
<element name="C7" library="library1" package="0805" value="1uF"/>
<element name="D1" library="library1" package="DO-15-V" value="DIODE">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="L2" pad="2"/>
<contactref element="U1" pad="19"/>
<contactref element="J2" pad="12"/>
<contactref element="Y1" pad="P$2"/>
<contactref element="SW1" pad="1" route="any" routetag="G$1.1"/>
<contactref element="SW1" pad="2" route="any" routetag="G$1.1"/>
<contactref element="J3" pad="13"/>
<contactref element="J3" pad="1"/>
<contactref element="LED1" pad="2"/>
<contactref element="LED2" pad="2"/>
<contactref element="C4" pad="-"/>
<contactref element="C6" pad="-"/>
<contactref element="U2" pad="1"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="!MCLR">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="SW1" pad="3" route="any" routetag="G$1.2"/>
<contactref element="SW1" pad="4" route="any" routetag="G$1.2"/>
</signal>
<signal name="PGED">
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="7"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="PGEC">
<contactref element="U1" pad="6"/>
<contactref element="J2" pad="6"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="VCAP">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="AVDD">
<contactref element="L1" pad="1"/>
<contactref element="U1" pad="28"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="OSC1">
<contactref element="U1" pad="9"/>
<contactref element="R5" pad="1"/>
<contactref element="Y1" pad="P$1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="OSC2">
<contactref element="U1" pad="10"/>
<contactref element="R5" pad="2"/>
<contactref element="Y1" pad="P$3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="AVSS">
<contactref element="C2" pad="2"/>
<contactref element="L2" pad="1"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="V+">
<contactref element="J2" pad="14"/>
<contactref element="D1" pad="P$2"/>
</signal>
<signal name="AN0">
<contactref element="U1" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="PWM1L">
<contactref element="U1" pad="26"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="PWM1H">
<contactref element="U1" pad="25"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="PWM2L">
<contactref element="U1" pad="24"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="PWM2H">
<contactref element="U1" pad="23"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="PWM3L">
<contactref element="U1" pad="22"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="PWM3H">
<contactref element="U1" pad="21"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="AN1">
<contactref element="U1" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="12"/>
<contactref element="J2" pad="11"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="18"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="17"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="16"/>
<contactref element="J3" pad="10"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="15"/>
<contactref element="J3" pad="11"/>
</signal>
<signal name="IC11">
<contactref element="U1" pad="11"/>
<contactref element="J2" pad="10"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="J1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="13"/>
<contactref element="C6" pad="+"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="J2" pad="13"/>
<contactref element="J3" pad="14"/>
<contactref element="R2" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="8"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="9"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="14"/>
<contactref element="J3" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="LED2" pad="1"/>
</signal>
<signal name="IC4">
<contactref element="U1" pad="4"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="IC5">
<contactref element="U1" pad="5"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="UNREG+">
<contactref element="C4" pad="+"/>
<contactref element="U2" pad="3" route="any" routetag="IC.VIN"/>
<contactref element="D1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
