(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 159)
    (tracks 1932)
    (zones 0)
    (modules 61)
    (nets 127)
  )
  (page A4 portrait)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.33)
    (user_trace_width 0.33)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.33)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.04876 4.04876)
    (pad_drill 3.05054)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 /~RESET)
  (net 4 "Net-(C16-Pad1)")
  (net 5 "Net-(C16-Pad2)")
  (net 6 "Net-(C17-Pad1)")
  (net 7 "Net-(C18-Pad1)")
  (net 8 "Net-(C18-Pad2)")
  (net 9 "Net-(C19-Pad1)")
  (net 10 "Net-(C20-Pad1)")
  (net 11 "Net-(C20-Pad2)")
  (net 12 "Net-(C21-Pad1)")
  (net 13 "Net-(C22-Pad1)")
  (net 14 "Net-(C22-Pad2)")
  (net 15 "Net-(C23-Pad1)")
  (net 16 /A15)
  (net 17 /A14)
  (net 18 /A13)
  (net 19 /A12)
  (net 20 /A11)
  (net 21 /A10)
  (net 22 /A9)
  (net 23 /A8)
  (net 24 /A7)
  (net 25 /A6)
  (net 26 /A5)
  (net 27 /A4)
  (net 28 /A3)
  (net 29 /A2)
  (net 30 /A1)
  (net 31 /A0)
  (net 32 /~M1)
  (net 33 /CPU_CLK)
  (net 34 /~MREQ)
  (net 35 /~WR)
  (net 36 /~RD)
  (net 37 /~IORQ)
  (net 38 /D0)
  (net 39 /D1)
  (net 40 /D2)
  (net 41 /D3)
  (net 42 /D4)
  (net 43 /D5)
  (net 44 /D6)
  (net 45 /D7)
  (net 46 /~RFSH)
  (net 47 "Net-(J2-Pad4)")
  (net 48 /~BUSACK)
  (net 49 /~HALT)
  (net 50 /~BUSREQ)
  (net 51 /~WAIT)
  (net 52 /~NMI)
  (net 53 "Net-(J3-Pad1)")
  (net 54 /RXA)
  (net 55 /TXA)
  (net 56 "Net-(J3-Pad4)")
  (net 57 "Net-(J3-Pad9)")
  (net 58 /CTSA)
  (net 59 /RTSA)
  (net 60 "Net-(J3-Pad6)")
  (net 61 /RXB)
  (net 62 /TXB)
  (net 63 /CTSB)
  (net 64 /RTSB)
  (net 65 /~INT)
  (net 66 /MA14)
  (net 67 /MA15)
  (net 68 /MA16)
  (net 69 /MA17)
  (net 70 /MA18)
  (net 71 /MA19)
  (net 72 /MA20)
  (net 73 /MA21)
  (net 74 "Net-(RV1-Pad2)")
  (net 75 "Net-(U2-Pad11)")
  (net 76 /~CTC_CS)
  (net 77 /CTC_CLK)
  (net 78 "Net-(U3-Pad10)")
  (net 79 "Net-(U3-Pad11)")
  (net 80 /RXDA)
  (net 81 /TXDA)
  (net 82 "Net-(U3-Pad16)")
  (net 83 /~RTSA)
  (net 84 /~CTSA)
  (net 85 "Net-(U3-Pad22)")
  (net 86 /~CTSB)
  (net 87 /~RTSB)
  (net 88 /TXDB)
  (net 89 /RXDB)
  (net 90 "Net-(U3-Pad29)")
  (net 91 "Net-(U3-Pad30)")
  (net 92 /~SIO_CS)
  (net 93 /~RAM_CS)
  (net 94 /VRAM)
  (net 95 /~ROM_CS)
  (net 96 "Net-(U6-Pad5)")
  (net 97 "Net-(U6-Pad6)")
  (net 98 "Net-(U6-Pad8)")
  (net 99 /WDOG)
  (net 100 /~RAM_CSI)
  (net 101 "Net-(U6-Pad14)")
  (net 102 "Net-(U6-Pad16)")
  (net 103 /~PGEN_WR)
  (net 104 /~PAGE_WR)
  (net 105 /~PAGE_EN)
  (net 106 /USR1)
  (net 107 "Net-(U6-Pad7)")
  (net 108 "Net-(U12-Pad5)")
  (net 109 "Net-(U12-Pad12)")
  (net 110 /VBAT)
  (net 111 /CH_B_CLKI)
  (net 112 /CH_A_CLK)
  (net 113 /CH_A_CLKI)
  (net 114 "Net-(U2-Pad20)")
  (net 115 "Net-(D1-Pad2)")
  (net 116 "Net-(J2-Pad1)")
  (net 117 "Net-(J2-Pad9)")
  (net 118 "Net-(J2-Pad6)")
  (net 119 "Net-(J6-Pad4)")
  (net 120 /USR5)
  (net 121 /USR6)
  (net 122 /USR7)
  (net 123 /IEI)
  (net 124 /IEO)
  (net 125 "Net-(R4-Pad1)")
  (net 126 "Net-(R5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.33)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CH_A_CLK)
    (add_net /CH_A_CLKI)
    (add_net /CH_B_CLKI)
    (add_net /CPU_CLK)
    (add_net /CTC_CLK)
    (add_net /CTSA)
    (add_net /CTSB)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /IEI)
    (add_net /IEO)
    (add_net /MA14)
    (add_net /MA15)
    (add_net /MA16)
    (add_net /MA17)
    (add_net /MA18)
    (add_net /MA19)
    (add_net /MA20)
    (add_net /MA21)
    (add_net /RTSA)
    (add_net /RTSB)
    (add_net /RXA)
    (add_net /RXB)
    (add_net /RXDA)
    (add_net /RXDB)
    (add_net /TXA)
    (add_net /TXB)
    (add_net /TXDA)
    (add_net /TXDB)
    (add_net /USR1)
    (add_net /USR5)
    (add_net /USR6)
    (add_net /USR7)
    (add_net /WDOG)
    (add_net /~BUSACK)
    (add_net /~BUSREQ)
    (add_net /~CTC_CS)
    (add_net /~CTSA)
    (add_net /~CTSB)
    (add_net /~HALT)
    (add_net /~INT)
    (add_net /~IORQ)
    (add_net /~M1)
    (add_net /~MREQ)
    (add_net /~NMI)
    (add_net /~PAGE_EN)
    (add_net /~PAGE_WR)
    (add_net /~PGEN_WR)
    (add_net /~RAM_CS)
    (add_net /~RAM_CSI)
    (add_net /~RD)
    (add_net /~RESET)
    (add_net /~RFSH)
    (add_net /~ROM_CS)
    (add_net /~RTSA)
    (add_net /~RTSB)
    (add_net /~SIO_CS)
    (add_net /~WAIT)
    (add_net /~WR)
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(U12-Pad12)")
    (add_net "Net-(U12-Pad5)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad22)")
    (add_net "Net-(U3-Pad29)")
    (add_net "Net-(U3-Pad30)")
    (add_net "Net-(U6-Pad14)")
    (add_net "Net-(U6-Pad16)")
    (add_net "Net-(U6-Pad5)")
    (add_net "Net-(U6-Pad6)")
    (add_net "Net-(U6-Pad7)")
    (add_net "Net-(U6-Pad8)")
  )
  (net_class GND ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.74)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /VBAT)
    (add_net /VRAM)
    (add_net VCC)
  )
  (module My_Components:Conn_Pin_Header_39x1_2.54mm (layer F.Cu) (tedit 5C6702D1)
    (at 127 175.26)
    (descr "Pin Header, 39x1, 2.54mm pitch")
    (tags "CONN 39x1")
    (fp_text reference J5 (at -48.26 -2.2225) (layer F.SilkS))
    (fp_text value RC2014_BUS (at -27.94 -2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -48.26 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A15))
    (pad 2 thru_hole circle (at -45.72 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A14))
    (pad 3 thru_hole circle (at -43.18 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A13))
    (pad 4 thru_hole circle (at -40.64 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A12))
    (pad 5 thru_hole circle (at -38.1 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A11))
    (pad 6 thru_hole circle (at -35.56 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A10))
    (pad 7 thru_hole circle (at -33.02 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A9))
    (pad 8 thru_hole circle (at -30.48 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 9 thru_hole circle (at -27.94 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A7))
    (pad 10 thru_hole circle (at -25.4 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A6))
    (pad 11 thru_hole circle (at -22.86 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A5))
    (pad 12 thru_hole circle (at -20.32 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A4))
    (pad 13 thru_hole circle (at -17.78 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /A3))
    (pad 14 thru_hole circle (at -15.24 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /A2))
    (pad 15 thru_hole circle (at -12.7 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /A1))
    (pad 16 thru_hole circle (at -10.16 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /A0))
    (pad 17 thru_hole circle (at -7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 18 thru_hole circle (at -5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 19 thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~M1))
    (pad 20 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~RESET))
    (pad 21 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /CPU_CLK))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 /~INT))
    (pad 23 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~MREQ))
    (pad 24 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~WR))
    (pad 25 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /~RD))
    (pad 26 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /~IORQ))
    (pad 27 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /D0))
    (pad 28 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D1))
    (pad 29 thru_hole circle (at 22.86 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /D2))
    (pad 30 thru_hole circle (at 25.4 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /D3))
    (pad 31 thru_hole circle (at 27.94 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /D4))
    (pad 32 thru_hole circle (at 30.48 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /D5))
    (pad 33 thru_hole circle (at 33.02 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D6))
    (pad 34 thru_hole circle (at 35.56 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D7))
    (pad 35 thru_hole circle (at 38.1 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 /TXDA))
    (pad 36 thru_hole circle (at 40.64 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 /RXDA))
    (pad 37 thru_hole circle (at 43.18 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 /USR1))
    (pad 38 thru_hole circle (at 45.72 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 123 /IEI))
    (pad 39 thru_hole circle (at 48.26 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 124 /IEO))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP40_600 (layer F.Cu) (tedit 5C4D6E37)
    (at 107.95 88.9)
    (descr "40 pins DIL package, round pads")
    (tags "DIP DIL DIP28 DIL28")
    (fp_text reference U3 (at -29.21 6.6675 270) (layer F.SilkS))
    (fp_text value Z84C40 (at -27.6225 6.6675 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -24.13 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D1))
    (pad 2 thru_hole circle (at -21.59 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /D3))
    (pad 3 thru_hole circle (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /D5))
    (pad 4 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D7))
    (pad 5 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 /~INT))
    (pad 6 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(U2-Pad11)"))
    (pad 7 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 124 /IEO))
    (pad 8 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~M1))
    (pad 9 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 10 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(U3-Pad10)"))
    (pad 11 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(U3-Pad11)"))
    (pad 12 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 /RXDA))
    (pad 13 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 /CH_A_CLK))
    (pad 14 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 /CH_A_CLK))
    (pad 15 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 /TXDA))
    (pad 16 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(U3-Pad16)"))
    (pad 17 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 /~RTSA))
    (pad 18 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 /~CTSA))
    (pad 19 thru_hole circle (at 21.59 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(U3-Pad16)"))
    (pad 20 thru_hole circle (at 24.13 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /CPU_CLK))
    (pad 21 thru_hole circle (at 24.13 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~RESET))
    (pad 22 thru_hole circle (at 21.59 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(U3-Pad22)"))
    (pad 23 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 /~CTSB))
    (pad 24 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 /~RTSB))
    (pad 25 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(U3-Pad22)"))
    (pad 26 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 /TXDB))
    (pad 27 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 /CH_A_CLK))
    (pad 28 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 /RXDB))
    (pad 29 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(U3-Pad29)"))
    (pad 30 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(U3-Pad30)"))
    (pad 31 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 32 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /~RD))
    (pad 33 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /A0))
    (pad 34 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /A1))
    (pad 35 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 92 /~SIO_CS))
    (pad 36 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /~IORQ))
    (pad 37 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D6))
    (pad 38 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /D4))
    (pad 39 thru_hole circle (at -21.59 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /D2))
    (pad 40 thru_hole circle (at -24.13 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /D0))
    (model dil/dil_40-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP40_600 (layer F.Cu) (tedit 5C4D6E09)
    (at 107.95 160.02)
    (descr "40 pins DIL package, round pads")
    (tags "DIP DIL DIP28 DIL28")
    (fp_text reference U1 (at -29.21 6.35 90) (layer F.SilkS))
    (fp_text value Z84C00 (at -27.6225 6.6675 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -24.13 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A11))
    (pad 2 thru_hole circle (at -21.59 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A12))
    (pad 3 thru_hole circle (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A13))
    (pad 4 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A14))
    (pad 5 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A15))
    (pad 6 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /CPU_CLK))
    (pad 7 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /D4))
    (pad 8 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /D3))
    (pad 9 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /D5))
    (pad 10 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D6))
    (pad 11 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 12 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /D2))
    (pad 13 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D7))
    (pad 14 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /D0))
    (pad 15 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D1))
    (pad 16 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 /~INT))
    (pad 17 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~NMI))
    (pad 18 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /~HALT))
    (pad 19 thru_hole circle (at 21.59 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~MREQ))
    (pad 20 thru_hole circle (at 24.13 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /~IORQ))
    (pad 21 thru_hole circle (at 24.13 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /~RD))
    (pad 22 thru_hole circle (at 21.59 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~WR))
    (pad 23 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /~BUSACK))
    (pad 24 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 /~WAIT))
    (pad 25 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /~BUSREQ))
    (pad 26 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~RESET))
    (pad 27 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~M1))
    (pad 28 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~RFSH))
    (pad 29 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 30 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /A0))
    (pad 31 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /A1))
    (pad 32 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /A2))
    (pad 33 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /A3))
    (pad 34 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A4))
    (pad 35 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A5))
    (pad 36 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A6))
    (pad 37 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A7))
    (pad 38 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 39 thru_hole circle (at -21.59 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A9))
    (pad 40 thru_hole circle (at -24.13 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A10))
    (model dil/dil_40-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6DF1)
    (at 80.01 160.02 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C1 (at 0 -1.905 90) (layer F.SilkS))
    (fp_text value 100n (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6DA5)
    (at 80.01 106.68 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C2 (at 0 1.905 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6DA0)
    (at 80.01 88.9 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C3 (at 0 -1.905 90) (layer F.SilkS))
    (fp_text value 100n (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6DE1)
    (at 80.01 142.24 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C4 (at 0 1.905 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 94 /VRAM))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6DC3)
    (at 80.01 124.46 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C5 (at 0 1.905 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6B2C)
    (at 156.21 158.75 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C6 (at 4.7625 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6AB6)
    (at 135.89 97.79 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C7 (at 4.445 0) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6AC9)
    (at 135.89 85.09 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C8 (at 4.445 0) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6A4D)
    (at 125.73 120.65 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C9 (at 4.445 0) (layer F.SilkS))
    (fp_text value 100n (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6A46)
    (at 125.73 146.05 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C10 (at 4.445 0) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6A49)
    (at 125.73 133.35 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C11 (at 4.445 0) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6A53)
    (at 138.43 110.49 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C12 (at 4.445 -0.635) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4F8495)
    (at 142.24 152.4)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C13 (at -5.715 0) (layer F.SilkS))
    (fp_text value 100n (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D43C8)
    (at 127 99.06)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C14 (at -5.3975 0) (layer F.SilkS))
    (fp_text value 100n (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C5B5473)
    (at 142.24 104.14 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C16 (at 6.35 -0.1905 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C16-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C16-Pad2)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6AB4)
    (at 138.43 97.79 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C17 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C5B5E1C)
    (at 149.86 104.14 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C18 (at 12.3825 -0.254 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C18-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C18-Pad2)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C5B5288)
    (at 157.48 104.14)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C19 (at 4.7625 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C19-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C5B3C9D)
    (at 142.24 91.44 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C20 (at 6.35 -0.635 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C20-Pad2)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C4D6ACC)
    (at 138.43 85.09 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C21 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C21-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C5B3C9E)
    (at 149.86 91.44 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C22 (at 12.3825 -0.635 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C22-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C22-Pad2)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 5C5B528A)
    (at 157.48 91.44)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C23 (at 4.7625 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0.3175 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C23-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Elec_Radial_6.3mm (layer F.Cu) (tedit 5D004485)
    (at 165.1 162.56)
    (descr "Electrolythic Capacitor, Radial, 6.3 mm diameter,  2.5 mm lead spacing")
    (tags "CAPACITOR CP")
    (fp_text reference C24 (at 0 4.1275) (layer F.SilkS))
    (fp_text value 47u (at 0 5.715) (layer F.SilkS))
    (fp_text user + (at -2.8575 -2.8575) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.25 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 1.25 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/c_vert_c2v10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Dsub_DE9M (layer F.Cu) (tedit 5C89716B)
    (at 167.3225 129.54 270)
    (descr "Connector, DE9, Male, Right Angle, Through Hole")
    (tags "CONN DSUB DE9M 9PIN")
    (fp_text reference J2 (at 16.51 -0.3175) (layer F.SilkS))
    (fp_text value SERIAL_A (at 16.51 -5.715) (layer F.SilkS))
    (pad GND thru_hole circle (at 12.49426 0 270) (size 4.04876 4.04876) (drill 3.05054) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad GND thru_hole circle (at -12.49426 0 270) (size 4.04876 4.04876) (drill 3.05054) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 5.4864 1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 2.7432 1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 54 /RXA))
    (pad 3 thru_hole circle (at 0 1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 55 /TXA))
    (pad 4 thru_hole circle (at -2.7432 1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at -5.4864 1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole circle (at -4.1148 -1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(J2-Pad9)"))
    (pad 8 thru_hole circle (at -1.3716 -1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 58 /CTSA))
    (pad 7 thru_hole circle (at 1.397 -1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RTSA))
    (pad 6 thru_hole circle (at 4.1148 -1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(J2-Pad6)"))
    (model conn_DBxx/db9_male_pin90deg.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Dsub_DE9M (layer F.Cu) (tedit 5C89715E)
    (at 167.3225 93.98 270)
    (descr "Connector, DE9, Male, Right Angle, Through Hole")
    (tags "CONN DSUB DE9M 9PIN")
    (fp_text reference J3 (at 16.51 0) (layer F.SilkS))
    (fp_text value SERIAL_B (at 16.51 -5.3975) (layer F.SilkS))
    (pad GND thru_hole circle (at 12.49426 0 270) (size 4.04876 4.04876) (drill 3.05054) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad GND thru_hole circle (at -12.49426 0 270) (size 4.04876 4.04876) (drill 3.05054) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 5.4864 1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(J3-Pad1)"))
    (pad 2 thru_hole circle (at 2.7432 1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 61 /RXB))
    (pad 3 thru_hole circle (at 0 1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 62 /TXB))
    (pad 4 thru_hole circle (at -2.7432 1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(J3-Pad4)"))
    (pad 5 thru_hole circle (at -5.4864 1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole circle (at -4.1148 -1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(J3-Pad9)"))
    (pad 8 thru_hole circle (at -1.3716 -1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 63 /CTSB))
    (pad 7 thru_hole circle (at 1.397 -1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 64 /RTSB))
    (pad 6 thru_hole circle (at 4.1148 -1.4224 270) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(J3-Pad6)"))
    (model conn_DBxx/db9_male_pin90deg.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Power_Jack_Circular_Pads (layer F.Cu) (tedit 5C5B0F49)
    (at 172.72 153.67 180)
    (descr "Connector, Power Jack")
    (tags "CONN POWER JACK")
    (fp_text reference J1 (at 3.81 -5.3975 180) (layer F.SilkS))
    (fp_text value POWER (at -1.27 -5.3975) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 0 180) (size 4 4) (drill 2.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 6.20014 0 180) (size 4.5 4.5) (drill 3.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3 thru_hole circle (at 2.99974 4.8006 180) (size 4 4) (drill 2.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model connectors/POWER_21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:OSC_Half_Can_DIP8 (layer F.Cu) (tedit 5C4D6AE4)
    (at 143.51 160.02)
    (descr "DIP8 package for half can OSC")
    (tags "OSC DIP")
    (fp_text reference QG1 (at -4.7625 7.62) (layer F.SilkS))
    (fp_text value 10MHz (at 4.1275 7.62) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /CPU_CLK))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:OSC_Half_Can_DIP8 (layer F.Cu) (tedit 5C5B548B)
    (at 128.27 106.68)
    (descr "DIP8 package for half can OSC")
    (tags "OSC DIP")
    (fp_text reference QG2 (at -6.0325 7.62) (layer F.SilkS))
    (fp_text value "1.8432 MHz" (at 0.3175 7.62) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 /CH_A_CLK))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Trimmer_Bourns_3362P (layer F.Cu) (tedit 5298DC3D)
    (at 156.21 130.81 90)
    (descr "Trimming Potentiometer - Bourns 3362P")
    (tags R)
    (autoplace_cost90 10)
    (autoplace_cost180 10)
    (fp_text reference RV1 (at -1.905 -4.445 90) (layer F.SilkS))
    (fp_text value 2k (at 1.905 -4.445 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(R5-Pad2)"))
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(RV1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(R4-Pad1)"))
    (model discret/adjustable_rx2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Switch_Tactile_6mm_Right (layer F.Cu) (tedit 5C5A05E3)
    (at 178.1175 166.37 270)
    (descr "Switch, Tactile, 6mm, Right Angle")
    (tags "SWITCH TACTILE 6MM RIGHT")
    (autoplace_cost180 10)
    (fp_text reference SW1 (at -5.715 8.5725) (layer F.SilkS))
    (fp_text value RESET (at -5.715 4.1275) (layer F.SilkS))
    (pad GND thru_hole circle (at 3.50266 6.35 90) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (pad GND thru_hole circle (at -3.49758 6.35 90) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.25298 3.85064 90) (size 1.80086 1.80086) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~RESET))
    (pad 2 thru_hole circle (at -2.2479 3.85064 90) (size 1.80086 1.80086) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model tactile_switches/bot_tact_cv1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.2 1.2 1.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP28_600 (layer F.Cu) (tedit 5C4D6E12)
    (at 100.33 106.68)
    (descr "28 pins DIL package, round pads, width 600mil")
    (tags "DIP DIL DIL28 DIL28")
    (fp_text reference U2 (at -22.225 6.35 90) (layer F.SilkS))
    (fp_text value Z84C30 (at -20.6375 6.985 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /D4))
    (pad 2 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /D5))
    (pad 3 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D6))
    (pad 4 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D7))
    (pad 5 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /~RD))
    (pad 7 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 113 /CH_A_CLKI))
    (pad 8 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 111 /CH_B_CLKI))
    (pad 9 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(U2-Pad20)"))
    (pad 10 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /~IORQ))
    (pad 11 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(U2-Pad11)"))
    (pad 12 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 /~INT))
    (pad 13 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 123 /IEI))
    (pad 14 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~M1))
    (pad 15 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /CPU_CLK))
    (pad 16 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 /~CTC_CS))
    (pad 17 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~RESET))
    (pad 18 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /A0))
    (pad 19 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /A1))
    (pad 20 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(U2-Pad20)"))
    (pad 21 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 /CTC_CLK))
    (pad 22 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 /CH_A_CLK))
    (pad 23 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 /CH_A_CLK))
    (pad 24 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 25 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /D0))
    (pad 26 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D1))
    (pad 27 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /D2))
    (pad 28 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /D3))
    (model dil/dil_28-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP32_600 (layer F.Cu) (tedit 5C4D6E0B)
    (at 102.87 142.24)
    (descr "32 pins DIL package, round pads")
    (tags "DIP DIL DIP32 DIL32")
    (fp_text reference U4 (at -24.13 6.35 270) (layer F.SilkS))
    (fp_text value AS6C4008 (at -22.5425 7.62 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 /MA18))
    (pad 2 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 /MA16))
    (pad 3 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 /MA14))
    (pad 4 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A12))
    (pad 5 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A7))
    (pad 6 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A6))
    (pad 7 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A5))
    (pad 8 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A4))
    (pad 9 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /A3))
    (pad 10 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /A2))
    (pad 11 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /A1))
    (pad 12 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /A0))
    (pad 13 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /D0))
    (pad 14 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D1))
    (pad 15 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /D2))
    (pad 16 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 17 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /D3))
    (pad 18 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /D4))
    (pad 19 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /D5))
    (pad 20 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D6))
    (pad 21 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D7))
    (pad 22 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 /~RAM_CS))
    (pad 23 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A10))
    (pad 24 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /~RD))
    (pad 25 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A11))
    (pad 26 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A9))
    (pad 27 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 28 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A13))
    (pad 29 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~WR))
    (pad 30 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 /MA17))
    (pad 31 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /MA15))
    (pad 32 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 94 /VRAM))
    (model dil/dil_32-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP32_600 (layer F.Cu) (tedit 5C4D6E0E)
    (at 102.87 124.46)
    (descr "32 pins DIL package, round pads")
    (tags "DIP DIL DIP32 DIL32")
    (fp_text reference U5 (at -24.13 6.35 90) (layer F.SilkS))
    (fp_text value SST39SF040 (at -22.5425 8.255 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 /MA18))
    (pad 2 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 /MA16))
    (pad 3 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /MA15))
    (pad 4 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A12))
    (pad 5 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A7))
    (pad 6 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A6))
    (pad 7 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A5))
    (pad 8 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A4))
    (pad 9 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /A3))
    (pad 10 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /A2))
    (pad 11 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /A1))
    (pad 12 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /A0))
    (pad 13 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /D0))
    (pad 14 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D1))
    (pad 15 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /D2))
    (pad 16 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 17 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /D3))
    (pad 18 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /D4))
    (pad 19 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /D5))
    (pad 20 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D6))
    (pad 21 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D7))
    (pad 22 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 95 /~ROM_CS))
    (pad 23 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A10))
    (pad 24 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /~RD))
    (pad 25 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A11))
    (pad 26 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A9))
    (pad 27 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 28 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A13))
    (pad 29 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 /MA14))
    (pad 30 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 /MA17))
    (pad 31 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~WR))
    (pad 32 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model dil/dil_32-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5C5A2F14)
    (at 156.21 146.05 90)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U6 (at 11.1125 5.08 90) (layer F.SilkS))
    (fp_text value MAX693 (at 15.5575 5.08 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 110 /VBAT))
    (pad 2 thru_hole circle (at -6.35 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 94 /VRAM))
    (pad 3 thru_hole circle (at -3.81 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 4 thru_hole circle (at -1.27 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 1.27 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(U6-Pad5)"))
    (pad 6 thru_hole circle (at 3.81 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(U6-Pad6)"))
    (pad 7 thru_hole circle (at 6.35 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(U6-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(U6-Pad8)"))
    (pad 9 thru_hole circle (at 8.89 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(RV1-Pad2)"))
    (pad 10 thru_hole circle (at 6.35 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~NMI))
    (pad 11 thru_hole circle (at 3.81 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 /WDOG))
    (pad 12 thru_hole circle (at 1.27 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 /~RAM_CS))
    (pad 13 thru_hole circle (at -1.27 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 /~RAM_CSI))
    (pad 14 thru_hole circle (at -3.81 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(U6-Pad14)"))
    (pad 15 thru_hole circle (at -6.35 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~RESET))
    (pad 16 thru_hole circle (at -8.89 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(U6-Pad16)"))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5C4D6E7A)
    (at 151.13 97.79)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U7 (at 11.7475 3.4925 90) (layer F.SilkS))
    (fp_text value MAX232A (at 11.7475 -1.27 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C16-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C17-Pad1)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C16-Pad1)"))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C18-Pad2)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C18-Pad1)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C19-Pad1)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 /TXA))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 /RXA))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 /RXDA))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 /TXDA))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 /~RTSA))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 /~CTSA))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 /CTSA))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RTSA))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5C4F9D69)
    (at 151.13 85.09)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U8 (at 11.7475 3.4925 90) (layer F.SilkS))
    (fp_text value MAX232A (at 11.7475 -0.9525 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C20-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C21-Pad1)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C20-Pad1)"))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C22-Pad2)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C22-Pad1)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C23-Pad1)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 62 /TXB))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 61 /RXB))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 /RXDB))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 /TXDB))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 /~RTSB))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 /~CTSB))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 /CTSB))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 /RTSB))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP20_300 (layer F.Cu) (tedit 5C4D6E8B)
    (at 140.97 120.65)
    (descr "20 pins DIL package, round pads")
    (tags "DIP DIL DIP20 DIL20")
    (fp_text reference U9 (at 14.605 3.81 90) (layer F.SilkS))
    (fp_text value ATF16V8B (at 14.605 -1.27 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~MREQ))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /~IORQ))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~WR))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~M1))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /A2))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /A3))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A4))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A5))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A6))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A7))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 /~RAM_CSI))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 /WDOG))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 /MA19))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 /~PGEN_WR))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 /~PAGE_WR))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 95 /~ROM_CS))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 92 /~SIO_CS))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 /~CTC_CS))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5C4D6EAC)
    (at 138.43 146.05)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U10 (at 11.7475 3.81 90) (layer F.SilkS))
    (fp_text value 74HC670 (at 11.7475 -1.5875 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D1))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /D2))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /D3))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A15))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A14))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 /MA17))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 /MA16))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /MA15))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 /MA14))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 /~PAGE_EN))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 /~PAGE_WR))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /A1))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /A0))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /D0))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5C4D6E99)
    (at 138.43 133.35)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U11 (at 11.7475 3.81 90) (layer F.SilkS))
    (fp_text value 74HC670 (at 11.7475 -1.5875 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /D5))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D6))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D7))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A15))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A14))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 73 /MA21))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 /MA20))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 /MA19))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 /MA18))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 /~PAGE_EN))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 /~PAGE_WR))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /A1))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /A0))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /D4))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP14_300 (layer F.Cu) (tedit 5C5BD2F7)
    (at 149.86 110.49)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U12 (at 11.1125 0 90) (layer F.SilkS))
    (fp_text value 74HC74 (at 12.7 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~RESET))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /D0))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 /~PGEN_WR))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(U12-Pad5)"))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 /~PAGE_EN))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(U12-Pad12)"))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 /CTC_CLK))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 /CH_A_CLK))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(U12-Pad12)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Friction_Lock_2P_2.54mm (layer F.Cu) (tedit 5C5B0F59)
    (at 154.94 165.1)
    (descr "Connector, Friction Lock, 2 Positions, 2.54mm Pitch")
    (tags "CONN FRICTION LOCK 2P")
    (fp_text reference J4 (at -1.905 -4.1275) (layer F.SilkS))
    (fp_text value VBAT (at 1.27 -4.1275) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 110 /VBAT))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5C5B549C)
    (at 157.48 120.65 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R4 (at -5.715 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(R4-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5C5B54B4)
    (at 160.02 120.65 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R5 (at -5.715 0 90) (layer F.SilkS))
    (fp_text value 29.4k (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(R5-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_SIL5 (layer F.Cu) (tedit 5C8936D2)
    (at 142.24 139.7)
    (descr "Footprint, SIL-5")
    (tags "CONN SIL-5")
    (fp_text reference RN2 (at -8.255 -0.635) (layer F.SilkS))
    (fp_text value 4.7k (at -8.255 0.9525) (layer F.SilkS))
    (pad 1 thru_hole rect (at -5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 /MA17))
    (pad 3 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 /MA16))
    (pad 4 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 /MA14))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /MA15))
  )
  (module My_Components:Conn_SIL5 (layer F.Cu) (tedit 5C8936D9)
    (at 142.24 127)
    (descr "Footprint, SIL-5")
    (tags "CONN SIL-5")
    (fp_text reference RN3 (at -8.255 -0.635) (layer F.SilkS))
    (fp_text value 4.7k (at -8.255 0.9525) (layer F.SilkS))
    (pad 1 thru_hole rect (at -5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 73 /MA21))
    (pad 3 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 /MA20))
    (pad 4 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 /MA18))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 /MA19))
  )
  (module Symbols:Symbol_GNU-Logo_SilkscreenTop (layer B.Cu) (tedit 5C6703C2)
    (at 96.52 87.63 180)
    (descr "GNU-Logo, GNU-Head, GNU-Kopf, Silkscreen,")
    (tags "GNU-Logo, GNU-Head, GNU-Kopf, Silkscreen,")
    (fp_text reference REF** (at 0 4.445 180) (layer B.SilkS) hide)
    (fp_text value Symbol_GNU-Logo_SilkscreenTop (at 0 -9.14908 180) (layer B.SilkS) hide)
  )
  (module Symbols:OSHW-Logo_11.4x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 124.46 88.5825 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_11.4x12mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 151.13 84.7725 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module My_Components:LED_3mm (layer F.Cu) (tedit 5C894A96)
    (at 160.02 165.1 180)
    (descr "LED 3mm, 100mil (2.54mm) lead spacing")
    (tags "LED 3mm T1")
    (fp_text reference D1 (at 0 2.8575) (layer F.SilkS))
    (fp_text value POWER (at 0 -2.8575) (layer F.SilkS))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5C5B54BF)
    (at 162.56 151.13 270)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R1 (at -0.3175 -1.905 270) (layer F.SilkS))
    (fp_text value 470 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(D1-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_SIL5 (layer F.Cu) (tedit 5C8952DB)
    (at 124.46 170.18)
    (descr "Footprint, SIL-5")
    (tags "CONN SIL-5")
    (fp_text reference RN1 (at -11.7475 0) (layer F.SilkS))
    (fp_text value 4.7k (at -8.255 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at -5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 /~INT))
    (pad 3 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~NMI))
    (pad 4 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /~BUSREQ))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 /~WAIT))
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5C5B54C9)
    (at 162.56 140.97 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 6.0325 0.3175 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~RESET))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5C5B5497)
    (at 135.89 110.49 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R3 (at -3.81 -1.905 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 123 /IEI))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Pin_Header_10x1_2.54mm (layer F.Cu) (tedit 5C670325)
    (at 130.81 172.72)
    (descr "Pin Header, 10x1, 2.54mm pitch")
    (tags "CONN 10x1")
    (fp_text reference J6 (at -13.97 0) (layer F.SilkS))
    (fp_text value RC2014_EXT (at -8.255 5.715) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -8.89 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3 thru_hole circle (at -6.35 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~RFSH))
    (pad 4 thru_hole circle (at -3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(J6-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 112 /CH_A_CLK))
    (pad 6 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /~BUSACK))
    (pad 7 thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /~HALT))
    (pad 8 thru_hole circle (at 6.35 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /~BUSREQ))
    (pad 9 thru_hole circle (at 8.89 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /~WAIT))
    (pad 10 thru_hole circle (at 11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~NMI))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Pin_Header_5x1_2.54mm (layer F.Cu) (tedit 5C670345)
    (at 170.18 172.72)
    (descr "Pin Header, 5x1, 2.54mm pitch")
    (tags "CONN 5x1")
    (fp_text reference J7 (at -7.62 0) (layer F.SilkS))
    (fp_text value RC2014_SPARE (at -0.9525 5.715) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 88 /TXDB))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 89 /RXDB))
    (pad 3 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 120 /USR5))
    (pad 4 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 121 /USR6))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 122 /USR7))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Pin_Header_3x1_2.54mm (layer B.Cu) (tedit 5C67037A)
    (at 111.76 102.87 180)
    (descr "Pin Header, 3x1, 2.54mm pitch")
    (tags "CONN 3x1")
    (fp_text reference JP1 (at -3.81 2.2225 180) (layer B.SilkS))
    (fp_text value CH_A_CLK (at 1.905 2.2225 180) (layer B.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 112 /CH_A_CLK))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 112 /CH_A_CLK))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 113 /CH_A_CLKI))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Pin_Header_3x1_2.54mm (layer B.Cu) (tedit 5C67039C)
    (at 111.76 92.71 180)
    (descr "Pin Header, 3x1, 2.54mm pitch")
    (tags "CONN 3x1")
    (fp_text reference JP2 (at -3.81 2.2225 180) (layer B.SilkS))
    (fp_text value CH_B_CLK (at 1.905 2.2225 180) (layer B.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 112 /CH_A_CLK))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 112 /CH_A_CLK))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 111 /CH_B_CLKI))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_SIL9 (layer F.Cu) (tedit 5C8952D1)
    (at 152.4 170.18)
    (descr "Footprint, SIL-9")
    (tags "CONN SIL-9")
    (fp_text reference RN4 (at -16.8275 0) (layer F.SilkS))
    (fp_text value 4.7k (at -13.335 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at -10.16 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -7.62 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /D0))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D1))
    (pad 4 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /D2))
    (pad 5 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /D3))
    (pad 6 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /D4))
    (pad 7 thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /D5))
    (pad 8 thru_hole circle (at 7.62 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D6))
    (pad 9 thru_hole circle (at 10.16 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D7))
  )
  (gr_text "Design files and documentation:\ngithub.com/skiselev/easy_z80" (at 103.1875 121.92) (layer B.SilkS))
  (gr_text IEO (at 175.5775 171.7675 90) (layer B.SilkS))
  (gr_text IEI (at 173.99 171.45 90) (layer B.SilkS))
  (gr_text "NVRAM Battery" (at 154.94 168.275) (layer B.SilkS))
  (gr_text - (at 156.21 166.6875) (layer B.SilkS))
  (gr_text + (at 153.67 166.6875) (layer B.SilkS))
  (gr_text RTSB (at 169.8625 95.5675) (layer B.SilkS))
  (gr_text CTSB (at 169.8625 92.71) (layer B.SilkS))
  (gr_text RXB (at 164.7825 96.8375) (layer B.SilkS))
  (gr_text TXB (at 164.7825 93.98) (layer B.SilkS))
  (gr_text GND (at 164.7825 88.5825) (layer B.SilkS))
  (gr_text RTSA (at 169.8625 131.1275) (layer B.SilkS))
  (gr_text CTSA (at 169.8625 128.27) (layer B.SilkS))
  (gr_text GND (at 164.7825 124.1425) (layer B.SilkS))
  (gr_text RXA (at 164.7825 132.3975) (layer B.SilkS))
  (gr_text TXA (at 164.7825 129.54) (layer B.SilkS))
  (gr_text UART_CLK (at 129.2225 161.925 90) (layer B.SilkS))
  (gr_text RX2 (at 167.9575 171.45 90) (layer B.SilkS))
  (gr_text RX1 (at 166.0525 168.91 90) (layer B.SilkS))
  (gr_text TX2 (at 165.4175 171.45 90) (layer B.SilkS))
  (gr_text TX1 (at 163.5125 168.91 90) (layer B.SilkS))
  (gr_text "JP1/JP2: SIO channel A/B clock select:\n  1-2 - 1.8432 MHz (default, trace connection)\n  2-3 - Programmable using CTC channel 0/1" (at 132.08 109.22) (layer B.SilkS))
  (gr_text "Easy Z80 - Version 1.1 - Copyright (C) 2019 Max Malinov & Sergey Kiselev" (at 121.92 78.74) (layer F.SilkS))
  (gr_text "Easy Z80 - Version 1.1 - Copyright (C) 2019 Max Malinov & Sergey Kiselev" (at 121.92 78.74) (layer B.SilkS))
  (gr_text ~NMI (at 140.97 167.64 90) (layer B.SilkS))
  (gr_text ~IORQ (at 140.335 171.45 90) (layer B.SilkS))
  (gr_text ~WAIT (at 138.43 167.64 90) (layer B.SilkS))
  (gr_text ~RD (at 137.795 171.45 90) (layer B.SilkS))
  (gr_text ~BUSREQ (at 135.89 167.64 90) (layer B.SilkS))
  (gr_text ~WR (at 135.255 171.45 90) (layer B.SilkS))
  (gr_text ~HALT (at 133.35 161.925 90) (layer B.SilkS))
  (gr_text ~MREQ (at 132.715 166.37 90) (layer B.SilkS))
  (gr_text ~BUSACK (at 130.81 161.925 90) (layer B.SilkS))
  (gr_text ~INT (at 130.175 166.37 90) (layer B.SilkS))
  (gr_text CPU_CLK (at 127.635 166.37 90) (layer B.SilkS))
  (gr_text ~RESET (at 125.095 166.37 90) (layer B.SilkS))
  (gr_text ~RFSH (at 123.19 161.925 90) (layer B.SilkS))
  (gr_text ~M1 (at 122.555 166.37 90) (layer B.SilkS))
  (gr_text VCC (at 120.65 166.37 90) (layer B.SilkS))
  (gr_text GND (at 118.11 166.37 90) (layer B.SilkS))
  (gr_text D7 (at 162.56 173.99 90) (layer B.SilkS))
  (gr_text D6 (at 160.02 173.99 90) (layer B.SilkS))
  (gr_text D5 (at 157.48 173.99 90) (layer B.SilkS))
  (gr_text D4 (at 154.94 173.99 90) (layer B.SilkS))
  (gr_text D3 (at 152.4 173.99 90) (layer B.SilkS))
  (gr_text D2 (at 149.86 173.99 90) (layer B.SilkS))
  (gr_text D1 (at 147.32 173.99 90) (layer B.SilkS))
  (gr_text D0 (at 144.78 173.99 90) (layer B.SilkS))
  (gr_text A0 (at 116.84 173.99 90) (layer B.SilkS))
  (gr_text A1 (at 114.3 173.99 90) (layer B.SilkS))
  (gr_text A2 (at 111.76 173.99 90) (layer B.SilkS))
  (gr_text A3 (at 109.22 173.99 90) (layer B.SilkS))
  (gr_text A4 (at 106.68 173.99 90) (layer B.SilkS))
  (gr_text A5 (at 104.14 173.99 90) (layer B.SilkS))
  (gr_text A6 (at 101.6 173.99 90) (layer B.SilkS))
  (gr_text A7 (at 99.06 173.99 90) (layer B.SilkS))
  (gr_text A8 (at 96.52 173.99 90) (layer B.SilkS))
  (gr_text A9 (at 93.98 173.99 90) (layer B.SilkS))
  (gr_text A10 (at 91.44 173.99 90) (layer B.SilkS))
  (gr_text A11 (at 88.9 173.99 90) (layer B.SilkS))
  (gr_text A12 (at 86.36 173.99 90) (layer B.SilkS))
  (gr_text A13 (at 83.82 173.99 90) (layer B.SilkS))
  (gr_text A14 (at 81.28 173.99 90) (layer B.SilkS))
  (gr_text A15 (at 78.74 173.99 90) (layer B.SilkS))
  (gr_line (start 176.9745 175.9585) (end 176.9745 78.0415) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.0415 176.9745) (end 175.9585 176.9745) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.0255 78.0415) (end 77.0255 175.9585) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.9585 77.0255) (end 78.0415 77.0255) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "NVRAM Bat." (at 151.13 164.1475 90) (layer F.SilkS))
  (gr_text - (at 156.21 168.275) (layer F.SilkS))
  (gr_text + (at 153.67 168.275) (layer F.SilkS))
  (gr_arc (start 175.9585 78.0415) (end 175.9585 77.0255) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 78.0415 78.0415) (end 77.0255 78.0415) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 175.9585 175.9585) (end 176.9745 175.9585) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 78.0415 175.9585) (end 78.0415 176.9745) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.33))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.9745 176.9745) (xy 77.0255 176.9745) (xy 77.0255 77.0255) (xy 176.9745 77.0255)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.33))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.9745 176.9745) (xy 77.0255 176.9745) (xy 77.0255 77.0255) (xy 176.9745 77.0255)
      )
    )
  )
)
