(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (grid_origin 123 108)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/SIG")
  (net 2 "/GND")
  (footprint "Library:COAX4_CONSMA002-L-G_LNX" (layer "F.Cu")
    (at 127.885 108.0508 -90)
    (tags "CONSMA002-L-G ")
    (attr through_hole)
    (fp_text reference "J2" (at 0 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "COAX4_CONSMA002-L-G_LNX" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 1 "/SIG"))
    (pad "2" thru_hole circle (at -2.55 -2.55 270) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask")
      (net 2 "/GND"))
    (pad "3" thru_hole circle (at -2.55 2.55 270) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask")
      (net 2 "/GND"))
    (pad "4" thru_hole circle (at 2.55 2.55 270) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask")
      (net 2 "/GND"))
    (pad "5" thru_hole circle (at 2.55 -2.55 270) (size 2.0066 2.0066) (drill 1.4986) (layers "*.Cu" "*.Mask")
      (net 2 "/GND"))
  )
  (footprint "Library:CONN_XF3M1-0515-1B_OMR" (layer "F.Cu")
    (at 121.275 110.0454 -90)
    (tags "XF3M1-0515-1B ")
    (property "Sheetfile" "1E 5Pin SMA.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "XF3M(1)-0515-1B")
    (attr smd)
    (fp_text reference "J1" (at -2 3.5 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "XF3M1-0515-1B" (at -2 1.599989 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at -4.000001 0 270) (size 0.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at -3.000001 0 270) (size 0.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/SIG") (pinfunction "2") (pintype "unspecified"))
    (pad "3" smd rect (at -2 0 270) (size 0.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/SIG") (pinfunction "3") (pintype "unspecified"))
    (pad "4" smd rect (at -0.999999 0 270) (size 0.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/SIG") (pinfunction "4") (pintype "unspecified"))
    (pad "5" smd rect (at 0.000001 0 270) (size 0.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "5") (pintype "unspecified"))
    (pad "6" smd rect (at -6.4 3.250001 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND"))
    (pad "7" smd rect (at 2.4 3.250001 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND"))
  )
  (gr_poly
    (pts
      (xy 115.75 102)
      (xy 132.5 102)
      (xy 132.5 114)
      (xy 115.75 114)
    )
    (fill none) (layer "Edge.Cuts"))
  (gr_text "XF3M(1)\n0515-1B" (at 118.1 107.8 -90) (layer "F.SilkS"))
  (zone (net 2) (net_name "/GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 115.75 102)
        (xy 132.5 102)
        (xy 132.5 114)
        (xy 115.75 114)
      )
    )
  )
  (zone (net 2) (net_name "/GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 132.5 102)
        (xy 115.75 102)
        (xy 115.75 114)
        (xy 132.5 114)
      )
    )
  )
)
