<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="12.68" y2="0" width="0" layer="20"/>
<wire x1="12.68" y1="0" x2="12.68" y2="25.705" width="0" layer="20"/>
<wire x1="12.68" y1="25.705" x2="0" y2="25.705" width="0" layer="20"/>
<wire x1="0" y1="25.705" x2="0" y2="0" width="0" layer="20"/>
<text>50mil header part number:
20021121-00010C4LF</text>
</plain>
<libraries>
<library name="talkbacksies">
<description>talkbacksies</description>
<packages>
<package name="DEBUG-HEADER-20021121-00010C4LF">
</package>
<package name="SINGLE-100MIL-HOLE">
</package>
<package name="JLINK-SEGGER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="DBGR" library="talkbacksies" package="DEBUG-HEADER-20021121-00010C4LF" value="DEBUG-HEADER-20021121-00010C4LF"/>
<element name="RX" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="TX" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="U$2" library="talkbacksies" package="JLINK-SEGGER" value="JLINK-SEGGER"/>
</elements>
<signals>
<signal name="N$32">
<contactref element="DBGR" pad="4"/>
<contactref element="U$2" pad="P$9"/>
</signal>
<signal name="N$34">
<contactref element="DBGR" pad="2"/>
<contactref element="U$2" pad="P$7"/>
</signal>
<signal name="N$35">
<contactref element="DBGR" pad="1"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="N$36">
<contactref element="DBGR" pad="10"/>
<contactref element="U$2" pad="P$15"/>
</signal>
<signal name="N$37">
<contactref element="DBGR" pad="6"/>
<contactref element="U$2" pad="P$13"/>
</signal>
<signal name="N$38">
<contactref element="DBGR" pad="7"/>
<contactref element="TX" pad="P$1"/>
</signal>
<signal name="N$39">
<contactref element="DBGR" pad="9"/>
<contactref element="RX" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="P$19"/>
<contactref element="DBGR" pad="8"/>
</signal>
<signal name="GND">
<contactref element="DBGR" pad="3"/>
<contactref element="DBGR" pad="5"/>
<contactref element="U$2" pad="P$4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
