(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.2)
    (grid_origin 123.444 73.025)
    (pcbplotparams
      (layerselection 0x0000030_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(U1-Pad12)")
  (net 2 "Net-(JP1-Pad1)")
  (net 3 "unconnected-(U1-Pad7)")
  (net 4 "unconnected-(U1-Pad6)")
  (net 5 "unconnected-(U1-Pad5)")
  (net 6 "unconnected-(U1-Pad15)")
  (net 7 "unconnected-(U1-Pad16)")
  (net 8 "unconnected-(U1-Pad17)")
  (net 9 "unconnected-(U1-Pad18)")
  (net 10 "unconnected-(U1-Pad19)")
  (net 11 "unconnected-(U1-Pad20)")
  (net 12 "+5V")
  (net 13 "/LED")
  (net 14 "GND")
  (net 15 "/MOSI")
  (net 16 "/MISO")
  (net 17 "/SCK")
  (net 18 "/DC")
  (net 19 "/RESET")
  (net 20 "/TFTCS")
  (net 21 "/TOUCHCS")
  (net 22 "/IRQ")
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.8 82.9 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "touchscreen_tester.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -2.8 -2.1) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 13 "/LED") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 12 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm" (layer "F.Cu")
    (tedit 5C756AB2)
    (at 136.144 98.425 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "touchscreen_tester.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text value "Jumper_2_Bridged" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "Net-(JP1-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0.65 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 22 "/IRQ") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.8 84.9)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "touchscreen_tester.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.8 -2) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 12 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 13 "/LED") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "dstahlke:Seeeduino XIAO-MOUDLE14P-2.54-21X17.8MM" (layer "F.Cu")
    (tedit 64278E3C)
    (at 138.38169 81.38559 -90)
    (property "Sheetfile" "touchscreen_tester.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 9.3345 -21.7805 90) (layer "F.SilkS"))
    (fp_text value "SeeeduinoXIAO" (at 8.89 -10.795 90) (layer "F.SilkS"))
    (pad "1" smd oval (at 0.83312 -18.11782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/TOUCHCS") (pinfunction "PA02_A0_D0") (pintype "unspecified"))
    (pad "2" smd oval (at 0.83312 -15.57782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/DC") (pinfunction "PA4_A1_D1") (pintype "unspecified"))
    (pad "3" smd oval (at 0.83312 -13.03782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/RESET") (pinfunction "PA10_A2_D2") (pintype "unspecified"))
    (pad "4" smd oval (at 0.83312 -10.49782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/TFTCS") (pinfunction "PA11_A3_D3") (pintype "unspecified"))
    (pad "5" smd oval (at 0.83312 -7.95782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "unconnected-(U1-Pad5)") (pinfunction "PA8_A4_D4_SDA") (pintype "unspecified+no_connect"))
    (pad "6" smd oval (at 0.83312 -5.41782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "unconnected-(U1-Pad6)") (pinfunction "PA9_A5_D5_SCL") (pintype "unspecified+no_connect"))
    (pad "7" smd oval (at 0.83312 -2.87782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "unconnected-(U1-Pad7)") (pinfunction "PB08_A6_D6_TX") (pintype "unspecified+no_connect"))
    (pad "8" smd oval (at 16.99768 -2.87782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(JP1-Pad1)") (pinfunction "PB09_A7_D7_RX") (pintype "unspecified"))
    (pad "9" smd oval (at 16.99768 -5.41782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/SCK") (pinfunction "PA7_A8_D8_SCK") (pintype "unspecified"))
    (pad "10" smd oval (at 16.99768 -7.95782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/MISO") (pinfunction "PA5_A9_D9_MISO") (pintype "unspecified"))
    (pad "11" smd oval (at 16.99768 -10.49782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/MOSI") (pinfunction "PA6_A10_D10_MOSI") (pintype "unspecified"))
    (pad "12" smd oval (at 16.99768 -13.03782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "unconnected-(U1-Pad12)") (pinfunction "3V3") (pintype "unspecified+no_connect"))
    (pad "13" smd oval (at 16.99768 -15.57782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "14" smd oval (at 16.99768 -18.11782 270) (size 2.74828 1.99898) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+5V") (pinfunction "5V") (pintype "unspecified"))
    (pad "15" smd oval (at 7.7 -1.8) (size 2.032 1.016) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "unconnected-(U1-Pad15)") (pinfunction "5V") (pintype "input+no_connect"))
    (pad "16" smd oval (at 10.25 -1.8) (size 2.032 1.016) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "unconnected-(U1-Pad16)") (pinfunction "GND") (pintype "input+no_connect"))
    (pad "17" smd circle (at 7.698803 -18.804187) (size 1.143 1.143) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "unconnected-(U1-Pad17)") (pinfunction "PA31_SWDIO") (pintype "input+no_connect"))
    (pad "18" smd circle (at 10.238803 -18.804187) (size 1.143 1.143) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "unconnected-(U1-Pad18)") (pinfunction "PA30_SWCLK") (pintype "input+no_connect"))
    (pad "19" smd circle (at 7.698803 -16.264187) (size 1.143 1.143) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "unconnected-(U1-Pad19)") (pinfunction "RESET") (pintype "input+no_connect"))
    (pad "20" smd circle (at 10.238803 -16.264187) (size 1.143 1.143) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "unconnected-(U1-Pad20)") (pinfunction "GND") (pintype "input+no_connect"))
  )
  (footprint "dstahlke:TJCTM24024-SPI-NODRILL" (layer "F.Cu")
    (tedit 642795A4)
    (at 118.6 75)
    (property "Sheetfile" "touchscreen_tester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0 0) (layer "Cmts.User") hide)
    (fp_text value "TJCTM24024-SPI" (at 0 0) (layer "Eco1.User") hide)
    (pad "P1" thru_hole oval (at 4.84886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "P2" thru_hole oval (at 7.38886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "P3" thru_hole oval (at 9.92886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "/TFTCS") (pinfunction "CS") (pintype "input"))
    (pad "P4" thru_hole oval (at 12.46886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "/RESET") (pinfunction "RESET") (pintype "input"))
    (pad "P5" thru_hole oval (at 15.00886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "/DC") (pinfunction "DC") (pintype "input"))
    (pad "P6" thru_hole oval (at 17.54886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "/MOSI") (pinfunction "SDI") (pintype "input"))
    (pad "P7" thru_hole oval (at 20.08886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "/SCK") (pinfunction "SCK") (pintype "input"))
    (pad "P8" thru_hole oval (at 22.62886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "/LED") (pinfunction "LED") (pintype "input"))
    (pad "P9" thru_hole oval (at 25.16886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "/MISO") (pinfunction "SDO") (pintype "tri_state"))
    (pad "P10" thru_hole oval (at 27.70886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "/SCK") (pinfunction "T_CLK") (pintype "input"))
    (pad "P11" thru_hole oval (at 30.24886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "/TOUCHCS") (pinfunction "T_CS") (pintype "input"))
    (pad "P12" thru_hole oval (at 32.78886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "/MOSI") (pinfunction "T_DIN") (pintype "input"))
    (pad "P13" thru_hole oval (at 35.32886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "/MISO") (pinfunction "T_DO") (pintype "tri_state"))
    (pad "P14" thru_hole oval (at 37.86886 -1.99898) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "/IRQ") (pinfunction "T_IRQ") (pintype "output"))
  )
  (gr_line (start 120.65 71.12) (end 120.65 104.775) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 158.75 96.901) (end 158.75 104.775) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 120.65 104.775) (end 122.555 104.775) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 158.75 71.12) (end 158.75 83.82) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 138.303 96.901) (end 138.303 83.82) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 158.75 83.82) (end 138.303 83.82) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 138.303 96.901) (end 158.75 96.901) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 158.75 104.775) (end 122.555 104.775) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 120.65 71.12) (end 158.75 71.12) (layer "Edge.Cuts") (width 0.15))
  (gr_text "MISO" (at 143.764 76.2 90) (layer "F.SilkS"))
  (gr_text "MOSI" (at 151.384 76.2 90) (layer "F.SilkS"))
  (gr_text "SCK" (at 138.684 76.2 90) (layer "F.SilkS"))
  (gr_text "GND" (at 125.984 76.2 90) (layer "F.SilkS"))
  (gr_text "+5" (at 123.444 76.2 90) (layer "F.SilkS"))
  (gr_text "SCK" (at 146.304 76.2 90) (layer "F.SilkS"))
  (gr_text "MISO" (at 153.924 76.2 90) (layer "F.SilkS"))
  (gr_text "TFTCS" (at 128.524 76.835 90) (layer "F.SilkS"))
  (gr_text "DC" (at 133.604 75.565 90) (layer "F.SilkS"))
  (gr_text "TOUCHCS" (at 148.844 77.47 90) (layer "F.SilkS"))
  (gr_text "MOSI" (at 136.144 76.2 90) (layer "F.SilkS"))
  (gr_text "LED" (at 141.224 76.2 90) (layer "F.SilkS"))
  (gr_text "RESET" (at 131.064 76.835 90) (layer "F.SilkS"))
  (zone (net 14) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.496 83.693)
        (xy 138.176 83.693)
        (xy 138.176 97.155)
        (xy 158.496 97.155)
        (xy 158.496 104.521)
        (xy 120.904 104.521)
        (xy 120.904 71.247)
        (xy 158.496 71.247)
      )
    )
  )
)
