(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu14.04.1-stable)
  (general
    (links 72)
    (no_connects 0)
    (area 129.54 53.34 191.77 119.38)
    (thickness 1.6)
    (drawings 4)
    (tracks 339)
    (zones 0)
    (modules 26)
    (nets 63)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(U2-Pad30)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(D3-Pad1)")
  (net 6 "Net-(U2-Pad34)")
  (net 7 6)
  (net 8 "Net-(LED_TEST1-Pad2)")
  (net 9 7)
  (net 10 "Net-(LED_TEST1-Pad4)")
  (net 11 8)
  (net 12 "Net-(LED_TEST1-Pad6)")
  (net 13 "Net-(R1-Pad1)")
  (net 14 20)
  (net 15 "Net-(R3-Pad1)")
  (net 16 15)
  (net 17 "Net-(R4-Pad1)")
  (net 18 16)
  (net 19 "Net-(SPKR_TEST1-Pad2)")
  (net 20 "Net-(SPKR_TEST1-Pad4)")
  (net 21 27)
  (net 22 "Net-(TEST1-Pad2)")
  (net 23 0)
  (net 24 "Net-(TEST1-Pad4)")
  (net 25 1)
  (net 26 "Net-(TEST1-Pad6)")
  (net 27 2)
  (net 28 "Net-(TEST1-Pad8)")
  (net 29 3)
  (net 30 "Net-(TEST1-Pad10)")
  (net 31 4)
  (net 32 "Net-(TEST1-Pad12)")
  (net 33 5)
  (net 34 "Net-(TEST1-Pad14)")
  (net 35 11)
  (net 36 "Net-(TEST2-Pad2)")
  (net 37 12)
  (net 38 "Net-(TEST2-Pad4)")
  (net 39 "Net-(TEST3-Pad1)")
  (net 40 25)
  (net 41 "Net-(TEST3-Pad3)")
  (net 42 24)
  (net 43 "Net-(TEST3-Pad5)")
  (net 44 23)
  (net 45 "Net-(TEST3-Pad7)")
  (net 46 22)
  (net 47 "Net-(TEST3-Pad9)")
  (net 48 21)
  (net 49 "Net-(TEST3-Pad11)")
  (net 50 19)
  (net 51 "Net-(TEST3-Pad13)")
  (net 52 18)
  (net 53 "Net-(TEST4-Pad1)")
  (net 54 14)
  (net 55 "Net-(TEST4-Pad3)")
  (net 56 13)
  (net 57 "Net-(TEST4-Pad5)")
  (net 58 A14)
  (net 59 "Net-(U1-Pad17)")
  (net 60 "Net-(U1-Pad10)")
  (net 61 "Net-(U1-Pad9)")
  (net 62 26)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 0)
    (add_net 1)
    (add_net 11)
    (add_net 12)
    (add_net 13)
    (add_net 14)
    (add_net 15)
    (add_net 16)
    (add_net 18)
    (add_net 19)
    (add_net 2)
    (add_net 20)
    (add_net 21)
    (add_net 22)
    (add_net 23)
    (add_net 24)
    (add_net 25)
    (add_net 26)
    (add_net 27)
    (add_net 3)
    (add_net 4)
    (add_net 5)
    (add_net 6)
    (add_net 7)
    (add_net 8)
    (add_net A14)
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(SPKR_TEST1-Pad2)")
    (add_net "Net-(SPKR_TEST1-Pad4)")
    (add_net "Net-(TEST1-Pad10)")
    (add_net "Net-(TEST1-Pad12)")
    (add_net "Net-(TEST1-Pad14)")
    (add_net "Net-(TEST1-Pad2)")
    (add_net "Net-(TEST1-Pad4)")
    (add_net "Net-(TEST1-Pad6)")
    (add_net "Net-(TEST1-Pad8)")
    (add_net "Net-(TEST2-Pad2)")
    (add_net "Net-(TEST2-Pad4)")
    (add_net "Net-(TEST3-Pad1)")
    (add_net "Net-(TEST3-Pad11)")
    (add_net "Net-(TEST3-Pad13)")
    (add_net "Net-(TEST3-Pad3)")
    (add_net "Net-(TEST3-Pad5)")
    (add_net "Net-(TEST3-Pad7)")
    (add_net "Net-(TEST3-Pad9)")
    (add_net "Net-(TEST4-Pad1)")
    (add_net "Net-(TEST4-Pad3)")
    (add_net "Net-(TEST4-Pad5)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad34)")
  )
  (net_class powa ""
    (clearance 0.2)
    (trace_width 0.8)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(LED_TEST1-Pad2)")
    (add_net "Net-(LED_TEST1-Pad4)")
    (add_net "Net-(LED_TEST1-Pad6)")
    (add_net "Net-(U2-Pad30)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 182.88 102.108 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference batt1 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(U2-Pad30)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 173.736 114.3 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at 1.91 3.06 270) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 270) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 168.656 114.3 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at 1.91 3.06 270) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 270) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 163.576 114.3 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.91 3.06 270) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 270) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 185.42 108.204 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference kill_jumper1 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(U2-Pad30)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(U2-Pad34)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 54EA0A4B)
    (at 153.924 99.06)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference LED_TEST1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 6))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(LED_TEST1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 7))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(LED_TEST1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 8))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(LED_TEST1-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 152.4 114.3 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.32892 -3.50012 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 20))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 149.352 103.124 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 5.32892 -3.50012 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 20))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 21 27))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 149.352 106.68 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 5.32892 -3.50012 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 16 15))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 152.4 110.49 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 5.32892 -3.50012 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(R4-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 18 16))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 582575DB)
    (at 163.576 101.092 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R5 (at 5.32892 -3.50012 270) (layer F.SilkS))
    (fp_text value 3ohm (at 5.08 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(LED_TEST1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 168.656 101.092 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R6 (at 5.32892 -3.50012 270) (layer F.SilkS))
    (fp_text value 3ohm (at 5.08 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(LED_TEST1-Pad4)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 173.736 101.092 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R7 (at 5.32892 -3.50012 270) (layer F.SilkS))
    (fp_text value 3ohm (at 5.08 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(LED_TEST1-Pad6)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 157.48 109.22)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference speaker1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(SPKR_TEST1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(SPKR_TEST1-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02 (layer F.Cu) (tedit 0)
    (at 153.924 90.424)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference SPKR_TEST1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_02X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(SPKR_TEST1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(R4-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(SPKR_TEST1-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x02.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x07 (layer F.Cu) (tedit 0)
    (at 153.67 59.69)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TEST1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_02X07 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 27))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(TEST1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 0))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(TEST1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 1))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(TEST1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 2))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(TEST1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 3))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(TEST1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 4))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(TEST1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 5))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "Net-(TEST1-Pad14)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x07.wrl
      (at (xyz 0.05 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02 (layer F.Cu) (tedit 0)
    (at 153.924 83.312)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TEST2 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_02X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 11))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "Net-(TEST2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 12))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(TEST2-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x02.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x07 (layer F.Cu) (tedit 0)
    (at 182.88 72.39)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TEST3 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_02X07 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(TEST3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 25))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "Net-(TEST3-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 24))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "Net-(TEST3-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 23))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "Net-(TEST3-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 22))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 "Net-(TEST3-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 21))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 49 "Net-(TEST3-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 19))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 "Net-(TEST3-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 18))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x07.wrl
      (at (xyz 0.05 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 54EA0A4B)
    (at 182.88 92.71)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TEST4 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 "Net-(TEST4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 14))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 "Net-(TEST4-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 13))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 "Net-(TEST4-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 A14))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lightsaber_parts:teensy32-basic (layer F.Cu) (tedit 58256F41)
    (at 140.208 83.82 270)
    (fp_text reference U1 (at 0 2.54 270) (layer F.SilkS))
    (fp_text value Teensy_3.1 (at 0 -2.54 270) (layer F.Fab))
    (pad 15 thru_hole circle (at 10.16 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 15))
    (pad 16 thru_hole circle (at 7.62 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 18 16))
    (pad 17 thru_hole circle (at 5.08 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(U1-Pad17)"))
    (pad 20 thru_hole circle (at -2.54 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 20))
    (pad 10 thru_hole circle (at 10.16 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(U1-Pad10)"))
    (pad 9 thru_hole circle (at 7.62 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(U1-Pad9)"))
    (pad 8 thru_hole circle (at 5.08 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 8))
    (pad 7 thru_hole circle (at 2.54 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 7))
    (pad 6 thru_hole circle (at 0 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 6))
    (pad 5 thru_hole circle (at -2.54 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 33 5))
    (pad 4 thru_hole circle (at -5.08 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 4))
    (pad 3 thru_hole circle (at -7.62 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 29 3))
    (pad 0 thru_hole circle (at -15.24 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 23 0))
    (pad 2 thru_hole circle (at -10.16 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 27 2))
    (pad 1 thru_hole circle (at -12.7 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 25 1))
    (pad 11 thru_hole circle (at 12.7 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 11))
    (pad 12 thru_hole circle (at 15.24 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 37 12))
    (pad 13 thru_hole circle (at 15.24 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 56 13))
    (pad 14 thru_hole circle (at 12.7 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 54 14))
    (pad 18 thru_hole circle (at 2.54 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 52 18))
    (pad 19 thru_hole circle (at 0 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 50 19))
    (pad 21 thru_hole circle (at -5.08 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 48 21))
    (pad 22 thru_hole circle (at -7.62 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 46 22))
    (pad 23 thru_hole circle (at -10.16 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 44 23))
    (pad 24 thru_hole circle (at -12.7 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 24))
    (pad 25 thru_hole circle (at -15.24 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 40 25))
    (pad 26 thru_hole circle (at -17.78 -7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 62 26))
    (pad 27 thru_hole circle (at -17.78 7.62 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 21 27))
    (pad 28 thru_hole circle (at 15.24 -5.08 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 58 A14))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 185.42 67.31 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference VIN_JUMP1 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 26))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(R1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lightsaber_parts:screw_hole (layer F.Cu) (tedit 582573F1)
    (at 184.15 114.3)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module lightsaber_parts:screw_hole (layer F.Cu) (tedit 582573F1)
    (at 134.62 114.3)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module lightsaber_parts:screw_hole (layer F.Cu) (tedit 582573F1)
    (at 134.62 60.96)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module lightsaber_parts:screw_hole (layer F.Cu) (tedit 582573F1)
    (at 184.15 60.96)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module lightsaber_parts:TeensySaberV2.1 (layer F.Cu) (tedit 5833F2C4)
    (at 168.656 76.708 270)
    (fp_text reference U2 (at 0 2.54 270) (layer F.SilkS))
    (fp_text value TeensySaberV2.1 (at 0 -2.54 270) (layer F.Fab))
    (pad 28 thru_hole circle (at 17.78 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(TEST4-Pad5)"))
    (pad 29 thru_hole circle (at 20.32 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (pad 30 thru_hole circle (at 20.32 -5.08 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(U2-Pad30)"))
    (pad 31 thru_hole circle (at 20.32 -2.54 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(LED_TEST1-Pad6)"))
    (pad 32 thru_hole circle (at 20.32 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(LED_TEST1-Pad4)"))
    (pad 33 thru_hole circle (at 20.32 2.54 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(LED_TEST1-Pad2)"))
    (pad 34 thru_hole circle (at 20.32 5.08 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U2-Pad34)"))
    (pad 35 thru_hole circle (at 20.32 7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(SPKR_TEST1-Pad2)"))
    (pad 36 thru_hole circle (at 17.78 7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(SPKR_TEST1-Pad4)"))
    (pad 5 thru_hole circle (at -2.54 7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(TEST1-Pad14)"))
    (pad 4 thru_hole circle (at -5.08 7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(TEST1-Pad12)"))
    (pad 3 thru_hole circle (at -7.62 7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(TEST1-Pad10)"))
    (pad 0 thru_hole circle (at -15.24 7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(TEST1-Pad4)"))
    (pad 2 thru_hole circle (at -10.16 7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(TEST1-Pad8)"))
    (pad 1 thru_hole circle (at -12.7 7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(TEST1-Pad6)"))
    (pad 11 thru_hole circle (at 12.7 7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(TEST2-Pad2)"))
    (pad 12 thru_hole circle (at 15.24 7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(TEST2-Pad4)"))
    (pad 13 thru_hole circle (at 15.24 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(TEST4-Pad3)"))
    (pad 14 thru_hole circle (at 12.7 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(TEST4-Pad1)"))
    (pad 18 thru_hole circle (at 2.54 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(TEST3-Pad13)"))
    (pad 19 thru_hole circle (at 0 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(TEST3-Pad11)"))
    (pad 21 thru_hole circle (at -5.08 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(TEST3-Pad9)"))
    (pad 22 thru_hole circle (at -7.62 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(TEST3-Pad7)"))
    (pad 23 thru_hole circle (at -10.16 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(TEST3-Pad5)"))
    (pad 24 thru_hole circle (at -12.7 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(TEST3-Pad3)"))
    (pad 25 thru_hole circle (at -15.24 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(TEST3-Pad1)"))
    (pad 26 thru_hole circle (at -17.78 -7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(R1-Pad1)"))
    (pad 27 thru_hole circle (at -17.78 7.62 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(TEST1-Pad2)"))
    (pad 28 thru_hole circle (at 15.24 -5.08 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(TEST4-Pad5)"))
  )
  (gr_line (start 130.81 118.11) (end 130.81 57.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 118.11) (end 130.81 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 57.15) (end 187.96 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 57.15) (end 187.96 57.15) (angle 90) (layer Edge.Cuts) (width 0.15))
)
