(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 108)
    (no_connects 0)
    (area 95.852857 67.215 219.107143 103.065)
    (thickness 1.6)
    (drawings 13)
    (tracks 319)
    (zones 0)
    (modules 59)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 76.2635 101.5365)
    (grid_origin 76.2635 101.5365)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(C6-Pad1)")
  (net 9 "Net-(C6-Pad2)")
  (net 10 "Net-(C7-Pad1)")
  (net 11 "Net-(C7-Pad2)")
  (net 12 "Net-(C8-Pad1)")
  (net 13 "Net-(C8-Pad2)")
  (net 14 VCC)
  (net 15 VSS)
  (net 16 "Net-(Cco1-Pad1)")
  (net 17 "Net-(Cco1-Pad2)")
  (net 18 "Net-(Cco2-Pad1)")
  (net 19 "Net-(Cco2-Pad2)")
  (net 20 "Net-(Cco3-Pad1)")
  (net 21 "Net-(Cco3-Pad2)")
  (net 22 "Net-(Cco4-Pad1)")
  (net 23 "Net-(Cco4-Pad2)")
  (net 24 bela_aout0)
  (net 25 bela_aout1)
  (net 26 bela_aout2)
  (net 27 bela_aout3)
  (net 28 "Net-(P2-Pad1)")
  (net 29 "Net-(P2-Pad4)")
  (net 30 modular_aout0)
  (net 31 modular_aout1)
  (net 32 modular_aout2)
  (net 33 modular_aout3)
  (net 34 "Net-(R9-Pad1)")
  (net 35 "Net-(R10-Pad1)")
  (net 36 "Net-(R11-Pad1)")
  (net 37 "Net-(R12-Pad1)")
  (net 38 outputoffset)
  (net 39 "Net-(R13-Pad2)")
  (net 40 "Net-(R14-Pad2)")
  (net 41 "Net-(R15-Pad2)")
  (net 42 "Net-(R16-Pad2)")
  (net 43 "Net-(R25-Pad1)")
  (net 44 "Net-(RoutF1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(Cco1-Pad1)")
    (add_net "Net-(Cco1-Pad2)")
    (add_net "Net-(Cco2-Pad1)")
    (add_net "Net-(Cco2-Pad2)")
    (add_net "Net-(Cco3-Pad1)")
    (add_net "Net-(Cco3-Pad2)")
    (add_net "Net-(Cco4-Pad1)")
    (add_net "Net-(Cco4-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(RoutF1-Pad1)")
    (add_net VCC)
    (add_net VSS)
    (add_net bela_aout0)
    (add_net bela_aout1)
    (add_net bela_aout2)
    (add_net bela_aout3)
    (add_net modular_aout0)
    (add_net modular_aout1)
    (add_net modular_aout2)
    (add_net modular_aout3)
    (add_net outputoffset)
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D91D9)
    (at 133.731 94.361 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 4.1275 0.0635 270) (layer F.SilkS))
    (fp_text value 220pF (at 1.3335 -2.413 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D9251)
    (at 136.144 94.361)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at -0.254 3.7465 180) (layer F.SilkS))
    (fp_text value 220pF (at 1.25 2.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D93A8)
    (at 188.786 93.7895 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at -0.317 -2.286 270) (layer F.SilkS))
    (fp_text value 220p (at 2.1595 -2.3495 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D93B4)
    (at 191.008 93.7895)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C4 (at 3.2385 2.2225 90) (layer F.SilkS))
    (fp_text value 220p (at 0.6985 2.3495) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D921E)
    (at 128.46 90.932 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at -1.6515 0.6985 270) (layer F.SilkS))
    (fp_text value 440p (at 4.1905 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D9235)
    (at 140.208 90.8685)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 4.318 1.0795) (layer F.SilkS))
    (fp_text value 440p (at -1.778 -0.0635 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(C6-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D9293)
    (at 184.531 90.6145)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 4.191 -0.5715 90) (layer F.SilkS))
    (fp_text value 440p (at -1.8415 0.0635 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(C7-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D92E3)
    (at 198.755 90.678)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at 1.397 -0.0635 90) (layer F.SilkS))
    (fp_text value 440p (at -1.778 -0.254 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(C8-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 584D9160)
    (at 114.744 81.9785 180)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C9 (at 3.6825 -2.667 270) (layer F.SilkS))
    (fp_text value 10uF (at -2.0325 -2.794 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 584D9145)
    (at 114.744 87.884 180)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C10 (at 3.8095 -2.794 270) (layer F.SilkS))
    (fp_text value 10uF (at -1.9055 -3.1115 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 VSS))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D8DA3)
    (at 162.116 80.391)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C11 (at -1.842 -0.0635 90) (layer F.SilkS))
    (fp_text value 10n (at 4.1905 -0.0635 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D9271)
    (at 167.259 94.615)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C12 (at 4.191 0 90) (layer F.SilkS))
    (fp_text value 10n (at 1.25 2.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 VSS))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D92D3)
    (at 192.024 90.6145)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C13 (at 1.397 0.0635 90) (layer F.SilkS))
    (fp_text value 10n (at -1.5875 -0.381 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D8D46)
    (at 131.191 76.6445)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C14 (at -0.254 -2.9845 90) (layer F.SilkS))
    (fp_text value 10n (at 2.0955 -2.2225 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 VSS))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D922E)
    (at 133.604 90.932)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C15 (at 1.27 0.0635 90) (layer F.SilkS))
    (fp_text value 10n (at -1.7145 -0.0635 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D8DD9)
    (at 189.674 76.6445)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C16 (at -0.317 -2.8575 90) (layer F.SilkS))
    (fp_text value 10n (at 1.9055 -2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 VSS))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D9447)
    (at 115.506 75.565 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference Cco1 (at -4.3815 -0.699 270) (layer F.SilkS))
    (fp_text value 1uF (at -1.7145 -0.2545 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(Cco1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(Cco1-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D8D92)
    (at 149.67 76.581 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference Cco2 (at 1.3335 2.222 90) (layer F.SilkS))
    (fp_text value 1uF (at 4.2545 0.063 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(Cco2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(Cco2-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D8DAB)
    (at 173.99 75.692 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference Cco3 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 1uF (at 4.191 0 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(Cco3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(Cco3-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584D8E1D)
    (at 210.248 77.6605 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference Cco4 (at 1.4605 -2.1595 270) (layer F.SilkS))
    (fp_text value 1uF (at 4.318 -0.064 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 "Net-(Cco4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 "Net-(Cco4-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 584D8FEF)
    (at 155.575 97.282 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -2.4765 8.5725 180) (layer F.SilkS) hide)
    (fp_text value in_bela (at -2.54 4.064 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 bela_aout0))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 bela_aout1))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 bela_aout2))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 bela_aout3))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mta-156:MTA-156-4 (layer F.Cu) (tedit 584D9186)
    (at 106.778 79.4175)
    (descr MTA-156-4)
    (tags MTA-156-4)
    (fp_text reference P2 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value MTA-156-4 (at 0 -3.1) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0) (size 5 2.5) (drill 1.68) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 3.96) (size 5 2.5) (drill 1.68) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 7.92) (size 5 2.5) (drill 1.68) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 11.88) (size 5 2.5) (drill 1.68) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P2-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 584D8D80)
    (at 155.575 76.327 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 4.8895 8.6995 180) (layer F.SilkS) hide)
    (fp_text value out_mod (at 5.1435 3.7465 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 modular_aout0))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 modular_aout1))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 modular_aout2))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 modular_aout3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module trim:trimmer (layer F.Cu) (tedit 584DAABF)
    (at 155.766 84.8995 90)
    (fp_text reference TR1 (at -4.2545 -1.461 180) (layer F.SilkS))
    (fp_text value 10k (at 0.2 -4.1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -2.5 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 0 -2.5 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 "Net-(RoutF1-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 -2.5 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 "Net-(RoutF1-Pad1)"))
  )
  (module Housings_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 584D90E4)
    (at 126.048 87.503 90)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 5.5245 -0.6355 180) (layer F.SilkS))
    (fp_text value TL074 (at 3.7465 8.191 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(Cco2-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(R14-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R10-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 VSS))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R9-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R13-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(Cco1-Pad2)"))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 584D9306)
    (at 184.531 87.503 90)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 1.3335 -1.524 90) (layer F.SilkS))
    (fp_text value TL074 (at 3.4925 7.5565 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(Cco4-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(R16-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R12-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 VSS))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R11-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(R15-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(Cco3-Pad2)"))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 584D8F83)
    (at 162.052 91.186 90)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U3 (at 2.032 -1.397 90) (layer F.SilkS))
    (fp_text value TL072 (at 3.8735 4.0005 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 outputoffset))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 outputoffset))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(R25-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 VSS))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5844C766)
    (at 209.55 72.39)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.SilkS) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5844C75E)
    (at 209.55 97.79)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.SilkS) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5844C755)
    (at 105.41 72.39)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.SilkS) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5844C748)
    (at 105.41 97.79)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.SilkS) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D910F)
    (at 121.984 89.916 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 6.858 0.063 180) (layer F.SilkS))
    (fp_text value 28k7 (at 4.445 0.063 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 24 bela_aout0))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8FB0)
    (at 145.478 89.916 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 6.7945 0.0005 180) (layer F.SilkS))
    (fp_text value 28k7 (at 4.445 0.0005 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(C6-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 25 bela_aout1))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8F4D)
    (at 180.34 90.043 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 6.7945 0 180) (layer F.SilkS))
    (fp_text value 28k7 (at 4.3815 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 26 bela_aout2))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8EA8)
    (at 195.961 93.726)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 6.9215 0 90) (layer F.SilkS))
    (fp_text value 28k7 (at 4.445 0.0635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(C8-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 27 bela_aout3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D9051)
    (at 126.302 94.361 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R5 (at 3.1755 0 270) (layer F.SilkS))
    (fp_text value 28k7 (at 5.7155 -0.0635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D901F)
    (at 141.16 97.155)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R6 (at 6.922 0.127 90) (layer F.SilkS))
    (fp_text value 28k7 (at 4.382 0.0635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(C6-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8EF5)
    (at 183.896 93.853 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R7 (at 3.2385 -0.0635 270) (layer F.SilkS))
    (fp_text value 28k7 (at 5.715 -0.0635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(C7-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8E3F)
    (at 203.898 90.1065 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R8 (at 6.9215 0.064 180) (layer F.SilkS))
    (fp_text value 28k7 (at 4.5085 0.064 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(C8-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D9048)
    (at 126.302 97.4725 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R9 (at 3.1755 0 270) (layer F.SilkS))
    (fp_text value 10k (at 6.2235 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 34 "Net-(R9-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D9025)
    (at 151.32 94.0435 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R10 (at 3.3015 0 270) (layer F.SilkS))
    (fp_text value 10k (at 6.159 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 35 "Net-(R10-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8EFD)
    (at 183.896 98.4885 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R11 (at 3.3655 0.0635 270) (layer F.SilkS))
    (fp_text value 10k (at 6.223 -0.0635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 36 "Net-(R11-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8E37)
    (at 207.01 79.9465 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R12 (at 3.3655 0 360) (layer F.SilkS))
    (fp_text value 10k (at 6.1595 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 37 "Net-(R12-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D9119)
    (at 118.745 89.916 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R13 (at 6.858 -0.0635 180) (layer F.SilkS))
    (fp_text value 10k (at 4.064 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 38 outputoffset))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 39 "Net-(R13-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8FA9)
    (at 148.717 89.916 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R14 (at 6.6675 -0.0635 180) (layer F.SilkS))
    (fp_text value 10k (at 4.0005 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 38 outputoffset))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 40 "Net-(R14-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8F2B)
    (at 177.102 90.043 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R15 (at 6.731 -0.0005 180) (layer F.SilkS))
    (fp_text value 10k (at 4.0005 -0.064 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 38 outputoffset))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 41 "Net-(R15-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8EC3)
    (at 186.69 98.4885)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R16 (at 6.858 0.0635 90) (layer F.SilkS))
    (fp_text value 10k (at 3.937 0.0635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 38 outputoffset))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 42 "Net-(R16-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8D20)
    (at 118.428 76.708)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R17 (at 6.794 0.0635 90) (layer F.SilkS))
    (fp_text value 10k (at 3.9365 0.0635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(Cco1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 39 "Net-(R13-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8D5D)
    (at 146.431 73.533 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R18 (at 3.175 -3.175 270) (layer F.SilkS))
    (fp_text value 10k (at 6.0325 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 19 "Net-(Cco2-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 40 "Net-(R14-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8DC1)
    (at 176.974 73.533)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R19 (at 6.795 0.0635 90) (layer F.SilkS))
    (fp_text value 10k (at 4.001 0.0635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 21 "Net-(Cco3-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 41 "Net-(R15-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8DF0)
    (at 204.66 73.533 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R20 (at 3.1745 -3.2385 270) (layer F.SilkS))
    (fp_text value 10k (at 6.159 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 23 "Net-(Cco4-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 42 "Net-(R16-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8D2D)
    (at 128.588 73.4695 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R21 (at 3.4295 0 270) (layer F.SilkS))
    (fp_text value 1k (at 6.414 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 30 modular_aout0))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 16 "Net-(Cco1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8D66)
    (at 136.271 76.6445)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R22 (at 6.9215 -3.1115 90) (layer F.SilkS))
    (fp_text value 1k (at 3.6195 -0.0635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 31 modular_aout1))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 18 "Net-(Cco2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8DCB)
    (at 187.134 76.6445 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R23 (at 3.3015 -0.127 270) (layer F.SilkS))
    (fp_text value 1k (at 6.667 -0.0635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 32 modular_aout2))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 20 "Net-(Cco3-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8DF9)
    (at 194.564 76.6445)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R24 (at 6.9215 -3.175 90) (layer F.SilkS))
    (fp_text value 1k (at 3.6195 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 33 modular_aout3))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 22 "Net-(Cco4-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D8F34)
    (at 173.863 90.1065 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R25 (at 6.7945 0 180) (layer F.SilkS))
    (fp_text value 10k (at 3.937 0.0635 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 43 "Net-(R25-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 584D9421)
    (at 157.607 79.756 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference RoutF1 (at 12.3825 0.6985 360) (layer F.SilkS))
    (fp_text value 16k9 (at 5.842 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 44 "Net-(RoutF1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 43 "Net-(R25-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 584D9178)
    (at 111.95 75.1205 270)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R26 (at -5.5245 2.095 360) (layer F.SilkS))
    (fp_text value bead (at -5.588 -1.7785 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.49936 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5019 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 28 "Net-(P2-Pad1)"))
  )
  (module Resistors_ThroughHole:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 584D906D)
    (at 111.887 95.631 90)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R27 (at -5.08 3.175 180) (layer F.SilkS))
    (fp_text value bead (at 1.2065 2.0955 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.49936 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 VSS))
    (pad 2 thru_hole circle (at 2.5019 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(P2-Pad4)"))
  )
  (gr_text gnd (at 165.3667 76.7461 90) (layer F.SilkS))
  (gr_text 0 (at 153.5811 72.6821) (layer F.SilkS))
  (gr_text 0 (at 155.4607 99.8601) (layer F.SilkS))
  (gr_text gnd (at 153.4287 94.7293 90) (layer F.SilkS))
  (gr_text - (at 109.347 93.853) (layer F.SilkS))
  (gr_text + (at 109.4105 76.454) (layer F.SilkS))
  (gr_text http://x37v.info (at 209.7405 87.503 90) (layer B.SilkS))
  (gr_text "xnor 12/2016" (at 211.6455 87.249 90) (layer B.SilkS))
  (gr_text "bela analog to modular" (at 190.881 70.612) (layer B.SilkS))
  (gr_line (start 101.6 68.58) (end 213.36 68.58) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.36 68.58) (end 213.36 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.36 101.6) (end 101.6 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 68.58) (end 101.6 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.854 68.707) (xy 212.979 68.707) (xy 213.106 101.346) (xy 101.727 101.346) (xy 101.854 68.8975)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.854 68.961) (xy 212.979 68.961) (xy 213.1695 101.092) (xy 101.854 101.4095) (xy 101.7905 68.8975)
      )
    )
  )
)
