(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 185)
    (no_connects 0)
    (area 12.5 12.975 105.075001 92.5)
    (thickness 1.6)
    (drawings 69)
    (tracks 834)
    (zones 0)
    (modules 77)
    (nets 58)
  )
  (page A4)
  (layers
    (0 F.Cu power)
    (31 B.Cu jumper)
    (33 F.Adhes user hide)
    (35 F.Paste user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (47 F.CrtYd user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.2)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.096 6.096)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 15 90)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (gerberprecision 5)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Output/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 PHR1)
  (net 4 "Net-(C7-Pad1)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(P5-Pad1)")
  (net 8 "Net-(P8-Pad2)")
  (net 9 "Net-(P9-Pad1)")
  (net 10 "Net-(P10-Pad1)")
  (net 11 "Net-(P10-Pad2)")
  (net 12 "Net-(P12-Pad2)")
  (net 13 "Net-(P13-Pad2)")
  (net 14 "Net-(P14-Pad2)")
  (net 15 "Net-(Q2-Pad1)")
  (net 16 "Net-(Q6-Pad1)")
  (net 17 RXD)
  (net 18 ~RST)
  (net 19 BOOT0)
  (net 20 TXD)
  (net 21 "Net-(R17-Pad2)")
  (net 22 "Net-(R18-Pad1)")
  (net 23 "Net-(R19-Pad2)")
  (net 24 "Net-(R20-Pad1)")
  (net 25 ADC3)
  (net 26 "Net-(U1-Pad10)")
  (net 27 "Net-(U1-Pad12)")
  (net 28 "Net-(U1-Pad13)")
  (net 29 "Net-(U1-Pad14)")
  (net 30 "Net-(C6-Pad2)")
  (net 31 "Net-(C8-Pad1)")
  (net 32 THR)
  (net 33 +12V)
  (net 34 VCC)
  (net 35 "Net-(D1-Pad2)")
  (net 36 "Net-(D4-Pad1)")
  (net 37 "Net-(L1-Pad1)")
  (net 38 "Net-(P1-Pad2)")
  (net 39 "Net-(P3-Pad1)")
  (net 40 "Net-(P3-Pad3)")
  (net 41 "Net-(P4-Pad7)")
  (net 42 "Net-(P11-Pad2)")
  (net 43 "Net-(P11-Pad3)")
  (net 44 RST)
  (net 45 SoftPWM)
  (net 46 "Net-(P15-Pad1)")
  (net 47 "Net-(P4-Pad8)")
  (net 48 DE/~RE)
  (net 49 "Net-(P17-Pad3)")
  (net 50 "Net-(Q1-Pad1)")
  (net 51 "Net-(Q3-Pad1)")
  (net 52 "Net-(Q4-Pad1)")
  (net 53 "Net-(Q5-Pad1)")
  (net 54 "Net-(U2-Pad7)")
  (net 55 "Net-(U2-Pad4)")
  (net 56 "Net-(U5-Pad8)")
  (net 57 "Net-(U6-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ADC3)
    (add_net BOOT0)
    (add_net DE/~RE)
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P10-Pad2)")
    (add_net "Net-(P11-Pad2)")
    (add_net "Net-(P11-Pad3)")
    (add_net "Net-(P17-Pad3)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P4-Pad7)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P9-Pad1)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U6-Pad8)")
    (add_net PHR1)
    (add_net RST)
    (add_net RXD)
    (add_net SoftPWM)
    (add_net THR)
    (add_net TXD)
    (add_net ~RST)
  )
  (net_class FETGate ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(P15-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R20-Pad1)")
    (add_net VCC)
  )
  (net_class HighPower ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net "Net-(P12-Pad2)")
    (add_net "Net-(P13-Pad2)")
    (add_net "Net-(P14-Pad2)")
    (add_net "Net-(P8-Pad2)")
  )
  (net_class MidPower ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P1-Pad2)")
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_SPTAF-3.5mm_4pol (layer F.Cu) (tedit 5925B487)
    (at 83 46.55 90)
    (descr "4-way 3.5mm pitch terminal block, Phoenix SPTAF series")
    (fp_text reference P14 (at 6.55 -2.3 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 5.25 6 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 10.5 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(P14-Pad2)") (zone_connect 2))
    (pad 4 thru_hole circle (at 10.5 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(P14-Pad2)") (zone_connect 2))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC))
    (pad 3 thru_hole circle (at 7 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(P14-Pad2)") (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(P14-Pad2)") (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_SPTAF-3.5mm_4pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_SMD:Choke_SMD_12x12mm_h8mm (layer F.Cu) (tedit 58D276B0)
    (at 54.5 68.5)
    (descr "Choke, SMD, 12x12mm 8mm height")
    (tags "Choke, SMD")
    (attr smd)
    (fp_text reference L2 (at -0.25 -2.75) (layer F.SilkS))
    (fp_text value 27uH (at 0 8.89) (layer F.Fab))
    (pad 1 smd rect (at -4.95046 0) (size 2.90068 5.40004) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 4.95046 0) (size 2.90068 5.40004) (layers F.Cu F.Paste F.Mask)
      (net 33 +12V))
    (model Choke_SMD.3dshapes/Choke_SMD_12x12mm_h8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_SPTAF-3.5mm_4pol (layer F.Cu) (tedit 5925B46F)
    (at 83.05 64.075 90)
    (descr "4-way 3.5mm pitch terminal block, Phoenix SPTAF series")
    (fp_text reference P8 (at 7.075 -2.25 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 5.25 6 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 10.5 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(P8-Pad2)") (zone_connect 2))
    (pad 4 thru_hole circle (at 10.5 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(P8-Pad2)") (zone_connect 2))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC))
    (pad 3 thru_hole circle (at 7 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(P8-Pad2)") (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(P8-Pad2)") (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_SPTAF-3.5mm_4pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_SPTAF-3.5mm_4pol (layer F.Cu) (tedit 5925B481)
    (at 83 29.8 90)
    (descr "4-way 3.5mm pitch terminal block, Phoenix SPTAF series")
    (zone_connect 2)
    (fp_text reference P13 (at 6.6 -2.3 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 5.25 6 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 10.5 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(P13-Pad2)") (zone_connect 2))
    (pad 4 thru_hole circle (at 10.5 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(P13-Pad2)") (zone_connect 2))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (pad 3 thru_hole circle (at 7 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(P13-Pad2)") (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(P13-Pad2)") (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_SPTAF-3.5mm_4pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_SPTAF-3.5mm_4pol (layer F.Cu) (tedit 5925B474)
    (at 83 81.8 90)
    (descr "4-way 3.5mm pitch terminal block, Phoenix SPTAF series")
    (fp_text reference P12 (at 6.9 -2.3 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 5.25 6 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 10.5 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(P12-Pad2)") (zone_connect 2))
    (pad 4 thru_hole circle (at 10.5 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(P12-Pad2)") (zone_connect 2))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC))
    (pad 3 thru_hole circle (at 7 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(P12-Pad2)") (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(P12-Pad2)") (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 5 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_SPTAF-3.5mm_4pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58D27C55)
    (at 31.1 51.84)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 2.7 -0.04) (layer F.SilkS))
    (fp_text value 1nF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 PHR1))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 31.29 55.92 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 1nF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 32 THR))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58D27553)
    (at 38.3 69.1)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0.95 -1.85) (layer F.SilkS))
    (fp_text value 1nF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_10x10.5 (layer F.Cu) (tedit 58D2758E)
    (at 44.4 83 270)
    (descr "SMT capacitor, aluminium electrolytic, 10x10.5")
    (attr smd)
    (fp_text reference C11 (at 0 -2.6 270) (layer F.SilkS))
    (fp_text value 820uF (at 0 6.35 270) (layer F.Fab))
    (pad 1 smd rect (at 4.0005 0 270) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 34 VCC))
    (pad 2 smd rect (at -4.0005 0 270) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 58D27C58)
    (at 37.75 50.25 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at 3.125 2.975 270) (layer F.SilkS))
    (fp_text value POWER (at 1.3 -2.9 270) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 64.75 29.75 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.91 3.06 90) (layer F.SilkS))
    (fp_text value ACTIVITY (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x08 (layer F.Cu) (tedit 58D27646)
    (at 26.5 35.75 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 6.75 1.25 180) (layer F.SilkS))
    (fp_text value TOZERO (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 TXD))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 BOOT0))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 RST))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P4-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P4-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled (layer F.Cu) (tedit 58D27587)
    (at 30 86.5 90)
    (descr "Molex Mini-Fit JR, PN:5569-04A2, dual row, side entry type, through hole, with plastic peg mount")
    (tags "connector molex mini-fit 5569")
    (zone_connect 2)
    (fp_text reference P7 (at 4.5 -4.25 90) (layer F.SilkS))
    (fp_text value "Molex 12V/24V" (at 2.1 10 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 4.2 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 0 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (pad 4 thru_hole circle (at 4.2 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 34 VCC) (zone_connect 2))
    (pad "" np_thru_hole circle (at 2.1 -7.3 90) (size 3 3) (drill 3) (layers *.Cu)
      (zone_connect 0))
    (model Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 58D275FB)
    (at 25.75 65.75 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 6.75 1.25 180) (layer F.SilkS))
    (fp_text value ADC3 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P9-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58D2760A)
    (at 30.55 39.225)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 1.45 -1.225) (layer F.SilkS))
    (fp_text value FDV303N (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P10-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D27697)
    (at 33.5 68.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.5 -0.25 270) (layer F.SilkS))
    (fp_text value 300 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 SoftPWM))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 58D275ED)
    (at 25.75 52.75 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference R6 (at 6.25 1.25 180) (layer F.SilkS))
    (fp_text value Photores (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 PHR1))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5925B003)
    (at 31.75 49.75)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2.15 -0.85) (layer F.SilkS))
    (fp_text value 5K1 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 PHR1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 58D275F7)
    (at 25.75 59.25 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference R9 (at 6.25 1.25 180) (layer F.SilkS))
    (fp_text value Thermistor (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 THR))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 31.71 53.94 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 5K1 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 THR))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58D27518)
    (at 73 62 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 1 -2.5 270) (layer F.SilkS))
    (fp_text value 6 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R17-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5925B455)
    (at 69 80 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 2.9 2.9 180) (layer F.SilkS))
    (fp_text value 6 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R18-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(Q3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58D27504)
    (at 69 33 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0.25 1.75 270) (layer F.SilkS))
    (fp_text value 6 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5925B407)
    (at 68.3 44.5 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 1.7 -2.3 270) (layer F.SilkS))
    (fp_text value 6 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R20-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(Q5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D27E24)
    (at 26 45.25 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 3.72 -1.89 180) (layer F.SilkS))
    (fp_text value 300 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(P4-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5925AFDF)
    (at 30.6 41.8)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 2.4 -1.5 90) (layer F.SilkS))
    (fp_text value 5K1 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58D27E1B)
    (at 30.7 43.9)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R23 (at -0.94 1.45) (layer F.SilkS))
    (fp_text value 50 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P10-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D2765B)
    (at 48.4 36.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at -0.4 1.85) (layer F.SilkS))
    (fp_text value 43K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P9-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 ADC3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D2765F)
    (at 51.1 36.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 0.4 1.85) (layer F.SilkS))
    (fp_text value 11K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 ADC3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D2755F)
    (at 38.7 71.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 3.3 0) (layer F.SilkS))
    (fp_text value 11K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 41.25 51 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5925B37F)
    (at 63.8 25 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at -2.1 1.3 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 TXD))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 58D275EA)
    (at 26.5 42.25 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P10 (at 7 1.25 180) (layer F.SilkS))
    (fp_text value IROUT (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P10-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P10-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 53 32)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -4.3) (layer F.SilkS))
    (fp_text value STM32F030F4 (at 0 4.3) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 BOOT0))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C6-Pad2)"))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C8-Pad1)"))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 ~RST))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad1)"))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 PHR1))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 THR))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 ADC3))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 SoftPWM))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 TXD))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 RXD))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P5-Pad1)"))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 DE/~RE))
    (model Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 48 26)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 18pF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58D27B73)
    (at 59 26 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 2.825 0.95 90) (layer F.SilkS))
    (fp_text value 18pF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bytelabs_ch_various:CRYSTAL_ABM3C (layer F.Cu) (tedit 58D27679)
    (at 54 26)
    (fp_text reference Y1 (at 0.5 -4.25) (layer F.SilkS))
    (fp_text value "8 MHz 18pF" (at 0.25 -2.75) (layer F.SilkS))
    (pad 4 smd rect (at -1.89992 -1.15062) (size 1.6002 1.30048) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.89992 -1.15062) (size 1.6002 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.89992 1.15062) (size 1.6002 1.30048) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.89992 1.15062) (size 1.6002 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C6-Pad2)"))
  )
  (module AC-Stuff:1Pin (layer F.Cu) (tedit 58D274EC)
    (at 59.4 28.7)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P5 (at 1.6 -0.2) (layer F.SilkS))
    (fp_text value SWD (at 0.24892 3.74904) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 7 "Net-(P5-Pad1)"))
  )
  (module AC-Stuff:1Pin (layer F.Cu) (tedit 58D274E6)
    (at 57.5 28.3)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P6 (at 0.75 1.45) (layer F.SilkS))
    (fp_text value SWC (at 0.24892 3.74904) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 48 DE/~RE))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58D274EF)
    (at 60 32.5 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 1.5 -2.25 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58D27653)
    (at 46 31.5)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -3.25 0.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58D2764D)
    (at 44 28.8 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 2.25 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 ~RST))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 RST))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_10x10.5 (layer F.Cu) (tedit 5925B3AA)
    (at 62.45 53.45 270)
    (descr "SMT capacitor, aluminium electrolytic, 10x10.5")
    (attr smd)
    (fp_text reference C16 (at 0.15 -1.95 270) (layer F.SilkS))
    (fp_text value 470uF (at 0 6.35 270) (layer F.Fab))
    (pad 1 smd rect (at 4.0005 0 270) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 33 +12V))
    (pad 2 smd rect (at -4.0005 0 270) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_10x10.5 (layer F.Cu) (tedit 58D27594)
    (at 62.175 83.025 270)
    (descr "SMT capacitor, aluminium electrolytic, 10x10.5")
    (attr smd)
    (fp_text reference C17 (at -0.25 -3.5 270) (layer F.SilkS))
    (fp_text value 820uF (at 0 6.35 270) (layer F.Fab))
    (pad 1 smd rect (at 4.0005 0 270) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 34 VCC))
    (pad 2 smd rect (at -4.0005 0 270) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5530FCB9)
    (at 29.5 75 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2 270) (layer F.SilkS))
    (fp_text value PMEG6010 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 33 +12V))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D1-Pad2)"))
  )
  (module Diodes_SMD:SMB_Standard (layer F.Cu) (tedit 58D27548)
    (at 44.75 66.25 90)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D4 (at -1 -3 90) (layer F.SilkS))
    (fp_text value SD2114 (at 0.05 4.7 90) (layer F.Fab))
    (fp_text user K (at -4.75 1.75 90) (layer F.SilkS))
    (fp_text user A (at 4.5 1.5 90) (layer F.SilkS))
    (pad 1 smd rect (at -2.14884 0 90) (size 2.49936 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 2.14884 0 90) (size 2.49936 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Diodes_SMD.3dshapes/SMB_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 58D27618)
    (at 32.5 35.7 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.5 -2.5 270) (layer F.SilkS))
    (fp_text value JP-3V3 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5925B4F3)
    (at 64.85 17.2)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0.05 4.7) (layer F.SilkS))
    (fp_text value TERMINATION (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P11-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P11-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58D27989)
    (at 36 17 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0.1 7.2 270) (layer F.SilkS))
    (fp_text value JP-DMX (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 RXD))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P3-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58D27564)
    (at 33 72.5 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 1.75 -2.25 90) (layer F.SilkS))
    (fp_text value FDV303N (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D27650)
    (at 47 29 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -0.25 -1.5 90) (layer F.SilkS))
    (fp_text value 5K1 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 ~RST))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58D276A0)
    (at 37.2 73.7)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0.05 2.05) (layer F.SilkS))
    (fp_text value 120K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 VCC))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:WSON-10-2x3 (layer F.Cu) (tedit 58D276BE)
    (at 42.5 42.5 90)
    (fp_text reference U2 (at 0 2.75 90) (layer F.SilkS))
    (fp_text value TPS62177 (at 0 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad "" smd rect (at 0 0.6 90) (size 0.84 1) (layers F.Paste))
    (pad 10 smd rect (at 0.95 -1 90) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 9 smd rect (at 0.95 -0.5 90) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(L1-Pad1)"))
    (pad 6 smd rect (at 0.95 1 90) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.95 0.5 90) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at 0.95 0 90) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -0.95 1 90) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.95 0.5 90) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U2-Pad4)"))
    (pad 1 smd rect (at -0.95 -1 90) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.95 -0.5 90) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 VCC))
    (pad PAD smd rect (at 0 0 90) (size 0.84 2.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.95 0 90) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 VCC))
    (pad "" smd rect (at 0 -0.6 90) (size 0.84 1) (layers F.Paste))
  )
  (module TO_SOT_Packages_SMD:TO-263-5Lead (layer F.Cu) (tedit 58D276DA)
    (at 51.25 59 90)
    (descr "D2PAK / TO-263 3-lead smd package")
    (tags "D2PAK D2PAK-3 TO-263AB TO-263")
    (attr smd)
    (fp_text reference U7 (at 11 7 180) (layer F.SilkS))
    (fp_text value AP1501-12K5G (at 15.25 -0.25 180) (layer F.Fab))
    (pad 5 smd rect (at 0 3.4 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0 1.7 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 +12V))
    (pad 2 smd rect (at 0 -1.7 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D4-Pad1)"))
    (pad 3 smd rect (at 9.15 0 90) (size 9.4 10.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 0 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -3.4 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(P15-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/TO-263-5Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeC_EIA-6032_Reflow (layer F.Cu) (tedit 58D276C5)
    (at 38.25 44.75 270)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow")
    (tags "Tantal Capacitor Size-C EIA-6032 Reflow")
    (attr smd)
    (fp_text reference C1 (at 0 0.25 270) (layer F.SilkS))
    (fp_text value 220uF (at 0 2.9 270) (layer F.Fab))
    (pad 2 smd rect (at 2.47 0 270) (size 2.37 2.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.47 0 270) (size 2.37 2.23) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeC_EIA-6032_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 58D27D96)
    (at 66 69 180)
    (attr smd)
    (fp_text reference C9 (at 3.85 0.15 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 33 +12V))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5925B415)
    (at 64.81 43.78 90)
    (attr smd)
    (fp_text reference C10 (at 1.58 -4.01 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 33 +12V))
    (pad 2 smd rect (at 1.651 0 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58D276CB)
    (at 43 45.5)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at 0.25 2) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 34 VCC))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 58D28226)
    (at 36.75 62.5 270)
    (attr smd)
    (fp_text reference C14 (at 0 2.25 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 34 VCC))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_Reflow (layer F.Cu) (tedit 5925B3BE)
    (at 65.94 62.08)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow")
    (tags "Tantal Capacitor Size-D EIA-7343 Reflow")
    (attr smd)
    (fp_text reference C15 (at -0.04 -0.28) (layer F.SilkS))
    (fp_text value 100uF (at -0.09906 3.59918) (layer F.Fab))
    (pad 2 smd rect (at 3.12 0) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.12 0) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 33 +12V))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58D27961)
    (at 46 18 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P11 (at 0.2 7.4 90) (layer F.SilkS))
    (fp_text value DMX-IN (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P11-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P11-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 592595EA)
    (at 56 18 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P16 (at -3.075 1.025 180) (layer F.SilkS))
    (fp_text value DMX-OUT (at 0.25 10.75 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P11-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P11-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 40 58.4)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P15 (at 0 -5.1) (layer F.SilkS))
    (fp_text value JP-12/24V (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P15-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 +12V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58D282A7)
    (at 25.75 75 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P17 (at 0 7 180) (layer F.SilkS))
    (fp_text value FAN (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 +12V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(P17-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Drills:1Pin (layer F.Cu) (tedit 587540D4)
    (at 100.25 20)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value 1Pin (at 0.24892 3.74904) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Drills:1Pin (layer F.Cu) (tedit 587540D4)
    (at 100 85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value 1Pin (at 0.24892 3.74904) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Drills:1Pin (layer F.Cu) (tedit 587540D4)
    (at 100 52)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value 1Pin (at 0.24892 3.74904) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Drills:1Pin (layer F.Cu) (tedit 587540D4)
    (at 70 20.2)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value 1Pin (at 0.24892 3.74904) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Drills:1Pin (layer F.Cu) (tedit 587540D4)
    (at 20 74)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value 1Pin (at 0.24892 3.74904) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer F.Cu) (tedit 5925B469)
    (at 69.8 55.32 270)
    (descr "DPAK / TO-252 2-lead smd package")
    (tags "dpak TO-252")
    (attr smd)
    (fp_text reference Q1 (at -4.62 -5.4 270) (layer F.SilkS))
    (fp_text value "IPD220N06L3 G" (at 0 -2.413 270) (layer F.Fab))
    (pad 1 smd rect (at -2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -6.35 270) (size 6.096 6.096) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P8-Pad2)") (zone_connect 2))
    (pad 3 smd rect (at 2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/TO-252-2Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer F.Cu) (tedit 5925B462)
    (at 69.74 79.99 270)
    (descr "DPAK / TO-252 2-lead smd package")
    (tags "dpak TO-252")
    (attr smd)
    (fp_text reference Q3 (at -4.89 -5.66 270) (layer F.SilkS))
    (fp_text value "IPD220N06L3 G" (at 0 -2.413 270) (layer F.Fab))
    (pad 1 smd rect (at -2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0 -6.35 270) (size 6.096 6.096) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P12-Pad2)") (zone_connect 2))
    (pad 3 smd rect (at 2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/TO-252-2Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer F.Cu) (tedit 5925B47E)
    (at 69.65 27.47 270)
    (descr "DPAK / TO-252 2-lead smd package")
    (tags "dpak TO-252")
    (attr smd)
    (fp_text reference Q4 (at -4.77 -5.25 270) (layer F.SilkS))
    (fp_text value "IPD220N06L3 G" (at 0 -2.413 270) (layer F.Fab))
    (pad 1 smd rect (at -2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 0 -6.35 270) (size 6.096 6.096) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P13-Pad2)") (zone_connect 2))
    (pad 3 smd rect (at 2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/TO-252-2Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer F.Cu) (tedit 5925B47A)
    (at 69.68 44.58 270)
    (descr "DPAK / TO-252 2-lead smd package")
    (tags "dpak TO-252")
    (attr smd)
    (fp_text reference Q5 (at -5.08 -5.32 270) (layer F.SilkS))
    (fp_text value "IPD220N06L3 G" (at 0 -2.413 270) (layer F.Fab))
    (pad 1 smd rect (at -2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at 0 -6.35 270) (size 6.096 6.096) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P14-Pad2)") (zone_connect 2))
    (pad 3 smd rect (at 2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/TO-252-2Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 5925B4AC)
    (at 41.45 22.475)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at -0.25 -3.375) (layer F.SilkS))
    (fp_text value ISL3172E (at 0 2.6) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at -2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 DE/~RE))
    (pad 3 smd rect (at -2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 DE/~RE))
    (pad 4 smd rect (at -2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 TXD))
    (pad 5 smd rect (at 2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(P11-Pad3)"))
    (pad 7 smd rect (at 2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(P11-Pad2)"))
    (pad 8 smd rect (at 2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 68.3 73.8)
    (descr "8-Lead Thermally Enhanced Plastic Small Outline (SE) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at 0 -3.5) (layer F.SilkS))
    (fp_text value ADP3624ARDZ (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad10)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad12)"))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R18-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 +12V))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R17-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U5-Pad8)"))
    (pad 9 smd rect (at 0.5875 0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.5875 -0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.5875 0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.5875 -0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_SOIC.3dshapes/SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 67 38)
    (descr "8-Lead Thermally Enhanced Plastic Small Outline (SE) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at 0 -3.5) (layer F.SilkS))
    (fp_text value ADP3624ARDZ (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad13)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad14)"))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R20-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 +12V))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R19-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U6-Pad8)"))
    (pad 9 smd rect (at 0.5875 0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.5875 -0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.5875 0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.5875 -0.5875) (size 1.175 1.175) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_SOIC.3dshapes/SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_SMD:Choke_SMD_3x3mm (layer F.Cu) (tedit 5925C3C9)
    (at 40.9 39.2 180)
    (descr "SMD Power Inductors 3x3mm")
    (tags "SMD inductor")
    (attr smd)
    (fp_text reference L1 (at -3.15 0.5 180) (layer F.SilkS))
    (fp_text value 10uH (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 0.8 2.7) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 0.8 2.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Choke_SMD.3dshapes/Choke_SMD_3x3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text RT (at 67.9 15.1) (layer F.SilkS))
  (gr_text * (at 40.6 21.8) (layer F.SilkS))
  (gr_text * (at 23.75 76) (layer F.SilkS))
  (target plus (at 15 90) (size 5) (width 0.15) (layer Edge.Cuts))
  (gr_text * (at 20.75 37.25) (layer F.SilkS))
  (gr_text + (at 22.75 68) (layer F.SilkS))
  (gr_text * (at 51.56 29.43) (layer F.SilkS))
  (gr_text 1nF (at 41.425 69.3) (layer F.SilkS))
  (gr_text 300R (at 35.5 67.5 90) (layer F.SilkS))
  (gr_text "120k 0805" (at 43.3 74.9) (layer F.SilkS))
  (gr_text 11k (at 42.025 72.975) (layer F.SilkS))
  (gr_text 27uH (at 55.05 71.675) (layer F.SilkS))
  (gr_text * (at 66.025 36.35) (layer F.SilkS))
  (gr_text * (at 67.25 72.275) (layer F.SilkS))
  (gr_text 10uF (at 65.65 66.625) (layer F.SilkS))
  (gr_text 10uF (at 62.1 42.4 90) (layer F.SilkS))
  (gr_text 10uF (at 43.075 48.9) (layer F.SilkS))
  (gr_text 10uH (at 40.95 36.6) (layer F.SilkS))
  (gr_text 0.1uF (at 44.375 33.8) (layer F.SilkS))
  (gr_text 5k1 (at 48.375 28.725 90) (layer F.SilkS))
  (gr_text "18pF\n" (at 48.325 22.4) (layer F.SilkS))
  (gr_text "0.1uF\n" (at 63.6 32.95 90) (layer F.SilkS))
  (gr_text "0.1uF\n" (at 42 30.5) (layer F.SilkS))
  (gr_text 1k (at 44.675 51.075 90) (layer F.SilkS))
  (gr_text "220uF\n" (at 35.75 43.2 90) (layer F.SilkS))
  (gr_text 300R (at 25.94 47.11) (layer F.SilkS))
  (gr_text 5k1 (at 33.3 42.1) (layer F.SilkS))
  (gr_text "50R 0805" (at 32.1 46.77) (layer F.SilkS))
  (gr_text "5k1\n" (at 34.475 49.775) (layer F.SilkS))
  (gr_text "5k1\n" (at 28.95 53.95) (layer F.SilkS))
  (gr_text "1nF\n" (at 28.25 51.6) (layer F.SilkS))
  (gr_text 1nF (at 30.725 59.45) (layer F.SilkS))
  (gr_text 10uF (at 34.5 58.75 90) (layer F.SilkS))
  (gr_text 100uF (at 66.2 59.3) (layer F.SilkS))
  (gr_text "470uF\n" (at 65.9 53.8 90) (layer F.SilkS))
  (gr_text 820uF (at 42.95 83.6) (layer F.SilkS))
  (gr_text 820uF (at 61 83.725) (layer F.SilkS))
  (gr_text 6R (at 71.3 80 90) (layer F.SilkS))
  (gr_text 6R (at 75.3 60.1 90) (layer F.SilkS))
  (gr_text 6R (at 70.5 44.5 90) (layer F.SilkS))
  (gr_text 6R (at 65.85 34.125 90) (layer F.SilkS))
  (gr_text 1k (at 62.9 23.7) (layer F.SilkS))
  (gr_text 18pf (at 61.3 22.55 90) (layer F.SilkS))
  (gr_text 11k (at 51.625 39.8) (layer F.SilkS))
  (gr_text 43k (at 48 39.875) (layer F.SilkS))
  (gr_text PWR (at 36.45 55.25) (layer F.SilkS))
  (gr_text TXD (at 68.2 25.7) (layer F.SilkS))
  (gr_text Ch3 (at 93.7 22.7) (layer F.SilkS))
  (gr_text Ch2 (at 93.9 39.1) (layer F.SilkS))
  (gr_text Ch1 (at 94 59) (layer F.SilkS))
  (gr_text Ch0 (at 93.8 78.2) (layer F.SilkS))
  (gr_text 12 (at 42.3 62.9 90) (layer F.SilkS))
  (gr_text 24 (at 42.3 59.3 90) (layer F.SilkS))
  (gr_text 12/24V (at 20.2 78.4) (layer F.SilkS))
  (gr_text FAN (at 29 69 90) (layer F.SilkS))
  (gr_text "<12V\n" (at 18.4 69.6) (layer F.SilkS))
  (gr_text ADC3 (at 18.6 67.6) (layer F.SilkS))
  (gr_text Thermistor (at 21.5 61.2) (layer F.SilkS))
  (gr_text Photores (at 20.5 54.5) (layer F.SilkS))
  (gr_text IR-OUT+ (at 20.2 45) (layer F.SilkS))
  (gr_text MCU-SERIAL (at 22.45 15.1) (layer F.SilkS))
  (gr_text MCU (at 30.8 19.9) (layer F.SilkS))
  (gr_text DMX (at 35.55 19.85) (layer F.SilkS))
  (gr_text DMX-IN (at 47.9 15.1) (layer F.SilkS))
  (gr_text DMX-OUT (at 58.9 15.1) (layer F.SilkS))
  (gr_line (start 105 90) (end 15 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105 14) (end 105 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 15 14) (end 105 14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 15 90) (end 15 14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 34) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.5 89.5) (xy 33.5 89.5) (xy 33.5 80.25) (xy 37.5 80.25) (xy 37.5 83.25)
        (xy 38.75 84.5) (xy 81.75 84.5) (xy 81.75 80.5) (xy 90.5 80.5) (xy 90.5 76.25)
        (xy 81.75 76.25) (xy 81.75 73.5) (xy 90.5 73.5) (xy 90.5 65.75) (xy 81.75 65.75)
        (xy 81.75 62.75) (xy 90.5 62.75) (xy 90.5 58.5) (xy 81.75 58.5) (xy 81.75 55.75)
        (xy 90.5 55.75) (xy 90.5 48) (xy 81.75 48) (xy 81.75 45.25) (xy 90.5 45.25)
        (xy 90.5 41) (xy 81.75 41) (xy 81.75 38.25) (xy 90.5 38.25) (xy 90.5 31.25)
        (xy 81.75 31.25) (xy 81.75 28.5) (xy 90.5 28.5) (xy 90.5 24.25) (xy 81.75 24.25)
        (xy 81.75 21.5) (xy 90.5 21.5) (xy 90.5 21.25) (xy 95.5 21.25) (xy 95.5 89.5)
      )
    )
  )
  (zone (net 34) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.5 89.5) (xy 33.5 89.5) (xy 33.5 80.25) (xy 37.5 80.25) (xy 37.5 83.25)
        (xy 38.75 84.5) (xy 81.75 84.5) (xy 81.75 80.5) (xy 90.5 80.5) (xy 90.5 76.25)
        (xy 81.75 76.25) (xy 81.75 73.5) (xy 90.5 73.5) (xy 90.5 65.75) (xy 81.75 65.75)
        (xy 81.75 62.75) (xy 90.5 62.75) (xy 90.5 58.5) (xy 81.75 58.5) (xy 81.75 55.75)
        (xy 90.5 55.75) (xy 90.5 48) (xy 81.75 48) (xy 81.75 45.25) (xy 90.5 45.25)
        (xy 90.5 41) (xy 81.75 41) (xy 81.75 38.25) (xy 90.5 38.25) (xy 90.5 31.25)
        (xy 81.75 31.25) (xy 81.75 28.5) (xy 90.5 28.5) (xy 90.5 24.25) (xy 81.75 24.25)
        (xy 81.75 21.5) (xy 90.5 21.5) (xy 90.5 21.25) (xy 95.5 21.25) (xy 95.5 89.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.5 82.75) (xy 39.25 82.75) (xy 39.25 80) (xy 38.25 79) (xy 33 79)
        (xy 32 80) (xy 32 89.5) (xy 27.5 89.5) (xy 27.5 77.5) (xy 27.75 77.25)
        (xy 27.75 72.75) (xy 29.25 72.75) (xy 32.75 69.25) (xy 38.15 69.25) (xy 40.4 67)
        (xy 43 67) (xy 43 56.2) (xy 45.8 56.2) (xy 45.8 45) (xy 62.8 45)
        (xy 62.8 37.6) (xy 69 31.4) (xy 69 24.5) (xy 79.5 24.5) (xy 79.5 82.75)
      )
    )
  )
  (zone (net 13) (net_name "Net-(P13-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79 30.5) (xy 79.75 29.75) (xy 79.75 28.25) (xy 80.25 27.75) (xy 89.5 27.75)
        (xy 89.5 25) (xy 81.25 25) (xy 80.5 24.25) (xy 80.5 21.75) (xy 81.5 20.75)
        (xy 89.5 20.75) (xy 89.5 18) (xy 80.25 18) (xy 76.75 21.5) (xy 76.75 30.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61.8 21.6) (xy 61.8 44.4) (xy 36.8 44.4) (xy 36.8 21.6) (xy 37 21.6)
      )
    )
  )
  (zone (net 14) (net_name "Net-(P14-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.5 34.6) (xy 89.5 37.4) (xy 89.5 37.5) (xy 80.6 37.5) (xy 80.6 41.6)
        (xy 89.5 41.6) (xy 89.5 44.5) (xy 80.7 44.5) (xy 79.1 46.1) (xy 74.9 41.9)
        (xy 77 39.8) (xy 77 34.6) (xy 77.7 34.6)
      )
    )
  )
  (zone (net 8) (net_name "Net-(P8-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.5 55) (xy 80.6 55) (xy 80.6 59.2) (xy 89.5 59.2) (xy 89.5 62)
        (xy 76.6 62) (xy 76.6 52.2) (xy 89.5 52.2) (xy 89.5 55)
      )
    )
  )
  (zone (net 12) (net_name "Net-(P12-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.4 72.7) (xy 80.5 72.7) (xy 80.5 76.8) (xy 89.5 76.8) (xy 89.5 79.7)
        (xy 77.4 79.7) (xy 77.4 69.9) (xy 89.4 69.9) (xy 89.4 72.7)
      )
    )
  )
)
