(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 516)
    (zones 0)
    (modules 41)
    (nets 22)
  )
  (page A4)
  (title_block
    (title "Pulse Extender V1.0")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 157.48 106.68)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 5V)
  (net 2 GND)
  (net 3 RC2)
  (net 4 RC1)
  (net 5 FlashLamp_IN)
  (net 6 Q-Switch_IN)
  (net 7 DISABLE_QS)
  (net 8 Q-Switch_OUT)
  (net 9 DIGITAL_ON_LEVEL)
  (net 10 QS_RC_Charge)
  (net 11 QS_OUT_AMP)
  (net 12 FL_RC_Charge)
  (net 13 "Net-(D1-Pad2)")
  (net 14 "Net-(R8-Pad1)")
  (net 15 "Net-(R10-Pad2)")
  (net 16 "Net-(R11-Pad2)")
  (net 17 "Net-(R12-Pad1)")
  (net 18 "Net-(R13-Pad1)")
  (net 19 "Net-(R17-Pad2)")
  (net 20 "Net-(Q2-Pad2)")
  (net 21 "Net-(R18-Pad2)")
  (net_class Default "Ceci est la Netclass par défaut."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5V)
    (add_net DIGITAL_ON_LEVEL)
    (add_net DISABLE_QS)
    (add_net FL_RC_Charge)
    (add_net FlashLamp_IN)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net Q-Switch_IN)
    (add_net Q-Switch_OUT)
    (add_net QS_OUT_AMP)
    (add_net QS_RC_Charge)
    (add_net RC1)
    (add_net RC2)
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer B.Cu) (tedit 5C13907B)
    (at 86.98 58.93 180)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J2 (at 0 -4) (layer B.SilkS))
    (fp_text value Conn_Coaxial (at 0 -6 180) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 6 Q-Switch_IN))
    (pad 2 thru_hole oval (at 5.08 5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at -5.08 5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer B.Cu) (tedit 5C13907B)
    (at 63.98 58.93 180)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J1 (at 0 -4) (layer B.SilkS))
    (fp_text value Conn_Coaxial (at 0 -6 180) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 FlashLamp_IN))
    (pad 2 thru_hole oval (at 5.08 5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at -5.08 5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer B.Cu) (tedit 5C13907B)
    (at 119.98 58.93 180)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J4 (at 0 -4) (layer B.SilkS))
    (fp_text value Conn_Coaxial (at 0 -6 180) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 8 Q-Switch_OUT))
    (pad 2 thru_hole oval (at 5.08 5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at -5.08 5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3006P_Horizontal (layer B.Cu) (tedit 5A3D4994)
    (at 94.98 86.93 90)
    (descr "Potentiometer, horizontal, Bourns 3006P, https://www.bourns.com/docs/Product-Datasheets/3006.pdf")
    (tags "Potentiometer horizontal Bourns 3006P")
    (fp_text reference RV2 (at -7.235 4.935 270) (layer B.SilkS))
    (fp_text value 50k (at -7.235 -2.395 270) (layer B.Fab))
    (fp_text user %R (at -6.475 1.27 270) (layer B.Fab))
    (pad 3 thru_hole circle (at -12.7 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -7.62 2.54 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(R18-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3006P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3006P_Horizontal (layer B.Cu) (tedit 5A3D4994)
    (at 119.48 86.93 90)
    (descr "Potentiometer, horizontal, Bourns 3006P, https://www.bourns.com/docs/Product-Datasheets/3006.pdf")
    (tags "Potentiometer horizontal Bourns 3006P")
    (fp_text reference RV1 (at -7.235 4.935 270) (layer B.SilkS))
    (fp_text value 50k (at -7.235 -2.395 270) (layer B.Fab))
    (fp_text user %R (at -6.475 1.27 270) (layer B.Fab))
    (pad 3 thru_hole circle (at -12.7 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -7.62 2.54 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(R17-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3006P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:USB_Micro_B_Female_10118192 (layer B.Cu) (tedit 5D27B4C3)
    (at 54.38 77.43 90)
    (descr http://portal.fciconnect.com/Comergent//fci/drawing/10118192.pdf)
    (fp_text reference J5 (at 0 5 -90) (layer B.SilkS))
    (fp_text value 10118192-0001LF (at 0 -4.25 -90) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad SH smd rect (at -3.8 0 90) (size 1.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad SH smd rect (at 3.8 0 90) (size 1.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad SH smd rect (at -1.2 0 90) (size 1.9 1.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad SH smd rect (at 1.2 0 90) (size 1.9 1.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad SH smd rect (at -3.1 2.55 90) (size 2.1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad SH smd rect (at 3.1 2.55 90) (size 2.1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.3 2.675 90) (size 0.4 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 5V))
    (pad 4 smd rect (at 0.65 2.675 90) (size 0.4 1.35) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.3 2.675 90) (size 0.4 1.35) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.65 2.675 90) (size 0.4 1.35) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at 0 2.675 90) (size 0.4 1.35) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (offset (xyz 0 1.22 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:PinHeader_1x2_P2.54mm (layer F.Cu) (tedit 5D27ABEF)
    (at 102.23 53.93)
    (fp_text reference J3 (at 1.37 -2.69) (layer F.SilkS))
    (fp_text value M20-9990246 (at 1.26 2.84) (layer F.Fab))
    (fp_text user %R (at 1.2 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0.02) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 DISABLE_QS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B4B45C9)
    (at 54.48 66.18 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value LED (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 55.48 66.78 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.9 90) (layer F.SilkS))
    (fp_text value 100 (at -0.1 -1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-7343-15_Kemet-W_Pad2.25x2.55mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 64.73 77.43 270)
    (descr "Tantalum Capacitor SMD Kemet-W (7343-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C1 (at 0 -3.1 90) (layer F.SilkS))
    (fp_text value 220u (at 0 3.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -3.2 0 270) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 1 5V))
    (pad 2 smd roundrect (at 3.2 0 270) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-15_Kemet-W.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 110.98 88.93 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 4.7n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 RC1))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 119.98 63.93 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 4.7n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 Q-Switch_OUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 105.48 63.93 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 470p (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 DISABLE_QS))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 105.73 88.93 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 4.7n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 RC2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D27AA37)
    (at 94.73 73.18 90)
    (fp_text reference Q1 (at 0 2.5 90) (layer F.SilkS))
    (fp_text value BC817-40_215 (at 0.025 3.25 90) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 QS_RC_Charge) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 RC1) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 5V) (solder_mask_margin 0.07))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D27AA37)
    (at 121.73 70.68 90)
    (fp_text reference Q2 (at 0.025 2.75 90) (layer F.SilkS))
    (fp_text value BC817-40_215 (at 0.025 3.25 90) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15 90) (layer F.Fab))
    (pad 3 smd rect (at 1.05 0 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 5V) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(Q2-Pad2)") (solder_mask_margin 0.07))
    (pad 1 smd rect (at -1.05 -0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 QS_OUT_AMP) (solder_mask_margin 0.07))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D27AA37)
    (at 94.73 78.93 90)
    (fp_text reference Q3 (at 0.025 -2.5 90) (layer F.SilkS))
    (fp_text value BC817-40_215 (at 0.025 3.25 90) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15 90) (layer F.Fab))
    (pad 3 smd rect (at 1.05 0 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 5V) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 RC2) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -1.05 -0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 FL_RC_Charge) (solder_mask_margin 0.07))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 60.48 63.93 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 5.1k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 5V))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 FlashLamp_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 63.98 63.93 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 FlashLamp_IN))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 90.73 63.93 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 5.1k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 5V))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 Q-Switch_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 86.98 63.93 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 Q-Switch_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 71.98 74.93)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 3.92k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 DIGITAL_ON_LEVEL))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 71.98 79.93 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 1.07k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 DIGITAL_ON_LEVEL))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 83.23 71.18 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 1.75) (layer F.SilkS))
    (fp_text value 200k (at 0 -1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 14 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 110.98 72.18 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 1.75) (layer F.SilkS))
    (fp_text value 200k (at -0.25 -1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 16 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 11 QS_OUT_AMP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 83.23 63.93 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 1.07k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 Q-Switch_IN))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 103.23 75.93)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 1.07k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 RC1))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 16 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 67.48 63.93 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 1.75 90) (layer F.SilkS))
    (fp_text value 1.07k (at 0 3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 FlashLamp_IN))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 17 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 103.23 78.43 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 1.07k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 RC2))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 83.23 82.18)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at 0 1.75) (layer F.SilkS))
    (fp_text value 200k (at 0 3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 17 "Net-(R12-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 FL_RC_Charge))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 110.98 82.18)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 0 1.75) (layer F.SilkS))
    (fp_text value 200k (at 0 3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 "Net-(R13-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 DISABLE_QS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 114.48 88.93 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 1.07k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 19 "Net-(R17-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 RC1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 102.23 88.93 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 1.07k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 RC2))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 21 "Net-(R18-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 90.73 72.93 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 200k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 QS_RC_Charge))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 116.98 70.18 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 200k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 11 QS_OUT_AMP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 123.48 63.93 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 200 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 Q-Switch_OUT))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 101.73 63.93 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R22 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 1.07k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 DISABLE_QS))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 90.73 81.68 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R23 (at 0 1.75 90) (layer F.SilkS))
    (fp_text value 200k (at 0 -1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 FL_RC_Charge))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SSOP-16_Custom (layer F.Cu) (tedit 5D28ED23)
    (at 83.23 77.18)
    (attr smd)
    (fp_text reference U1 (at 0 -3.9003) (layer F.SilkS))
    (fp_text value LT1714CGNTR (at 0 3.81) (layer F.Fab))
    (pad 16 smd rect (at 2.458 -2.2225 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 7 DISABLE_QS) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 1 smd rect (at -2.458 -2.2225 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 9 DIGITAL_ON_LEVEL) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 15 smd rect (at 2.458 -1.5875 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 2 smd rect (at -2.458 -1.5875 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R10-Pad2)") (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 14 smd rect (at 2.458 -0.9525 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R8-Pad1)") (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 3 smd rect (at -2.458 -0.9525 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 13 smd rect (at 2.458 -0.3175 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 10 QS_RC_Charge) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 4 smd rect (at -2.458 -0.3175 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 1 5V) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 12 smd rect (at 2.458 0.3175 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 5 smd rect (at -2.458 0.3175 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 1 5V) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 11 smd rect (at 2.458 0.9525 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 12 FL_RC_Charge) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 6 smd rect (at -2.458 0.9525 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 10 smd rect (at 2.458 1.5875 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 7 smd rect (at -2.458 1.5875 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R12-Pad1)") (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 9 smd rect (at 2.458 2.2225 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 8 smd rect (at -2.458 2.2225 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 9 DIGITAL_ON_LEVEL) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-16_3.9x4.9mm_P0.635mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SSOP-16_Custom (layer F.Cu) (tedit 5D28ED23)
    (at 110.98 77.18)
    (attr smd)
    (fp_text reference U2 (at 0 -3.9003) (layer F.SilkS))
    (fp_text value LT1714CGNTR (at 0 3.81) (layer F.Fab))
    (pad 8 smd rect (at -2.458 2.2225 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 9 DIGITAL_ON_LEVEL) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 9 smd rect (at 2.458 2.2225 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 7 smd rect (at -2.458 1.5875 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R13-Pad1)") (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 10 smd rect (at 2.458 1.5875 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 6 smd rect (at -2.458 0.9525 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 11 smd rect (at 2.458 0.9525 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 7 DISABLE_QS) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 5 smd rect (at -2.458 0.3175 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 1 5V) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 12 smd rect (at 2.458 0.3175 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 4 smd rect (at -2.458 -0.3175 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 1 5V) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 13 smd rect (at 2.458 -0.3175 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 3 smd rect (at -2.458 -0.9525 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 14 smd rect (at 2.458 -0.9525 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 11 QS_OUT_AMP) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 2 smd rect (at -2.458 -1.5875 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R11-Pad2)") (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 15 smd rect (at 2.458 -1.5875 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 1 smd rect (at -2.458 -2.2225 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 9 DIGITAL_ON_LEVEL) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (pad 16 smd rect (at 2.458 -2.2225 270) (size 0.3556 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.01) (solder_paste_margin -0.01))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-16_3.9x4.9mm_P0.635mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 126.73 70.18 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 3 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 Q-Switch_OUT))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 20 "Net-(Q2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Q-Switch Disable\nTest Pins" (at 103.48 58.18) (layer F.SilkS))
  (gr_line (start 51.98 45.43) (end 51.98 105.43) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.98 45.43) (end 51.98 45.43) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.98 105.43) (end 131.98 45.43) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 51.98 105.43) (end 131.98 105.43) (layer Edge.Cuts) (width 0.05))
  (gr_text "Q-Switch\nExtended Pulse\nOUT" (at 119.98 48.93) (layer F.SilkS))
  (gr_text "Q-Switch\nInverted Pulse\nIN" (at 86.98 48.93) (layer F.SilkS))
  (gr_text "Flashlamp\nPulse\nIN" (at 63.98 48.93) (layer F.SilkS))
  (gr_text GND (at 107.48 53.93 90) (layer F.SilkS))
  (gr_text "Q-Switch Extended Width" (at 124.48 93.43 90) (layer F.SilkS))
  (gr_text "Q-Switch Disable Width" (at 99.98 93.43 90) (layer F.SilkS))
  (gr_text "Designed By\nEtienne Santoul\n20190722" (at 72.23 97.93) (layer B.SilkS))
  (gr_text "BU Neurophotonics Center" (at 72.48 99.93) (layer F.SilkS))
  (gr_text "Pulse Extender v2.1" (at 72.23 95.93) (layer F.SilkS))
  (zone (net 1) (net_name 5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 52.98 46.43) (xy 52.98 104.43) (xy 130.98 104.43) (xy 130.98 46.43)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 52.98 46.43) (xy 52.98 104.43) (xy 130.98 104.43) (xy 130.98 46.43)
      )
    )
  )
)
