(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 45)
    (no_connects 0)
    (area 38.049999 39.649999 94.150001 69.750001)
    (thickness 1.6)
    (drawings 38)
    (tracks 214)
    (zones 0)
    (modules 24)
    (nets 15)
  )
  (page A4)
  (title_block
    (title "Raspberry Pi Hat Template")
    (date 2015-12-24)
    (rev 0.1)
    (company OpenFet)
    (comment 1 "Author: Julien")
    (comment 2 "License: CERN OHL V1.2")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.1)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.15)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1)
    (segment_width 0.35)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.26)
    (via_min_drill 0.16)
    (user_via 0.6 0.32)
    (user_via 1.5 0.8)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.69926 1.69926)
    (pad_drill 0.9652)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 211.1 101.7)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(P3-Pad7)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(P3-Pad12)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 +12V)
  (net 8 +5V)
  (net 9 "Net-(D4-Pad2)")
  (net 10 "Net-(P3-Pad13)")
  (net 11 "Net-(P3-Pad15)")
  (net 12 /3V3)
  (net 13 /SDA)
  (net 14 /SCL)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +12V)
    (add_net +5V)
    (add_net /3V3)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(P3-Pad12)")
    (add_net "Net-(P3-Pad13)")
    (add_net "Net-(P3-Pad15)")
    (add_net "Net-(P3-Pad7)")
  )
  (module project_footprints:R-78-E (layer B.Cu) (tedit 5A051E7E)
    (at 83.465 62.965 90)
    (descr "TO-220, Horizontal, RM 2.54mm")
    (tags "TO-220 Horizontal RM 2.54mm")
    (fp_text reference U1 (at -4 5.5 90) (layer B.SilkS) hide)
    (fp_text value R-78-E (at 0 2.54 90) (layer B.SilkS))
    (fp_text user %R (at -4 5.5 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 +12V))
    (pad 2 thru_hole oval (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Horizontal.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Horizontal (layer B.Cu) (tedit 5A052CC8)
    (at 78.385 66.14 180)
    (descr "TO-220, Horizontal, RM 2.54mm")
    (tags "TO-220 Horizontal RM 2.54mm")
    (fp_text reference Q1 (at 1.905 9.525 180) (layer B.SilkS) hide)
    (fp_text value IRLB8271 (at 2.54 5.08 180) (layer B.SilkS))
    (fp_text user %R (at 2.54 20.58 180) (layer B.Fab))
    (pad 0 np_thru_hole oval (at 2.54 16.66 180) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(P3-Pad12)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Horizontal.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Horizontal.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x10 (layer F.Cu) (tedit 5828EB59)
    (at 46.4318 44.4738 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value Raspberry_Pi_+_Conn (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SDA))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 +5V))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SCL))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SCL))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P3-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P3-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P3-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /3V3))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model 3D/pin_socket_2mm_7x2.wrl
      (at (xyz 0.05 -0.3 -0.05))
      (scale (xyz 1.25 1.25 1.25))
      (rotate (xyz 0 180 90))
    )
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5687A909)
    (at 41.6 43.2)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5687A904)
    (at 41.6 66.2)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module myFootPrints:MadeInOregonRev25 (layer F.Cu) (tedit 0)
    (at 86.005 54.71)
    (fp_text reference VAL (at 0 0) (layer F.SilkS) hide)
    (fp_text value MadeInOregonRev25 (at 0 0) (layer F.SilkS) hide)
  )
  (module w_logo:Logo_silk_polarity_center_10x2.8mm (layer B.Cu) (tedit 0)
    (at 54.001 52.297 270)
    (descr "Polarity logo, positive center, 10x2.8mm")
    (fp_text reference G*** (at -1.8 -0.4 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 1.5 -0.4 270) (layer B.SilkS) hide)
  )
  (module myFootPrints:MB225rev (layer F.Cu) (tedit 0)
    (at 45.492 60.679)
    (fp_text reference VAL (at 0 0) (layer F.SilkS) hide)
    (fp_text value MB225rev (at 0 0) (layer F.SilkS) hide)
  )
  (module project_footprints:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer B.Cu) (tedit 592E3582)
    (at 59.97 54.075 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at 1.25 1.86 270) (layer B.SilkS) hide)
    (fp_text value 10uF (at -2.54 0.635 270) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 +12V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D7.5_P5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module project_footprints:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer B.Cu) (tedit 592E357B)
    (at 59.97 61.695 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C2 (at 1.25 2.06 90) (layer B.SilkS) hide)
    (fp_text value 10uF (at -1.27 1.905 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module project_footprints:LED-3MM (layer F.Cu) (tedit 57578FCB)
    (at 59.97 65.505 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at 1.91 3.06 180) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 180) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad2)"))
    (model 3D/led_3mm_yellow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module project_footprints:LED-3MM (layer F.Cu) (tedit 57578FCB)
    (at 52.35 65.505 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at 1.91 3.06 180) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 180) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole rect (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 8 +5V))
    (model 3D/led_3mm_red.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module project_footprints:LED-3MM (layer F.Cu) (tedit 57578FCB)
    (at 68.225 65.505 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.91 3.06 180) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 180) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D3-Pad2)"))
    (model 3D/led_3mm_green.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module project_footprints:Diode_DO-35_SOD27_Horizontal_RM10 (layer B.Cu) (tedit 5A051BCF)
    (at 73.94 44.55)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D4 (at 5.715 0) (layer B.SilkS))
    (fp_text value D (at 4.41452 3.55854) (layer B.Fab) hide)
    (pad 2 thru_hole circle (at 10.16052 0.00254 180) (size 1.69926 1.69926) (drill 0.9652) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(D4-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 0.00254 180) (size 1.69926 1.69926) (drill 0.9652) (layers *.Cu *.Mask B.SilkS)
      (net 7 +12V))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module project_footprints:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer B.Cu) (tedit 5925AAFB)
    (at 86.1 47.7 270)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P4 (at 1.27 1.905 270) (layer B.SilkS))
    (fp_text value CONN_01X02 (at 1.27 -4.50088 270) (layer B.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 7 +12V))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module project_footprints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 53.62 58.52 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at 0 -1.905 180) (layer F.Fab))
    (fp_text value 180 (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 3.175 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(P3-Pad7)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz -0.125 0 0))
      (scale (xyz 0.325 0.325 0.325))
      (rotate (xyz 0 0 0))
    )
  )
  (module project_footprints:Resistor_Horz (layer B.Cu) (tedit 5664956A)
    (at 77.115 42.01)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R2 (at 0 1.905) (layer B.Fab))
    (fp_text value 10K (at 0 0) (layer B.SilkS))
    (pad 1 thru_hole circle (at -3.175 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(P3-Pad12)"))
    (pad 2 thru_hole circle (at 3.175 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz -0.125 0 0))
      (scale (xyz 0.325 0.325 0.325))
      (rotate (xyz 0 0 0))
    )
  )
  (module project_footprints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 53.62 55.345 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R3 (at 0 -1.905 180) (layer F.Fab))
    (fp_text value 330 (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 3.175 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz -0.125 0 0))
      (scale (xyz 0.325 0.325 0.325))
      (rotate (xyz 0 0 0))
    )
  )
  (module project_footprints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 53.62 61.695 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R4 (at 0 -1.905 180) (layer F.Fab))
    (fp_text value 180 (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 thru_hole circle (at 3.175 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(P3-Pad12)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz -0.125 0 0))
      (scale (xyz 0.325 0.325 0.325))
      (rotate (xyz 0 0 0))
    )
  )
  (module project_footprints:SW_PUSH_SMALL (layer F.Cu) (tedit 592B3239)
    (at 54.255 50.265)
    (fp_text reference SW1 (at 0 0) (layer F.SilkS))
    (fp_text value SPST (at 0 2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 3.25 -2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 14 /SCL))
    (pad 2 thru_hole circle (at 3.25 2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.25 -2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 14 /SCL))
    (pad 2 thru_hole circle (at -3.25 2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 1 GND))
    (model ../../../../../../Users/MakersBox/Dropbox/KiCad2015/3D/pcb_push.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module project_footprints:SW_PUSH_SMALL (layer F.Cu) (tedit 592B3239)
    (at 65.685 57.885)
    (fp_text reference SW2 (at 0 0) (layer F.SilkS))
    (fp_text value SPST (at 0 2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 3.25 -2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 11 "Net-(P3-Pad15)"))
    (pad 2 thru_hole circle (at 3.25 2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.25 -2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 11 "Net-(P3-Pad15)"))
    (pad 2 thru_hole circle (at -3.25 2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 1 GND))
    (model ../../../../../../Users/MakersBox/Dropbox/KiCad2015/3D/pcb_push.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module project_footprints:SW_PUSH_SMALL (layer F.Cu) (tedit 592B3239)
    (at 65.685 50.265)
    (fp_text reference SW3 (at 0 0) (layer F.SilkS))
    (fp_text value SPST (at 0 2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 3.25 -2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 10 "Net-(P3-Pad13)"))
    (pad 2 thru_hole circle (at 3.25 2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.25 -2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 10 "Net-(P3-Pad13)"))
    (pad 2 thru_hole circle (at -3.25 2.25) (size 1.8 1.8) (drill 1.0668) (layers *.Cu B.Mask)
      (net 1 GND))
    (model ../../../../../../Users/MakersBox/Dropbox/KiCad2015/3D/pcb_push.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module project_footprints:BARREL_JACK (layer F.Cu) (tedit 5925BBD6)
    (at 42.825 48.995 90)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J1 (at -8.89 3.175 90) (layer F.SilkS) hide)
    (fp_text value BARREL_JACK (at -6.2 -5.5 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 3.75 3.75) (drill 2.75) (layers *.Cu *.Mask)
      (net 7 +12V))
    (pad 2 thru_hole circle (at -6 0 90) (size 3.75 3.75) (drill 2.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3 4.7 90) (size 3.25 3.25) (drill 2.5) (layers *.Cu *.Mask))
    (model 3D/dc_socket.wrl
      (at (xyz -0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5A05204A)
    (at 91.72 56.615)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value I2C (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SDA))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SCL))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "3V3\nGND\nSDA\nSCL" (at 89.815 60.425) (layer F.SilkS))
  (gr_text + (at 65.177 63.6) (layer B.SilkS))
  (gr_text + (at 56.922 63.6) (layer B.SilkS))
  (gr_text + (at 49.302 63.6) (layer B.SilkS))
  (gr_text -12V+ (at 92.736 49.122 90) (layer F.SilkS))
  (gr_text MOSFET (at 66.955 62.33) (layer F.SilkS))
  (gr_text GPIO22 (at 70.765 57.885 90) (layer F.SilkS))
  (gr_text GPIO27 (at 70.765 50.265 90) (layer F.SilkS))
  (gr_line (start 83.1 69.7) (end 91.1 69.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.1 39.7) (end 91.1 39.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79.1 39.7) (end 83.1 39.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79.1 69.7) (end 83.1 69.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text +12V- (at 92.482 49.122 90) (layer B.SilkS))
  (gr_text GPIO18 (at 66.955 68.68) (layer F.SilkS))
  (gr_text www.MakersBox.us (at 57.811 68.172) (layer B.SilkS))
  (gr_text PiFET (at 76.48 62.965) (layer F.SilkS))
  (gr_text PWR (at 51.1 68.7) (layer F.SilkS))
  (gr_line (start 68.1 39.7) (end 79.1 39.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.1 69.7) (end 79.1 69.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "Rev 0.3\nNov 17" (at 88.418 42.899) (layer B.SilkS))
  (gr_line (start 66.1 39.7) (end 68.1 39.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 66.1 69.7) (end 68.1 69.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 41.1 39.7) (end 66.1 39.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 41.1 69.7) (end 66.1 69.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text GPIO4 (at 58.7 68.68) (layer F.SilkS))
  (gr_text GPIO17 (at 59.335 50.265 90) (layer F.SilkS))
  (dimension 30 (width 0.3) (layer Dwgs.User)
    (gr_text "30.000 mm" (at 117.45 54.7 270) (layer Dwgs.User))
    (feature1 (pts (xy 100.1 69.7) (xy 118.8 69.7)))
    (feature2 (pts (xy 100.1 39.7) (xy 118.8 39.7)))
    (crossbar (pts (xy 116.1 39.7) (xy 116.1 69.7)))
    (arrow1a (pts (xy 116.1 69.7) (xy 115.513579 68.573496)))
    (arrow1b (pts (xy 116.1 69.7) (xy 116.686421 68.573496)))
    (arrow2a (pts (xy 116.1 39.7) (xy 115.513579 40.826504)))
    (arrow2b (pts (xy 116.1 39.7) (xy 116.686421 40.826504)))
  )
  (dimension 65 (width 0.3) (layer Dwgs.User)
    (gr_text "65.000 mm" (at 70.6 15.850001) (layer Dwgs.User))
    (feature1 (pts (xy 38.1 42.7) (xy 38.1 14.500001)))
    (feature2 (pts (xy 103.1 42.7) (xy 103.1 14.500001)))
    (crossbar (pts (xy 103.1 17.200001) (xy 38.1 17.200001)))
    (arrow1a (pts (xy 38.1 17.200001) (xy 39.226504 16.61358)))
    (arrow1b (pts (xy 38.1 17.200001) (xy 39.226504 17.786422)))
    (arrow2a (pts (xy 103.1 17.200001) (xy 101.973496 16.61358)))
    (arrow2b (pts (xy 103.1 17.200001) (xy 101.973496 17.786422)))
  )
  (dimension 23 (width 0.3) (layer Dwgs.User)
    (gr_text "23.000 mm" (at 109.45 54.7 270) (layer Dwgs.User))
    (feature1 (pts (xy 99.6 66.2) (xy 110.8 66.2)))
    (feature2 (pts (xy 99.6 43.2) (xy 110.8 43.2)))
    (crossbar (pts (xy 108.1 43.2) (xy 108.1 66.2)))
    (arrow1a (pts (xy 108.1 66.2) (xy 107.513579 65.073496)))
    (arrow1b (pts (xy 108.1 66.2) (xy 108.686421 65.073496)))
    (arrow2a (pts (xy 108.1 43.2) (xy 107.513579 44.326504)))
    (arrow2b (pts (xy 108.1 43.2) (xy 108.686421 44.326504)))
  )
  (gr_line (start 38.1 42.7) (end 38.1 66.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.1 66.7) (end 94.1 42.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 91.1 42.7) (end 91.1 39.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 91.1 66.7) (end 94.1 66.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 41.1 66.7) (end 41.1 69.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 58 (width 0.3) (layer Dwgs.User)
    (gr_text "58.000 mm" (at 70.6 26.35) (layer Dwgs.User))
    (feature1 (pts (xy 99.6 43.2) (xy 99.6 25)))
    (feature2 (pts (xy 41.6 43.2) (xy 41.6 25)))
    (crossbar (pts (xy 41.6 27.7) (xy 99.6 27.7)))
    (arrow1a (pts (xy 99.6 27.7) (xy 98.473496 28.286421)))
    (arrow1b (pts (xy 99.6 27.7) (xy 98.473496 27.113579)))
    (arrow2a (pts (xy 41.6 27.7) (xy 42.726504 28.286421)))
    (arrow2b (pts (xy 41.6 27.7) (xy 42.726504 27.113579)))
  )
  (gr_arc (start 41.1 42.7) (end 38.1 42.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.403 69.569) (xy 65.177 69.696) (xy 65.05 39.343) (xy 95.276 39.216)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.003 39.724) (xy 103.15 39.851) (xy 95.403 70.712) (xy 65.05 71.093) (xy 65.05 40.359)
      )
    )
  )
)
