(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 478)
    (no_connects 0)
    (area 58.218999 48.069499 211.324 150.241001)
    (thickness 1.6002)
    (drawings 42)
    (tracks 3240)
    (zones 0)
    (modules 72)
    (nets 179)
  )
  (page USLetter)
  (title_block
    (date "27 sep 2012")
  )
  (layers
    (0 Front signal)
    (31 Back signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.25146)
    (user_trace_width 1.26746)
    (trace_clearance 0.254)
    (zone_clearance 0.31496)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.1905)
    (edge_width 0.381)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.254)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 4.0005 4.0005)
    (pad_drill 2.29108)
    (pad_to_mask_clearance 0.254)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 /A0)
  (net 2 /A1)
  (net 3 /A10)
  (net 4 /A11)
  (net 5 /A12)
  (net 6 /A13)
  (net 7 /A14)
  (net 8 /A15)
  (net 9 /A16)
  (net 10 /A17)
  (net 11 /A18)
  (net 12 /A19)
  (net 13 /A2)
  (net 14 /A3)
  (net 15 /A4)
  (net 16 /A5)
  (net 17 /A6)
  (net 18 /A7)
  (net 19 /A8)
  (net 20 /A9)
  (net 21 /AA10)
  (net 22 /AA11)
  (net 23 /AA12)
  (net 24 /AA13)
  (net 25 /AA14)
  (net 26 /AA15)
  (net 27 /AA16)
  (net 28 /AA17)
  (net 29 /AA18)
  (net 30 /AA19)
  (net 31 /AA8)
  (net 32 /AA9)
  (net 33 /AD0)
  (net 34 /AD1)
  (net 35 /AD2)
  (net 36 /AD3)
  (net 37 /AD4)
  (net 38 /AD5)
  (net 39 /AD6)
  (net 40 /AD7)
  (net 41 /AEN)
  (net 42 /ALE)
  (net 43 /CLK)
  (net 44 /CLK88)
  (net 45 /D0)
  (net 46 /D1)
  (net 47 /D2)
  (net 48 /D3)
  (net 49 /D4)
  (net 50 /D5)
  (net 51 /D6)
  (net 52 /D7)
  (net 53 /DRQ1)
  (net 54 /DRQ2)
  (net 55 /DRQ3)
  (net 56 /INT)
  (net 57 /IRQ3)
  (net 58 /IRQ4)
  (net 59 /IRQ5)
  (net 60 /IRQ6)
  (net 61 /IRQ7)
  (net 62 /NMI)
  (net 63 /OSC)
  (net 64 /QS0)
  (net 65 /QS1)
  (net 66 /READY)
  (net 67 /RESET)
  (net 68 /TC)
  (net 69 /~DACK0)
  (net 70 /~DACK1)
  (net 71 /~DACK2)
  (net 72 /~DACK3)
  (net 73 /~IOCHK)
  (net 74 /~IOR)
  (net 75 /~IOW)
  (net 76 /~MEMR)
  (net 77 /~MEMW)
  (net 78 /~RQ/GT0)
  (net 79 /~RQ/GT1)
  (net 80 /~S0)
  (net 81 /~S1)
  (net 82 /~S2)
  (net 83 /~TEST)
  (net 84 /~XIOR)
  (net 85 /~XIOW)
  (net 86 /~XMEMR)
  (net 87 /~XMEMW)
  (net 88 GND)
  (net 89 VCC)
  (net 90 /RSTDRV)
  (net 91 /IRQ2)
  (net 92 "Net-(BUS1-Pad5)")
  (net 93 "Net-(BUS1-Pad7)")
  (net 94 "Net-(BUS1-Pad8)")
  (net 95 "Net-(BUS1-Pad9)")
  (net 96 /OSCDRV)
  (net 97 /IORDY)
  (net 98 "Net-(C20-Pad1)")
  (net 99 "Net-(C21-Pad1)")
  (net 100 /AT_KBCLK)
  (net 101 "Net-(D1-Pad1)")
  (net 102 "Net-(D2-Pad2)")
  (net 103 /~VID0)
  (net 104 /~VID1)
  (net 105 /XSEL)
  (net 106 /E0_PASS)
  (net 107 "Net-(P1-Pad2)")
  (net 108 /AT_KBDATA)
  (net 109 "Net-(P1-Pad6)")
  (net 110 "Net-(P2-Pad1)")
  (net 111 "Net-(P2-Pad2)")
  (net 112 /~RESIN)
  (net 113 "Net-(Q1-Pad2)")
  (net 114 "Net-(R2-Pad2)")
  (net 115 "Net-(R3-Pad2)")
  (net 116 /~RQ/GT2)
  (net 117 /KBCLK)
  (net 118 /KBDATA)
  (net 119 "Net-(U1-Pad29)")
  (net 120 "Net-(U1-Pad32)")
  (net 121 "Net-(U1-Pad34)")
  (net 122 /APNMI)
  (net 123 "Net-(U3-Pad3)")
  (net 124 "Net-(U3-Pad4)")
  (net 125 /~RAMCS)
  (net 126 /~ROMCS)
  (net 127 "Net-(U3-Pad7)")
  (net 128 "Net-(U3-Pad8)")
  (net 129 "Net-(U3-Pad9)")
  (net 130 /SPKR)
  (net 131 /XAEN)
  (net 132 "Net-(U3-Pad33)")
  (net 133 /EOP)
  (net 134 /~XDACK3)
  (net 135 /~XDACK2)
  (net 136 /~XDACK1)
  (net 137 /~XDACK0)
  (net 138 /XALE)
  (net 139 /LE)
  (net 140 /~DEN)
  (net 141 /DTR)
  (net 142 "Net-(U3-Pad82)")
  (net 143 "Net-(U3-Pad83)")
  (net 144 "Net-(U3-Pad84)")
  (net 145 /MD0)
  (net 146 /MD1)
  (net 147 /MD2)
  (net 148 /MD3)
  (net 149 /MD4)
  (net 150 /MD5)
  (net 151 /MD6)
  (net 152 /MD7)
  (net 153 "Net-(C22-Pad1)")
  (net 154 /~RAMCS2)
  (net 155 "Net-(U9-Pad16)")
  (net 156 "Net-(U9-Pad17)")
  (net 157 "Net-(U9-Pad18)")
  (net 158 "Net-(U9-Pad19)")
  (net 159 "Net-(U14-Pad3)")
  (net 160 "Net-(U14-Pad8)")
  (net 161 "Net-(RR5-Pad2)")
  (net 162 "Net-(RR5-Pad3)")
  (net 163 "Net-(RR5-Pad4)")
  (net 164 "Net-(RR5-Pad5)")
  (net 165 "Net-(RR5-Pad6)")
  (net 166 /~SPKR)
  (net 167 /~RAMENA)
  (net 168 "Net-(C21-Pad2)")
  (net 169 "Net-(C23-Pad1)")
  (net 170 "Net-(U12-Pad7)")
  (net 171 "Net-(U12-Pad9)")
  (net 172 "Net-(P2-Pad3)")
  (net 173 /KBD_VCC)
  (net 174 "Net-(U16-Pad19)")
  (net 175 "Net-(U16-Pad11)")
  (net 176 "Net-(U16-Pad1)")
  (net 177 /ROM_A16)
  (net 178 /~EPSL)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.25146)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AA10)
    (add_net /AA11)
    (add_net /AA12)
    (add_net /AA13)
    (add_net /AA14)
    (add_net /AA15)
    (add_net /AA16)
    (add_net /AA17)
    (add_net /AA18)
    (add_net /AA19)
    (add_net /AA8)
    (add_net /AA9)
    (add_net /AD0)
    (add_net /AD1)
    (add_net /AD2)
    (add_net /AD3)
    (add_net /AD4)
    (add_net /AD5)
    (add_net /AD6)
    (add_net /AD7)
    (add_net /AEN)
    (add_net /ALE)
    (add_net /APNMI)
    (add_net /AT_KBCLK)
    (add_net /AT_KBDATA)
    (add_net /CLK)
    (add_net /CLK88)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /DRQ1)
    (add_net /DRQ2)
    (add_net /DRQ3)
    (add_net /DTR)
    (add_net /E0_PASS)
    (add_net /EOP)
    (add_net /INT)
    (add_net /IORDY)
    (add_net /IRQ2)
    (add_net /IRQ3)
    (add_net /IRQ4)
    (add_net /IRQ5)
    (add_net /IRQ6)
    (add_net /IRQ7)
    (add_net /KBCLK)
    (add_net /KBDATA)
    (add_net /LE)
    (add_net /MD0)
    (add_net /MD1)
    (add_net /MD2)
    (add_net /MD3)
    (add_net /MD4)
    (add_net /MD5)
    (add_net /MD6)
    (add_net /MD7)
    (add_net /NMI)
    (add_net /OSC)
    (add_net /OSCDRV)
    (add_net /QS0)
    (add_net /QS1)
    (add_net /READY)
    (add_net /RESET)
    (add_net /ROM_A16)
    (add_net /RSTDRV)
    (add_net /SPKR)
    (add_net /TC)
    (add_net /XAEN)
    (add_net /XALE)
    (add_net /XSEL)
    (add_net /~DACK0)
    (add_net /~DACK1)
    (add_net /~DACK2)
    (add_net /~DACK3)
    (add_net /~DEN)
    (add_net /~EPSL)
    (add_net /~IOCHK)
    (add_net /~IOR)
    (add_net /~IOW)
    (add_net /~MEMR)
    (add_net /~MEMW)
    (add_net /~RAMCS)
    (add_net /~RAMCS2)
    (add_net /~RAMENA)
    (add_net /~RESIN)
    (add_net /~ROMCS)
    (add_net /~RQ/GT0)
    (add_net /~RQ/GT1)
    (add_net /~RQ/GT2)
    (add_net /~S0)
    (add_net /~S1)
    (add_net /~S2)
    (add_net /~SPKR)
    (add_net /~TEST)
    (add_net /~VID0)
    (add_net /~VID1)
    (add_net /~XDACK0)
    (add_net /~XDACK1)
    (add_net /~XDACK2)
    (add_net /~XDACK3)
    (add_net /~XIOR)
    (add_net /~XIOW)
    (add_net /~XMEMR)
    (add_net /~XMEMW)
    (add_net "Net-(BUS1-Pad5)")
    (add_net "Net-(BUS1-Pad7)")
    (add_net "Net-(BUS1-Pad8)")
    (add_net "Net-(BUS1-Pad9)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(RR5-Pad2)")
    (add_net "Net-(RR5-Pad3)")
    (add_net "Net-(RR5-Pad4)")
    (add_net "Net-(RR5-Pad5)")
    (add_net "Net-(RR5-Pad6)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U12-Pad7)")
    (add_net "Net-(U12-Pad9)")
    (add_net "Net-(U14-Pad3)")
    (add_net "Net-(U14-Pad8)")
    (add_net "Net-(U16-Pad1)")
    (add_net "Net-(U16-Pad11)")
    (add_net "Net-(U16-Pad19)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad33)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U3-Pad82)")
    (add_net "Net-(U3-Pad83)")
    (add_net "Net-(U3-Pad84)")
    (add_net "Net-(U3-Pad9)")
    (add_net "Net-(U9-Pad16)")
    (add_net "Net-(U9-Pad17)")
    (add_net "Net-(U9-Pad18)")
    (add_net "Net-(U9-Pad19)")
  )
  (net_class GND ""
    (clearance 0.254)
    (trace_width 0.50546)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
  )
  (net_class KBD_VCC ""
    (clearance 0.254)
    (trace_width 0.50546)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /KBD_VCC)
  )
  (net_class VCC ""
    (clearance 0.254)
    (trace_width 0.63246)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net VCC)
  )
  (module my_components:IC_DIP32_600 (layer Front) (tedit 59EFBB18)
    (at 85.09 83.82)
    (descr "32 pins DIL package, round pads")
    (tags "DIP DIL DIP32 DIL32")
    (fp_text reference U4 (at -18.7325 9.525) (layer F.SilkS))
    (fp_text value SST39SF010A (at 14.2875 9.525) (layer F.SilkS))
    (pad 1 thru_hole rect (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 177 /ROM_A16))
    (pad 3 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A15))
    (pad 4 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A12))
    (pad 5 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A7))
    (pad 6 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A6))
    (pad 7 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A5))
    (pad 8 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A4))
    (pad 9 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A3))
    (pad 10 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A2))
    (pad 11 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /A1))
    (pad 12 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /A0))
    (pad 13 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /AD0))
    (pad 14 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /AD1))
    (pad 15 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /AD2))
    (pad 16 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 17 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /AD3))
    (pad 18 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /AD4))
    (pad 19 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /AD5))
    (pad 20 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /AD6))
    (pad 21 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /AD7))
    (pad 22 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 126 /~ROMCS))
    (pad 23 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /A10))
    (pad 24 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 /~MEMR))
    (pad 25 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /A11))
    (pad 26 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A9))
    (pad 27 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A8))
    (pad 28 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A13))
    (pad 29 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A14))
    (pad 30 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 31 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 /~MEMW))
    (pad 32 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_32-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Speaker_12mm (layer Front) (tedit 59E15036)
    (at 68.58 68.58)
    (descr "Speaker 12mm")
    (tags "SPEAKER 12MM")
    (fp_text reference SP1 (at 4.7625 5.715) (layer F.SilkS))
    (fp_text value SPEAKER (at 9.8425 5.715) (layer F.SilkS))
    (fp_text user + (at -5.08 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at -3.2512 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 1 thru_hole circle (at 3.2512 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(P2-Pad2)"))
  )
  (module my_components:IC_PLCC84_TH (layer Front) (tedit 59E1608C)
    (at 162.56 109.22 180)
    (descr "PLCC84 Socket, Through Hole")
    (tags "PLCC PLCC84")
    (fp_text reference U3 (at 14.2875 -19.3675 180) (layer F.SilkS))
    (fp_text value FE2010A (at 8.89 -19.3675 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 -15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 0 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 3 thru_hole circle (at -2.54 -15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 123 "Net-(U3-Pad3)"))
    (pad 4 thru_hole circle (at -2.54 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(U3-Pad4)"))
    (pad 5 thru_hole circle (at -5.08 -15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 125 /~RAMCS))
    (pad 6 thru_hole circle (at -5.08 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 178 /~EPSL))
    (pad 7 thru_hole circle (at -7.62 -15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 127 "Net-(U3-Pad7)"))
    (pad 8 thru_hole circle (at -7.62 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 128 "Net-(U3-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 -15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 129 "Net-(U3-Pad9)"))
    (pad 10 thru_hole circle (at -10.16 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 /INT))
    (pad 11 thru_hole circle (at -12.7 -15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 12 thru_hole circle (at -15.24 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 /~VID0))
    (pad 13 thru_hole circle (at -12.7 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 /~VID1))
    (pad 14 thru_hole circle (at -15.24 -10.16 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 130 /SPKR))
    (pad 15 thru_hole circle (at -12.7 -10.16 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(C20-Pad1)"))
    (pad 16 thru_hole circle (at -15.24 -7.62 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 /XSEL))
    (pad 17 thru_hole circle (at -12.7 -7.62 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 /READY))
    (pad 18 thru_hole circle (at -15.24 -5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /RESET))
    (pad 19 thru_hole circle (at -12.7 -5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /CLK88))
    (pad 20 thru_hole circle (at -15.24 -2.54 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 /OSC))
    (pad 21 thru_hole circle (at -12.7 -2.54 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 168 "Net-(C21-Pad2)"))
    (pad 22 thru_hole circle (at -15.24 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 23 thru_hole circle (at -12.7 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(C22-Pad1)"))
    (pad 24 thru_hole circle (at -15.24 2.54 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 /~RQ/GT0))
    (pad 25 thru_hole circle (at -12.7 2.54 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 117 /KBCLK))
    (pad 26 thru_hole circle (at -15.24 5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 118 /KBDATA))
    (pad 27 thru_hole circle (at -12.7 5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 73 /~IOCHK))
    (pad 28 thru_hole circle (at -15.24 7.62 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 97 /IORDY))
    (pad 29 thru_hole circle (at -12.7 7.62 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 122 /APNMI))
    (pad 30 thru_hole circle (at -15.24 10.16 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 131 /XAEN))
    (pad 31 thru_hole circle (at -12.7 10.16 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 62 /NMI))
    (pad 32 thru_hole circle (at -15.24 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 33 thru_hole circle (at -12.7 15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 132 "Net-(U3-Pad33)"))
    (pad 34 thru_hole circle (at -12.7 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /AD0))
    (pad 35 thru_hole circle (at -10.16 15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /AD1))
    (pad 36 thru_hole circle (at -10.16 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /AD2))
    (pad 37 thru_hole circle (at -7.62 15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /AD3))
    (pad 38 thru_hole circle (at -7.62 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /AD4))
    (pad 39 thru_hole circle (at -5.08 15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /AD5))
    (pad 40 thru_hole circle (at -5.08 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /AD6))
    (pad 41 thru_hole circle (at -2.54 15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /AD7))
    (pad 42 thru_hole circle (at -2.54 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 43 thru_hole circle (at 0 15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 44 thru_hole circle (at 0 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /AA8))
    (pad 45 thru_hole circle (at 2.54 15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /AA9))
    (pad 46 thru_hole circle (at 2.54 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /AA10))
    (pad 47 thru_hole circle (at 5.08 15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /AA11))
    (pad 48 thru_hole circle (at 5.08 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /AA12))
    (pad 49 thru_hole circle (at 7.62 15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /AA13))
    (pad 50 thru_hole circle (at 7.62 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AA14))
    (pad 51 thru_hole circle (at 10.16 15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /AA15))
    (pad 52 thru_hole circle (at 10.16 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /AA16))
    (pad 53 thru_hole circle (at 12.7 15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /AA17))
    (pad 54 thru_hole circle (at 15.24 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /AA18))
    (pad 55 thru_hole circle (at 12.7 12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /AA19))
    (pad 56 thru_hole circle (at 15.24 10.16 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 /DRQ3))
    (pad 57 thru_hole circle (at 12.7 10.16 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 /DRQ2))
    (pad 58 thru_hole circle (at 15.24 7.62 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 /DRQ1))
    (pad 59 thru_hole circle (at 12.7 7.62 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 133 /EOP))
    (pad 60 thru_hole circle (at 15.24 5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 134 /~XDACK3))
    (pad 61 thru_hole circle (at 12.7 5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 135 /~XDACK2))
    (pad 62 thru_hole circle (at 15.24 2.54 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 136 /~XDACK1))
    (pad 63 thru_hole circle (at 12.7 2.54 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 137 /~XDACK0))
    (pad 64 thru_hole circle (at 15.24 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 65 thru_hole circle (at 12.7 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 /~XIOR))
    (pad 66 thru_hole circle (at 15.24 -2.54 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 85 /~XIOW))
    (pad 67 thru_hole circle (at 12.7 -2.54 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 /~XMEMR))
    (pad 68 thru_hole circle (at 15.24 -5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 /~XMEMW))
    (pad 69 thru_hole circle (at 12.7 -5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 138 /XALE))
    (pad 70 thru_hole circle (at 15.24 -7.62 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 139 /LE))
    (pad 71 thru_hole circle (at 12.7 -7.62 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 140 /~DEN))
    (pad 72 thru_hole circle (at 15.24 -10.16 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 141 /DTR))
    (pad 73 thru_hole circle (at 12.7 -10.16 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 /~S2))
    (pad 74 thru_hole circle (at 15.24 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 /~S1))
    (pad 75 thru_hole circle (at 12.7 -15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 /~S0))
    (pad 76 thru_hole circle (at 12.7 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 91 /IRQ2))
    (pad 77 thru_hole circle (at 10.16 -15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 /IRQ3))
    (pad 78 thru_hole circle (at 10.16 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 /IRQ4))
    (pad 79 thru_hole circle (at 7.62 -15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 /IRQ5))
    (pad 80 thru_hole circle (at 7.62 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /IRQ6))
    (pad 81 thru_hole circle (at 5.08 -15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 61 /IRQ7))
    (pad 82 thru_hole circle (at 5.08 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 142 "Net-(U3-Pad82)"))
    (pad 83 thru_hole circle (at 2.54 -15.24 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 143 "Net-(U3-Pad83)"))
    (pad 84 thru_hole circle (at 2.54 -12.7 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 144 "Net-(U3-Pad84)"))
    (model Sockets.3dshapes/PLCC84.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP32_600 (layer Front) (tedit 59926921)
    (at 85.09 104.14)
    (descr "32 pins DIL package, round pads")
    (tags "DIP DIL DIP32 DIL32")
    (fp_text reference U6 (at -17.78 9.525) (layer F.SilkS))
    (fp_text value AS6C4008 (at 15.5575 9.525) (layer F.SilkS))
    (pad 1 thru_hole rect (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A18))
    (pad 2 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A16))
    (pad 3 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A14))
    (pad 4 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A12))
    (pad 5 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A7))
    (pad 6 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A6))
    (pad 7 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A5))
    (pad 8 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A4))
    (pad 9 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A3))
    (pad 10 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A2))
    (pad 11 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /A1))
    (pad 12 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /A0))
    (pad 13 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 145 /MD0))
    (pad 14 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 146 /MD1))
    (pad 15 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 147 /MD2))
    (pad 16 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 17 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 148 /MD3))
    (pad 18 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 149 /MD4))
    (pad 19 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 150 /MD5))
    (pad 20 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 151 /MD6))
    (pad 21 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 152 /MD7))
    (pad 22 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 154 /~RAMCS2))
    (pad 23 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /A10))
    (pad 24 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 /~MEMR))
    (pad 25 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /A11))
    (pad 26 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A9))
    (pad 27 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A8))
    (pad 28 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A13))
    (pad 29 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 /~MEMW))
    (pad 30 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A17))
    (pad 31 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A15))
    (pad 32 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_32-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP14_300 (layer Front) (tedit 59E16058)
    (at 96.52 67.31)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U14 (at -6.0325 5.715) (layer F.SilkS))
    (fp_text value 74F00 (at 5.3975 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 167 /~RAMENA))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 167 /~RAMENA))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 159 "Net-(U14-Pad3)"))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 159 "Net-(U14-Pad3)"))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A19))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 154 /~RAMCS2))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 160 "Net-(U14-Pad8)"))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 166 /~SPKR))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 130 /SPKR))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 130 /SPKR))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 59E55BAA)
    (at 92.71 60.96)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R6 (at 6.35 -0.3175) (layer F.SilkS))
    (fp_text value 1k (at 8.5725 -0.3175) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 166 /~SPKR))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP40_600 (layer Front) (tedit 59E1883C)
    (at 171.45 58.42)
    (descr "40 pins DIL package, round pads")
    (tags "DIP DIL DIP28 DIL28")
    (fp_text reference U2 (at -23.1775 9.525) (layer F.SilkS))
    (fp_text value 8087 (at 22.5425 9.525) (layer F.SilkS))
    (pad 1 thru_hole rect (at -24.13 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at -21.59 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AA14))
    (pad 3 thru_hole circle (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /AA13))
    (pad 4 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /AA12))
    (pad 5 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /AA11))
    (pad 6 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /AA10))
    (pad 7 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /AA9))
    (pad 8 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /AA8))
    (pad 9 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /AD7))
    (pad 10 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /AD6))
    (pad 11 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /AD5))
    (pad 12 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /AD4))
    (pad 13 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /AD3))
    (pad 14 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /AD2))
    (pad 15 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /AD1))
    (pad 16 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /AD0))
    (pad 17 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole circle (at 21.59 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /CLK88))
    (pad 20 thru_hole circle (at 24.13 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 21 thru_hole circle (at 24.13 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /RESET))
    (pad 22 thru_hole circle (at 21.59 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 /READY))
    (pad 23 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 /~TEST))
    (pad 24 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 /QS1))
    (pad 25 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 /QS0))
    (pad 26 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 /~S0))
    (pad 27 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 /~S1))
    (pad 28 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 /~S2))
    (pad 29 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 30 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 31 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 /~RQ/GT1))
    (pad 32 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 122 /APNMI))
    (pad 33 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 116 /~RQ/GT2))
    (pad 34 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 35 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /AA19))
    (pad 36 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /AA18))
    (pad 37 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /AA17))
    (pad 38 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /AA16))
    (pad 39 thru_hole circle (at -21.59 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /AA15))
    (pad 40 thru_hole circle (at -24.13 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_40-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Transistor_TO92_EBC_254 (layer Front) (tedit 59E1881B)
    (at 78.74 63.5)
    (descr "Transistor, TO92, 2.54mm lead spacing")
    (tags TO92)
    (fp_text reference Q1 (at -2.54 -3.175) (layer F.SilkS))
    (fp_text value PN2222A (at 2.2225 -3.175 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 169 "Net-(C23-Pad1)"))
    (model discret/to98.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Edge_PCB_ISA8 (layer Front) (tedit 5298E0D8)
    (at 147.32 146.05)
    (descr "Connector, PCB Edge, ISA8")
    (tags "CONN BUS ISA")
    (fp_text reference BUS1 (at -36.83 -6.35) (layer F.SilkS) hide)
    (fp_text value BUSPC_HOST (at -29.21 -6.35) (layer F.SilkS) hide)
    (pad 1 connect rect (at 38.1 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 88 GND))
    (pad 2 connect rect (at 35.56 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 90 /RSTDRV))
    (pad 3 connect rect (at 33.02 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 89 VCC))
    (pad 4 connect rect (at 30.48 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 91 /IRQ2))
    (pad 5 connect rect (at 27.94 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 92 "Net-(BUS1-Pad5)"))
    (pad 6 connect rect (at 25.4 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 54 /DRQ2))
    (pad 7 connect rect (at 22.86 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 93 "Net-(BUS1-Pad7)"))
    (pad 8 connect rect (at 20.32 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 94 "Net-(BUS1-Pad8)"))
    (pad 9 connect rect (at 17.78 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 95 "Net-(BUS1-Pad9)"))
    (pad 10 connect rect (at 15.24 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 88 GND))
    (pad 11 connect rect (at 12.7 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 77 /~MEMW))
    (pad 12 connect rect (at 10.16 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 76 /~MEMR))
    (pad 13 connect rect (at 7.62 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 75 /~IOW))
    (pad 14 connect rect (at 5.08 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 74 /~IOR))
    (pad 15 connect rect (at 2.54 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 72 /~DACK3))
    (pad 16 connect rect (at 0 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 55 /DRQ3))
    (pad 17 connect rect (at -2.54 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 70 /~DACK1))
    (pad 18 connect rect (at -5.08 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 53 /DRQ1))
    (pad 19 connect rect (at -7.62 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 69 /~DACK0))
    (pad 20 connect rect (at -10.16 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 43 /CLK))
    (pad 21 connect rect (at -12.7 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 61 /IRQ7))
    (pad 22 connect rect (at -15.24 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 60 /IRQ6))
    (pad 23 connect rect (at -17.78 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 59 /IRQ5))
    (pad 24 connect rect (at -20.32 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 58 /IRQ4))
    (pad 25 connect rect (at -22.86 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 57 /IRQ3))
    (pad 26 connect rect (at -25.4 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 71 /~DACK2))
    (pad 27 connect rect (at -27.94 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 68 /TC))
    (pad 28 connect rect (at -30.48 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 42 /ALE))
    (pad 29 connect rect (at -33.02 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 89 VCC))
    (pad 30 connect rect (at -35.56 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 96 /OSCDRV))
    (pad 31 connect rect (at -38.1 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 88 GND))
    (pad 32 connect rect (at 38.1 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 73 /~IOCHK))
    (pad 33 connect rect (at 35.56 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 52 /D7))
    (pad 34 connect rect (at 33.02 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 51 /D6))
    (pad 35 connect rect (at 30.48 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 50 /D5))
    (pad 36 connect rect (at 27.94 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 49 /D4))
    (pad 37 connect rect (at 25.4 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 48 /D3))
    (pad 38 connect rect (at 22.86 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 47 /D2))
    (pad 39 connect rect (at 20.32 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 46 /D1))
    (pad 40 connect rect (at 17.78 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 45 /D0))
    (pad 41 connect rect (at 15.24 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 97 /IORDY))
    (pad 42 connect rect (at 12.7 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 41 /AEN))
    (pad 43 connect rect (at 10.16 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 12 /A19))
    (pad 44 connect rect (at 7.62 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 11 /A18))
    (pad 45 connect rect (at 5.08 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 10 /A17))
    (pad 46 connect rect (at 2.54 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 9 /A16))
    (pad 47 connect rect (at 0 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 8 /A15))
    (pad 48 connect rect (at -2.54 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 7 /A14))
    (pad 49 connect rect (at -5.08 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 6 /A13))
    (pad 50 connect rect (at -7.62 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 5 /A12))
    (pad 51 connect rect (at -10.16 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 4 /A11))
    (pad 52 connect rect (at -12.7 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 3 /A10))
    (pad 53 connect rect (at -15.24 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 20 /A9))
    (pad 54 connect rect (at -17.78 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 19 /A8))
    (pad 55 connect rect (at -20.32 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 18 /A7))
    (pad 56 connect rect (at -22.86 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 17 /A6))
    (pad 57 connect rect (at -25.4 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 16 /A5))
    (pad 58 connect rect (at -27.94 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 15 /A4))
    (pad 59 connect rect (at -30.48 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 14 /A3))
    (pad 60 connect rect (at -33.02 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 13 /A2))
    (pad 61 connect rect (at -35.56 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 2 /A1))
    (pad 62 connect rect (at -38.1 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 1 /A0))
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E15580)
    (at 142.24 73.66 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C1 (at 2.54 1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.5875 1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59926C3A)
    (at 142.24 53.34 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C2 (at 2.54 1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.5875 1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E16181)
    (at 165.1 88.9)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C3 (at -9.525 0) (layer F.SilkS))
    (fp_text value 0.1uF (at -5.715 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59EFBD11)
    (at 61.595 78.74 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C4 (at 2.54 1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.5875 1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E155D1)
    (at 61.595 119.38 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C5 (at 2.54 1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.5875 1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59926C22)
    (at 61.595 99.06 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C6 (at 2.54 1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.5875 1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E15615)
    (at 109.22 78.74 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C7 (at 2.54 -1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.5875 -1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E15624)
    (at 109.22 66.04 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C8 (at 2.54 -1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.5875 -1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E15642)
    (at 109.22 91.44 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C10 (at 2.2225 -1.905 450) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.905 -1.905 450) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E15650)
    (at 109.22 104.14 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C11 (at 2.2225 -1.905 450) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.905 -1.905 450) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E15658)
    (at 109.22 129.54 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C12 (at 2.2225 -1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.905 -1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E15661)
    (at 109.22 116.84 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C13 (at 2.2225 -1.905 450) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.905 -1.905 450) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E1569C)
    (at 83.82 66.04 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C14 (at 2.2225 -1.8415 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.905 -1.8415 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59926AF6)
    (at 185.42 99.06 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C15 (at -2.2225 -1.905 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.905 -1.905 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 59E158BF)
    (at 61.595 134.9375 270)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C18 (at -5.3975 0.9525 270) (layer F.SilkS))
    (fp_text value 10uF (at -5.3975 -0.635 270) (layer F.SilkS))
    (fp_text user + (at -2.8575 -2.2225 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 59E15707)
    (at 142.24 66.04 270)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C19 (at -5.3975 0.635 270) (layer F.SilkS))
    (fp_text value 10uF (at -5.3975 -0.9525 270) (layer F.SilkS))
    (fp_text user + (at -2.54 2.54 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 59E15715)
    (at 205.74 53.6575 270)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C20 (at 1.905 3.81 270) (layer F.SilkS))
    (fp_text value 10uF (at -2.2225 3.81 270) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:C_Trim_Murata (layer Front) (tedit 59E1576C)
    (at 186.69 121.92 180)
    (descr "Trimmer Capacitor Murata")
    (tags "Trimmer Capacitor Murata")
    (fp_text reference C21 (at 4.7625 -4.7625 270) (layer F.SilkS))
    (fp_text value 5-30pF (at 3.175 -4.445 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(C21-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.99898 1.99898) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 168 "Net-(C21-Pad2)"))
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E52FB8)
    (at 193.04 111.76 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C22 (at 2.54 -1.905 270) (layer F.SilkS))
    (fp_text value 47pF (at -1.27 -1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(C22-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E15790)
    (at 78.74 68.58 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C23 (at 2.8575 1.778 180) (layer F.SilkS))
    (fp_text value 0.01uF (at -1.5875 1.778 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 169 "Net-(C23-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Diode_762 (layer Front) (tedit 59926A50)
    (at 194.31 93.98 180)
    (descr "Diode, 7.62mm lead spacing")
    (tags "DIODE 7.62mm")
    (fp_text reference D1 (at 3.4925 1.905 180) (layer F.SilkS))
    (fp_text value 1N4148 (at -1.27 1.905 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 /AT_KBCLK))
    (pad 1 thru_hole rect (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(D1-Pad1)"))
    (model discret/diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:LED_3mm (layer Front) (tedit 59E17371)
    (at 204.47 88.9 90)
    (descr "LED 3mm, 100mil (2.54mm) lead spacing")
    (tags "LED 3mm T1")
    (fp_text reference D2 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value POWER_LED (at -3.175 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Hole_3mm (layer Front) (tedit 52CC20B5)
    (at 206.121 81.28)
    (descr "Mounting Hole, 3mm")
    (tags "HOLE 3MM")
    (fp_text reference HOLE1 (at 0 -3.175) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.175) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
  )
  (module my_components:Hole_3mm (layer Front) (tedit 52CC20B5)
    (at 206.121 137.795)
    (descr "Mounting Hole, 3mm")
    (tags "HOLE 3MM")
    (fp_text reference HOLE2 (at 0 -3.175) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.175) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
  )
  (module my_components:Conn_Mini_DIN_6pin (layer Front) (tedit 59F9507A)
    (at 210.82 116.84 270)
    (descr "Connector, Mini-DIN, 6 pin")
    (tags "MINI DIN CONN 6PIN")
    (fp_text reference P1 (at 5.3975 13.97 270) (layer F.SilkS))
    (fp_text value KEYBOARD (at -2.8575 13.97 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 1.30048 8.509 90) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(P1-Pad2)"))
    (pad 1 thru_hole circle (at -1.30048 8.509 90) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 108 /AT_KBDATA))
    (pad 5 thru_hole circle (at -3.35026 11.00074 90) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 100 /AT_KBCLK))
    (pad 6 thru_hole circle (at 3.35026 11.00074 90) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(P1-Pad6)"))
    (pad 4 thru_hole circle (at 3.35026 8.509 90) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 173 /KBD_VCC))
    (pad 3 thru_hole circle (at -3.35026 8.509 90) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad ~ thru_hole circle (at 0 4.699 90) (size 4.0005 4.0005) (drill 2.29108) (layers *.Cu *.SilkS *.Mask)
      (net 88 GND))
    (pad ~ thru_hole circle (at -6.75894 5.50926 90) (size 4.0005 4.0005) (drill 2.29108) (layers *.Cu *.SilkS *.Mask)
      (net 88 GND))
    (pad ~ thru_hole circle (at 6.75894 5.50926 90) (size 4.0005 4.0005) (drill 2.29108) (layers *.Cu *.SilkS *.Mask)
      (net 88 GND))
    (model r_mini_dins/minidin_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Pin_Header_4x1_2.54mm (layer Front) (tedit 59F01F80)
    (at 60.96 68.58 90)
    (descr "Pin Header, 4x1, 2.54mm pitch")
    (tags "CONN 4x1")
    (fp_text reference P2 (at -4.572 2.286 180) (layer F.SilkS))
    (fp_text value SPEAKER (at -5.9055 0.9525 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(P2-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(P2-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 172 "Net-(P2-Pad3)"))
    (pad 4 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Pin_Header_2x1_2.54mm (layer Front) (tedit 59E17390)
    (at 204.47 71.4375)
    (descr "Pin Header, 2x1, 2.54mm pitch")
    (tags "CONN 2x1")
    (fp_text reference P3 (at -2.8575 -2.2225) (layer F.SilkS))
    (fp_text value RESET (at 1.27 -2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 112 /~RESIN))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 59D2956D)
    (at 78.74 71.12)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R1 (at -1.5875 1.905) (layer F.SilkS))
    (fp_text value 33 (at 1.905 1.905) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(P2-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 169 "Net-(C23-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 59E1588D)
    (at 125.73 124.46)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 5.715 0) (layer F.SilkS))
    (fp_text value 47 (at 8.128 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /CLK))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(R2-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 59E13FC1)
    (at 115.57 124.46)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R3 (at -7.3025 -1.27) (layer F.SilkS))
    (fp_text value 47 (at -4.7625 -1.27) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 /OSCDRV))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(R3-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 59E13FE9)
    (at 203.2 62.23 270)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R4 (at 1.905 1.905 270) (layer F.SilkS))
    (fp_text value 470 (at -1.5875 1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(D2-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 59E13FE1)
    (at 205.74 62.23 270)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R5 (at 1.905 -1.905 270) (layer F.SilkS))
    (fp_text value 470 (at -1.5875 -1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 /~RESIN))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 59EFBC39)
    (at 72.39 93.98 180)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R7 (at -6.0325 0 180) (layer F.SilkS))
    (fp_text value 10k (at -8.89 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 177 /ROM_A16))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_SIL10 (layer Front) (tedit 59E1615A)
    (at 179.07 68.58)
    (descr "Footprint, SIL-10")
    (tags "CONN SIL-10")
    (fp_text reference RR1 (at -18.0975 0) (layer F.SilkS))
    (fp_text value 4.7k (at -14.605 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at -8.89 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 /~RQ/GT0))
    (pad 3 thru_hole circle (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 116 /~RQ/GT2))
    (pad 4 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 /~RQ/GT1))
    (pad 5 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 /~S2))
    (pad 6 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 /~S1))
    (pad 7 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 /~S0))
    (pad 8 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 117 /KBCLK))
    (pad 9 thru_hole circle (at 8.89 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 118 /KBDATA))
    (pad 10 thru_hole circle (at 11.43 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 /~TEST))
  )
  (module my_components:Conn_SIL10 (layer Front) (tedit 59E140CC)
    (at 173.99 134.62)
    (descr "Footprint, SIL-10")
    (tags "CONN SIL-10")
    (fp_text reference RR2 (at -10.795 2.2225) (layer F.SilkS))
    (fp_text value 10k (at 11.43 2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at -8.89 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D0))
    (pad 3 thru_hole circle (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /D1))
    (pad 4 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /D2))
    (pad 5 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /D3))
    (pad 6 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /D4))
    (pad 7 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /D5))
    (pad 8 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 /D6))
    (pad 9 thru_hole circle (at 8.89 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /D7))
    (pad 10 thru_hole circle (at 11.43 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 /~RESIN))
  )
  (module my_components:Switch_Tactile_6mm_Right (layer Front) (tedit 59E17367)
    (at 210.82 99.06 270)
    (descr "Switch, Tactile, 6mm, Right Angle")
    (tags "SWITCH TACTILE 6MM RIGHT")
    (autoplace_cost180 10)
    (fp_text reference SW1 (at -5.08 2.8575 360) (layer F.SilkS))
    (fp_text value RESET (at 5.08 2.8575 360) (layer F.SilkS))
    (pad GND thru_hole circle (at 3.50266 6.35 90) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.SilkS *.Mask)
      (net 88 GND))
    (pad GND thru_hole circle (at -3.49758 6.35 90) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.SilkS *.Mask)
      (net 88 GND))
    (pad 1 thru_hole circle (at 2.25298 3.85064 90) (size 1.80086 1.80086) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at -2.2479 3.85064 90) (size 1.80086 1.80086) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 112 /~RESIN))
    (model tactile_switches/bot_tact_cv1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.2 1.2 1.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP40_600 (layer Front) (tedit 59E160AE)
    (at 171.45 78.74)
    (descr "40 pins DIL package, round pads")
    (tags "DIP DIL DIP28 DIL28")
    (fp_text reference U1 (at -23.1775 9.525) (layer F.SilkS))
    (fp_text value 8088 (at 22.225 9.525) (layer F.SilkS))
    (pad 1 thru_hole rect (at -24.13 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at -21.59 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AA14))
    (pad 3 thru_hole circle (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /AA13))
    (pad 4 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /AA12))
    (pad 5 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /AA11))
    (pad 6 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /AA10))
    (pad 7 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /AA9))
    (pad 8 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /AA8))
    (pad 9 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /AD7))
    (pad 10 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /AD6))
    (pad 11 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /AD5))
    (pad 12 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /AD4))
    (pad 13 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /AD3))
    (pad 14 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /AD2))
    (pad 15 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /AD1))
    (pad 16 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /AD0))
    (pad 17 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 62 /NMI))
    (pad 18 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 /INT))
    (pad 19 thru_hole circle (at 21.59 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /CLK88))
    (pad 20 thru_hole circle (at 24.13 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 21 thru_hole circle (at 24.13 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /RESET))
    (pad 22 thru_hole circle (at 21.59 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 /READY))
    (pad 23 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 /~TEST))
    (pad 24 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 /QS1))
    (pad 25 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 /QS0))
    (pad 26 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 /~S0))
    (pad 27 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 /~S1))
    (pad 28 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 /~S2))
    (pad 29 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(U1-Pad29)"))
    (pad 30 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 /~RQ/GT1))
    (pad 31 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 /~RQ/GT0))
    (pad 32 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(U1-Pad32)"))
    (pad 33 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 34 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(U1-Pad34)"))
    (pad 35 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /AA19))
    (pad 36 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /AA18))
    (pad 37 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /AA17))
    (pad 38 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /AA16))
    (pad 39 thru_hole circle (at -21.59 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /AA15))
    (pad 40 thru_hole circle (at -24.13 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_40-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP32_600 (layer Front) (tedit 59E1607D)
    (at 85.09 124.46)
    (descr "32 pins DIL package, round pads")
    (tags "DIP DIL DIP32 DIL32")
    (fp_text reference U5 (at -18.0975 9.525) (layer F.SilkS))
    (fp_text value AS6C4008 (at 15.5575 9.525) (layer F.SilkS))
    (pad 1 thru_hole rect (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A18))
    (pad 2 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A16))
    (pad 3 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A14))
    (pad 4 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A12))
    (pad 5 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A7))
    (pad 6 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A6))
    (pad 7 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A5))
    (pad 8 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A4))
    (pad 9 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A3))
    (pad 10 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A2))
    (pad 11 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /A1))
    (pad 12 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /A0))
    (pad 13 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 145 /MD0))
    (pad 14 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 146 /MD1))
    (pad 15 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 147 /MD2))
    (pad 16 thru_hole circle (at 19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 17 thru_hole circle (at 19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 148 /MD3))
    (pad 18 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 149 /MD4))
    (pad 19 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 150 /MD5))
    (pad 20 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 151 /MD6))
    (pad 21 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 152 /MD7))
    (pad 22 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A19))
    (pad 23 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /A10))
    (pad 24 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 /~MEMR))
    (pad 25 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /A11))
    (pad 26 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A9))
    (pad 27 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A8))
    (pad 28 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A13))
    (pad 29 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 /~MEMW))
    (pad 30 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A17))
    (pad 31 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A15))
    (pad 32 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_32-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP20_300 (layer Front) (tedit 59E16037)
    (at 125.73 80.01)
    (descr "20 pins DIL package, round pads")
    (tags "DIP DIL DIP20 DIL20")
    (fp_text reference U7 (at -10.16 5.715) (layer F.SilkS))
    (fp_text value 74F573 (at 8.89 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /AD0))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /AD1))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /AD2))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /AD3))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /AD4))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /AD5))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /AD6))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /AD7))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 139 /LE))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A7))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A6))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A5))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A4))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A3))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A2))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /A1))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /A0))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP20_300 (layer Front) (tedit 59E16034)
    (at 125.73 67.31)
    (descr "20 pins DIL package, round pads")
    (tags "DIP DIL DIP20 DIL20")
    (fp_text reference U8 (at -10.16 5.715) (layer F.SilkS))
    (fp_text value 74F573 (at 8.89 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /AA8))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /AA9))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /AA10))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /AA11))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /AA12))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /AA13))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AA14))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /AA15))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 139 /LE))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A15))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A14))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A13))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A12))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /A11))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /A10))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A9))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A8))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP20_300 (layer Front) (tedit 59E16063)
    (at 125.73 92.71)
    (descr "20 pins DIL package, round pads")
    (tags "DIP DIL DIP20 DIL20")
    (fp_text reference U10 (at -9.8425 5.715) (layer F.SilkS))
    (fp_text value 74F245 (at 8.89 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 141 /DTR))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /AD0))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /AD1))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /AD2))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /AD3))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /AD4))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /AD5))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /AD6))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /AD7))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /D7))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 /D6))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /D5))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /D4))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /D3))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /D2))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /D1))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D0))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 140 /~DEN))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP20_300 (layer Front) (tedit 59E16040)
    (at 125.73 105.41)
    (descr "20 pins DIL package, round pads")
    (tags "DIP DIL DIP20 DIL20")
    (fp_text reference U11 (at -9.8425 5.715) (layer F.SilkS))
    (fp_text value 74F245 (at 8.89 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 /~MEMR))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D0))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /D1))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /D2))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /D3))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /D4))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /D5))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 /D6))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /D7))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 152 /MD7))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 151 /MD6))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 150 /MD5))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 149 /MD4))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 148 /MD3))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 147 /MD2))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 146 /MD1))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 145 /MD0))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 167 /~RAMENA))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP20_300 (layer Front) (tedit 59E1606C)
    (at 125.73 130.81)
    (descr "20 pins DIL package, round pads")
    (tags "DIP DIL DIP20 DIL20")
    (fp_text reference U12 (at -9.8425 5.715) (layer F.SilkS))
    (fp_text value 74F244 (at 8.89 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 /OSC))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /ALE))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 133 /EOP))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 /~DACK2))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 137 /~XDACK0))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 170 "Net-(U12-Pad7)"))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /CLK88))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 171 "Net-(U12-Pad9)"))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(R2-Pad2)"))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 /~DACK0))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 135 /~XDACK2))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 /TC))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 138 /XALE))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(R3-Pad2)"))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP20_300 (layer Front) (tedit 59E16042)
    (at 125.73 118.11)
    (descr "20 pins DIL package, round pads")
    (tags "DIP DIL DIP20 DIL20")
    (fp_text reference U13 (at -9.8425 -5.3975) (layer F.SilkS))
    (fp_text value 74F244 (at 8.89 -5.3975) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 /~XIOR))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 /~DACK1))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 85 /~XIOW))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 /~DACK3))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 /~XMEMR))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /AEN))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 /~XMEMW))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 90 /RSTDRV))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /RESET))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 /~MEMW))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 131 /XAEN))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 /~MEMR))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 134 /~XDACK3))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 /~IOW))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 136 /~XDACK1))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 /~IOR))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP8_300 (layer Front) (tedit 59E18873)
    (at 194.31 100.33)
    (descr "8 pins DIL package, round pads")
    (tags "DIP DIL DIP8 DIL8")
    (fp_text reference U15 (at -6.6675 3.81) (layer F.SilkS))
    (fp_text value PIC12F629 (at 6.096 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 117 /KBCLK))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 118 /KBDATA))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 /E0_PASS))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 /AT_KBCLK))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 108 /AT_KBDATA))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(D1-Pad1)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Crystal_HC-49U_Vert (layer Front) (tedit 59E15747)
    (at 185.42 111.76 90)
    (descr "Quartz Crystal, HC-49U, Vertical")
    (tags "QUARTZ CRYSTAL HC49U VERT")
    (autoplace_cost180 10)
    (fp_text reference X1 (at -6.6675 -1.905 90) (layer F.SilkS))
    (fp_text value 28.63636MHz (at -2.8575 -3.4925 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.44094 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(C21-Pad1)"))
    (pad 2 thru_hole circle (at 2.44094 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(C22-Pad1)"))
    (model discret/crystal_hc18u_vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 599268F4)
    (at 165.1 129.54)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C16 (at -2.2225 1.905) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.905 1.905) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_SIL6 (layer Front) (tedit 59E16909)
    (at 153.67 134.62)
    (descr "Footprint, SIL-6")
    (tags "CONN SIL-6")
    (fp_text reference RR3 (at -4.1275 2.2225) (layer F.SilkS))
    (fp_text value 4.7k (at 5.715 2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 /~IOR))
    (pad 3 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 /~IOW))
    (pad 4 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 /~MEMR))
    (pad 5 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 /~MEMW))
    (pad 6 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 /XSEL))
  )
  (module my_components:Conn_SIL6 (layer Front) (tedit 59E14046)
    (at 196.85 106.68)
    (descr "Footprint, SIL-6")
    (tags "CONN SIL-6")
    (fp_text reference RR4 (at 0.9525 2.2225) (layer F.SilkS))
    (fp_text value 4.7k (at 4.7625 2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 /~VID0))
    (pad 3 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 /~VID1))
    (pad 4 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 /E0_PASS))
    (pad 5 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 108 /AT_KBDATA))
    (pad 6 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 /AT_KBCLK))
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E17326)
    (at 109.22 53.34 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C9 (at 2.54 -1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.5875 -1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP20_300 (layer Front) (tedit 59E1602C)
    (at 125.73 54.61)
    (descr "20 pins DIL package, round pads")
    (tags "DIP DIL DIP20 DIL20")
    (fp_text reference U9 (at -10.16 5.715) (layer F.SilkS))
    (fp_text value 74F573 (at 8.89 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /AA16))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /AA17))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /AA18))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /AA19))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 139 /LE))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A19))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A18))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A17))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A16))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 155 "Net-(U9-Pad16)"))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 156 "Net-(U9-Pad17)"))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 157 "Net-(U9-Pad18)"))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 158 "Net-(U9-Pad19)"))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_DIP20_300 (layer Front) (tedit 59E1886F)
    (at 92.71 54.61)
    (descr "20 pins DIL package, round pads")
    (tags "DIP DIL DIP20 DIL20")
    (fp_text reference U16 (at -14.2875 3.81) (layer F.SilkS))
    (fp_text value ATF16V8B (at 14.4145 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 176 "Net-(U16-Pad1)"))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 165 "Net-(RR5-Pad6)"))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 164 "Net-(RR5-Pad5)"))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 163 "Net-(RR5-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A16))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A17))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A18))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A19))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A15))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 175 "Net-(U16-Pad11)"))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 126 /~ROMCS))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 154 /~RAMCS2))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 130 /SPKR))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 166 /~SPKR))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 167 /~RAMENA))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 162 "Net-(RR5-Pad3)"))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 161 "Net-(RR5-Pad2)"))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 174 "Net-(U16-Pad19)"))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_SIL6 (layer Front) (tedit 59EF9C60)
    (at 67.31 60.96)
    (descr "Footprint, SIL-6")
    (tags "CONN SIL-6")
    (fp_text reference RR5 (at -3.81 2.2225) (layer F.SilkS))
    (fp_text value 10k (at 6.35 2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 161 "Net-(RR5-Pad2)"))
    (pad 3 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 162 "Net-(RR5-Pad3)"))
    (pad 4 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 163 "Net-(RR5-Pad4)"))
    (pad 5 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 164 "Net-(RR5-Pad5)"))
    (pad 6 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 165 "Net-(RR5-Pad6)"))
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E174AA)
    (at 76.2 53.34 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C17 (at 2.2225 -1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.905 -1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 59E4F3E7)
    (at 202.565 129.54 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference F1 (at 2.54 -1.905 180) (layer F.SilkS))
    (fp_text value 1.1A (at -1.905 -1.905 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 173 /KBD_VCC))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Switch_DIP_3_Positions (layer Front) (tedit 59E52FDB)
    (at 193.04 130.81)
    (descr "DIP Switch, 3 Positions")
    (tags "SWITCH DIP 3POS")
    (fp_text reference SW2 (at -3.175 6.35) (layer F.SilkS))
    (fp_text value CONFIG (at 2.2225 6.35) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 3 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 4 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 /E0_PASS))
    (pad 5 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 /~VID1))
    (pad 6 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 /~VID0))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Switch_DIP_5_Positions (layer Front) (tedit 59E55D4B)
    (at 66.04 54.61)
    (descr "DIP Switch, 5 Positions")
    (tags "SWITCH DIP 5POS")
    (fp_text reference SW3 (at 8.3185 2.2225 90) (layer F.SilkS))
    (fp_text value UMB (at 8.3185 -2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 161 "Net-(RR5-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 162 "Net-(RR5-Pad3)"))
    (pad 3 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 163 "Net-(RR5-Pad4)"))
    (pad 4 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 164 "Net-(RR5-Pad5)"))
    (pad 5 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 165 "Net-(RR5-Pad6)"))
    (pad 6 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 7 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 8 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 9 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 10 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Pin_Header_2x1_2.54mm_NoKey (layer Front) (tedit 59F95240)
    (at 141.9225 97.79 90)
    (descr "Pin Header, 2x1, 2.54mm pitch, no key")
    (tags "CONN 2x1 NOKEY")
    (fp_text reference JP3 (at -5.08 -0.9525 90) (layer F.SilkS))
    (fp_text value RAMCS (at -5.08 0.635 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 125 /~RAMCS))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 167 /~RAMENA))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Pin_Header_2x1_2.54mm_NoKey (layer Front) (tedit 59EFA7AE)
    (at 193.04 121.92 270)
    (descr "Pin Header, 2x1, 2.54mm pitch, no key")
    (tags "CONN 2x1 NOKEY")
    (fp_text reference JP2 (at 2.2225 -2.2225 270) (layer F.SilkS))
    (fp_text value XSEL (at -1.5875 -2.2225 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 88 GND))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 /XSEL))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 59EFBA62)
    (at 190.5 113.03 270)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R8 (at 1.905 1.778 270) (layer F.SilkS))
    (fp_text value 1M (at -1.905 1.778 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(C22-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 168 "Net-(C21-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Pin_Header_2x1_2.54mm_NoKey (layer Front) (tedit 59F01FA8)
    (at 61.595 91.44 90)
    (descr "Pin Header, 2x1, 2.54mm pitch, no key")
    (tags "CONN 2x1 NOKEY")
    (fp_text reference JP1 (at 5.715 -0.9525 90) (layer F.SilkS))
    (fp_text value ROM_A16 (at 5.715 0.635 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 177 /ROM_A16))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 89 VCC))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer Front) (tedit 59F95DD8)
    (at 142.5575 133.6675)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference GPLv3 (at 0 5.715) (layer F.SilkS))
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082) (layer F.Fab))
  )
  (module my_components:Conn_Pin_Header_2x1_2.54mm_NoKey (layer Front) (tedit 59F95276)
    (at 141.9225 92.71 90)
    (descr "Pin Header, 2x1, 2.54mm pitch, no key")
    (tags "CONN 2x1 NOKEY")
    (fp_text reference JP4 (at 4.445 -0.9525 90) (layer F.SilkS))
    (fp_text value ROMCS (at 9.2075 -0.9525 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 178 /~EPSL))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 126 /~ROMCS))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "JP3, JP4 - RAM and ROM Chip Select Generation:\n  Open:  Use SPLD (U16)\n  Closed: Use FE2010 (U3)" (at 102.87 136.525) (layer B.SilkS))
  (gr_text "JP1 - Flash ROM Mapping to 0xF0000-0xFFFFF:\n  Open:  Map lower 64 KiB of Flash ROM (default)\n  Closed: Map upper 64 KiB of Flash ROM\nJP2 - Crystal (X1) Frequency Select:\n  Open:  14.31818 MHz (default)\n  Closed: 28.63636 MHz" (at 102.87 124.1425) (layer B.SilkS))
  (gr_text "SW3 - UMB Configuration:\n  SW3.1 = ON: Enable 0xC0000-0xC7FFF\n  SW3.2 = ON: Enable 0xC8000-0xCFFFF\n  SW3.3 = ON: Enable 0xD0000-0xD7FFF\n  SW3.4 = ON: Enable 0xD8000-0xDFFFF\n  SW3.5 = ON: Enable 0xE0000-0xEFFFF\n" (at 102.87 103.8225) (layer B.SilkS))
  (gr_text "Copyright (C) 2017 Sergey Kiselev" (at 168.91 139.065) (layer F.SilkS))
  (gr_text "SW2.3 - Keyboard 0xE0 scan code pass through:\n  SW2.3 = OFF: Disable; SW1.3 = ON: Enable" (at 190.5 76.2) (layer B.SilkS))
  (gr_text "Micro 8088 - Version 1.1" (at 85.09 136.144) (layer F.SilkS))
  (gr_text "SW2.1, SW2.2 - Video mode select:\n  SW2.1 = OFF, SW2.2 = OFF: MDA or Hercules\n  SW2.1 = ON,  SW2.2 = OFF: 80x25 CGA\n  SW2.1 = OFF, SW2.2 = ON:  40x25 CGA\n  SW2.1 = ON,  SW2.2 = ON:  None, EGA or VGA" (at 191.135 58.42) (layer B.SilkS))
  (gr_line (start 187.96 142.24) (end 187.96 149.225) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 107.315 149.86) (end 187.325 149.86) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 106.68 142.24) (end 106.68 149.225) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 187.325 149.225) (end 187.96 149.225) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 107.315 149.225) (end 107.315 149.86) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60.96 48.26) (end 208.28 48.26) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 58.42 139.7) (end 58.42 50.8) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60.96 142.24) (end 106.68 142.24) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 187.96 142.24) (end 208.28 142.24) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 210.82 50.8) (end 210.82 139.7) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 208.28 50.8) (end 208.28 48.26) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 208.28 139.7) (end 210.82 139.7) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 60.96 139.7) (end 60.96 142.24) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 60.96 50.8) (end 58.42 50.8) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_text www.malinov.com (at 88.265 140.081) (layer F.SilkS))
  (zone (net 88) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.31496))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 210.82 142.24) (xy 210.82 48.26) (xy 58.42 48.26) (xy 58.42 142.24) (xy 106.68 142.24)
        (xy 106.68 140.97) (xy 187.96 140.97) (xy 187.96 142.24)
      )
    )
  )
  (zone (net 88) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.31496))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 210.82 142.24) (xy 210.82 48.26) (xy 58.42 48.26) (xy 58.42 142.24) (xy 106.68 142.24)
        (xy 106.68 140.97) (xy 187.96 140.97) (xy 187.96 142.24)
      )
    )
  )
)
