(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 24)
    (zones 0)
    (modules 32)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (user_trace_width 1.016)
    (user_trace_width 1.524)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.7366 0.381)
    (user_via 0.8636 0.50038)
    (user_via 0.8636 0.508)
    (uvia_size 0.8)
    (uvia_drill 0.4)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.8)
    (uvia_drill 0.4)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (net_class 43V ""
    (clearance 0.1524)
    (trace_width 2.54)
    (via_dia 0.70104)
    (via_drill 0.59944)
    (uvia_dia 0.70104)
    (uvia_drill 0.59944)
    (diff_pair_width 1.016)
    (diff_pair_gap 0.8636)
  )
  (net_class Spindle ""
    (clearance 0.6858)
    (trace_width 1.016)
    (via_dia 0.70104)
    (via_drill 0.59944)
    (uvia_dia 0.70104)
    (uvia_drill 0.59944)
    (diff_pair_width 1.016)
    (diff_pair_gap 0.8636)
  )
  (net_class Stepper ""
    (clearance 0.2286)
    (trace_width 0.6096)
    (via_dia 0.7366)
    (via_drill 0.381)
    (uvia_dia 0.7366)
    (uvia_drill 0.381)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 60.198 26.67)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -7.874 0.034) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 62.738 26.67)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -11.176 1.27) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 60.198 24.13)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -7.874 0.034) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 62.738 24.13)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -11.176 1.27) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 65.278 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 57.658 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 65.278 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 60.198 21.59)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -7.874 0.034) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 57.658 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 65.278 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 65.278 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 62.738 29.21)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -11.176 1.27) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 60.198 29.21)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -7.874 0.034) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 62.738 21.59)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -11.176 1.27) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 57.658 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 57.658 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 60.198 21.59)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -7.874 -0.034) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 62.738 21.59)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -11.176 -1.27) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 65.278 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 65.278 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 57.658 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 57.658 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 65.278 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 57.658 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 57.658 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 65.278 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 60.198 29.21)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -7.874 -0.034) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 62.738 29.21)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -11.176 -1.27) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 62.738 26.67)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -11.176 -1.27) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 60.198 26.67)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -7.874 -0.034) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 62.738 24.13)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -11.176 -1.27) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 60.198 24.13)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -7.874 -0.034) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Billy Bogardus" (at 61.468 30.734 180) (layer B.SilkS))
  (gr_text 9/25/2019 (at 61.468 30.734) (layer F.SilkS))
  (gr_text "0201 Practice" (at 61.468 20.066) (layer F.SilkS))
  (gr_line (start 55.118 31.75) (end 67.818 31.75) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 55.118 19.05) (end 67.818 19.05) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 67.818 19.05) (end 67.818 31.75) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 55.118 19.05) (end 55.118 31.75) (layer Edge.Cuts) (width 0.12))
)
